libao documentation | libao version 1.2.0 - 20130122

# libao Drivers

Libao supports both live output drivers and file output drivers. Live output drivers send audio data to sound cards and sound daemons. File output drivers write audio to disk using a particular file format (such as WAV, AU, etc.). You must invoke the ao_open_????() function that corresponds to the type of driver you are using, but otherwise live and file drivers are treated identically in libao.

Driver options may be passed to the drivers via the `*options` argument to ao_open_live() and ao_open_file(), or they may be set in the configuration file as `name=value` pairs.

## Options Understood by All Drivers

- "debug" - (value not required) Requests driver print detailed debugging information.
- "matrix" - Set an output channel mapping similar to the use of the matrix field in ao_sample_format. The specified matrix overrides the backend's native channel ordering/numbering. The channel numbering used by the driver does not necessarily reflect the physical ordering; for example, the fourth PulseAudio channel is always 'Center' by default whether the channel physically exists or not.
- "quiet" - (value not required) Requests the driver print no output whatsoever, even in the event of error.
- "verbose" - (value not required) Requests that the driver print more detailed information concerning normal operation.

## Standard Driver Options

These are options that have the same use in each driver, but may not be supported by all drivers (due to the option being meaningless or unimplemented for a given audio backend).

- "id" - Request a specific playback device/sink/output by number. In most audio backends, this will correspond to a specific output device, but for all devices, this means 'give me the Nth output'.
- "dev" - Request a specific playback device/sink/output by name. This name will be in a format determined by the specific driver backend (eg, the first hardware device in ALSA format would be 'hw:0', and for OSS it would be '/dev/dsp').
- "server" - Daemon-based sound subsystems often support connecting to non-default local or remote servers. The "server" option allows specifying the connection for a given driver in a format specific to that system.
- "client_name" - specify a descriptive name for the application; this is often used by sound backends to display status information about which applications are currently making use of playback.

## Live Output Drivers

### aixs

IBM AIX sound driver. According to the author, "tested on AIX 5.1 with the Crystal chipsets only (found as internal audio in the 7043-140 and on the MCA adapter DFE5 (7-6)), but it should work with other AIX releases and the ACPA also."

Option keys:

- "dev" - (see 'Standard Driver Options' above). By default, the driver tries "/dev/baud0/1" (device for MCA machines with the Crystal chipset). Other possible devices are "/dev/paud0/1" for PCI machines with the Crystal chipset, and "/dev/acpa0/1" for MCA machines with the ACPA.
- "id" - (see 'Standard Driver Options' above).

### alsa

Advanced Linux Sound Architecture (API versions 0.9.x/1.x.x; earlier API versions are now deprecated).

Option keys:

- "buffer_time" - Override the default hardware buffer size (in milliseconds).
- "dev" - (see 'Standard Driver Options' above). ALSA device label to use. Examples include "hw:0" for the first soundcard and "hw:1" for the second. The alsa driver normally chooses one of "surround71", "surround51", "surround40", "front", or "default" automatically depending on number of output channels.
- "id" - (see 'Standard Driver Options' above).
- "period_time" - Override the default hardware period size (in microseconds).
- "use_mmap" - set to "yes" or "no" to override the compiled-in default to use or not use mmap device access. In the past, some buggy alsa drivers have behaved better when not using mmap access at the penalty of slightly higher CPU usage.

### arts

aRts Sound Daemon live output driver.

Option keys:

- "multi" - set to "yes" to allow opening the aRts playback device for multiply concurrent playback. Although the driver works properly in multi mode, it is known to occasionally crash the aRts server itself. Default behavior is "no".

### esd

ESounD audio driver. Although declining in poularity, this sound daemon is still used on some Linux systems. It permits multiple programs to play sound simultaneously and sound to be sent to networked computers.

Option keys:

- "host" - Deprecated synonym for 'server' below.
- "server" - (see 'Standard Driver Options' above). The hostname where esd is running. By default sound is played on the local host. A port number can be specified after a colon, as in "whizbang.com:555".
- "client_name" - descriptive name for this client (eg, the application name).

### irix

IRIX audio driver. This was inherited from the original libao, but has not been tested. Use at your own risk. (Better yet, fix it! I don't have access to an IRIX system.)

### macosx

MacOS X AUHAL live output driver. This driver supports MacOS X 10.5 and later (10.4 and earlier uses an earlier, incompatable interface).

Option keys:

- "buffer_time" - Set the hardware buffer size to the equivalent of value in milliseconds.
- "dev" - specify the audio device to use by name (eg, 'speaker', 'headphones', 'hdmi' or 'iMic'), or by audio device UID (eg 'AppleHDAEngineOutputDP:8,5,1,0:0:{2D4C-05ED-00000000}'). Partial matches are allowed, matching is case insensivtive.

### nas

Network Audio System live output driver.

Option keys:

- "buf_size" - Set size of audio buffer on server in bytes.
- "host" - Deprecated synonym for 'server' below.
- "server" - (see 'Standard Driver Options' above). Set location of NAS server; See nas(1) for format.

### null

Null driver. This is just a test device which does not write the audio data anywhere.

### oss

Open Sound System driver. This is the audio system for older Linux and FreeBSD as well as some other UNIX-like systems.

Option keys:

- "buffer_time" - Override the default hardware buffer size (in milliseconds).
- "dev" - (see 'Standard Driver Options' above). By default, the driver tries "/dev/sound/dsp", followed by "/dev/dsp".
- "dsp" - Deprecated synonym for "dev".
- "id" - (see 'Standard Driver Options' above).

### pulse

PulseAudio live audio sound driver. Pulse is a sound server daemon used by the modern Gnome desktop on UNIX-like systems.

Option keys:

- "buffer_time" - Override the default hardware buffer size (in milliseconds).
- "dev" - (see 'Standard Driver Options' above). This maps to a specific Pulse sink; it may be specified by Pulse sink name, or by number.
- "id" - (see 'Standard Driver Options' above). Maps to a specific pulse sink number.
- "server" - Specifies Pulseaudio server to use.
- "sink" - Deprecated synonym for "dev".

### roar

RoarAudio live audio sound driver.

Option keys:

- "server" - Specifies Roar server to use.
- "host" - Specifies Roar server to use (legacy synonym for 'server').
- "id" - Selects audio device to use for playback by number. For a roar server, this is mapped to a given output mixer.
- "dev" - Selects audio device to use for playback by name. For a roar server, this is a number and thus synonymous with 'id' above.
- "client_name" - descriptive name for this client (eg, the application name).
- "role" - stream type as enumerated by Roar; see RoarAudio documentation.

### sndio

SNDIO is the modern audio interface used by OpenBSD.

Option keys:

- "dev" - (see 'Standard Driver Options' above).
- "id" - (see 'Standard Driver Options' above).

### sun

Sun audio driver. This is the audio system for NetBSD, OpenBSD, and Solaris.

Option keys:

- "dev" - (see 'Standard Driver Options' above). By default, the driver tries "/dev/sound/0"
- "id" - (see 'Standard Driver Options' above).

### wmm

Windows MMSound output driver for Win98 and later.

Option keys:

- "dev" - (see 'Standard Driver Options' above).
- "id" - (see 'Standard Driver Options' above).

## File Output Drivers

### au

Sun audio file driver. Writes a .au file from audio output. This driver can write usable data to unseekable files (like standard out), which the wav driver cannot do.

### raw

Raw sample driver. Writes the sound to disk in uncompressed, headerless form using the byte order specified.

Option keys:

- "byteorder" - Byte order used in the output. Use "native" for native machine byte order, "big" for big-endian order, and "little" for little-endian order. By default this is "native".

### wav

Windows 'WAV' sound file output. Because of the way WAV files are structured, this driver cannot correct files unless the target file is seekable. Writing WAVs to stdout will result in broken files. Use either the raw or the au driver instead.

## Default Driver Detection

In the absence of configuration files to explicit identify a default driver, the library will try to detect a suitable default driver. It does this by testing every available live output driver (using ao_plugin_test()) and finding the driver with the highest priority (see the ao_info struct) that works. Drivers with priority 0, such as the null and file output drivers, are never selected as the default.

The ranking system currently used is:

Priority | Drivers
--- | ---
50 | pulse, roar
45 | arts*
40 | esd
35 | alsa
30 | macosx, sndio
20 | aixs, oss, irix, sun, wmm
15 | arts*
10 | nas
0 | null, all file output

*arts priority depends on whether or not the arts install was built with `HAVE_ARTS_SUSPENDED`; when present, the default aRts priority is 45, else it is 15.

Clearly, any ranking scheme will fail to make everybody happy. For such cases, the configuration files can be easily used to define an appropriate default output device.

Adding `debug` to the libao configuration file on a line by itself will cause libao to print what static and dynamic drivers are available for use, as well as print the testing order.

copyright © 2001-2003 Stan Seibert, 2010-2013 Monty | xiph.org monty@xiph.org
libao documentation | libao version 1.2.0 - 20130122