This is doc/gcc.info, produced by makeinfo version 4.0 from
doc/gcc.texi.

INFO-DIR-SECTION Programming
START-INFO-DIR-ENTRY
* gcc: (gcc).                  The GNU Compiler Collection.
END-INFO-DIR-ENTRY
   This file documents the use and the internals of the GNU compiler.


   Published by the Free Software Foundation
59 Temple Place - Suite 330
Boston, MA 02111-1307 USA


   Copyright (C) 1988, 1989, 1992, 1993, 1994, 1995, 1996, 1997, 1998,
1999, 2000, 2001 Free Software Foundation, Inc.


   Permission is granted to copy, distribute and/or modify this document
under the terms of the GNU Free Documentation License, Version 1.1 or
any later version published by the Free Software Foundation; with the
Invariant Sections being "GNU General Public License" and "Funding Free
Software", the Front-Cover texts being (a) (see below), and with the
Back-Cover Texts being (b) (see below).  A copy of the license is
included in the section entitled "GNU Free Documentation License".

   (a) The FSF's Front-Cover Text is:

   A GNU Manual

   (b) The FSF's Back-Cover Text is:

   You have freedom to copy and modify this GNU Manual, like GNU
software.  Copies published by the Free Software Foundation raise
funds for GNU development.


File: gcc.info,  Node: DEC Alpha Options,  Next: Clipper Options,  Prev: Intel 960 Options,  Up: Submodel Options

DEC Alpha Options
-----------------

   These `-m' options are defined for the DEC Alpha implementations:

`-mno-soft-float'
`-msoft-float'
     Use (do not use) the hardware floating-point instructions for
     floating-point operations.  When `-msoft-float' is specified,
     functions in `libgcc1.c' will be used to perform floating-point
     operations.  Unless they are replaced by routines that emulate the
     floating-point operations, or compiled in such a way as to call
     such emulations routines, these routines will issue floating-point
     operations.   If you are compiling for an Alpha without
     floating-point operations, you must ensure that the library is
     built so as not to call them.

     Note that Alpha implementations without floating-point operations
     are required to have floating-point registers.

`-mfp-reg'
`-mno-fp-regs'
     Generate code that uses (does not use) the floating-point register
     set.  `-mno-fp-regs' implies `-msoft-float'.  If the floating-point
     register set is not used, floating point operands are passed in
     integer registers as if they were integers and floating-point
     results are passed in $0 instead of $f0.  This is a non-standard
     calling sequence, so any function with a floating-point argument
     or return value called by code compiled with `-mno-fp-regs' must
     also be compiled with that option.

     A typical use of this option is building a kernel that does not
     use, and hence need not save and restore, any floating-point
     registers.

`-mieee'
     The Alpha architecture implements floating-point hardware
     optimized for maximum performance.  It is mostly compliant with
     the IEEE floating point standard.  However, for full compliance,
     software assistance is required.  This option generates code fully
     IEEE compliant code _except_ that the INEXACT-FLAG is not
     maintained (see below).  If this option is turned on, the CPP
     macro `_IEEE_FP' is defined during compilation.  The option is a
     shorthand for: `-D_IEEE_FP -mfp-trap-mode=su -mtrap-precision=i
     -mieee-conformant'.  The resulting code is less efficient but is
     able to correctly support denormalized numbers and exceptional
     IEEE values such as not-a-number and plus/minus infinity.  Other
     Alpha compilers call this option `-ieee_with_no_inexact'.

`-mieee-with-inexact'
     This is like `-mieee' except the generated code also maintains the
     IEEE INEXACT-FLAG.  Turning on this option causes the generated
     code to implement fully-compliant IEEE math.  The option is a
     shorthand for `-D_IEEE_FP -D_IEEE_FP_INEXACT' plus the three
     following: `-mieee-conformant', `-mfp-trap-mode=sui', and
     `-mtrap-precision=i'.  On some Alpha implementations the resulting
     code may execute significantly slower than the code generated by
     default.  Since there is very little code that depends on the
     INEXACT-FLAG, you should normally not specify this option.  Other
     Alpha compilers call this option `-ieee_with_inexact'.

`-mfp-trap-mode=TRAP-MODE'
     This option controls what floating-point related traps are enabled.
     Other Alpha compilers call this option `-fptm TRAP-MODE'.  The
     trap mode can be set to one of four values:

    `n'
          This is the default (normal) setting.  The only traps that
          are enabled are the ones that cannot be disabled in software
          (e.g., division by zero trap).

    `u'
          In addition to the traps enabled by `n', underflow traps are
          enabled as well.

    `su'
          Like `su', but the instructions are marked to be safe for
          software completion (see Alpha architecture manual for
          details).

    `sui'
          Like `su', but inexact traps are enabled as well.

`-mfp-rounding-mode=ROUNDING-MODE'
     Selects the IEEE rounding mode.  Other Alpha compilers call this
     option `-fprm ROUNDING-MODE'.  The ROUNDING-MODE can be one of:

    `n'
          Normal IEEE rounding mode.  Floating point numbers are
          rounded towards the nearest machine number or towards the
          even machine number in case of a tie.

    `m'
          Round towards minus infinity.

    `c'
          Chopped rounding mode.  Floating point numbers are rounded
          towards zero.

    `d'
          Dynamic rounding mode.  A field in the floating point control
          register (FPCR, see Alpha architecture reference manual)
          controls the rounding mode in effect.  The C library
          initializes this register for rounding towards plus infinity.
          Thus, unless your program modifies the FPCR, `d' corresponds
          to round towards plus infinity.

`-mtrap-precision=TRAP-PRECISION'
     In the Alpha architecture, floating point traps are imprecise.
     This means without software assistance it is impossible to recover
     from a floating trap and program execution normally needs to be
     terminated.  GCC can generate code that can assist operating
     system trap handlers in determining the exact location that caused
     a floating point trap.  Depending on the requirements of an
     application, different levels of precisions can be selected:

    `p'
          Program precision.  This option is the default and means a
          trap handler can only identify which program caused a
          floating point exception.

    `f'
          Function precision.  The trap handler can determine the
          function that caused a floating point exception.

    `i'
          Instruction precision.  The trap handler can determine the
          exact instruction that caused a floating point exception.

     Other Alpha compilers provide the equivalent options called
     `-scope_safe' and `-resumption_safe'.

`-mieee-conformant'
     This option marks the generated code as IEEE conformant.  You must
     not use this option unless you also specify `-mtrap-precision=i'
     and either `-mfp-trap-mode=su' or `-mfp-trap-mode=sui'.  Its only
     effect is to emit the line `.eflag 48' in the function prologue of
     the generated assembly file.  Under DEC Unix, this has the effect
     that IEEE-conformant math library routines will be linked in.

`-mbuild-constants'
     Normally GCC examines a 32- or 64-bit integer constant to see if
     it can construct it from smaller constants in two or three
     instructions.  If it cannot, it will output the constant as a
     literal and generate code to load it from the data segment at
     runtime.

     Use this option to require GCC to construct _all_ integer constants
     using code, even if it takes more instructions (the maximum is
     six).

     You would typically use this option to build a shared library
     dynamic loader.  Itself a shared library, it must relocate itself
     in memory before it can find the variables and constants in its
     own data segment.

`-malpha-as'
`-mgas'
     Select whether to generate code to be assembled by the
     vendor-supplied assembler (`-malpha-as') or by the GNU assembler
     `-mgas'.

`-mbwx'
`-mno-bwx'
`-mcix'
`-mno-cix'
`-mmax'
`-mno-max'
     Indicate whether GCC should generate code to use the optional BWX,
     CIX, and MAX instruction sets.  The default is to use the
     instruction sets supported by the CPU type specified via `-mcpu='
     option or that of the CPU on which GCC was built if none was
     specified.

`-mcpu=CPU_TYPE'
     Set the instruction set, register set, and instruction scheduling
     parameters for machine type CPU_TYPE.  You can specify either the
     `EV' style name or the corresponding chip number.  GCC supports
     scheduling parameters for the EV4 and EV5 family of processors and
     will choose the default values for the instruction set from the
     processor you specify.  If you do not specify a processor type,
     GCC will default to the processor on which the compiler was built.

     Supported values for CPU_TYPE are

    `ev4'
    `21064'
          Schedules as an EV4 and has no instruction set extensions.

    `ev5'
    `21164'
          Schedules as an EV5 and has no instruction set extensions.

    `ev56'
    `21164a'
          Schedules as an EV5 and supports the BWX extension.

    `pca56'
    `21164pc'
    `21164PC'
          Schedules as an EV5 and supports the BWX and MAX extensions.

    `ev6'
    `21264'
          Schedules as an EV5 (until Digital releases the scheduling
          parameters for the EV6) and supports the BWX, CIX, and MAX
          extensions.

`-mmemory-latency=TIME'
     Sets the latency the scheduler should assume for typical memory
     references as seen by the application.  This number is highly
     dependent on the memory access patterns used by the application
     and the size of the external cache on the machine.

     Valid options for TIME are

    `NUMBER'
          A decimal number representing clock cycles.

    `L1'
    `L2'
    `L3'
    `main'
          The compiler contains estimates of the number of clock cycles
          for "typical" EV4 & EV5 hardware for the Level 1, 2 & 3 caches
          (also called Dcache, Scache, and Bcache), as well as to main
          memory.  Note that L3 is only valid for EV5.


File: gcc.info,  Node: Clipper Options,  Next: H8/300 Options,  Prev: DEC Alpha Options,  Up: Submodel Options

Clipper Options
---------------

   These `-m' options are defined for the Clipper implementations:

`-mc300'
     Produce code for a C300 Clipper processor.  This is the default.

`-mc400'
     Produce code for a C400 Clipper processor i.e. use floating point
     registers f8--f15.


File: gcc.info,  Node: H8/300 Options,  Next: SH Options,  Prev: Clipper Options,  Up: Submodel Options

H8/300 Options
--------------

   These `-m' options are defined for the H8/300 implementations:

`-mrelax'
     Shorten some address references at link time, when possible; uses
     the linker option `-relax'.  *Note `ld' and the H8/300:
     (ld.info)H8/300, for a fuller description.

`-mh'
     Generate code for the H8/300H.

`-ms'
     Generate code for the H8/S.

`-ms2600'
     Generate code for the H8/S2600.  This switch must be used with
     `-ms'.

`-mint32'
     Make `int' data 32 bits by default.

`-malign-300'
     On the H8/300H and H8/S, use the same alignment rules as for the
     H8/300.  The default for the H8/300H and H8/S is to align longs
     and floats on 4 byte boundaries.  `-malign-300' causes them to be
     aligned on 2 byte boundaries.  This option has no effect on the
     H8/300.


File: gcc.info,  Node: SH Options,  Next: System V Options,  Prev: H8/300 Options,  Up: Submodel Options

SH Options
----------

   These `-m' options are defined for the SH implementations:

`-m1'
     Generate code for the SH1.

`-m2'
     Generate code for the SH2.

`-m3'
     Generate code for the SH3.

`-m3e'
     Generate code for the SH3e.

`-m4-nofpu'
     Generate code for the SH4 without a floating-point unit.

`-m4-single-only'
     Generate code for the SH4 with a floating-point unit that only
     supports single-precision arithmetic.

`-m4-single'
     Generate code for the SH4 assuming the floating-point unit is in
     single-precision mode by default.

`-m4'
     Generate code for the SH4.

`-mb'
     Compile code for the processor in big endian mode.

`-ml'
     Compile code for the processor in little endian mode.

`-mdalign'
     Align doubles at 64-bit boundaries.  Note that this changes the
     calling conventions, and thus some functions from the standard C
     library will not work unless you recompile it first with
     `-mdalign'.

`-mrelax'
     Shorten some address references at link time, when possible; uses
     the linker option `-relax'.

`-mbigtable'
     Use 32-bit offsets in `switch' tables.  The default is to use
     16-bit offsets.

`-mfmovd'
     Enable the use of the instruction `fmovd'.

`-mhitachi'
     Comply with the calling conventions defined by Hitachi.

`-mnomacsave'
     Mark the `MAC' register as call-clobbered, even if `-mhitachi' is
     given.

`-mieee'
     Increase IEEE-compliance of floating-point code.

`-misize'
     Dump instruction size and location in the assembly code.

`-mpadstruct'
     This option is deprecated.  It pads structures to multiple of 4
     bytes, which is incompatible with the SH ABI.

`-mspace'
     Optimize for space instead of speed.  Implied by `-Os'.

`-mprefergot'
     When generating position-independent code, emit function calls
     using the Global Offset Table instead of the Procedure Linkage
     Table.

`-musermode'
     Generate a library function call to invalidate instruction cache
     entries, after fixing up a trampoline.  This library function call
     doesn't assume it can write to the whole memory address space.
     This is the default when the target is `sh-*-linux*'.


File: gcc.info,  Node: System V Options,  Next: TMS320C3x/C4x Options,  Prev: SH Options,  Up: Submodel Options

Options for System V
--------------------

   These additional options are available on System V Release 4 for
compatibility with other compilers on those systems:

`-G'
     Create a shared object.  It is recommended that `-symbolic' or
     `-shared' be used instead.

`-Qy'
     Identify the versions of each tool used by the compiler, in a
     `.ident' assembler directive in the output.

`-Qn'
     Refrain from adding `.ident' directives to the output file (this is
     the default).

`-YP,DIRS'
     Search the directories DIRS, and no others, for libraries
     specified with `-l'.

`-Ym,DIR'
     Look in the directory DIR to find the M4 preprocessor.  The
     assembler uses this option.


File: gcc.info,  Node: TMS320C3x/C4x Options,  Next: V850 Options,  Prev: System V Options,  Up: Submodel Options

TMS320C3x/C4x Options
---------------------

   These `-m' options are defined for TMS320C3x/C4x implementations:

`-mcpu=CPU_TYPE'
     Set the instruction set, register set, and instruction scheduling
     parameters for machine type CPU_TYPE.  Supported values for
     CPU_TYPE are `c30', `c31', `c32', `c40', and `c44'.  The default
     is `c40' to generate code for the TMS320C40.

`-mbig-memory'

`-mbig'
`-msmall-memory'
`-msmall'
     Generates code for the big or small memory model.  The small memory
     model assumed that all data fits into one 64K word page.  At
     run-time the data page (DP) register must be set to point to the
     64K page containing the .bss and .data program sections.  The big
     memory model is the default and requires reloading of the DP
     register for every direct memory access.

`-mbk'
`-mno-bk'
     Allow (disallow) allocation of general integer operands into the
     block count register BK.

`-mdb'
`-mno-db'
     Enable (disable) generation of code using decrement and branch,
     DBcond(D), instructions.  This is enabled by default for the C4x.
     To be on the safe side, this is disabled for the C3x, since the
     maximum iteration count on the C3x is 2^23 + 1 (but who iterates
     loops more than 2^23 times on the C3x?).  Note that GCC will try
     to reverse a loop so that it can utilise the decrement and branch
     instruction, but will give up if there is more than one memory
     reference in the loop.  Thus a loop where the loop counter is
     decremented can generate slightly more efficient code, in cases
     where the RPTB instruction cannot be utilised.

`-mdp-isr-reload'
`-mparanoid'
     Force the DP register to be saved on entry to an interrupt service
     routine (ISR), reloaded to point to the data section, and restored
     on exit from the ISR.  This should not be required unless someone
     has violated the small memory model by modifying the DP register,
     say within an object library.

`-mmpyi'
`-mno-mpyi'
     For the C3x use the 24-bit MPYI instruction for integer multiplies
     instead of a library call to guarantee 32-bit results.  Note that
     if one of the operands is a constant, then the multiplication will
     be performed using shifts and adds.  If the `-mmpyi' option is not
     specified for the C3x, then squaring operations are performed
     inline instead of a library call.

`-mfast-fix'
`-mno-fast-fix'
     The C3x/C4x FIX instruction to convert a floating point value to an
     integer value chooses the nearest integer less than or equal to the
     floating point value rather than to the nearest integer.  Thus if
     the floating point number is negative, the result will be
     incorrectly truncated an additional code is necessary to detect
     and correct this case.  This option can be used to disable
     generation of the additional code required to correct the result.

`-mrptb'
`-mno-rptb'
     Enable (disable) generation of repeat block sequences using the
     RPTB instruction for zero overhead looping.  The RPTB construct is
     only used for innermost loops that do not call functions or jump
     across the loop boundaries.  There is no advantage having nested
     RPTB loops due to the overhead required to save and restore the
     RC, RS, and RE registers.  This is enabled by default with `-O2'.

`-mrpts=COUNT'
`-mno-rpts'
     Enable (disable) the use of the single instruction repeat
     instruction RPTS.  If a repeat block contains a single
     instruction, and the loop count can be guaranteed to be less than
     the value COUNT, GCC will emit a RPTS instruction instead of a
     RPTB.  If no value is specified, then a RPTS will be emitted even
     if the loop count cannot be determined at compile time.  Note that
     the repeated instruction following RPTS does not have to be
     reloaded from memory each iteration, thus freeing up the CPU buses
     for operands.  However, since interrupts are blocked by this
     instruction, it is disabled by default.

`-mloop-unsigned'
`-mno-loop-unsigned'
     The maximum iteration count when using RPTS and RPTB (and DB on
     the C40) is 2^31 + 1 since these instructions test if the
     iteration count is negative to terminate the loop.  If the
     iteration count is unsigned there is a possibility than the 2^31 +
     1 maximum iteration count may be exceeded.  This switch allows an
     unsigned iteration count.

`-mti'
     Try to emit an assembler syntax that the TI assembler (asm30) is
     happy with.  This also enforces compatibility with the API
     employed by the TI C3x C compiler.  For example, long doubles are
     passed as structures rather than in floating point registers.

`-mregparm'
`-mmemparm'
     Generate code that uses registers (stack) for passing arguments to
     functions.  By default, arguments are passed in registers where
     possible rather than by pushing arguments on to the stack.

`-mparallel-insns'
`-mno-parallel-insns'
     Allow the generation of parallel instructions.  This is enabled by
     default with `-O2'.

`-mparallel-mpy'
`-mno-parallel-mpy'
     Allow the generation of MPY||ADD and MPY||SUB parallel
     instructions, provided `-mparallel-insns' is also specified.
     These instructions have tight register constraints which can
     pessimize the code generation of large functions.


File: gcc.info,  Node: V850 Options,  Next: ARC Options,  Prev: TMS320C3x/C4x Options,  Up: Submodel Options

V850 Options
------------

   These `-m' options are defined for V850 implementations:

`-mlong-calls'
`-mno-long-calls'
     Treat all calls as being far away (near).  If calls are assumed to
     be far away, the compiler will always load the functions address
     up into a register, and call indirect through the pointer.

`-mno-ep'
`-mep'
     Do not optimize (do optimize) basic blocks that use the same index
     pointer 4 or more times to copy pointer into the `ep' register, and
     use the shorter `sld' and `sst' instructions.  The `-mep' option
     is on by default if you optimize.

`-mno-prolog-function'
`-mprolog-function'
     Do not use (do use) external functions to save and restore
     registers at the prolog and epilog of a function.  The external
     functions are slower, but use less code space if more than one
     function saves the same number of registers.  The
     `-mprolog-function' option is on by default if you optimize.

`-mspace'
     Try to make the code as small as possible.  At present, this just
     turns on the `-mep' and `-mprolog-function' options.

`-mtda=N'
     Put static or global variables whose size is N bytes or less into
     the tiny data area that register `ep' points to.  The tiny data
     area can hold up to 256 bytes in total (128 bytes for byte
     references).

`-msda=N'
     Put static or global variables whose size is N bytes or less into
     the small data area that register `gp' points to.  The small data
     area can hold up to 64 kilobytes.

`-mzda=N'
     Put static or global variables whose size is N bytes or less into
     the first 32 kilobytes of memory.

`-mv850'
     Specify that the target processor is the V850.

`-mbig-switch'
     Generate code suitable for big switch tables.  Use this option
     only if the assembler/linker complain about out of range branches
     within a switch table.


File: gcc.info,  Node: ARC Options,  Next: NS32K Options,  Prev: V850 Options,  Up: Submodel Options

ARC Options
-----------

   These options are defined for ARC implementations:

`-EL'
     Compile code for little endian mode.  This is the default.

`-EB'
     Compile code for big endian mode.

`-mmangle-cpu'
     Prepend the name of the cpu to all public symbol names.  In
     multiple-processor systems, there are many ARC variants with
     different instruction and register set characteristics.  This flag
     prevents code compiled for one cpu to be linked with code compiled
     for another.  No facility exists for handling variants that are
     "almost identical".  This is an all or nothing option.

`-mcpu=CPU'
     Compile code for ARC variant CPU.  Which variants are supported
     depend on the configuration.  All variants support `-mcpu=base',
     this is the default.

`-mtext=TEXT-SECTION'
`-mdata=DATA-SECTION'
`-mrodata=READONLY-DATA-SECTION'
     Put functions, data, and readonly data in TEXT-SECTION,
     DATA-SECTION, and READONLY-DATA-SECTION respectively by default.
     This can be overridden with the `section' attribute.  *Note
     Variable Attributes::.


File: gcc.info,  Node: NS32K Options,  Next: AVR Options,  Prev: ARC Options,  Up: Submodel Options

NS32K Options
-------------

   These are the `-m' options defined for the 32000 series.  The default
values for these options depends on which style of 32000 was selected
when the compiler was configured; the defaults for the most common
choices are given below.

`-m32032'
`-m32032'
     Generate output for a 32032.  This is the default when the
     compiler is configured for 32032 and 32016 based systems.

`-m32332'
`-m32332'
     Generate output for a 32332.  This is the default when the
     compiler is configured for 32332-based systems.

`-m32532'
`-m32532'
     Generate output for a 32532.  This is the default when the
     compiler is configured for 32532-based systems.

`-m32081'
     Generate output containing 32081 instructions for floating point.
     This is the default for all systems.

`-m32381'
     Generate output containing 32381 instructions for floating point.
     This also implies `-m32081'.  The 32381 is only compatible with
     the 32332 and 32532 cpus.  This is the default for the
     pc532-netbsd configuration.

`-mmulti-add'
     Try and generate multiply-add floating point instructions `polyF'
     and `dotF'.  This option is only available if the `-m32381' option
     is in effect.  Using these instructions requires changes to
     register allocation which generally has a negative impact on
     performance.  This option should only be enabled when compiling
     code particularly likely to make heavy use of multiply-add
     instructions.

`-mnomulti-add'
     Do not try and generate multiply-add floating point instructions
     `polyF' and `dotF'.  This is the default on all platforms.

`-msoft-float'
     Generate output containing library calls for floating point.
     *Warning:* the requisite libraries may not be available.

`-mnobitfield'
     Do not use the bit-field instructions.  On some machines it is
     faster to use shifting and masking operations.  This is the
     default for the pc532.

`-mbitfield'
     Do use the bit-field instructions.  This is the default for all
     platforms except the pc532.

`-mrtd'
     Use a different function-calling convention, in which functions
     that take a fixed number of arguments return pop their arguments
     on return with the `ret' instruction.

     This calling convention is incompatible with the one normally used
     on Unix, so you cannot use it if you need to call libraries
     compiled with the Unix compiler.

     Also, you must provide function prototypes for all functions that
     take variable numbers of arguments (including `printf'); otherwise
     incorrect code will be generated for calls to those functions.

     In addition, seriously incorrect code will result if you call a
     function with too many arguments.  (Normally, extra arguments are
     harmlessly ignored.)

     This option takes its name from the 680x0 `rtd' instruction.

`-mregparam'
     Use a different function-calling convention where the first two
     arguments are passed in registers.

     This calling convention is incompatible with the one normally used
     on Unix, so you cannot use it if you need to call libraries
     compiled with the Unix compiler.

`-mnoregparam'
     Do not pass any arguments in registers.  This is the default for
     all targets.

`-msb'
     It is OK to use the sb as an index register which is always loaded
     with zero.  This is the default for the pc532-netbsd target.

`-mnosb'
     The sb register is not available for use or has not been
     initialized to zero by the run time system.  This is the default
     for all targets except the pc532-netbsd.  It is also implied
     whenever `-mhimem' or `-fpic' is set.

`-mhimem'
     Many ns32000 series addressing modes use displacements of up to
     512MB.  If an address is above 512MB then displacements from zero
     can not be used.  This option causes code to be generated which
     can be loaded above 512MB.  This may be useful for operating
     systems or ROM code.

`-mnohimem'
     Assume code will be loaded in the first 512MB of virtual address
     space.  This is the default for all platforms.


File: gcc.info,  Node: AVR Options,  Next: MCore Options,  Prev: NS32K Options,  Up: Submodel Options

AVR Options
-----------

   These options are defined for AVR implementations:

`-mmcu=MCU'
     Specify ATMEL AVR instruction set or MCU type.

     Instruction set avr1 is for the minimal AVR core, not supported by
     the C compiler, only for assembler programs (MCU types: at90s1200,
     attiny10, attiny11, attiny12, attiny15, attiny28).

     Instruction set avr2 (default) is for the classic AVR core with up
     to 8K program memory space (MCU types: at90s2313, at90s2323,
     attiny22, at90s2333, at90s2343, at90s4414, at90s4433, at90s4434,
     at90s8515, at90c8534, at90s8535).

     Instruction set avr3 is for the classic AVR core with up to 128K
     program memory space (MCU types: atmega103, atmega603).

     Instruction set avr4 is for the enhanced AVR core with up to 8K
     program memory space (MCU types: atmega83, atmega85).

     Instruction set avr5 is for the enhanced AVR core with up to 128K
     program memory space (MCU types: atmega161, atmega163, atmega32,
     at94k).

`-msize'
     Output instruction sizes to the asm file.

`-minit-stack=N'
     Specify the initial stack address, which may be a symbol or
     numeric value, `__stack' is the default.

`-mno-interrupts'
     Generated code is not compatible with hardware interrupts.  Code
     size will be smaller.

`-mcall-prologues'
     Functions prologues/epilogues expanded as call to appropriate
     subroutines.  Code size will be smaller.

`-mno-tablejump'
     Do not generate tablejump insns which sometimes increase code size.

`-mtiny-stack'
     Change only the low 8 bits of the stack pointer.


File: gcc.info,  Node: MCore Options,  Next: IA-64 Options,  Prev: AVR Options,  Up: Submodel Options

MCore Options
-------------

   These are the `-m' options defined for the Motorola M*Core
processors.

`-mhardlit'
`-mhardlit'
`-mno-hardlit'
     Inline constants into the code stream if it can be done in two
     instructions or less.

`-mdiv'
`-mdiv'
`-mno-div'
     Use the divide instruction.  (Enabled by default).

`-mrelax-immediate'
`-mrelax-immediate'
`-mno-relax-immediate'
     Allow arbitrary sized immediates in bit operations.

`-mwide-bitfields'
`-mwide-bitfields'
`-mno-wide-bitfields'
     Always treat bit-fields as int-sized.

`-m4byte-functions'
`-m4byte-functions'
`-mno-4byte-functions'
     Force all functions to be aligned to a four byte boundary.

`-mcallgraph-data'
`-mcallgraph-data'
`-mno-callgraph-data'
     Emit callgraph information.

`-mslow-bytes'
`-mslow-bytes'
`-mno-slow-bytes'
     Prefer word access when reading byte quantities.

`-mlittle-endian'
`-mlittle-endian'
`-mbig-endian'
     Generate code for a little endian target.

`-m210'
`-m210'
`-m340'
     Generate code for the 210 processor.


File: gcc.info,  Node: IA-64 Options,  Next: D30V Options,  Prev: MCore Options,  Up: Submodel Options

IA-64 Options
-------------

   These are the `-m' options defined for the Intel IA-64 architecture.

`-mbig-endian'
     Generate code for a big endian target.  This is the default for
     HPUX.

`-mlittle-endian'
     Generate code for a little endian target.  This is the default for
     AIX5 and Linux.

`-mgnu-as'
`-mno-gnu-as'
     Generate (or don't) code for the GNU assembler.  This is the
     default.

`-mgnu-ld'
`-mno-gnu-ld'
     Generate (or don't) code for the GNU linker.  This is the default.

`-mno-pic'
     Generate code that does not use a global pointer register.  The
     result is not position independent code, and violates the IA-64
     ABI.

`-mvolatile-asm-stop'
`-mno-volatile-asm-stop'
     Generate (or don't) a stop bit immediately before and after
     volatile asm statements.

`-mb-step'
     Generate code that works around Itanium B step errata.

`-mregister-names'
`-mno-register-names'
     Generate (or don't) `in', `loc', and `out' register names for the
     stacked registers.  This may make assembler output more readable.

`-mno-sdata'
`-msdata'
     Disable (or enable) optimizations that use the small data section.
     This may be useful for working around optimizer bugs.

`-mconstant-gp'
     Generate code that uses a single constant global pointer value.
     This is useful when compiling kernel code.

`-mauto-pic'
     Generate code that is self-relocatable.  This implies
     `-mconstant-gp'.  This is useful when compiling firmware code.

`-minline-divide-min-latency'
     Generate code for inline divides using the minimum latency
     algorithm.

`-minline-divide-max-throughput'
     Generate code for inline divides using the maximum throughput
     algorithm.

`-mno-dwarf2-asm'
`-mdwarf2-asm'
     Don't (or do) generate assembler code for the DWARF2 line number
     debugging info.  This may be useful when not using the GNU
     assembler.

`-mfixed-range=REGISTER-RANGE'
     Generate code treating the given register range as fixed registers.
     A fixed register is one that the register allocator can not use.
     This is useful when compiling kernel code.  A register range is
     specified as two registers separated by a dash.  Multiple register
     ranges can be specified separated by a comma.


File: gcc.info,  Node: D30V Options,  Next: S/390 and zSeries Options,  Prev: IA-64 Options,  Up: Submodel Options

D30V Options
------------

   These `-m' options are defined for D30V implementations:

`-mextmem'
     Link the `.text', `.data', `.bss', `.strings', `.rodata',
     `.rodata1', `.data1' sections into external memory, which starts
     at location `0x80000000'.

`-mextmemory'
     Same as the `-mextmem' switch.

`-monchip'
     Link the `.text' section into onchip text memory, which starts at
     location `0x0'.  Also link `.data', `.bss', `.strings', `.rodata',
     `.rodata1', `.data1' sections into onchip data memory, which
     starts at location `0x20000000'.

`-mno-asm-optimize'
`-masm-optimize'
     Disable (enable) passing `-O' to the assembler when optimizing.
     The assembler uses the `-O' option to automatically parallelize
     adjacent short instructions where possible.

`-mbranch-cost=N'
     Increase the internal costs of branches to N.  Higher costs means
     that the compiler will issue more instructions to avoid doing a
     branch.  The default is 2.

`-mcond-exec=N'
     Specify the maximum number of conditionally executed instructions
     that replace a branch.  The default is 4.


File: gcc.info,  Node: S/390 and zSeries Options,  Prev: D30V Options,  Up: Submodel Options

S/390 and zSeries Options
-------------------------

   These are the `-m' options defined for the S/390 and zSeries
architecture.

`-mhard-float'
`-msoft-float'
     Use (do not use) the hardware floating-point instructions and
     registers for floating-point operations.  When `-msoft-float' is
     specified, functions in `libgcc.a' will be used to perform
     floating-point operations.  When `-mhard-float' is specified, the
     compiler generates IEEE floating-point instructions.  This is the
     default.

`-mbackchain'
`-mno-backchain'
     Generate (or do not generate) code which maintains an explicit
     backchain within the stack frame that points to the caller's frame.
     This is currently needed to allow debugging.  The default is to
     generate the backchain.

`-msmall-exec'
`-mno-small-exec'
     Generate (or do not generate) code using the `bras' instruction to
     do subroutine calls.  This only works reliably if the total
     executable size does not exceed 64k.  The default is to use the
     `basr' instruction instead, which does not have this limitation.

`-m64'
`-m31'
     When `-m31' is specified, generate code compliant to the Linux for
     S/390 ABI.  When `-m64' is specified, generate code compliant to
     the Linux for zSeries ABI.  This allows GCC in particular to
     generate 64-bit instructions.  For the `s390' targets, the default
     is `-m31', while the `s390x' targets default to `-m64'.

`-mmvcle'
`-mno-mvcle'
     Generate (or do not generate) code using the `mvcle' instruction
     to perform block moves.  When `-mno-mvcle' is specifed, use a
     `mvc' loop instead.  This is the default.

`-mdebug'
`-mno-debug'
     Print (or do not print) additional debug information when
     compiling.  The default is to not print debug information.

