;; Machine Descriptions for R8C/M16C/M32C
;; Copyright (C) 2005, 2007
;; Free Software Foundation, Inc.
;; Contributed by Red Hat.
;;
;; This file is part of GCC.
;;
;; GCC is free software; you can redistribute it and/or modify it
;; under the terms of the GNU General Public License as published
;; by the Free Software Foundation; either version 3, or (at your
;; option) any later version.
;;
;; GCC is distributed in the hope that it will be useful, but WITHOUT
;; ANY WARRANTY; without even the implied warranty of MERCHANTABILITY
;; or FITNESS FOR A PARTICULAR PURPOSE.  See the GNU General Public
;; License for more details.
;;
;; You should have received a copy of the GNU General Public License
;; along with GCC; see the file COPYING3.  If not see
;; <http://www.gnu.org/licenses/>.

;; add, sub

(define_insn "addqi3"
  [(set (match_operand:QI 0 "mra_or_sp_operand"
		  "=SdRhl,SdRhl,??Rmm,??Rmm, *Raa,*Raa,SdRhl,??Rmm")
	(plus:QI (match_operand:QI 1 "mra_operand"
		  "%0,0,0,0, 0,0,0,0")
		 (match_operand:QI 2 "mrai_operand"
		  "iSdRhl,?Rmm,iSdRhl,?Rmm, iSdRhl,?Rmm,*Raa,*Raa")))]
  ""
  "add.b\t%2,%0"
  [(set_attr "flags" "oszc")]
  )

(define_insn "addhi3"
  [(set (match_operand:HI 0 "m32c_nonimmediate_operand"
	 	  "=SdRhi,SdRhi,??Rmm,??Rmm, SdRhi,??Rmm, Rhi, Raw, Raw, !Rsp")
	(plus:HI (match_operand:HI 1 "m32c_any_operand"
		  "%0,0,0,0, 0,0, Raw, Rfb, Rfb, 0")
		 (match_operand:HI 2 "m32c_any_operand"
		  "IU2sSdRhi,?Rmm,IU2sSdRhi,?Rmm, IM2,IM2, IS2IU2, I00, IS1, i")))]
  ""
  "@
   add.w\t%2,%0
   add.w\t%2,%0
   add.w\t%2,%0
   add.w\t%2,%0
   sub.w\t%m2,%0
   sub.w\t%m2,%0
   mova\t%d2[%1],%0
   stc\t%1,%0
   mova\t%D2[%1],%0
   add.w\t%2,%0"
  [(set_attr "flags" "oszc,oszc,oszc,oszc,oszc,oszc,n,n,n,oszc")]
  )

(define_insn "addpsi3"
  [(set (match_operand:PSI 0 "m32c_nonimmediate_operand" "=Rpi,Raa,SdRpi,SdRpi,Rsp*Rmm, Rpi,Rpi")
	(plus:PSI (match_operand:PSI 1 "m32c_nonimmediate_operand" "0,0,0,0,0, Raa,Rad")
		  (match_operand:PSI 2 "m32c_any_operand" "Is3,IS1,iSdRpi,?Rmm,i, i,IS2")))]
  "TARGET_A24"
  "@
   add.l:q\t%2,%0
   addx\t%2,%0
   add.l\t%2,%0
   add.l\t%2,%0
   add.l\t%2,%0
   mova\t%d2[%1],%0
   mova\t%D2[%1],%0"
  [(set_attr "flags" "oszc,oszc,oszc,oszc,oszc,n,n")]
  )

(define_expand "addsi3"
  [(set (match_operand:SI 0 "mra_operand" "=RsiSd,RsiSd,??Rmm,??Rmm")
        (plus:SI (match_operand:SI 1 "mra_operand" "%0,0,0,0")
                 (match_operand:SI 2 "mrai_operand" "iRsiSd,?Rmm,iRsiSd,?Rmm")))]
  "TARGET_A24 ||TARGET_A16"
  ""
  )

(define_insn "addsi3_1"
  [(set (match_operand:SI 0 "mra_operand" "=RsiSd,??Rmm,RsiSd,RsiSd,??Rmm,??Rmm,??Rmm,RsiSd")
        (plus:SI (match_operand:SI 1 "mra_operand" "%0,0,0,0,0,0,0,0")
                 (match_operand 2 "mrai_operand" "IU2,IU2,i,?Rmm,i,RsiSd,?Rmm,RsiSd")))]
  "TARGET_A16"
  "*
  
  switch (which_alternative)
    { 
    case 0:
      return \"add.w %X2,%h0\;adcf.w %H0\";
    case 1:
      return \"add.w %X2,%h0\;adcf.w %H0\";
    case 2:
      output_asm_insn (\"add.w %X2,%h0\",operands);
      operands[2]= GEN_INT (INTVAL (operands[2]) >> 16);
      return \"adc.w %X2,%H0\";
    case 3:
      return \"add.w %h2,%h0\;adc.w %H2,%H0\";
    case 4:
      output_asm_insn (\"add.w %X2,%h0\",operands);
      operands[2]= GEN_INT (INTVAL (operands[2]) >> 16);
      return \"adc.w %X2,%H0\";
    case 5:
      return \"add.w %h2,%h0\;adc.w %H2,%H0\";
    case 6:
      return \"add.w %h2,%h0\;adc.w %H2,%H0\";
    case 7:
      return \"add.w %h2,%h0\;adc.w %H2,%H0\";
    }"
  [(set_attr "flags" "x,x,x,x,x,x,x,x")]
)

(define_insn "addsi3_2"
  [(set (match_operand:SI 0 "mra_operand" "=RsiSd,RsiSd,??Rmm,??Rmm")
        (plus:SI (match_operand:SI 1 "mra_operand" "%0,0,0,0")
                 (match_operand:SI 2 "mrai_operand" "iRsiSd,?Rmm,iRsiSd,?Rmm")))]
  "TARGET_A24"
  "add.l\t%2,%0"
  [(set_attr "flags" "oszc")]
)

(define_insn "subqi3"
  [(set (match_operand:QI 0 "mra_or_sp_operand"
		   "=SdRhl,SdRhl,??Rmm,??Rmm, Raa,Raa,SdRhl,??Rmm, *Rsp")
	(minus:QI (match_operand:QI 1 "mra_operand"
		   "0,0,0,0, 0,0,0,0, 0")
		  (match_operand:QI 2 "mrai_operand"
		   "iSdRhl,?Rmm,iSdRhl,?Rmm, iSdRhl,?Rmm,Raa,Raa, i")))]
  ""
  "sub.b\t%2,%0"
  [(set_attr "flags" "oszc")]
  )

(define_insn "subhi3"
  [(set (match_operand:HI 0 "mra_operand"
		   "=SdRhi,SdRhi,??Rmm,??Rmm, SdRhi,??Rmm")
	(minus:HI (match_operand:HI 1 "mras_operand"
		   "0,0,0,0, 0,0")
		  (match_operand:HI 2 "mrai_operand"
		   "IU2SdRhi,?Rmm,IU2SdRhi,?Rmm, IM2,IM2")))]
  ""
  "@
   sub.w\t%2,%0
   sub.w\t%2,%0
   sub.w\t%2,%0
   sub.w\t%2,%0
   add.w\t%m2,%0
   add.w\t%m2,%0"
  [(set_attr "flags" "oszc,oszc,oszc,oszc,oszc,oszc")]
  )

(define_insn "subpsi3"
  [(set (match_operand:PSI 0 "mra_operand" "=RpiSd,RpiSd,??Rmm,??Rmm")
	(minus:PSI (match_operand:PSI 1 "mra_operand" "0,0,0,0")
		   (match_operand:PSI 2 "mrai_operand" "iRpiSd,?Rmm,iRpiSd,?Rmm")))]
  "TARGET_A24"
  "sub.%&\t%2,%0"
  [(set_attr "flags" "oszc")]
  )

(define_expand "subsi3"
  [(set (match_operand:SI 0 "mra_operand" "=RsiSd,RsiSd,??Rmm,??Rmm")
        (minus:SI (match_operand:SI 1 "mra_operand" "0,0,0,0")
                  (match_operand:SI 2 "mrai_operand" "iRsiSd,?Rmm,iRsiSd,?Rmm")))]
  "TARGET_A24 ||TARGET_A16"
  ""
)

(define_insn "subsi3_1"
  [(set (match_operand:SI 0 "mra_operand" "=RsiSd,RsiSd,??Rmm,??Rmm,??Rmm,RsiSd")
        (minus:SI (match_operand:SI 1 "mra_operand" "0,0,0,0,0,0")
                  (match_operand:SI 2 "mrai_operand" "i,?Rmm,i,RsiSd,?Rmm,RsiSd")))]
  "TARGET_A16"
  "*
  switch (which_alternative)
    {
    case 0:
      output_asm_insn (\"sub.w %X2,%h0\",operands);
      operands[2]= GEN_INT (INTVAL (operands[2]) >> 16);
      return \"sbb.w %X2,%H0\";
    case 1:
      return \"sub.w %h2,%h0\;sbb.w %H2,%H0\";
    case 2:
      output_asm_insn (\"sub.w %X2,%h0\",operands);
      operands[2]= GEN_INT (INTVAL (operands[2]) >> 16);
      return \"sbb.w %X2,%H0\";
    case 3:
      return \"sub.w %h2,%h0\;sbb.w %H2,%H0\";
    case 4:
      return \"sub.w %h2,%h0\;sbb.w %H2,%H0\";
    case 5:
      return \"sub.w %h2,%h0\;sbb.w %H2,%H0\";
    }"
  [(set_attr "flags" "x,x,x,x,x,x")]
)

(define_insn "subsi3_2"
  [(set (match_operand:SI 0 "mra_operand" "=RsiSd,RsiSd,??Rmm,??Rmm")
        (minus:SI (match_operand:SI 1 "mra_operand" "0,0,0,0")
                  (match_operand:SI 2 "mrai_operand" "iRsiSd,?Rmm,iRsiSd,?Rmm")))]
  "TARGET_A24"
  "sub.l\t%2,%0"
  [(set_attr "flags" "oszc,oszc,oszc,oszc")]
)

(define_insn "negqi2"
  [(set (match_operand:QI 0 "mra_operand" "=SdRhl,??Rmm")
	(neg:QI (match_operand:QI 1 "mra_operand" "0,0")))]
  ""
  "neg.b\t%0"
  [(set_attr "flags" "oszc,oszc")]
  )

(define_insn "neghi2"
  [(set (match_operand:HI 0 "mra_operand" "=SdRhi,??Rmm")
	(neg:HI (match_operand:HI 1 "mra_operand" "0,0")))]
  ""
  "neg.w\t%0"
  [(set_attr "flags" "oszc,oszc")]
  )

; We can negate an SImode by operating on the subparts.  GCC deals
; with this itself for larger modes, but not SI.
(define_insn "negsi2"
  [(set (match_operand:SI 0 "mra_operand" "=SdR03,??Rmm")
	(neg:SI (match_operand:SI 1 "mra_operand" "0,0")))]
  ""
  "not.w %h0 | not.w %H0 | add.w #1,%h0 | adcf.w %H0"
  [(set_attr "flags" "x")]
  )

(define_insn "absqi2"
  [(set (match_operand:QI 0 "mra_operand" "=RhlSd,??Rmm")
	(abs:QI (match_operand:QI 1 "mra_operand" "0,0")))]
  ""
  "abs.b\t%0"
  [(set_attr "flags" "oszc")]
  )

(define_insn "abshi2"
  [(set (match_operand:HI 0 "mra_operand" "=RhiSd,??Rmm")
	(abs:HI (match_operand:HI 1 "mra_operand" "0,0")))]
  ""
  "abs.w\t%0"
  [(set_attr "flags" "oszc")]
  )
