@c Copyright (C) 2012-2015 Free Software Foundation, Inc.
@c This is part of the GCC manual.
@c For copying conditions, see the file gcc/doc/include/fdl.texi.

@c This file is generated automatically using
@c gcc/config/avr/gen-avr-mmcu-texi.c from:
@c    gcc/config/avr/avr-arch.h
@c    gcc/config/avr/avr-devices.c
@c    gcc/config/avr/avr-mcus.def

@c Please do not edit manually.

@table @code

@item avr2
``Classic'' devices with up to 8@tie{}KiB of program memory.
@*@var{mcu}@tie{}= @code{attiny22}, @code{attiny26}, @code{at90c8534}, @code{at90s2313}, @code{at90s2323}, @code{at90s2333}, @code{at90s2343}, @code{at90s4414}, @code{at90s4433}, @code{at90s4434}, @code{at90s8515}, @code{at90s8535}.

@item avr25
``Classic'' devices with up to 8@tie{}KiB of program memory and with the @code{MOVW} instruction.
@*@var{mcu}@tie{}= @code{ata5272}, @code{ata6616c}, @code{attiny13}, @code{attiny13a}, @code{attiny2313}, @code{attiny2313a}, @code{attiny24}, @code{attiny24a}, @code{attiny25}, @code{attiny261}, @code{attiny261a}, @code{attiny43u}, @code{attiny4313}, @code{attiny44}, @code{attiny44a}, @code{attiny441}, @code{attiny45}, @code{attiny461}, @code{attiny461a}, @code{attiny48}, @code{attiny828}, @code{attiny84}, @code{attiny84a}, @code{attiny841}, @code{attiny85}, @code{attiny861}, @code{attiny861a}, @code{attiny87}, @code{attiny88}, @code{at86rf401}.

@item avr3
``Classic'' devices with 16@tie{}KiB up to 64@tie{}KiB of  program memory.
@*@var{mcu}@tie{}= @code{at43usb355}, @code{at76c711}.

@item avr31
``Classic'' devices with 128@tie{}KiB of program memory.
@*@var{mcu}@tie{}= @code{atmega103}, @code{at43usb320}.

@item avr35
``Classic'' devices with 16@tie{}KiB up to 64@tie{}KiB of program memory and with the @code{MOVW} instruction.
@*@var{mcu}@tie{}= @code{ata5505}, @code{ata6617c}, @code{ata664251}, @code{atmega16u2}, @code{atmega32u2}, @code{atmega8u2}, @code{attiny1634}, @code{attiny167}, @code{at90usb162}, @code{at90usb82}.

@item avr4
``Enhanced'' devices with up to 8@tie{}KiB of program memory.
@*@var{mcu}@tie{}= @code{ata6285}, @code{ata6286}, @code{ata6289}, @code{ata6612c}, @code{atmega48}, @code{atmega48a}, @code{atmega48p}, @code{atmega48pa}, @code{atmega8}, @code{atmega8a}, @code{atmega8hva}, @code{atmega8515}, @code{atmega8535}, @code{atmega88}, @code{atmega88a}, @code{atmega88p}, @code{atmega88pa}, @code{at90pwm1}, @code{at90pwm2}, @code{at90pwm2b}, @code{at90pwm3}, @code{at90pwm3b}, @code{at90pwm81}.

@item avr5
``Enhanced'' devices with 16@tie{}KiB up to 64@tie{}KiB of program memory.
@*@var{mcu}@tie{}= @code{ata5702m322}, @code{ata5782}, @code{ata5790}, @code{ata5790n}, @code{ata5795}, @code{ata5831}, @code{ata6613c}, @code{ata6614q}, @code{atmega16}, @code{atmega16a}, @code{atmega16hva}, @code{atmega16hva2}, @code{atmega16hvb}, @code{atmega16hvbrevb}, @code{atmega16m1}, @code{atmega16u4}, @code{atmega161}, @code{atmega162}, @code{atmega163}, @code{atmega164a}, @code{atmega164p}, @code{atmega164pa}, @code{atmega165}, @code{atmega165a}, @code{atmega165p}, @code{atmega165pa}, @code{atmega168}, @code{atmega168a}, @code{atmega168p}, @code{atmega168pa}, @code{atmega169}, @code{atmega169a}, @code{atmega169p}, @code{atmega169pa}, @code{atmega32}, @code{atmega32a}, @code{atmega32c1}, @code{atmega32hvb}, @code{atmega32hvbrevb}, @code{atmega32m1}, @code{atmega32u4}, @code{atmega32u6}, @code{atmega323}, @code{atmega324a}, @code{atmega324p}, @code{atmega324pa}, @code{atmega325}, @code{atmega325a}, @code{atmega325p}, @code{atmega325pa}, @code{atmega3250}, @code{atmega3250a}, @code{atmega3250p}, @code{atmega3250pa}, @code{atmega328}, @code{atmega328p}, @code{atmega329}, @code{atmega329a}, @code{atmega329p}, @code{atmega329pa}, @code{atmega3290}, @code{atmega3290a}, @code{atmega3290p}, @code{atmega3290pa}, @code{atmega406}, @code{atmega64}, @code{atmega64a}, @code{atmega64c1}, @code{atmega64hve}, @code{atmega64hve2}, @code{atmega64m1}, @code{atmega64rfr2}, @code{atmega640}, @code{atmega644}, @code{atmega644a}, @code{atmega644p}, @code{atmega644pa}, @code{atmega644rfr2}, @code{atmega645}, @code{atmega645a}, @code{atmega645p}, @code{atmega6450}, @code{atmega6450a}, @code{atmega6450p}, @code{atmega649}, @code{atmega649a}, @code{atmega649p}, @code{atmega6490}, @code{atmega6490a}, @code{atmega6490p}, @code{at90can32}, @code{at90can64}, @code{at90pwm161}, @code{at90pwm216}, @code{at90pwm316}, @code{at90scr100}, @code{at90usb646}, @code{at90usb647}, @code{at94k}, @code{m3000}.

@item avr51
``Enhanced'' devices with 128@tie{}KiB of program memory.
@*@var{mcu}@tie{}= @code{atmega128}, @code{atmega128a}, @code{atmega128rfa1}, @code{atmega128rfr2}, @code{atmega1280}, @code{atmega1281}, @code{atmega1284}, @code{atmega1284p}, @code{atmega1284rfr2}, @code{at90can128}, @code{at90usb1286}, @code{at90usb1287}.

@item avr6
``Enhanced'' devices with 3-byte PC, i.e.@: with more than 128@tie{}KiB of program memory.
@*@var{mcu}@tie{}= @code{atmega256rfr2}, @code{atmega2560}, @code{atmega2561}, @code{atmega2564rfr2}.

@item avrxmega2
``XMEGA'' devices with more than 8@tie{}KiB and up to 64@tie{}KiB of program memory.
@*@var{mcu}@tie{}= @code{atxmega16a4}, @code{atxmega16a4u}, @code{atxmega16c4}, @code{atxmega16d4}, @code{atxmega16e5}, @code{atxmega32a4}, @code{atxmega32a4u}, @code{atxmega32c3}, @code{atxmega32c4}, @code{atxmega32d3}, @code{atxmega32d4}, @code{atxmega32e5}, @code{atxmega8e5}.

@item avrxmega4
``XMEGA'' devices with more than 64@tie{}KiB and up to 128@tie{}KiB of program memory.
@*@var{mcu}@tie{}= @code{atxmega64a3}, @code{atxmega64a3u}, @code{atxmega64a4u}, @code{atxmega64b1}, @code{atxmega64b3}, @code{atxmega64c3}, @code{atxmega64d3}, @code{atxmega64d4}.

@item avrxmega5
``XMEGA'' devices with more than 64@tie{}KiB and up to 128@tie{}KiB of program memory and more than 64@tie{}KiB of RAM.
@*@var{mcu}@tie{}= @code{atxmega64a1}, @code{atxmega64a1u}.

@item avrxmega6
``XMEGA'' devices with more than 128@tie{}KiB of program memory.
@*@var{mcu}@tie{}= @code{atxmega128a3}, @code{atxmega128a3u}, @code{atxmega128b1}, @code{atxmega128b3}, @code{atxmega128c3}, @code{atxmega128d3}, @code{atxmega128d4}, @code{atxmega192a3}, @code{atxmega192a3u}, @code{atxmega192c3}, @code{atxmega192d3}, @code{atxmega256a3}, @code{atxmega256a3b}, @code{atxmega256a3bu}, @code{atxmega256a3u}, @code{atxmega256c3}, @code{atxmega256d3}, @code{atxmega384c3}, @code{atxmega384d3}.

@item avrxmega7
``XMEGA'' devices with more than 128@tie{}KiB of program memory and more than 64@tie{}KiB of RAM.
@*@var{mcu}@tie{}= @code{atxmega128a1}, @code{atxmega128a1u}, @code{atxmega128a4u}.

@item avrtiny
``TINY'' Tiny core devices with 512@tie{}B up to 4@tie{}KiB of program memory.
@*@var{mcu}@tie{}= @code{attiny10}, @code{attiny20}, @code{attiny4}, @code{attiny40}, @code{attiny5}, @code{attiny9}.

@item avr1
This ISA is implemented by the minimal AVR core and supported for assembler only.
@*@var{mcu}@tie{}= @code{attiny11}, @code{attiny12}, @code{attiny15}, @code{attiny28}, @code{at90s1200}.

@end table
