Next: i386-Regs, Previous: i386-Syntax, Up: i386-Dependent

#### 8.11.3 Instruction Naming

Instruction mnemonics are suffixed with one character modifiers which specify the size of operands. The letters ``b`', ``w`', ``l`' and ``q`' specify byte, word, long and quadruple word operands. If no suffix is specified by an instruction then `as` tries to fill in the missing suffix based on the destination register operand (the last one by convention). Thus, ``mov %ax, %bx`' is equivalent to ``movw %ax, %bx`'; also, ``mov $1, %bx`' is equivalent to ``movw $1, bx`'. Note that this is incompatible with the AT&T Unix assembler which assumes that a missing mnemonic suffix implies long operand size. (This incompatibility does not affect compiler output since compilers always explicitly specify the mnemonic suffix.)

Almost all instructions have the same names in AT&T and Intel format. There are a few exceptions. The sign extend and zero extend instructions need two sizes to specify them. They need a size to sign/zero extend from and a size to zero extend to. This is accomplished by using two instruction mnemonic suffixes in AT&T syntax. Base names for sign extend and zero extend are ``movs...`' and ``movz...`' in AT&T syntax (``movsx`' and ``movzx`' in Intel syntax). The instruction mnemonic suffixes are tacked on to this base name, the from suffix before the to suffix. Thus, ``movsbl %al, %edx`' is AT&T syntax for “move sign extend from %al to %edx.” Possible suffixes, thus, are ``bl`' (from byte to long), ``bw`' (from byte to word), ``wl`' (from word to long), ``bq`' (from byte to quadruple word), ``wq`' (from word to quadruple word), and ``lq`' (from long to quadruple word).

The Intel-syntax conversion instructions

- ``cbw`' — sign-extend byte in ``%al`' to word in ``%ax`',
- ``cwde`' — sign-extend word in ``%ax`' to long in ``%eax`',
- ``cwd`' — sign-extend word in ``%ax`' to long in ``%dx:%ax`',
- ``cdq`' — sign-extend dword in ``%eax`' to quad in ``%edx:%eax`',
- ``cdqe`' — sign-extend dword in ``%eax`' to quad in ``%rax`' (x86-64 only),
- ``cqo`' — sign-extend quad in ``%rax`' to octuple in ``%rdx:%rax`' (x86-64 only),

are called ``cbtw`', ``cwtl`', ``cwtd`', ``cltd`', ``cltq`', and ``cqto`' in AT&T naming. `as` accepts either naming for these instructions.

Far call/jump instructions are ``lcall`' and ``ljmp`' in AT&T syntax, but are ``call far`' and ``jump far`' in Intel convention.