Next: M68HC11-Modifiers, Previous: M68HC11-Opts, Up: M68HC11-Dependent

#### 8.19.2 Syntax

In the M68HC11 syntax, the instruction name comes first and it may be followed by one or several operands (up to three). Operands are separated by comma (``,`'). In the normal mode, `as` will complain if too many operands are specified for a given instruction. In the MRI mode (turned on with ``-M`' option), it will treat them as comments. Example:

         inx
         lda  #23
         bset 2,x #4
         brclr *bot #8 foo

The following addressing modes are understood for 68HC11 and 68HC12:

Immediate
  ``#number`'
Address Register
  ``number,X`', ``number,Y`'

  The number may be omitted in which case 0 is assumed.

Direct Addressing mode
  ``*symbol`', or ``*digits`'
Absolute
  ``symbol`', or ``digits`'

The M68HC12 has other more complex addressing modes. All of them are supported and they are represented below:

Constant Offset Indexed Addressing Mode
  ``number,reg`'

  The number may be omitted in which case 0 is assumed. The register can be either ``X`', ``Y`', ``SP`' or ``PC`'. The assembler will use the smaller post-byte definition according to the constant value (5-bit constant offset, 9-bit constant offset or 16-bit constant offset). If the constant is not known by the assembler it will use the 16-bit constant offset post-byte and the value will be resolved at link time.

Offset Indexed Indirect
  ``[number,reg]`'

  The register can be either ``X`', ``Y`', ``SP`' or ``PC`'.

Auto Pre-Increment/Pre-Decrement/Post-Increment/Post-Decrement
  ``number,-reg`' ``number,+reg`' ``number,reg-`' ``number,reg+`'

  The number must be in the range ``-8`'..``+8`' and must not be 0. The register can be either ``X`', ``Y`', ``SP`' or ``PC`'.

Accumulator Offset
  ``acc,reg`'

  The accumulator register can be either ``A`', ``B`' or ``D`'. The register can be either ``X`', ``Y`', ``SP`' or ``PC`'.

Accumulator D offset indexed-indirect
  ``[D,reg]`'

  The register can be either ``X`', ``Y`', ``SP`' or ``PC`'.

For example:

         ldab 1024,sp
         ldd [10,x]
         orab 3,+x
         stab -2,y-
         ldx a,pc
         sty [d,sp]