This is doc/gcc.info, produced by makeinfo version 4.2 from
doc/gcc.texi.

INFO-DIR-SECTION Programming
START-INFO-DIR-ENTRY
* gcc: (gcc).                  The GNU Compiler Collection.
END-INFO-DIR-ENTRY
   This file documents the use of the GNU compilers.

   Published by the Free Software Foundation
59 Temple Place - Suite 330
Boston, MA 02111-1307 USA

   Copyright (C) 1988, 1989, 1992, 1993, 1994, 1995, 1996, 1997, 1998,
1999, 2000, 2001, 2002 Free Software Foundation, Inc.

   Permission is granted to copy, distribute and/or modify this document
under the terms of the GNU Free Documentation License, Version 1.1 or
any later version published by the Free Software Foundation; with the
Invariant Sections being "GNU General Public License" and "Funding Free
Software", the Front-Cover texts being (a) (see below), and with the
Back-Cover Texts being (b) (see below).  A copy of the license is
included in the section entitled "GNU Free Documentation License".

   (a) The FSF's Front-Cover Text is:

   A GNU Manual

   (b) The FSF's Back-Cover Text is:

   You have freedom to copy and modify this GNU Manual, like GNU
software.  Copies published by the Free Software Foundation raise
funds for GNU development.


File: gcc.info,  Node: TMS320C3x/C4x Options,  Next: V850 Options,  Prev: System V Options,  Up: Submodel Options

TMS320C3x/C4x Options
---------------------

   These `-m' options are defined for TMS320C3x/C4x implementations:

`-mcpu=CPU_TYPE'
     Set the instruction set, register set, and instruction scheduling
     parameters for machine type CPU_TYPE.  Supported values for
     CPU_TYPE are `c30', `c31', `c32', `c40', and `c44'.  The default
     is `c40' to generate code for the TMS320C40.

`-mbig-memory'

`-mbig'
`-msmall-memory'
`-msmall'
     Generates code for the big or small memory model.  The small memory
     model assumed that all data fits into one 64K word page.  At
     run-time the data page (DP) register must be set to point to the
     64K page containing the .bss and .data program sections.  The big
     memory model is the default and requires reloading of the DP
     register for every direct memory access.

`-mbk'
`-mno-bk'
     Allow (disallow) allocation of general integer operands into the
     block count register BK.

`-mdb'
`-mno-db'
     Enable (disable) generation of code using decrement and branch,
     DBcond(D), instructions.  This is enabled by default for the C4x.
     To be on the safe side, this is disabled for the C3x, since the
     maximum iteration count on the C3x is 2^23 + 1 (but who iterates
     loops more than 2^23 times on the C3x?).  Note that GCC will try
     to reverse a loop so that it can utilise the decrement and branch
     instruction, but will give up if there is more than one memory
     reference in the loop.  Thus a loop where the loop counter is
     decremented can generate slightly more efficient code, in cases
     where the RPTB instruction cannot be utilised.

`-mdp-isr-reload'
`-mparanoid'
     Force the DP register to be saved on entry to an interrupt service
     routine (ISR), reloaded to point to the data section, and restored
     on exit from the ISR.  This should not be required unless someone
     has violated the small memory model by modifying the DP register,
     say within an object library.

`-mmpyi'
`-mno-mpyi'
     For the C3x use the 24-bit MPYI instruction for integer multiplies
     instead of a library call to guarantee 32-bit results.  Note that
     if one of the operands is a constant, then the multiplication will
     be performed using shifts and adds.  If the `-mmpyi' option is not
     specified for the C3x, then squaring operations are performed
     inline instead of a library call.

`-mfast-fix'
`-mno-fast-fix'
     The C3x/C4x FIX instruction to convert a floating point value to an
     integer value chooses the nearest integer less than or equal to the
     floating point value rather than to the nearest integer.  Thus if
     the floating point number is negative, the result will be
     incorrectly truncated an additional code is necessary to detect
     and correct this case.  This option can be used to disable
     generation of the additional code required to correct the result.

`-mrptb'
`-mno-rptb'
     Enable (disable) generation of repeat block sequences using the
     RPTB instruction for zero overhead looping.  The RPTB construct is
     only used for innermost loops that do not call functions or jump
     across the loop boundaries.  There is no advantage having nested
     RPTB loops due to the overhead required to save and restore the
     RC, RS, and RE registers.  This is enabled by default with `-O2'.

`-mrpts=COUNT'
`-mno-rpts'
     Enable (disable) the use of the single instruction repeat
     instruction RPTS.  If a repeat block contains a single
     instruction, and the loop count can be guaranteed to be less than
     the value COUNT, GCC will emit a RPTS instruction instead of a
     RPTB.  If no value is specified, then a RPTS will be emitted even
     if the loop count cannot be determined at compile time.  Note that
     the repeated instruction following RPTS does not have to be
     reloaded from memory each iteration, thus freeing up the CPU buses
     for operands.  However, since interrupts are blocked by this
     instruction, it is disabled by default.

`-mloop-unsigned'
`-mno-loop-unsigned'
     The maximum iteration count when using RPTS and RPTB (and DB on
     the C40) is 2^31 + 1 since these instructions test if the
     iteration count is negative to terminate the loop.  If the
     iteration count is unsigned there is a possibility than the 2^31 +
     1 maximum iteration count may be exceeded.  This switch allows an
     unsigned iteration count.

`-mti'
     Try to emit an assembler syntax that the TI assembler (asm30) is
     happy with.  This also enforces compatibility with the API
     employed by the TI C3x C compiler.  For example, long doubles are
     passed as structures rather than in floating point registers.

`-mregparm'
`-mmemparm'
     Generate code that uses registers (stack) for passing arguments to
     functions.  By default, arguments are passed in registers where
     possible rather than by pushing arguments on to the stack.

`-mparallel-insns'
`-mno-parallel-insns'
     Allow the generation of parallel instructions.  This is enabled by
     default with `-O2'.

`-mparallel-mpy'
`-mno-parallel-mpy'
     Allow the generation of MPY||ADD and MPY||SUB parallel
     instructions, provided `-mparallel-insns' is also specified.
     These instructions have tight register constraints which can
     pessimize the code generation of large functions.


File: gcc.info,  Node: V850 Options,  Next: ARC Options,  Prev: TMS320C3x/C4x Options,  Up: Submodel Options

V850 Options
------------

   These `-m' options are defined for V850 implementations:

`-mlong-calls'
`-mno-long-calls'
     Treat all calls as being far away (near).  If calls are assumed to
     be far away, the compiler will always load the functions address
     up into a register, and call indirect through the pointer.

`-mno-ep'
`-mep'
     Do not optimize (do optimize) basic blocks that use the same index
     pointer 4 or more times to copy pointer into the `ep' register, and
     use the shorter `sld' and `sst' instructions.  The `-mep' option
     is on by default if you optimize.

`-mno-prolog-function'
`-mprolog-function'
     Do not use (do use) external functions to save and restore
     registers at the prolog and epilog of a function.  The external
     functions are slower, but use less code space if more than one
     function saves the same number of registers.  The
     `-mprolog-function' option is on by default if you optimize.

`-mspace'
     Try to make the code as small as possible.  At present, this just
     turns on the `-mep' and `-mprolog-function' options.

`-mtda=N'
     Put static or global variables whose size is N bytes or less into
     the tiny data area that register `ep' points to.  The tiny data
     area can hold up to 256 bytes in total (128 bytes for byte
     references).

`-msda=N'
     Put static or global variables whose size is N bytes or less into
     the small data area that register `gp' points to.  The small data
     area can hold up to 64 kilobytes.

`-mzda=N'
     Put static or global variables whose size is N bytes or less into
     the first 32 kilobytes of memory.

`-mv850'
     Specify that the target processor is the V850.

`-mbig-switch'
     Generate code suitable for big switch tables.  Use this option
     only if the assembler/linker complain about out of range branches
     within a switch table.


File: gcc.info,  Node: ARC Options,  Next: NS32K Options,  Prev: V850 Options,  Up: Submodel Options

ARC Options
-----------

   These options are defined for ARC implementations:

`-EL'
     Compile code for little endian mode.  This is the default.

`-EB'
     Compile code for big endian mode.

`-mmangle-cpu'
     Prepend the name of the cpu to all public symbol names.  In
     multiple-processor systems, there are many ARC variants with
     different instruction and register set characteristics.  This flag
     prevents code compiled for one cpu to be linked with code compiled
     for another.  No facility exists for handling variants that are
     "almost identical".  This is an all or nothing option.

`-mcpu=CPU'
     Compile code for ARC variant CPU.  Which variants are supported
     depend on the configuration.  All variants support `-mcpu=base',
     this is the default.

`-mtext=TEXT-SECTION'
`-mdata=DATA-SECTION'
`-mrodata=READONLY-DATA-SECTION'
     Put functions, data, and readonly data in TEXT-SECTION,
     DATA-SECTION, and READONLY-DATA-SECTION respectively by default.
     This can be overridden with the `section' attribute.  *Note
     Variable Attributes::.


File: gcc.info,  Node: NS32K Options,  Next: AVR Options,  Prev: ARC Options,  Up: Submodel Options

NS32K Options
-------------

   These are the `-m' options defined for the 32000 series.  The default
values for these options depends on which style of 32000 was selected
when the compiler was configured; the defaults for the most common
choices are given below.

`-m32032'
`-m32032'
     Generate output for a 32032.  This is the default when the
     compiler is configured for 32032 and 32016 based systems.

`-m32332'
`-m32332'
     Generate output for a 32332.  This is the default when the
     compiler is configured for 32332-based systems.

`-m32532'
`-m32532'
     Generate output for a 32532.  This is the default when the
     compiler is configured for 32532-based systems.

`-m32081'
     Generate output containing 32081 instructions for floating point.
     This is the default for all systems.

`-m32381'
     Generate output containing 32381 instructions for floating point.
     This also implies `-m32081'.  The 32381 is only compatible with
     the 32332 and 32532 cpus.  This is the default for the
     pc532-netbsd configuration.

`-mmulti-add'
     Try and generate multiply-add floating point instructions `polyF'
     and `dotF'.  This option is only available if the `-m32381' option
     is in effect.  Using these instructions requires changes to
     register allocation which generally has a negative impact on
     performance.  This option should only be enabled when compiling
     code particularly likely to make heavy use of multiply-add
     instructions.

`-mnomulti-add'
     Do not try and generate multiply-add floating point instructions
     `polyF' and `dotF'.  This is the default on all platforms.

`-msoft-float'
     Generate output containing library calls for floating point.
     *Warning:* the requisite libraries may not be available.

`-mnobitfield'
     Do not use the bit-field instructions.  On some machines it is
     faster to use shifting and masking operations.  This is the
     default for the pc532.

`-mbitfield'
     Do use the bit-field instructions.  This is the default for all
     platforms except the pc532.

`-mrtd'
     Use a different function-calling convention, in which functions
     that take a fixed number of arguments return pop their arguments
     on return with the `ret' instruction.

     This calling convention is incompatible with the one normally used
     on Unix, so you cannot use it if you need to call libraries
     compiled with the Unix compiler.

     Also, you must provide function prototypes for all functions that
     take variable numbers of arguments (including `printf'); otherwise
     incorrect code will be generated for calls to those functions.

     In addition, seriously incorrect code will result if you call a
     function with too many arguments.  (Normally, extra arguments are
     harmlessly ignored.)

     This option takes its name from the 680x0 `rtd' instruction.

`-mregparam'
     Use a different function-calling convention where the first two
     arguments are passed in registers.

     This calling convention is incompatible with the one normally used
     on Unix, so you cannot use it if you need to call libraries
     compiled with the Unix compiler.

`-mnoregparam'
     Do not pass any arguments in registers.  This is the default for
     all targets.

`-msb'
     It is OK to use the sb as an index register which is always loaded
     with zero.  This is the default for the pc532-netbsd target.

`-mnosb'
     The sb register is not available for use or has not been
     initialized to zero by the run time system.  This is the default
     for all targets except the pc532-netbsd.  It is also implied
     whenever `-mhimem' or `-fpic' is set.

`-mhimem'
     Many ns32000 series addressing modes use displacements of up to
     512MB.  If an address is above 512MB then displacements from zero
     can not be used.  This option causes code to be generated which
     can be loaded above 512MB.  This may be useful for operating
     systems or ROM code.

`-mnohimem'
     Assume code will be loaded in the first 512MB of virtual address
     space.  This is the default for all platforms.


File: gcc.info,  Node: AVR Options,  Next: MCore Options,  Prev: NS32K Options,  Up: Submodel Options

AVR Options
-----------

   These options are defined for AVR implementations:

`-mmcu=MCU'
     Specify ATMEL AVR instruction set or MCU type.

     Instruction set avr1 is for the minimal AVR core, not supported by
     the C compiler, only for assembler programs (MCU types: at90s1200,
     attiny10, attiny11, attiny12, attiny15, attiny28).

     Instruction set avr2 (default) is for the classic AVR core with up
     to 8K program memory space (MCU types: at90s2313, at90s2323,
     attiny22, at90s2333, at90s2343, at90s4414, at90s4433, at90s4434,
     at90s8515, at90c8534, at90s8535).

     Instruction set avr3 is for the classic AVR core with up to 128K
     program memory space (MCU types: atmega103, atmega603, at43usb320,
     at76c711).

     Instruction set avr4 is for the enhanced AVR core with up to 8K
     program memory space (MCU types: atmega8, atmega83, atmega85).

     Instruction set avr5 is for the enhanced AVR core with up to 128K
     program memory space (MCU types: atmega16, atmega161, atmega163,
     atmega32, atmega323, atmega64, atmega128, at43usb355, at94k).

`-msize'
     Output instruction sizes to the asm file.

`-minit-stack=N'
     Specify the initial stack address, which may be a symbol or
     numeric value, `__stack' is the default.

`-mno-interrupts'
     Generated code is not compatible with hardware interrupts.  Code
     size will be smaller.

`-mcall-prologues'
     Functions prologues/epilogues expanded as call to appropriate
     subroutines.  Code size will be smaller.

`-mno-tablejump'
     Do not generate tablejump insns which sometimes increase code size.

`-mtiny-stack'
     Change only the low 8 bits of the stack pointer.


File: gcc.info,  Node: MCore Options,  Next: IA-64 Options,  Prev: AVR Options,  Up: Submodel Options

MCore Options
-------------

   These are the `-m' options defined for the Motorola M*Core
processors.

`-mhardlit'
`-mhardlit'
`-mno-hardlit'
     Inline constants into the code stream if it can be done in two
     instructions or less.

`-mdiv'
`-mdiv'
`-mno-div'
     Use the divide instruction.  (Enabled by default).

`-mrelax-immediate'
`-mrelax-immediate'
`-mno-relax-immediate'
     Allow arbitrary sized immediates in bit operations.

`-mwide-bitfields'
`-mwide-bitfields'
`-mno-wide-bitfields'
     Always treat bit-fields as int-sized.

`-m4byte-functions'
`-m4byte-functions'
`-mno-4byte-functions'
     Force all functions to be aligned to a four byte boundary.

`-mcallgraph-data'
`-mcallgraph-data'
`-mno-callgraph-data'
     Emit callgraph information.

`-mslow-bytes'
`-mslow-bytes'
`-mno-slow-bytes'
     Prefer word access when reading byte quantities.

`-mlittle-endian'
`-mlittle-endian'
`-mbig-endian'
     Generate code for a little endian target.

`-m210'
`-m210'
`-m340'
     Generate code for the 210 processor.


File: gcc.info,  Node: IA-64 Options,  Next: D30V Options,  Prev: MCore Options,  Up: Submodel Options

IA-64 Options
-------------

   These are the `-m' options defined for the Intel IA-64 architecture.

`-mbig-endian'
     Generate code for a big endian target.  This is the default for
     HPUX.

`-mlittle-endian'
     Generate code for a little endian target.  This is the default for
     AIX5 and Linux.

`-mgnu-as'
`-mno-gnu-as'
     Generate (or don't) code for the GNU assembler.  This is the
     default.

`-mgnu-ld'
`-mno-gnu-ld'
     Generate (or don't) code for the GNU linker.  This is the default.

`-mno-pic'
     Generate code that does not use a global pointer register.  The
     result is not position independent code, and violates the IA-64
     ABI.

`-mvolatile-asm-stop'
`-mno-volatile-asm-stop'
     Generate (or don't) a stop bit immediately before and after
     volatile asm statements.

`-mb-step'
     Generate code that works around Itanium B step errata.

`-mregister-names'
`-mno-register-names'
     Generate (or don't) `in', `loc', and `out' register names for the
     stacked registers.  This may make assembler output more readable.

`-mno-sdata'
`-msdata'
     Disable (or enable) optimizations that use the small data section.
     This may be useful for working around optimizer bugs.

`-mconstant-gp'
     Generate code that uses a single constant global pointer value.
     This is useful when compiling kernel code.

`-mauto-pic'
     Generate code that is self-relocatable.  This implies
     `-mconstant-gp'.  This is useful when compiling firmware code.

`-minline-divide-min-latency'
     Generate code for inline divides using the minimum latency
     algorithm.

`-minline-divide-max-throughput'
     Generate code for inline divides using the maximum throughput
     algorithm.

`-mno-dwarf2-asm'
`-mdwarf2-asm'
     Don't (or do) generate assembler code for the DWARF2 line number
     debugging info.  This may be useful when not using the GNU
     assembler.

`-mfixed-range=REGISTER-RANGE'
     Generate code treating the given register range as fixed registers.
     A fixed register is one that the register allocator can not use.
     This is useful when compiling kernel code.  A register range is
     specified as two registers separated by a dash.  Multiple register
     ranges can be specified separated by a comma.


File: gcc.info,  Node: D30V Options,  Next: S/390 and zSeries Options,  Prev: IA-64 Options,  Up: Submodel Options

D30V Options
------------

   These `-m' options are defined for D30V implementations:

`-mextmem'
     Link the `.text', `.data', `.bss', `.strings', `.rodata',
     `.rodata1', `.data1' sections into external memory, which starts
     at location `0x80000000'.

`-mextmemory'
     Same as the `-mextmem' switch.

`-monchip'
     Link the `.text' section into onchip text memory, which starts at
     location `0x0'.  Also link `.data', `.bss', `.strings', `.rodata',
     `.rodata1', `.data1' sections into onchip data memory, which
     starts at location `0x20000000'.

`-mno-asm-optimize'
`-masm-optimize'
     Disable (enable) passing `-O' to the assembler when optimizing.
     The assembler uses the `-O' option to automatically parallelize
     adjacent short instructions where possible.

`-mbranch-cost=N'
     Increase the internal costs of branches to N.  Higher costs means
     that the compiler will issue more instructions to avoid doing a
     branch.  The default is 2.

`-mcond-exec=N'
     Specify the maximum number of conditionally executed instructions
     that replace a branch.  The default is 4.


File: gcc.info,  Node: S/390 and zSeries Options,  Next: CRIS Options,  Prev: D30V Options,  Up: Submodel Options

S/390 and zSeries Options
-------------------------

   These are the `-m' options defined for the S/390 and zSeries
architecture.

`-mhard-float'
`-msoft-float'
     Use (do not use) the hardware floating-point instructions and
     registers for floating-point operations.  When `-msoft-float' is
     specified, functions in `libgcc.a' will be used to perform
     floating-point operations.  When `-mhard-float' is specified, the
     compiler generates IEEE floating-point instructions.  This is the
     default.

`-mbackchain'
`-mno-backchain'
     Generate (or do not generate) code which maintains an explicit
     backchain within the stack frame that points to the caller's frame.
     This is currently needed to allow debugging.  The default is to
     generate the backchain.

`-msmall-exec'
`-mno-small-exec'
     Generate (or do not generate) code using the `bras' instruction to
     do subroutine calls.  This only works reliably if the total
     executable size does not exceed 64k.  The default is to use the
     `basr' instruction instead, which does not have this limitation.

`-m64'
`-m31'
     When `-m31' is specified, generate code compliant to the Linux for
     S/390 ABI.  When `-m64' is specified, generate code compliant to
     the Linux for zSeries ABI.  This allows GCC in particular to
     generate 64-bit instructions.  For the `s390' targets, the default
     is `-m31', while the `s390x' targets default to `-m64'.

`-mmvcle'
`-mno-mvcle'
     Generate (or do not generate) code using the `mvcle' instruction
     to perform block moves.  When `-mno-mvcle' is specifed, use a
     `mvc' loop instead.  This is the default.

`-mdebug'
`-mno-debug'
     Print (or do not print) additional debug information when
     compiling.  The default is to not print debug information.


File: gcc.info,  Node: CRIS Options,  Next: MMIX Options,  Prev: S/390 and zSeries Options,  Up: Submodel Options

CRIS Options
------------

   These options are defined specifically for the CRIS ports.

`-march=ARCHITECTURE-TYPE'
`-mcpu=ARCHITECTURE-TYPE'
     Generate code for the specified architecture.  The choices for
     ARCHITECTURE-TYPE are `v3', `v8' and `v10' for respectively
     ETRAX 4, ETRAX 100, and ETRAX 100 LX.  Default is `v0' except for
     cris-axis-linux-gnu, where the default is `v10'.

`-mtune=ARCHITECTURE-TYPE'
     Tune to ARCHITECTURE-TYPE everything applicable about the generated
     code, except for the ABI and the set of available instructions.
     The choices for ARCHITECTURE-TYPE are the same as for
     `-march=ARCHITECTURE-TYPE'.

`-mmax-stack-frame=N'
     Warn when the stack frame of a function exceeds N bytes.

`-melinux-stacksize=N'
     Only available with the `cris-axis-aout' target.  Arranges for
     indications in the program to the kernel loader that the stack of
     the program should be set to N bytes.

`-metrax4'
`-metrax100'
     The options `-metrax4' and `-metrax100' are synonyms for
     `-march=v3' and `-march=v8' respectively.

`-mpdebug'
     Enable CRIS-specific verbose debug-related information in the
     assembly code.  This option also has the effect to turn off the
     `#NO_APP' formatted-code indicator to the assembler at the
     beginning of the assembly file.

`-mcc-init'
     Do not use condition-code results from previous instruction;
     always emit compare and test instructions before use of condition
     codes.

`-mno-side-effects'
     Do not emit instructions with side-effects in addressing modes
     other than post-increment.

`-mstack-align'
`-mno-stack-align'
`-mdata-align'
`-mno-data-align'
`-mconst-align'
`-mno-const-align'
     These options (no-options) arranges (eliminate arrangements) for
     the stack-frame, individual data and constants to be aligned for
     the maximum single data access size for the chosen CPU model.  The
     default is to arrange for 32-bit alignment.  ABI details such as
     structure layout are not affected by these options.

`-m32-bit'
`-m16-bit'
`-m8-bit'
     Similar to the stack- data- and const-align options above, these
     options arrange for stack-frame, writable data and constants to
     all be 32-bit, 16-bit or 8-bit aligned.  The default is 32-bit
     alignment.

`-mno-prologue-epilogue'
`-mprologue-epilogue'
     With `-mno-prologue-epilogue', the normal function prologue and
     epilogue that sets up the stack-frame are omitted and no return
     instructions or return sequences are generated in the code.  Use
     this option only together with visual inspection of the compiled
     code: no warnings or errors are generated when call-saved
     registers must be saved, or storage for local variable needs to be
     allocated.

`-mno-gotplt'
`-mgotplt'
     With `-fpic' and `-fPIC', don't generate (do generate) instruction
     sequences that load addresses for functions from the PLT part of
     the GOT rather than (traditional on other architectures) calls to
     the PLT.  The default is `-mgotplt'.

`-maout'
     Legacy no-op option only recognized with the cris-axis-aout target.

`-melf'
     Legacy no-op option only recognized with the cris-axis-elf and
     cris-axis-linux-gnu targets.

`-melinux'
     Only recognized with the cris-axis-aout target, where it selects a
     GNU/linux-like multilib, include files and instruction set for
     `-march=v8'.

`-mlinux'
     Legacy no-op option only recognized with the cris-axis-linux-gnu
     target.

`-sim'
     This option, recognized for the cris-axis-aout and cris-axis-elf
     arranges to link with input-output functions from a simulator
     library.  Code, initialized data and zero-initialized data are
     allocated consecutively.

`-sim2'
     Like `-sim', but pass linker options to locate initialized data at
     0x40000000 and zero-initialized data at 0x80000000.


File: gcc.info,  Node: MMIX Options,  Next: PDP-11 Options,  Prev: CRIS Options,  Up: Submodel Options

MMIX Options
------------

   These options are defined for the MMIX:

`-mlibfuncs'
`-mno-libfuncs'
     Specify that intrinsic library functions are being compiled,
     passing all values in registers, no matter the size.

`-mepsilon'
`-mno-epsilon'
     Generate floating-point comparison instructions that compare with
     respect to the `rE' epsilon register.

`-mabi=mmixware'
`-mabi=gnu'
     Generate code that passes function parameters and return values
     that (in the called function) are seen as registers `$0' and up,
     as opposed to the GNU ABI which uses global registers `$231' and
     up.

`-mzero-extend'
`-mno-zero-extend'
     When reading data from memory in sizes shorter than 64 bits, use
     (do not use) zero-extending load instructions by default, rather
     than sign-extending ones.

`-mknuthdiv'
`-mno-knuthdiv'
     Make the result of a division yielding a remainder have the same
     sign as the divisor.  With the default, `-mno-knuthdiv', the sign
     of the remainder follows the sign of the dividend.  Both methods
     are arithmetically valid, the latter being almost exclusively used.

`-mtoplevel-symbols'
`-mno-toplevel-symbols'
     Prepend (do not prepend) a `:' to all global symbols, so the
     assembly code can be used with the `PREFIX' assembly directive.

`-melf'
     Generate an executable in the ELF format, rather than the default
     `mmo' format used by the `mmix' simulator.

`-mbranch-predict'
`-mno-branch-predict'
     Use (do not use) the probable-branch instructions, when static
     branch prediction indicates a probable branch.

`-mbase-addresses'
`-mno-base-addresses'
     Generate (do not generate) code that uses _base addresses_.  Using
     a base address automatically generates a request (handled by the
     assembler and the linker) for a constant to be set up in a global
     register.  The register is used for one or more base address
     requests within the range 0 to 255 from the value held in the
     register.  The generally leads to short and fast code, but the
     number of different data items that can be addressed is limited.
     This means that a program that uses lots of static data may
     require `-mno-base-addresses'.


File: gcc.info,  Node: PDP-11 Options,  Next: Xstormy16 Options,  Prev: MMIX Options,  Up: Submodel Options

PDP-11 Options
--------------

   These options are defined for the PDP-11:

`-mfpu'
     Use hardware FPP floating point.  This is the default.  (FIS
     floating point on the PDP-11/40 is not supported.)

`-msoft-float'
     Do not use hardware floating point.

`-mac0'
     Return floating-point results in ac0 (fr0 in Unix assembler
     syntax).

`-mno-ac0'
     Return floating-point results in memory.  This is the default.

`-m40'
     Generate code for a PDP-11/40.

`-m45'
     Generate code for a PDP-11/45.  This is the default.

`-m10'
     Generate code for a PDP-11/10.

`-mbcopy-builtin'
     Use inline `movstrhi' patterns for copying memory.  This is the
     default.

`-mbcopy'
     Do not use inline `movstrhi' patterns for copying memory.

`-mint16'
`-mno-int32'
     Use 16-bit `int'.  This is the default.

`-mint32'
`-mno-int16'
     Use 32-bit `int'.

`-mfloat64'
`-mno-float32'
     Use 64-bit `float'.  This is the default.

`-mfloat32'

`-mno-float64'
     Use 32-bit `float'.

`-mabshi'
     Use `abshi2' pattern.  This is the default.

`-mno-abshi'
     Do not use `abshi2' pattern.

`-mbranch-expensive'
     Pretend that branches are expensive.  This is for experimenting
     with code generation only.

`-mbranch-cheap'
     Do not pretend that branches are expensive.  This is the default.

`-msplit'
     Generate code for a system with split I&D.

`-mno-split'
     Generate code for a system without split I&D.  This is the default.

`-munix-asm'
     Use Unix assembler syntax.  This is the default when configured for
     `pdp11-*-bsd'.

`-mdec-asm'
     Use DEC assembler syntax.  This is the default when configured for
     any PDP-11 target other than `pdp11-*-bsd'.


File: gcc.info,  Node: Xstormy16 Options,  Next: Xtensa Options,  Prev: PDP-11 Options,  Up: Submodel Options

Xstormy16 Options
-----------------

   These options are defined for Xstormy16:

`-msim'
     Choose startup files and linker script suitable for the simulator.


File: gcc.info,  Node: Xtensa Options,  Prev: Xstormy16 Options,  Up: Submodel Options

Xtensa Options
--------------

   The Xtensa architecture is designed to support many different
configurations.  The compiler's default options can be set to match a
particular Xtensa configuration by copying a configuration file into the
GCC sources when building GCC.  The options below may be used to
override the default options.

`-mbig-endian'
`-mlittle-endian'
     Specify big-endian or little-endian byte ordering for the target
     Xtensa processor.

`-mdensity'
`-mno-density'
     Enable or disable use of the optional Xtensa code density
     instructions.

`-mmac16'
`-mno-mac16'
     Enable or disable use of the Xtensa MAC16 option.  When enabled,
     GCC will generate MAC16 instructions from standard C code, with the
     limitation that it will use neither the MR register file nor any
     instruction that operates on the MR registers.  When this option is
     disabled, GCC will translate 16-bit multiply/accumulate operations
     to a combination of core instructions and library calls, depending
     on whether any other multiplier options are enabled.

`-mmul16'
`-mno-mul16'
     Enable or disable use of the 16-bit integer multiplier option.
     When enabled, the compiler will generate 16-bit multiply
     instructions for multiplications of 16 bits or smaller in standard
     C code.  When this option is disabled, the compiler will either
     use 32-bit multiply or MAC16 instructions if they are available or
     generate library calls to perform the multiply operations using
     shifts and adds.

`-mmul32'
`-mno-mul32'
     Enable or disable use of the 32-bit integer multiplier option.
     When enabled, the compiler will generate 32-bit multiply
     instructions for multiplications of 32 bits or smaller in standard
     C code.  When this option is disabled, the compiler will generate
     library calls to perform the multiply operations using either
     shifts and adds or 16-bit multiply instructions if they are
     available.

`-mnsa'
`-mno-nsa'
     Enable or disable use of the optional normalization shift amount
     (`NSA') instructions to implement the built-in `ffs' function.

`-mminmax'
`-mno-minmax'
     Enable or disable use of the optional minimum and maximum value
     instructions.

`-msext'
`-mno-sext'
     Enable or disable use of the optional sign extend (`SEXT')
     instruction.

`-mbooleans'
`-mno-booleans'
     Enable or disable support for the boolean register file used by
     Xtensa coprocessors.  This is not typically useful by itself but
     may be required for other options that make use of the boolean
     registers (e.g., the floating-point option).

`-mhard-float'
`-msoft-float'
     Enable or disable use of the floating-point option.  When enabled,
     GCC generates floating-point instructions for 32-bit `float'
     operations.  When this option is disabled, GCC generates library
     calls to emulate 32-bit floating-point operations using integer
     instructions.  Regardless of this option, 64-bit `double'
     operations are always emulated with calls to library functions.

`-mfused-madd'
`-mno-fused-madd'
     Enable or disable use of fused multiply/add and multiply/subtract
     instructions in the floating-point option.  This has no effect if
     the floating-point option is not also enabled.  Disabling fused
     multiply/add and multiply/subtract instructions forces the
     compiler to use separate instructions for the multiply and
     add/subtract operations.  This may be desirable in some cases
     where strict IEEE 754-compliant results are required: the fused
     multiply add/subtract instructions do not round the intermediate
     result, thereby producing results with _more_ bits of precision
     than specified by the IEEE standard.  Disabling fused multiply
     add/subtract instructions also ensures that the program output is
     not sensitive to the compiler's ability to combine multiply and
     add/subtract operations.

`-mserialize-volatile'
`-mno-serialize-volatile'
     When this option is enabled, GCC inserts `MEMW' instructions before
     `volatile' memory references to guarantee sequential consistency.
     The default is `-mserialize-volatile'.  Use
     `-mno-serialize-volatile' to omit the `MEMW' instructions.

`-mtext-section-literals'
`-mno-text-section-literals'
     Control the treatment of literal pools.  The default is
     `-mno-text-section-literals', which places literals in a separate
     section in the output file.  This allows the literal pool to be
     placed in a data RAM/ROM, and it also allows the linker to combine
     literal pools from separate object files to remove redundant
     literals and improve code size.  With `-mtext-section-literals',
     the literals are interspersed in the text section in order to keep
     them as close as possible to their references.  This may be
     necessary for large assembly files.

`-mtarget-align'
`-mno-target-align'
     When this option is enabled, GCC instructs the assembler to
     automatically align instructions to reduce branch penalties at the
     expense of some code density.  The assembler attempts to widen
     density instructions to align branch targets and the instructions
     following call instructions.  If there are not enough preceding
     safe density instructions to align a target, no widening will be
     performed.  The default is `-mtarget-align'.  These options do not
     affect the treatment of auto-aligned instructions like `LOOP',
     which the assembler will always align, either by widening density
     instructions or by inserting no-op instructions.

`-mlongcalls'
`-mno-longcalls'
     When this option is enabled, GCC instructs the assembler to
     translate direct calls to indirect calls unless it can determine
     that the target of a direct call is in the range allowed by the
     call instruction.  This translation typically occurs for calls to
     functions in other source files.  Specifically, the assembler
     translates a direct `CALL' instruction into an `L32R' followed by
     a `CALLX' instruction.  The default is `-mno-longcalls'.  This
     option should be used in programs where the call target can
     potentially be out of range.  This option is implemented in the
     assembler, not the compiler, so the assembly code generated by GCC
     will still show direct call instructions--look at the disassembled
     object code to see the actual instructions.  Note that the
     assembler will use an indirect call for every cross-file call, not
     just those that really will be out of range.

