;; This file contains MIPS instructions that support fixed-point operations.

;; All supported fixed-point modes
(define_mode_iterator FIXED [(QQ "") (HQ "") (SQ "") (DQ "TARGET_64BIT")
			     (UQQ "") (UHQ "") (USQ "") (UDQ "TARGET_64BIT")
			     (HA "") (SA "") (DA "TARGET_64BIT")
			     (UHA "") (USA "") (UDA "TARGET_64BIT")])

;; For signed add/sub with saturation
(define_mode_iterator ADDSUB [(HQ "") (SQ "") (HA "") (SA "") (V2HQ "")
			      (V2HA "")])
(define_mode_attr addsubfmt [(HQ "ph") (SQ "w") (HA "ph") (SA "w")
			     (V2HQ "ph") (V2HA "ph")])

;; For unsigned add/sub with saturation
(define_mode_iterator UADDSUB [(UQQ "ISA_HAS_DSP") (UHQ "ISA_HAS_DSPR2")
			       (UHA "ISA_HAS_DSPR2") (V4UQQ "ISA_HAS_DSP")
			       (V2UHQ "ISA_HAS_DSPR2") (V2UHA "ISA_HAS_DSPR2")])
(define_mode_attr uaddsubfmt [(UQQ "qb") (UHQ "ph") (UHA "ph")
			      (V4UQQ "qb") (V2UHQ "ph") (V2UHA "ph")])

;; For signed multiplication with saturation
(define_mode_iterator MULQ [(V2HQ "ISA_HAS_DSP") (HQ "ISA_HAS_DSP")
			    (SQ "ISA_HAS_DSPR2")])
(define_mode_attr mulqfmt [(V2HQ "ph") (HQ "ph") (SQ "w")])

(define_insn "add<mode>3"
  [(set (match_operand:FIXED 0 "register_operand" "=d")
	(plus:FIXED (match_operand:FIXED 1 "register_operand" "d")
		    (match_operand:FIXED 2 "register_operand" "d")))]
  ""
  "<d>addu\t%0,%1,%2"
  [(set_attr "type" "arith")
   (set_attr "mode" "<IMODE>")])

(define_insn "usadd<mode>3"
  [(parallel
    [(set (match_operand:UADDSUB 0 "register_operand" "=d")
	  (us_plus:UADDSUB (match_operand:UADDSUB 1 "register_operand" "d")
			   (match_operand:UADDSUB 2 "register_operand" "d")))
     (set (reg:CCDSP CCDSP_OU_REGNUM)
	  (unspec:CCDSP [(match_dup 1) (match_dup 2)] UNSPEC_ADDQ_S))])]
  ""
  "addu_s.<uaddsubfmt>\t%0,%1,%2"
  [(set_attr "type" "arith")
   (set_attr "mode" "<IMODE>")])

(define_insn "ssadd<mode>3"
  [(parallel
    [(set (match_operand:ADDSUB 0 "register_operand" "=d")
	  (ss_plus:ADDSUB (match_operand:ADDSUB 1 "register_operand" "d")
			  (match_operand:ADDSUB 2 "register_operand" "d")))
     (set (reg:CCDSP CCDSP_OU_REGNUM)
	  (unspec:CCDSP [(match_dup 1) (match_dup 2)] UNSPEC_ADDQ_S))])]
  "ISA_HAS_DSP"
  "addq_s.<addsubfmt>\t%0,%1,%2"
  [(set_attr "type" "arith")
   (set_attr "mode" "<IMODE>")])

(define_insn "sub<mode>3"
  [(set (match_operand:FIXED 0 "register_operand" "=d")
        (minus:FIXED (match_operand:FIXED 1 "register_operand" "d")
		     (match_operand:FIXED 2 "register_operand" "d")))]
  ""
  "<d>subu\t%0,%1,%2"
  [(set_attr "type" "arith")
   (set_attr "mode" "<IMODE>")])

(define_insn "ussub<mode>3"
  [(parallel
    [(set (match_operand:UADDSUB 0 "register_operand" "=d")
	  (us_minus:UADDSUB (match_operand:UADDSUB 1 "register_operand" "d")
			    (match_operand:UADDSUB 2 "register_operand" "d")))
     (set (reg:CCDSP CCDSP_OU_REGNUM)
	  (unspec:CCDSP [(match_dup 1) (match_dup 2)] UNSPEC_SUBQ_S))])]
  ""
  "subu_s.<uaddsubfmt>\t%0,%1,%2"
  [(set_attr "type" "arith")
   (set_attr "mode" "<IMODE>")])

(define_insn "sssub<mode>3"
  [(parallel
    [(set (match_operand:ADDSUB 0 "register_operand" "=d")
	  (ss_minus:ADDSUB (match_operand:ADDSUB 1 "register_operand" "d")
			   (match_operand:ADDSUB 2 "register_operand" "d")))
     (set (reg:CCDSP CCDSP_OU_REGNUM)
	  (unspec:CCDSP [(match_dup 1) (match_dup 2)] UNSPEC_SUBQ_S))])]
  "ISA_HAS_DSP"
  "subq_s.<addsubfmt>\t%0,%1,%2"
  [(set_attr "type" "arith")
   (set_attr "mode" "<IMODE>")])

(define_insn "ssmul<mode>3"
  [(parallel
    [(set (match_operand:MULQ 0 "register_operand" "=d")
          (ss_mult:MULQ (match_operand:MULQ 1 "register_operand" "d")
			(match_operand:MULQ 2 "register_operand" "d")))
     (set (reg:CCDSP CCDSP_OU_REGNUM)
          (unspec:CCDSP [(match_dup 1) (match_dup 2)] UNSPEC_MULQ_RS_PH))
     (clobber (match_scratch:DI 3 "=x"))])]
  ""
  "mulq_rs.<mulqfmt>\t%0,%1,%2"
  [(set_attr "type"     "imul3")
   (set_attr "mode"     "<IMODE>")])

(define_insn "ssmaddsqdq4"
  [(parallel
    [(set (match_operand:DQ 0 "register_operand" "=a")
	  (ss_plus:DQ
	  (ss_mult:DQ (sat_fract:DQ (match_operand:SQ 1
				     "register_operand" "d"))
                      (sat_fract:DQ (match_operand:SQ 2
				     "register_operand" "d")))
          (match_operand:DQ 3 "register_operand" "0")))
     (set (reg:CCDSP CCDSP_OU_REGNUM)
	  (unspec:CCDSP [(match_dup 1) (match_dup 2) (match_dup 3)]
			UNSPEC_DPAQ_SA_L_W))])]
  "ISA_HAS_DSP && !TARGET_64BIT"
  "dpaq_sa.l.w\t%q0,%1,%2"
  [(set_attr "type" "imadd")
   (set_attr "mode" "SI")])

(define_insn "ssmsubsqdq4"
  [(parallel
    [(set (match_operand:DQ 0 "register_operand" "=a")
          (ss_minus:DQ
	   (match_operand:DQ 3 "register_operand" "0")
           (ss_mult:DQ (sat_fract:DQ (match_operand:SQ 1
				      "register_operand" "d"))
                       (sat_fract:DQ (match_operand:SQ 2
				      "register_operand" "d")))))
     (set (reg:CCDSP CCDSP_OU_REGNUM)
	  (unspec:CCDSP [(match_dup 1) (match_dup 2) (match_dup 3)]
			UNSPEC_DPSQ_SA_L_W))])]
  "ISA_HAS_DSP && !TARGET_64BIT"
  "dpsq_sa.l.w\t%q0,%1,%2"
  [(set_attr "type" "imadd")
   (set_attr "mode" "SI")])
