This directory contains minimal loader utilities that talk to Fujitsu's
boot monitor.

aload:	Download using a serial line.
	Syntax is "aload <program> <device>", where <device> is the
	serial port, such as /dev/ttya.

eload:	Download using Ethernet.
	Syntax is "eload <program> <host>", where <host> is a host name
	or IP address.
