libao documentation | libao version 1.2.0 - 201401271

# ao_plugin_open

declared in "ao/plugin.h";

Open the device for playback. All of the device options will have already been set by previous calls to ao_plugin_set_option(). If this is a file output driver, the file itself will have be already opened and a pointer to a `FILE` structure stored in `device->file`.

If the plugin wishes to support automatic channel mapping, but it was not possible to set `device->output_matrix` in ao_plugin_device_init(), the plugin should now set `device->inter_matrix` to the channel ordering that will be expected for buffers submitted to ao_plugin_play().

Plugins should use `device->output_channels` to determine the number of output channels to configure, not `format->channels`. `device->output_channels` is the number of channels libao will be submitting upon each call to ao_plugin_play(). A plugin may alter the value of `device->output_channels` to demand a different number of channels if necessary (such as if a plugin is manufacturing a channel mapping manually).

    int ao_plugin_open(ao_device *device, ao_sample_format *format);

### Parameters

device
  Pointer to pre-allocated device structure. The plugin should set its desired byte format in `device->driver_byte_format`.
format
  Output device sample format. `format->byte_format` should be ignored as it is relevant only to the library core. `format->channels` is relevant only if a plugin is constructing a channel mapping manually; otherwise `device->output` should be used as it is the actual number of channels that will be sent to ao_plugin_play().

### Return Values

> - 1 indicates success.
> - 0 indicates failure to open the device. ao_plugin_device_clear() should be called to ensure the deallocate of all private data structures.

copyright © 2001-2003 Stan Seibert, 2010-2011 Monty | xiph.org monty@xiph.org
libao documentation | libao version 1.2.0 - 201401271