;;- Machine description for GNU compiler, Motorola 68000 Version
;;  Copyright (C) 1987-2014 Free Software Foundation, Inc.

;; This file is part of GCC.

;; GCC is free software; you can redistribute it and/or modify
;; it under the terms of the GNU General Public License as published by
;; the Free Software Foundation; either version 3, or (at your option)
;; any later version.

;; GCC is distributed in the hope that it will be useful,
;; but WITHOUT ANY WARRANTY; without even the implied warranty of
;; MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
;; GNU General Public License for more details.

;; You should have received a copy of the GNU General Public License
;; along with GCC; see the file COPYING3.  If not see
;; <http://www.gnu.org/licenses/>.

;;- Information about MCF5200 port.

;;- The MCF5200 "ColdFire" architecture is a reduced version of the
;;- 68k ISA.  Differences include reduced support for byte and word
;;- operands and the removal of BCD, bitfield, rotate, and integer
;;- divide instructions.  The TARGET_COLDFIRE flag turns the use of the
;;- removed opcodes and addressing modes off.
;;- 


;;- instruction definitions

;;- @@The original PO technology requires these to be ordered by speed,
;;- @@    so that assigner will pick the fastest.

;;- See file "rtl.def" for documentation on define_insn, match_*, et. al.

;;- When naming insn's (operand 0 of define_insn) be careful about using
;;- names from other targets machine descriptions.

;;- cpp macro #define NOTICE_UPDATE_CC in file tm.h handles condition code
;;- updates for most instructions.

;;- Operand classes for the register allocator:
;;- 'a' one of the address registers can be used.
;;- 'd' one of the data registers can be used.
;;- 'f' one of the m68881/fpu registers can be used
;;- 'r' either a data or an address register can be used.

;;- Immediate Floating point operator constraints
;;- 'G' a floating point constant that is *NOT* one of the standard
;;   68881 constant values (to force calling output_move_const_double
;;   to get it from rom if it is a 68881 constant).
;;
;;   See the functions standard_XXX_constant_p in output-m68k.c for more
;; info.

;;- Immediate integer operand constraints:
;;- 'I'  1 .. 8
;;- 'J'  -32768 .. 32767
;;- 'K'  all integers EXCEPT -128 .. 127
;;- 'L'  -8 .. -1
;;- 'M'  all integers EXCEPT -256 .. 255
;;- 'N'  24 .. 31
;;- 'O'  16
;;- 'P'  8 .. 15

;;- Assembler specs:
;;- "%."    size separator ("." or "")			move%.l d0,d1
;;- "%-"    push operand "sp@-"				move%.l d0,%-
;;- "%+"    pop operand "sp@+"				move%.l d0,%+
;;- "%@"    top of stack "sp@"				move%.l d0,%@
;;- "%!"    fpcr register
;;- "%$"    single-precision fp specifier ("s" or "")	f%$add.x fp0,fp1
;;- "%&"    double-precision fp specifier ("d" or "")	f%&add.x fp0,fp1

;;- Information about 68040 port.

;;- The 68040 executes all 68030 and 68881/2 instructions, but some must
;;- be emulated in software by the OS.  It is faster to avoid these
;;- instructions and issue a library call rather than trapping into
;;- the kernel.  The affected instructions are fintrz and fscale.  The
;;- TUNE_68040 flag turns the use of the opcodes off.

;;- The '040 also implements a set of new floating-point instructions
;;- which specify the rounding precision in the opcode.  This finally
;;- permit the 68k series to be truly IEEE compliant, and solves all
;;- issues of excess precision accumulating in the extended registers.
;;- By default, GCC does not use these instructions, since such code will
;;- not run on an '030.  To use these instructions, use the -m68040-only
;;- switch.

;;- These new instructions aren't directly in the md.  They are brought
;;- into play by defining "%$" and "%&" to expand to "s" and "d" rather
;;- than "".

;;- Information about 68060 port.

;;- The 68060 executes all 68030 and 68881/2 instructions, but some must
;;- be emulated in software by the OS.  It is faster to avoid these
;;- instructions and issue a library call rather than trapping into
;;- the kernel.  The affected instructions are: divs.l <ea>,Dr:Dq;
;;- divu.l <ea>,Dr:Dq; muls.l <ea>,Dr:Dq; mulu.l <ea>,Dr:Dq; and
;;- fscale.  The TUNE_68060 flag turns the use of the opcodes off.

;;- Some of these insn's are composites of several m68000 op codes.
;;- The assembler (or final @@??) insures that the appropriate one is
;;- selected.

;; UNSPEC usage:

(define_constants
  [(UNSPEC_SIN 1)
   (UNSPEC_COS 2)
   (UNSPEC_GOT 3)
   (UNSPEC_IB 4)
   (UNSPEC_TIE 5)
   (UNSPEC_RELOC16 6)
   (UNSPEC_RELOC32 7)
  ])

;; UNSPEC_VOLATILE usage:

(define_constants
  [(UNSPECV_BLOCKAGE	0)
   (UNSPECV_CAS_1	1)
   (UNSPECV_CAS_2	2)
   (UNSPECV_TAS_1	3)
   (UNSPECV_TAS_2	4)
  ])

;; Registers by name.
(define_constants
  [(D0_REG		0)
   (A0_REG		8)
   (A1_REG		9)
   (PIC_REG		13)
   (A6_REG		14)
   (SP_REG		15)
   (FP0_REG		16)
  ])

(include "predicates.md")
(include "constraints.md")

;; ::::::::::::::::::::
;; ::
;; :: Attributes
;; ::
;; ::::::::::::::::::::

;; Processor type.
(define_attr "cpu" "cfv1, cfv2, cfv3, cfv4, unknown"
  (const (symbol_ref "m68k_sched_cpu")))

;; MAC type.
(define_attr "mac" "no, cf_mac, cf_emac"
  (const (symbol_ref "m68k_sched_mac")))

;; Instruction type for use in scheduling description.
;; _l and _w suffixes indicate size of the operands of instruction.
;; alu - usual arithmetic or logic instruction.
;; aluq - arithmetic or logic instruction which has a quick immediate (the one
;;        that is encoded in the instruction word) for its Y operand.
;; alux - Arithmetic instruction that uses carry bit (e.g., addx and subx).
;; bcc - conditional branch.
;; bitr - bit operation that only updates flags.
;; bitrw - bit operation that updates flags and output operand.
;; bra, bsr, clr, cmp, div, ext - corresponding instruction.
;; falu, fbcc, fcmp, fdiv, fmove, fmul, fneg, fsqrt, ftst - corresponding
;;                                                          instruction.
;; ib - fake instruction to subscribe slots in ColdFire V1,V2,V3 instruction
;;      buffer.
;; ignore - fake instruction.
;; jmp, jsr, lea, link, mov3q, move, moveq, mul - corresponding instruction.
;; mvsz - mvs or mvz instruction.
;; neg, nop, pea, rts, scc - corresponding instruction.
;; shift - arithmetic or logical shift instruction.
;; trap, tst, unlk - corresponding instruction.
(define_attr "type"
  "alu_l,aluq_l,alux_l,bcc,bitr,bitrw,bra,bsr,clr,clr_l,cmp,cmp_l,
   div_w,div_l,ext,
   falu,fbcc,fcmp,fdiv,fmove,fmul,fneg,fsqrt,ftst,
   ib,ignore,
   jmp,jsr,lea,link,mov3q_l,move,move_l,moveq_l,mul_w,mul_l,mvsz,neg_l,nop,
   pea,rts,scc,shift,
   trap,tst,tst_l,unlk,
   unknown"
  (const_string "unknown"))

;; Index of the X or Y operand in recog_data.operand[].
;; Should be used only within opx_type and opy_type.
(define_attr "opx" "" (const_int 0))
(define_attr "opy" "" (const_int 1))

;; Type of the Y operand.
;; See m68k.c: enum attr_op_type.
(define_attr "opy_type"
  "none,Rn,FPn,mem1,mem234,mem5,mem6,mem7,imm_q,imm_w,imm_l"
  (cond [(eq_attr "type" "ext,fbcc,ftst,neg_l,bcc,bra,bsr,clr,clr_l,ib,ignore,
                          jmp,jsr,nop,rts,scc,trap,tst,tst_l,
                          unlk,unknown") (const_string "none")
	 (eq_attr "type" "lea,pea")
	 (symbol_ref "m68k_sched_attr_opy_type (insn, 1)")]
	(symbol_ref "m68k_sched_attr_opy_type (insn, 0)")))

;; Type of the X operand.
;; See m68k.c: enum attr_op_type.
(define_attr "opx_type"
  "none,Rn,FPn,mem1,mem234,mem5,mem6,mem7,imm_q,imm_w,imm_l"
  (cond [(eq_attr "type" "ib,ignore,nop,rts,trap,unlk,
                          unknown") (const_string "none")
	 (eq_attr "type" "pea") (const_string "mem1")
	 (eq_attr "type" "jmp,jsr")
	 (symbol_ref "m68k_sched_attr_opx_type (insn, 1)")]
	(symbol_ref "m68k_sched_attr_opx_type (insn, 0)")))

;; Access to the X operand: none, read, write, read/write, unknown.
;; Access to the Y operand is either none (if opy_type is none)
;; or read otherwise.
(define_attr "opx_access" "none, r, w, rw"
  (cond [(eq_attr "type" "ib,ignore,nop,rts,trap,unlk,
                          unknown") (const_string "none")
	 (eq_attr "type" "bcc,bra,bsr,bitr,cmp,cmp_l,fbcc,fcmp,ftst,
                          jmp,jsr,tst,tst_l") (const_string "r")
	 (eq_attr "type" "clr,clr_l,fneg,fmove,lea,
                          mov3q_l,move,move_l,moveq_l,mvsz,
                          pea,scc") (const_string "w")
	 (eq_attr "type" "alu_l,aluq_l,alux_l,bitrw,div_w,div_l,ext,
                          falu,fdiv,fmul,fsqrt,link,mul_w,mul_l,
                          neg_l,shift") (const_string "rw")]
	;; Should never be used.
	(symbol_ref "(gcc_unreachable (), OPX_ACCESS_NONE)")))

;; Memory accesses of the insn.
;; 00 - no memory references
;; 10 - memory is read
;; i0 - indexed memory is read
;; 01 - memory is written
;; 0i - indexed memory is written
;; 11 - memory is read, memory is written
;; i1 - indexed memory is read, memory is written
;; 1i - memory is read, indexed memory is written
(define_attr "op_mem" "00, 10, i0, 01, 0i, 11, i1, 1i"
  (symbol_ref "m68k_sched_attr_op_mem (insn)"))

;; Instruction size in words.
(define_attr "size" "1,2,3"
  (symbol_ref "m68k_sched_attr_size (insn)"))

;; Alternative is OK for ColdFire.
(define_attr "ok_for_coldfire" "yes,no" (const_string "yes"))

;; Define 'enabled' attribute.
(define_attr "enabled" ""
  (cond [(and (match_test "TARGET_COLDFIRE")
	      (eq_attr "ok_for_coldfire" "no"))
	 (const_int 0)]
 	(const_int 1)))

;; Mode macros for integer operations.
(define_mode_iterator I [QI HI SI])
(define_mode_attr sz [(QI "%.b") (HI "%.w") (SI "%.l")])

;; Mode macros for floating point operations.
;; Valid floating point modes
(define_mode_iterator FP [SF DF (XF "TARGET_68881")])
;; Mnemonic infix to round result
(define_mode_attr round [(SF "%$") (DF "%&") (XF "")])
;; Mnemonic infix to round result for mul or div instruction
(define_mode_attr round_mul [(SF "sgl") (DF "%&") (XF "")])
;; Suffix specifying source operand format
(define_mode_attr prec [(SF "s") (DF "d") (XF "x")])
;; Allowable D registers
(define_mode_attr dreg [(SF "d") (DF "") (XF "")])
;; Allowable 68881 constant constraints
(define_mode_attr const [(SF "F") (DF "G") (XF "")])


(define_insn_and_split "*movdf_internal"
  [(set (match_operand:DF 0 "push_operand"   "=m, m")
	(match_operand:DF 1 "general_operand" "f, ro<>E"))]
  ""
  "@
   fmove%.d %f1,%0
   #"
  "&& reload_completed && (extract_constrain_insn_cached (insn), which_alternative == 1)"
  [(const_int 0)]
{
  m68k_emit_move_double (operands);
  DONE;
}
  [(set_attr "type" "fmove,*")])

(define_insn_and_split "pushdi"
  [(set (match_operand:DI 0 "push_operand" "=m")
	(match_operand:DI 1 "general_operand" "ro<>Fi"))]
  ""
  "#"
  "&& reload_completed"
  [(const_int 0)]
{
  m68k_emit_move_double (operands);
  DONE;
})

;; We don't want to allow a constant operand for test insns because
;; (set (cc0) (const_int foo)) has no mode information.  Such insns will
;; be folded while optimizing anyway.

(define_insn "tstdi"
  [(set (cc0)
	(compare (match_operand:DI 0 "nonimmediate_operand" "am,d")
		 (const_int 0)))
   (clobber (match_scratch:SI 1 "=X,d"))
   (clobber (match_scratch:DI 2 "=d,X"))]
  ""
{
  if (which_alternative == 0)
    {
      rtx xoperands[2];

      xoperands[0] = operands[2];
      xoperands[1] = operands[0];
      output_move_double (xoperands);
      cc_status.flags |= CC_REVERSED; /*|*/
      return "neg%.l %R2\;negx%.l %2";
    }
  if (find_reg_note (insn, REG_DEAD, operands[0]))
    {
      cc_status.flags |= CC_REVERSED; /*|*/
      return "neg%.l %R0\;negx%.l %0";
    }
  else
    /*
       'sub' clears %1, and also clears the X cc bit
       'tst' sets the Z cc bit according to the low part of the DImode operand
       'subx %1' (i.e. subx #0) acts as a (non-existent) tstx on the high part.
    */
    return "sub%.l %1,%1\;tst%.l %R0\;subx%.l %1,%0";
})

;; If you think that the 68020 does not support tstl a0,
;; reread page B-167 of the 68020 manual more carefully.
(define_insn "*tstsi_internal_68020_cf"
  [(set (cc0)
	(compare (match_operand:SI 0 "nonimmediate_operand" "rm")
		 (const_int 0)))]
  "TARGET_68020 || TARGET_COLDFIRE"
  "tst%.l %0"
  [(set_attr "type" "tst_l")])

;; On an address reg, cmpw may replace cmpl.
(define_insn "*tstsi_internal"
  [(set (cc0)
	(compare (match_operand:SI 0 "nonimmediate_operand" "dm,r")
		 (const_int 0)))]
  "!(TARGET_68020 || TARGET_COLDFIRE)"
  "@
   tst%.l %0
   cmp%.w #0,%0"
  [(set_attr "type" "tst_l,cmp")])

;; This can't use an address register, because comparisons
;; with address registers as second operand always test the whole word.
(define_insn "*tsthi_internal"
  [(set (cc0)
	(compare (match_operand:HI 0 "nonimmediate_operand" "dm")
		 (const_int 0)))]
  ""
  "tst%.w %0"
  [(set_attr "type" "tst")])

(define_insn "*tstqi_internal"
  [(set (cc0)
	(compare (match_operand:QI 0 "nonimmediate_operand" "dm")
		 (const_int 0)))]
  ""
  "tst%.b %0"
  [(set_attr "type" "tst")])

(define_insn "tst<mode>_68881"
  [(set (cc0)
	(compare (match_operand:FP 0 "general_operand" "f<FP:dreg>m")
		 (match_operand:FP 1 "const0_operand" "H")))]
  "TARGET_68881"
{
  cc_status.flags = CC_IN_68881;
  if (FP_REG_P (operands[0]))
    return "ftst%.x %0";
  return "ftst%.<FP:prec> %0";
}
  [(set_attr "type" "ftst")])

(define_insn "tst<mode>_cf"
  [(set (cc0)
	(compare (match_operand:FP 0 "general_operand" "f<FP:dreg><Q>U")
		 (match_operand:FP 1 "const0_operand" "H")))]
  "TARGET_COLDFIRE_FPU"
{
  cc_status.flags = CC_IN_68881;
  if (FP_REG_P (operands[0]))
    return "ftst%.d %0";
  return "ftst%.<FP:prec> %0";
}
  [(set_attr "type" "ftst")])


;; compare instructions.

(define_insn "*cmpdi_internal"
 [(set (cc0)
       (compare (match_operand:DI 1 "nonimmediate_operand" "0,d")
                (match_operand:DI 2 "general_operand" "d,0")))
  (clobber (match_scratch:DI 0 "=d,d"))]
  ""
{
  if (rtx_equal_p (operands[0], operands[1]))
    return "sub%.l %R2,%R0\;subx%.l %2,%0";
  else
    {
      cc_status.flags |= CC_REVERSED; /*|*/
      return "sub%.l %R1,%R0\;subx%.l %1,%0";
    }
})

(define_insn "cmpdi"
 [(set (cc0)
       (compare (match_operand:DI 0 "nonimmediate_operand")
                (match_operand:DI 1 "general_operand")))
  (clobber (match_scratch:DI 2))]
  ""
  "")


(define_expand "cbranchdi4"
  [(set (pc)
	(if_then_else (match_operator 0 "ordered_comparison_operator"
		       [(match_operand:DI 1 "nonimmediate_operand")
			(match_operand:DI 2 "general_operand")])
		      (label_ref (match_operand 3 ""))
		      (pc)))]
  ""
{
  if (operands[2] == const0_rtx)
    emit_insn (gen_tstdi (operands[1]));
  else
    emit_insn (gen_cmpdi (operands[1], operands[2]));
  operands[1] = cc0_rtx;
  operands[2] = const0_rtx;
})

(define_expand "cstoredi4"
  [(set (match_operand:QI 0 "register_operand")
	(match_operator:QI 1 "ordered_comparison_operator"
	 [(match_operand:DI 2 "nonimmediate_operand")
	  (match_operand:DI 3 "general_operand")]))]
  ""
{
  if (operands[3] == const0_rtx)
    emit_insn (gen_tstdi (operands[2]));
  else
    emit_insn (gen_cmpdi (operands[2], operands[3]));
  operands[2] = cc0_rtx;
  operands[3] = const0_rtx;
})


(define_expand "cbranchsi4"
  [(set (cc0)
	(compare (match_operand:SI 1 "nonimmediate_operand" "")
		 (match_operand:SI 2 "general_operand" "")))
   (set (pc)
	(if_then_else (match_operator 0 "ordered_comparison_operator"
                       [(cc0) (const_int 0)])
		      (label_ref (match_operand 3 ""))
		      (pc)))]
  ""
  "")

(define_expand "cstoresi4"
  [(set (cc0)
	(compare (match_operand:SI 2 "nonimmediate_operand" "")
		 (match_operand:SI 3 "general_operand" "")))
   (set (match_operand:QI 0 "register_operand")
	(match_operator:QI 1 "ordered_comparison_operator"
         [(cc0) (const_int 0)]))]
  ""
  "")


;; A composite of the cmp, cmpa, cmpi & cmpm m68000 op codes.
(define_insn ""
  [(set (cc0)
        (compare (match_operand:SI 0 "nonimmediate_operand" "rKT,rKs,mSr,mSa,>")
                 (match_operand:SI 1 "general_src_operand" "mSr,mSa,KTr,Ksr,>")))]
  "!TARGET_COLDFIRE"
{
  if (GET_CODE (operands[0]) == MEM && GET_CODE (operands[1]) == MEM)
    return "cmpm%.l %1,%0";
  if (REG_P (operands[1])
      || (!REG_P (operands[0]) && GET_CODE (operands[0]) != MEM))
    {
      cc_status.flags |= CC_REVERSED; /*|*/
      return "cmp%.l %d0,%d1";
    }
  if (ADDRESS_REG_P (operands[0])
      && GET_CODE (operands[1]) == CONST_INT
      && INTVAL (operands[1]) < 0x8000
      && INTVAL (operands[1]) >= -0x8000)
    return "cmp%.w %1,%0";
  return "cmp%.l %d1,%d0";
})

(define_insn "*cmpsi_cf"
  [(set (cc0)
	(compare (match_operand:SI 0 "nonimmediate_operand" "mrKs,r")
		 (match_operand:SI 1 "general_operand" "r,mrKs")))]
  "TARGET_COLDFIRE"
{
  if (REG_P (operands[1])
      || (!REG_P (operands[0]) && GET_CODE (operands[0]) != MEM))
    {
      cc_status.flags |= CC_REVERSED; /*|*/
      return "cmp%.l %d0,%d1";
    }
  return "cmp%.l %d1,%d0";
}
  [(set_attr "type" "cmp_l")])

(define_expand "cbranchhi4"
  [(set (cc0)
	(compare (match_operand:HI 1 "nonimmediate_src_operand" "")
		 (match_operand:HI 2 "m68k_subword_comparison_operand" "")))
   (set (pc)
	(if_then_else (match_operator 0 "ordered_comparison_operator"
                       [(cc0) (const_int 0)])
		      (label_ref (match_operand 3 ""))
		      (pc)))]
  ""
  "")

(define_expand "cstorehi4"
  [(set (cc0)
	(compare (match_operand:HI 2 "nonimmediate_operand" "")
		 (match_operand:HI 3 "m68k_subword_comparison_operand" "")))
   (set (match_operand:QI 0 "register_operand")
	(match_operator:QI 1 "ordered_comparison_operator"
         [(cc0) (const_int 0)]))]
  ""
  "")

(define_insn ""
  [(set (cc0)
        (compare (match_operand:HI 0 "nonimmediate_src_operand" "rnmS,d,n,mS,>")
                 (match_operand:HI 1 "general_src_operand" "d,rnmS,mS,n,>")))]
  "!TARGET_COLDFIRE"
{
  if (GET_CODE (operands[0]) == MEM && GET_CODE (operands[1]) == MEM)
    return "cmpm%.w %1,%0";
  if ((REG_P (operands[1]) && !ADDRESS_REG_P (operands[1]))
      || (!REG_P (operands[0]) && GET_CODE (operands[0]) != MEM))
    {
      cc_status.flags |= CC_REVERSED; /*|*/
      return "cmp%.w %d0,%d1";
    }
  return "cmp%.w %d1,%d0";
})

(define_expand "cbranchqi4"
  [(set (cc0)
	(compare (match_operand:QI 1 "nonimmediate_src_operand" "")
		 (match_operand:QI 2 "m68k_subword_comparison_operand" "")))
   (set (pc)
	(if_then_else (match_operator 0 "ordered_comparison_operator"
                       [(cc0) (const_int 0)])
		      (label_ref (match_operand 3 ""))
		      (pc)))]
  ""
  "")

(define_expand "cstoreqi4"
  [(set (cc0)
	(compare (match_operand:QI 2 "nonimmediate_src_operand" "")
		 (match_operand:QI 3 "m68k_subword_comparison_operand" "")))
   (set (match_operand:QI 0 "register_operand")
	(match_operator:QI 1 "ordered_comparison_operator"
         [(cc0) (const_int 0)]))]
  ""
  "")

(define_insn ""
  [(set (cc0)
        (compare (match_operand:QI 0 "nonimmediate_src_operand" "dn,dmS,>")
                 (match_operand:QI 1 "general_src_operand" "dmS,nd,>")))]
  "!TARGET_COLDFIRE"
{
  if (GET_CODE (operands[0]) == MEM && GET_CODE (operands[1]) == MEM)
    return "cmpm%.b %1,%0";
  if (REG_P (operands[1])
      || (!REG_P (operands[0]) && GET_CODE (operands[0]) != MEM))
    {
      cc_status.flags |= CC_REVERSED; /*|*/
      return "cmp%.b %d0,%d1";
    }
  return "cmp%.b %d1,%d0";
})

(define_expand "cbranch<mode>4"
  [(set (cc0)
	(compare (match_operand:FP 1 "register_operand" "")
		 (match_operand:FP 2 "fp_src_operand" "")))
   (set (pc)
	(if_then_else (match_operator 0 "comparison_operator"
                       [(cc0) (const_int 0)])
		      (label_ref (match_operand 3 ""))
		      (pc)))]
  "TARGET_HARD_FLOAT"
  "")

(define_expand "cstore<mode>4"
  [(set (cc0)
	(compare (match_operand:FP 2 "register_operand" "")
		 (match_operand:FP 3 "fp_src_operand" "")))
   (set (match_operand:QI 0 "register_operand")
	(match_operator:QI 1 "m68k_cstore_comparison_operator"
         [(cc0) (const_int 0)]))]
  "TARGET_HARD_FLOAT && !(TUNE_68060 || TARGET_COLDFIRE_FPU)"
  "if (TARGET_COLDFIRE && operands[2] != const0_rtx)
     FAIL;")

(define_insn "*cmp<mode>_68881"
  [(set (cc0)
	(compare (match_operand:FP 0 "fp_src_operand" "f,f,<FP:dreg>mF")
		 (match_operand:FP 1 "fp_src_operand" "f,<FP:dreg>mF,f")))]
  "TARGET_68881
   && (register_operand (operands[0], <MODE>mode)
       || register_operand (operands[1], <MODE>mode))"
  "@
   fcmp%.x %1,%0
   fcmp%.<FP:prec> %f1,%0
   fcmp%.<FP:prec> %0,%f1"
  [(set_attr "type" "fcmp")])

(define_insn "*cmp<mode>_cf"
  [(set (cc0)
	(compare (match_operand:FP 0 "fp_src_operand" "f,f,<FP:dreg><Q>U")
		 (match_operand:FP 1 "fp_src_operand" "f,<FP:dreg><Q>U,f")))]
  "TARGET_COLDFIRE_FPU
   && (register_operand (operands[0], <MODE>mode)
       || register_operand (operands[1], <MODE>mode))"
  "@
   fcmp%.d %1,%0
   fcmp%.<FP:prec> %f1,%0
   fcmp%.<FP:prec> %0,%f1"
  [(set_attr "type" "fcmp")])

;; Recognizers for btst instructions.

;; ColdFire/5200 only allows "<Q>" type addresses when the bit position is
;; specified as a constant, so we must disable all patterns that may extract
;; from a MEM at a constant bit position if we can't use this as a constraint.

(define_insn ""
  [(set
    (cc0)
    (compare (zero_extract:SI (match_operand:QI 0 "memory_src_operand" "oS")
			       (const_int 1)
			       (minus:SI (const_int 7)
				         (match_operand:SI 1 "general_operand" "di")))
	     (const_int 0)))]
  "!TARGET_COLDFIRE"
{
  return output_btst (operands, operands[1], operands[0], insn, 7);
})

;; This is the same as the above pattern except for the constraints.  The 'i'
;; has been deleted.

(define_insn ""
  [(set
    (cc0)
    (compare (zero_extract:SI (match_operand:QI 0 "memory_operand" "o")
			       (const_int 1)
			       (minus:SI (const_int 7)
				         (match_operand:SI 1 "general_operand" "d")))
	     (const_int 0)))]
  "TARGET_COLDFIRE"
{
  return output_btst (operands, operands[1], operands[0], insn, 7);
})

(define_insn ""
  [(set
    (cc0)
    (compare (zero_extract:SI (match_operand:SI 0 "register_operand" "d")
			       (const_int 1)
			       (minus:SI (const_int 31)
				         (match_operand:SI 1 "general_operand" "di")))
	     (const_int 0)))]
  ""
{
  return output_btst (operands, operands[1], operands[0], insn, 31);
})

;; The following two patterns are like the previous two
;; except that they use the fact that bit-number operands
;; are automatically masked to 3 or 5 bits.

(define_insn ""
  [(set
    (cc0)
    (compare (zero_extract:SI (match_operand:QI 0 "memory_operand" "o")
			       (const_int 1)
			       (minus:SI (const_int 7)
				         (and:SI
				          (match_operand:SI 1 "register_operand" "d")
				          (const_int 7))))
	     (const_int 0)))]
  ""
{
  return output_btst (operands, operands[1], operands[0], insn, 7);
})

(define_insn ""
  [(set
    (cc0)
    (compare (zero_extract:SI (match_operand:SI 0 "register_operand" "d")
			       (const_int 1)
			       (minus:SI (const_int 31)
				         (and:SI
				          (match_operand:SI 1 "register_operand" "d")
				          (const_int 31))))
	     (const_int 0)))]
  ""
{
  return output_btst (operands, operands[1], operands[0], insn, 31);
})

;; Nonoffsettable mem refs are ok in this one pattern
;; since we don't try to adjust them.
(define_insn ""
  [(set
    (cc0)
    (compare (zero_extract:SI (match_operand:QI 0 "memory_operand" "m")
			      (const_int 1)
			      (match_operand:SI 1 "const_int_operand" "n"))
	     (const_int 0)))]
  "(unsigned) INTVAL (operands[1]) < 8 && !TARGET_COLDFIRE"
{
  operands[1] = GEN_INT (7 - INTVAL (operands[1]));
  return output_btst (operands, operands[1], operands[0], insn, 7);
})

(define_insn ""
  [(set
    (cc0)
    (compare (zero_extract:SI (match_operand:SI 0 "register_operand" "do")
			      (const_int 1)
			    (match_operand:SI 1 "const_int_operand" "n"))
	     (const_int 0)))]
  "!TARGET_COLDFIRE"
{
  if (GET_CODE (operands[0]) == MEM)
    {
      operands[0] = adjust_address (operands[0], QImode,
				    INTVAL (operands[1]) / 8);
      operands[1] = GEN_INT (7 - INTVAL (operands[1]) % 8);
      return output_btst (operands, operands[1], operands[0], insn, 7);
    }
  operands[1] = GEN_INT (31 - INTVAL (operands[1]));
  return output_btst (operands, operands[1], operands[0], insn, 31);
})

;; This is the same as the above pattern except for the constraints.
;; The 'o' has been replaced with 'Q'.

(define_insn ""
  [(set
    (cc0)
    (compare (zero_extract:SI (match_operand:SI 0 "register_operand" "dQ")
			      (const_int 1)
			      (match_operand:SI 1 "const_int_operand" "n"))
	     (const_int 0)))]
  "TARGET_COLDFIRE"
{
  if (GET_CODE (operands[0]) == MEM)
    {
      operands[0] = adjust_address (operands[0], QImode,
				    INTVAL (operands[1]) / 8);
      operands[1] = GEN_INT (7 - INTVAL (operands[1]) % 8);
      return output_btst (operands, operands[1], operands[0], insn, 7);
    }
  operands[1] = GEN_INT (31 - INTVAL (operands[1]));
  return output_btst (operands, operands[1], operands[0], insn, 31);
})


;; move instructions

;; A special case in which it is not desirable
;; to reload the constant into a data register.
(define_insn "pushexthisi_const"
  [(set (match_operand:SI 0 "push_operand" "=m,m,m")
	(match_operand:SI 1 "const_int_operand" "C0,R,J"))]
  "INTVAL (operands[1]) >= -0x8000 && INTVAL (operands[1]) < 0x8000"
  "@
   clr%.l %0
   mov3q%.l %1,%-
   pea %a1"
  [(set_attr "type" "clr_l,mov3q_l,pea")])

;This is never used.
;(define_insn "swapsi"
;  [(set (match_operand:SI 0 "nonimmediate_operand" "+r")
;	(match_operand:SI 1 "general_operand" "+r"))
;   (set (match_dup 1) (match_dup 0))]
;  ""
;  "exg %1,%0")

;; Special case of fullword move when source is zero for 68000_10.
;; moveq is faster on the 68000.
(define_insn "*movsi_const0_68000_10"
  [(set (match_operand:SI 0 "movsi_const0_operand" "=d,a,g")
	(const_int 0))]
  "TUNE_68000_10"
  "@
   moveq #0,%0
   sub%.l %0,%0
   clr%.l %0"
  [(set_attr "type" "moveq_l,alu_l,clr_l")
   (set_attr "opy" "*,0,*")])

;; Special case of fullword move when source is zero for 68040_60.
;; On the '040, 'subl an,an' takes 2 clocks while lea takes only 1
(define_insn "*movsi_const0_68040_60"
  [(set (match_operand:SI 0 "movsi_const0_operand" "=a,g")
	(const_int 0))]
  "TUNE_68040_60"
{
  if (which_alternative == 0)
    return MOTOROLA ? "lea 0.w,%0" : "lea 0:w,%0";
  else if (which_alternative == 1)
    return "clr%.l %0";
  else
    {
      gcc_unreachable ();
      return "";
    }
}
  [(set_attr "type" "lea,clr_l")])

;; Special case of fullword move when source is zero.
(define_insn "*movsi_const0"
  [(set (match_operand:SI 0 "movsi_const0_operand" "=a,g")
	(const_int 0))]
  "!(TUNE_68000_10 || TUNE_68040_60)"
  "@
   sub%.l %0,%0
   clr%.l %0"
  [(set_attr "type" "alu_l,clr_l")
   (set_attr "opy" "0,*")])

;; General case of fullword move.
;;
;; This is the main "hook" for PIC code.  When generating
;; PIC, movsi is responsible for determining when the source address
;; needs PIC relocation and appropriately calling legitimize_pic_address
;; to perform the actual relocation.
;;
;; In both the PIC and non-PIC cases the patterns generated will
;; matched by the next define_insn.
(define_expand "movsi"
  [(set (match_operand:SI 0 "" "")
	(match_operand:SI 1 "" ""))]
  ""
{
  rtx tmp, base, offset;

  /* Recognize the case where operand[1] is a reference to thread-local
     data and load its address to a register.  */
  if (!TARGET_PCREL && m68k_tls_reference_p (operands[1], false))
    {
      rtx tmp = operands[1];
      rtx addend = NULL;

      if (GET_CODE (tmp) == CONST && GET_CODE (XEXP (tmp, 0)) == PLUS)
        {
          addend = XEXP (XEXP (tmp, 0), 1);
          tmp = XEXP (XEXP (tmp, 0), 0);
        }

      gcc_assert (GET_CODE (tmp) == SYMBOL_REF);
      gcc_assert (SYMBOL_REF_TLS_MODEL (tmp) != 0);

      tmp = m68k_legitimize_tls_address (tmp);

      if (addend)
        {
	  if (!REG_P (tmp))
	    {
	      rtx reg;

	      reg = gen_reg_rtx (Pmode);
	      emit_move_insn (reg, tmp);
	      tmp = reg;
	    }

          tmp = gen_rtx_PLUS (SImode, tmp, addend);
	}

      operands[1] = tmp;
    }
  else if (flag_pic && !TARGET_PCREL && symbolic_operand (operands[1], SImode))
    {
      /* The source is an address which requires PIC relocation.
         Call legitimize_pic_address with the source, mode, and a relocation
         register (a new pseudo, or the final destination if reload_in_progress
         is set).   Then fall through normally */
      rtx temp = reload_in_progress ? operands[0] : gen_reg_rtx (Pmode);
      operands[1] = legitimize_pic_address (operands[1], SImode, temp);
    }
  else if (flag_pic && TARGET_PCREL && ! reload_in_progress)
    {
      /* Don't allow writes to memory except via a register;
	 the m68k doesn't consider PC-relative addresses to be writable.  */
      if (symbolic_operand (operands[0], SImode))
	operands[0] = force_reg (SImode, XEXP (operands[0], 0));
      else if (GET_CODE (operands[0]) == MEM
	       && symbolic_operand (XEXP (operands[0], 0), SImode))
	operands[0] = gen_rtx_MEM (SImode,
			       force_reg (SImode, XEXP (operands[0], 0)));
    }
  if (M68K_OFFSETS_MUST_BE_WITHIN_SECTIONS_P)
    {
      split_const (operands[1], &base, &offset);
      if (GET_CODE (base) == SYMBOL_REF
	  && !offset_within_block_p (base, INTVAL (offset)))
	{
	  tmp = !can_create_pseudo_p () ? operands[0] : gen_reg_rtx (SImode);
	  emit_move_insn (tmp, base);
	  emit_insn (gen_addsi3 (operands[0], tmp, offset));
	  DONE;
	}
    }
})

;; General case of fullword move.
(define_insn "*movsi_m68k"
  ;; Notes: make sure no alternative allows g vs g.
  ;; We don't allow f-regs since fixed point cannot go in them.
  [(set (match_operand:SI 0 "nonimmediate_operand" "=g,d,a<")
        (match_operand:SI 1 "general_src_operand" "damSnT,n,i"))]
  "!TARGET_COLDFIRE && reload_completed"
{
  return output_move_simode (operands);
})

;; Before reload is completed the register constraints
;; force integer constants in range for a moveq to be reloaded
;; if they are headed for memory.
(define_insn "*movsi_m68k2"
  [(set (match_operand:SI 0 "nonimmediate_operand" "=g,d,a<")
        (match_operand:SI 1 "general_src_operand" "damSKT,n,i"))]

  "!TARGET_COLDFIRE"
{
  return output_move_simode (operands);
})

;; ColdFire move instructions can have at most one operand of mode >= 6.
(define_insn "*movsi_cf"
  [(set (match_operand:SI 0 "nonimmediate_operand" "=g,d, d, d, d, d, a,Ap,  a,  r<Q>,g,    U")
	(match_operand:SI 1 "general_operand"      " R,CQ,CW,CZ,CS,Ci,J,J Cs,Cs, g,   Rr<Q>,U"))]
  "TARGET_COLDFIRE"
{
  switch (which_alternative)
    {
    case 0:
      return "mov3q%.l %1,%0";

    case 1:
      return "moveq %1,%0";

    case 2:
      {
	unsigned u = INTVAL (operands[1]);

	operands[1] = GEN_INT ((u << 16) | (u >> 16));  /*|*/
	return "moveq %1,%0\n\tswap %0";
      }

    case 3:
      return "mvz%.w %1,%0";

    case 4:
      return "mvs%.w %1,%0";

    case 5:
      return "move%.l %1,%0";

    case 6:
      return "move%.w %1,%0";

    case 7:
      return "pea %a1";

    case 8:
      return "lea %a1,%0";

    case 9:
    case 10:
    case 11:
      return "move%.l %1,%0";

    default:
      gcc_unreachable ();
      return "";
    }
}
  [(set_attr "type" "mov3q_l,moveq_l,*,mvsz,mvsz,move_l,move,pea,lea,move_l,move_l,move_l")])

;; Special case of fullword move, where we need to get a non-GOT PIC
;; reference into an address register.
(define_insn ""
  [(set (match_operand:SI 0 "nonimmediate_operand" "=a<")
        (match_operand:SI 1 "pcrel_address" ""))]
  "TARGET_PCREL"
{
  if (push_operand (operands[0], SImode))
    return "pea %a1";
  return "lea %a1,%0";
})

(define_expand "movhi"
  [(set (match_operand:HI 0 "nonimmediate_operand" "")
	(match_operand:HI 1 "general_operand" ""))]
  ""
  "")

(define_insn ""
  [(set (match_operand:HI 0 "nonimmediate_operand" "=g")
        (match_operand:HI 1 "general_src_operand" "gS"))]
  "!TARGET_COLDFIRE"
  "* return output_move_himode (operands);")

(define_insn ""
  [(set (match_operand:HI 0 "nonimmediate_operand" "=r<Q>,g,U")
	(match_operand:HI 1 "general_operand" "g,r<Q>,U"))]
  "TARGET_COLDFIRE"
  "* return output_move_himode (operands);")

(define_expand "movstricthi"
  [(set (strict_low_part (match_operand:HI 0 "nonimmediate_operand" ""))
        (match_operand:HI 1 "general_src_operand" ""))]
  ""
  "")

(define_insn ""
  [(set (strict_low_part (match_operand:HI 0 "nonimmediate_operand" "+dm"))
	(match_operand:HI 1 "general_src_operand" "rmSn"))]
  "!TARGET_COLDFIRE"
  "* return output_move_stricthi (operands);")

(define_insn ""
  [(set (strict_low_part (match_operand:HI 0 "nonimmediate_operand" "+d,m"))
	(match_operand:HI 1 "general_src_operand" "rmn,r"))]
  "TARGET_COLDFIRE"
  "* return output_move_stricthi (operands);")

(define_expand "movqi"
  [(set (match_operand:QI 0 "nonimmediate_operand" "")
        (match_operand:QI 1 "general_src_operand" ""))]
  ""
  "")

(define_insn ""
  [(set (match_operand:QI 0 "nonimmediate_operand" "=d,*a,m")
	(match_operand:QI 1 "general_src_operand" "dmSi*a,di*a,dmSi"))]
  "!TARGET_COLDFIRE"
  "* return output_move_qimode (operands);")

(define_insn ""
  [(set (match_operand:QI 0 "nonimmediate_operand" "=d<Q>,dm,U,d*a")
	(match_operand:QI 1 "general_src_operand" "dmi,d<Q>,U,di*a"))]
  "TARGET_COLDFIRE"
  "* return output_move_qimode (operands);")

(define_expand "movstrictqi"
  [(set (strict_low_part (match_operand:QI 0 "nonimmediate_operand" ""))
        (match_operand:QI 1 "general_src_operand" ""))]
  ""
  "")

(define_insn ""
  [(set (strict_low_part (match_operand:QI 0 "nonimmediate_operand" "+dm"))
	(match_operand:QI 1 "general_src_operand" "dmSn"))]
  "!TARGET_COLDFIRE"
  "* return output_move_strictqi (operands);")

(define_insn "*movstrictqi_cf"
  [(set (strict_low_part (match_operand:QI 0 "nonimmediate_operand" "+d, Ac, d,m"))
	(match_operand:QI 1 "general_src_operand"                    "C0,C0, dmn,d"))]
  "TARGET_COLDFIRE"
  "@
   clr%.b %0
   clr%.b %0
   move%.b %1,%0
   move%.b %1,%0"
  [(set_attr "type" "clr,clr,move,move")])

(define_expand "pushqi1"
  [(set (reg:SI SP_REG) (plus:SI (reg:SI SP_REG) (const_int -2)))
   (set (mem:QI (plus:SI (reg:SI SP_REG) (const_int 1)))
	(match_operand:QI 0 "general_operand" ""))]
  "!TARGET_COLDFIRE"
  "")

(define_expand "reload_insf"
  [(set (match_operand:SF 0 "nonimmediate_operand" "=f")
        (match_operand:SF 1 "general_operand" "mf"))
   (clobber (match_operand:SI 2 "register_operand" "=&a"))]
  "TARGET_COLDFIRE_FPU"
{
  if (emit_move_sequence (operands, SFmode, operands[2]))
    DONE;

  /* We don't want the clobber emitted, so handle this ourselves. */
  emit_insn (gen_rtx_SET (VOIDmode, operands[0], operands[1]));
  DONE;
})

(define_expand "reload_outsf"
  [(set (match_operand:SF 0 "general_operand" "")
        (match_operand:SF 1 "register_operand" "f"))
   (clobber (match_operand:SI 2 "register_operand" "=&a"))]
  "TARGET_COLDFIRE_FPU"
{
  if (emit_move_sequence (operands, SFmode, operands[2]))
    DONE;

  /* We don't want the clobber emitted, so handle this ourselves. */
  emit_insn (gen_rtx_SET (VOIDmode, operands[0], operands[1]));
  DONE;
})

(define_expand "movsf"
  [(set (match_operand:SF 0 "nonimmediate_operand" "")
	(match_operand:SF 1 "general_operand" ""))]
  ""
  "")

(define_insn ""
  [(set (match_operand:SF 0 "nonimmediate_operand" "=rmf")
	(match_operand:SF 1 "general_operand" "rmfF"))]
  "!TARGET_COLDFIRE"
{
  if (FP_REG_P (operands[0]))
    {
      if (FP_REG_P (operands[1]))
	return "f%$move%.x %1,%0";
      else if (ADDRESS_REG_P (operands[1]))
	return "move%.l %1,%-\;f%$move%.s %+,%0";
      else if (GET_CODE (operands[1]) == CONST_DOUBLE)
	return output_move_const_single (operands);
      return "f%$move%.s %f1,%0";
    }
  if (FP_REG_P (operands[1]))
    {
      if (ADDRESS_REG_P (operands[0]))
	return "fmove%.s %1,%-\;move%.l %+,%0";
      return "fmove%.s %f1,%0";
    }
  if (operands[1] == CONST0_RTX (SFmode)
      /* clr insns on 68000 read before writing.  */
      && ((TARGET_68010 || TARGET_COLDFIRE)
	  || !(GET_CODE (operands[0]) == MEM && MEM_VOLATILE_P (operands[0]))))
    {
      if (ADDRESS_REG_P (operands[0]))
	{
	  /* On the '040, 'subl an,an' takes 2 clocks while lea takes only 1 */
	  if (TUNE_68040_60)
	    return MOTOROLA ? "lea 0.w,%0" : "lea 0:w,%0";
	  else
	    return "sub%.l %0,%0";
	}
      /* moveq is faster on the 68000.  */
      if (DATA_REG_P (operands[0]) && TUNE_68000_10)
	return "moveq #0,%0";
      return "clr%.l %0";
    }
  return "move%.l %1,%0";
})

(define_insn "movsf_cf_soft"
  [(set (match_operand:SF 0 "nonimmediate_operand" "=r<Q>,g,U")
	(match_operand:SF 1 "general_operand" "g,r<Q>,U"))]
  "TARGET_COLDFIRE && !TARGET_COLDFIRE_FPU"
  "move%.l %1,%0"
  [(set_attr "type" "move_l")])

;; SFmode MEMs are restricted to modes 2-4 if TARGET_COLDFIRE_FPU.
;; The move instructions can handle all combinations.
(define_insn "movsf_cf_hard"
  [(set (match_operand:SF 0 "nonimmediate_operand" "=r<Q>U, f,    f,mr,f,r<Q>,f
,m")
        (match_operand:SF 1 "general_operand"      " f,     r<Q>U,f,rm,F,F,   m
,f"))]
  "TARGET_COLDFIRE_FPU"
{
  if (which_alternative == 4 || which_alternative == 5) {
    rtx xoperands[2];
    REAL_VALUE_TYPE r;
    long l;
    REAL_VALUE_FROM_CONST_DOUBLE (r, operands[1]);
    REAL_VALUE_TO_TARGET_SINGLE (r, l);
    xoperands[0] = operands[0];
    xoperands[1] = GEN_INT (l);
    if (which_alternative == 5) {
      if (l == 0) {
        if (ADDRESS_REG_P (xoperands[0]))
          output_asm_insn ("sub%.l %0,%0", xoperands);
        else
          output_asm_insn ("clr%.l %0", xoperands);
      } else
        if (GET_CODE (operands[0]) == MEM
            && symbolic_operand (XEXP (operands[0], 0), SImode))
          output_asm_insn ("move%.l %1,%-;move%.l %+,%0", xoperands);
        else
          output_asm_insn ("move%.l %1,%0", xoperands);
      return "";
    }
    if (l != 0)
      output_asm_insn ("move%.l %1,%-;fsmove%.s %+,%0", xoperands);
    else
      output_asm_insn ("clr%.l %-;fsmove%.s %+,%0", xoperands);
    return "";
  }
  if (FP_REG_P (operands[0]))
    {
      if (ADDRESS_REG_P (operands[1]))
        return "move%.l %1,%-;fsmove%.s %+,%0";
      if (FP_REG_P (operands[1]))
        return "fsmove%.d %1,%0";
      return "fsmove%.s %f1,%0";
    }
  if (FP_REG_P (operands[1]))
    {
      if (ADDRESS_REG_P (operands[0]))
        return "fmove%.s %1,%-;move%.l %+,%0";
      return "fmove%.s %f1,%0";
    }
  if (operands[1] == CONST0_RTX (SFmode))
    {
      if (ADDRESS_REG_P (operands[0]))
	return "sub%.l %0,%0";
      return "clr%.l %0";
    }
  return "move%.l %1,%0";
})

(define_expand "reload_indf"
  [(set (match_operand:DF 0 "nonimmediate_operand" "=f")
        (match_operand:DF 1 "general_operand" "mf"))
   (clobber (match_operand:SI 2 "register_operand" "=&a"))]
  "TARGET_COLDFIRE_FPU"
{
  if (emit_move_sequence (operands, DFmode, operands[2]))
    DONE;

  /* We don't want the clobber emitted, so handle this ourselves. */
  emit_insn (gen_rtx_SET (VOIDmode, operands[0], operands[1]));
  DONE;
})

(define_expand "reload_outdf"
  [(set (match_operand:DF 0 "general_operand" "")
        (match_operand:DF 1 "register_operand" "f"))
   (clobber (match_operand:SI 2 "register_operand" "=&a"))]
  "TARGET_COLDFIRE_FPU"
{
  if (emit_move_sequence (operands, DFmode, operands[2]))
    DONE;

  /* We don't want the clobber emitted, so handle this ourselves. */
  emit_insn (gen_rtx_SET (VOIDmode, operands[0], operands[1]));
  DONE;
})

(define_expand "movdf"
  [(set (match_operand:DF 0 "nonimmediate_operand" "")
	(match_operand:DF 1 "general_operand" ""))]
  ""
{
  if (TARGET_COLDFIRE_FPU)
    if (emit_move_sequence (operands, DFmode, 0))
      DONE;
})

(define_insn ""
  [(set (match_operand:DF 0 "nonimmediate_operand" "=rm,rf,rf,&rof<>")
	(match_operand:DF 1 "general_operand" "*rf,m,0,*rofE<>"))]
;  [(set (match_operand:DF 0 "nonimmediate_operand" "=rm,&rf,&rof<>")
;	(match_operand:DF 1 "general_operand" "rf,m,rofF<>"))]
  "!TARGET_COLDFIRE"
{
  if (FP_REG_P (operands[0]))
    {
      if (FP_REG_P (operands[1]))
	return "f%&move%.x %1,%0";
      if (REG_P (operands[1]))
	{
	  rtx xoperands[2];
	  xoperands[1] = gen_rtx_REG (SImode, REGNO (operands[1]) + 1);
	  output_asm_insn ("move%.l %1,%-", xoperands);
	  output_asm_insn ("move%.l %1,%-", operands);
	  return "f%&move%.d %+,%0";
	}
      if (GET_CODE (operands[1]) == CONST_DOUBLE)
	return output_move_const_double (operands);
      return "f%&move%.d %f1,%0";
    }
  else if (FP_REG_P (operands[1]))
    {
      if (REG_P (operands[0]))
	{
	  output_asm_insn ("fmove%.d %f1,%-\;move%.l %+,%0", operands);
	  operands[0] = gen_rtx_REG (SImode, REGNO (operands[0]) + 1);
	  return "move%.l %+,%0";
	}
      else
        return "fmove%.d %f1,%0";
    }
  return output_move_double (operands);
})

(define_insn_and_split "movdf_cf_soft"
  [(set (match_operand:DF 0 "nonimmediate_operand" "=r,g")
	(match_operand:DF 1 "general_operand" "g,r"))]
  "TARGET_COLDFIRE && !TARGET_COLDFIRE_FPU"
  "#"
  "&& reload_completed"
  [(const_int 0)]
{
  m68k_emit_move_double (operands);
  DONE;
})

(define_insn "movdf_cf_hard"
  [(set (match_operand:DF 0 "nonimmediate_operand" "=f,    <Q>U,r,f,r,r,m,f")
        (match_operand:DF 1 "general_operand"      " f<Q>U,f,   f,r,r,m,r,E"))]
  "TARGET_COLDFIRE_FPU"
{
  rtx xoperands[3];
  REAL_VALUE_TYPE r;
  long l[2];

  switch (which_alternative)
    {
    default:
      return "fdmove%.d %1,%0";
    case 1:
      return "fmove%.d %1,%0";
    case 2:
      return "fmove%.d %1,%-;move%.l %+,%0;move%.l %+,%R0";
    case 3:
      return "move%.l %R1,%-;move%.l %1,%-;fdmove%.d %+,%0";
    case 4: case 5: case 6:
      return output_move_double (operands);
    case 7:
      REAL_VALUE_FROM_CONST_DOUBLE (r, operands[1]);
      REAL_VALUE_TO_TARGET_DOUBLE (r, l);
      xoperands[0] = operands[0];
      xoperands[1] = GEN_INT (l[0]);
      xoperands[2] = GEN_INT (l[1]);
      if (operands[1] == CONST0_RTX (DFmode))
	output_asm_insn ("clr%.l %-;clr%.l %-;fdmove%.d %+,%0",
			xoperands);
      else
	if (l[1] == 0)
	  output_asm_insn ("clr%.l %-;move%.l %1,%-;fdmove%.d %+,%0",
			  xoperands);
	else
	  output_asm_insn ("move%.l %2,%-;move%.l %1,%-;fdmove%.d %+,%0",
			  xoperands);
      return "";
    }
})

;; ??? The XFmode patterns are schizophrenic about whether constants are
;; allowed.  Most but not all have predicates and constraint that disallow
;; constants.  Most but not all have output templates that handle constants.
;; See also TARGET_LEGITIMATE_CONSTANT_P.

(define_expand "movxf"
  [(set (match_operand:XF 0 "nonimmediate_operand" "")
	(match_operand:XF 1 "general_operand" ""))]
  ""
{
  /* We can't rewrite operands during reload.  */
  if (! reload_in_progress)
    {
      if (CONSTANT_P (operands[1]))
	{
	  operands[1] = force_const_mem (XFmode, operands[1]);
	  if (! memory_address_p (XFmode, XEXP (operands[1], 0)))
	    operands[1] = adjust_address (operands[1], XFmode, 0);
	}
      if (flag_pic && TARGET_PCREL)
	{
	  /* Don't allow writes to memory except via a register; the
	     m68k doesn't consider PC-relative addresses to be writable.  */
	  if (GET_CODE (operands[0]) == MEM
	      && symbolic_operand (XEXP (operands[0], 0), SImode))
	    operands[0] = gen_rtx_MEM (XFmode,
				   force_reg (SImode, XEXP (operands[0], 0)));
	}
    }
})

(define_insn ""
  [(set (match_operand:XF 0 "nonimmediate_operand" "=f,m,f,!r,!f,!r,m,!r")
	(match_operand:XF 1 "nonimmediate_operand" "m,f,f,f,r,!r,!r,m"))]
  "TARGET_68881"
{
  if (FP_REG_P (operands[0]))
    {
      if (FP_REG_P (operands[1]))
	return "fmove%.x %1,%0";
      if (REG_P (operands[1]))
	{
	  rtx xoperands[2];
	  xoperands[1] = gen_rtx_REG (SImode, REGNO (operands[1]) + 2);
	  output_asm_insn ("move%.l %1,%-", xoperands);
	  xoperands[1] = gen_rtx_REG (SImode, REGNO (operands[1]) + 1);
	  output_asm_insn ("move%.l %1,%-", xoperands);
	  output_asm_insn ("move%.l %1,%-", operands);
	  return "fmove%.x %+,%0";
	}
      if (GET_CODE (operands[1]) == CONST_DOUBLE)
        return "fmove%.x %1,%0";
      return "fmove%.x %f1,%0";
    }
  if (FP_REG_P (operands[1]))
    {
      if (REG_P (operands[0]))
	{
	  output_asm_insn ("fmove%.x %f1,%-\;move%.l %+,%0", operands);
	  operands[0] = gen_rtx_REG (SImode, REGNO (operands[0]) + 1);
	  output_asm_insn ("move%.l %+,%0", operands);
	  operands[0] = gen_rtx_REG (SImode, REGNO (operands[0]) + 1);
	  return "move%.l %+,%0";
	}
      /* Must be memory destination.  */
      return "fmove%.x %f1,%0";
    }
  return output_move_double (operands);
})

(define_insn ""
  [(set (match_operand:XF 0 "nonimmediate_operand" "=rm,rf,&rof<>")
	(match_operand:XF 1 "nonimmediate_operand" "rf,m,rof<>"))]
  "! TARGET_68881 && ! TARGET_COLDFIRE"
{
  if (FP_REG_P (operands[0]))
    {
      if (FP_REG_P (operands[1]))
	return "fmove%.x %1,%0";
      if (REG_P (operands[1]))
	{
	  rtx xoperands[2];
	  xoperands[1] = gen_rtx_REG (SImode, REGNO (operands[1]) + 2);
	  output_asm_insn ("move%.l %1,%-", xoperands);
	  xoperands[1] = gen_rtx_REG (SImode, REGNO (operands[1]) + 1);
	  output_asm_insn ("move%.l %1,%-", xoperands);
	  output_asm_insn ("move%.l %1,%-", operands);
	  return "fmove%.x %+,%0";
	}
      if (GET_CODE (operands[1]) == CONST_DOUBLE)
        return "fmove%.x %1,%0";
      return "fmove%.x %f1,%0";
    }
  if (FP_REG_P (operands[1]))
    {
      if (REG_P (operands[0]))
        {
          output_asm_insn ("fmove%.x %f1,%-\;move%.l %+,%0", operands);
          operands[0] = gen_rtx_REG (SImode, REGNO (operands[0]) + 1);
          output_asm_insn ("move%.l %+,%0", operands);
          operands[0] = gen_rtx_REG (SImode, REGNO (operands[0]) + 1);
          return "move%.l %+,%0";
        }
      else
        return "fmove%.x %f1,%0";
    }
  return output_move_double (operands);
})

(define_insn ""
  [(set (match_operand:XF 0 "nonimmediate_operand" "=r,g")
	(match_operand:XF 1 "nonimmediate_operand" "g,r"))]
  "! TARGET_68881 && TARGET_COLDFIRE"
  "* return output_move_double (operands);")

(define_expand "movdi"
  ;; Let's see if it really still needs to handle fp regs, and, if so, why.
  [(set (match_operand:DI 0 "nonimmediate_operand" "")
	(match_operand:DI 1 "general_operand" ""))]
  ""
  "")

;; movdi can apply to fp regs in some cases
(define_insn ""
  ;; Let's see if it really still needs to handle fp regs, and, if so, why.
  [(set (match_operand:DI 0 "nonimmediate_operand" "=rm,r,&ro<>")
	(match_operand:DI 1 "general_operand" "rF,m,roi<>F"))]
;  [(set (match_operand:DI 0 "nonimmediate_operand" "=rm,&r,&ro<>,!&rm,!&f")
;	(match_operand:DI 1 "general_operand" "r,m,roi<>,fF"))]
;  [(set (match_operand:DI 0 "nonimmediate_operand" "=rm,&rf,&ro<>,!&rm,!&f")
;	(match_operand:DI 1 "general_operand" "r,m,roi<>,fF,rfF"))]
  "!TARGET_COLDFIRE"
{
  if (FP_REG_P (operands[0]))
    {
      if (FP_REG_P (operands[1]))
	return "fmove%.x %1,%0";
      if (REG_P (operands[1]))
	{
	  rtx xoperands[2];
	  xoperands[1] = gen_rtx_REG (SImode, REGNO (operands[1]) + 1);
	  output_asm_insn ("move%.l %1,%-", xoperands);
	  output_asm_insn ("move%.l %1,%-", operands);
	  return "fmove%.d %+,%0";
	}
      if (GET_CODE (operands[1]) == CONST_DOUBLE)
	return output_move_const_double (operands);
      return "fmove%.d %f1,%0";
    }
  else if (FP_REG_P (operands[1]))
    {
      if (REG_P (operands[0]))
	{
	  output_asm_insn ("fmove%.d %f1,%-\;move%.l %+,%0", operands);
	  operands[0] = gen_rtx_REG (SImode, REGNO (operands[0]) + 1);
	  return "move%.l %+,%0";
	}
      else
        return "fmove%.d %f1,%0";
    }
  return output_move_double (operands);
})

(define_insn ""
  [(set (match_operand:DI 0 "nonimmediate_operand" "=r,g")
	(match_operand:DI 1 "general_operand" "g,r"))]
  "TARGET_COLDFIRE"
  "* return output_move_double (operands);")

;; Thus goes after the move instructions
;; because the move instructions are better (require no spilling)
;; when they can apply.  It goes before the add/sub insns
;; so we will prefer it to them.

(define_insn "pushasi"
  [(set (match_operand:SI 0 "push_operand" "=m")
	(match_operand:SI 1 "address_operand" "p"))]
  ""
  "pea %a1"
  [(set_attr "type" "pea")])

;; truncation instructions
(define_insn "truncsiqi2"
  [(set (match_operand:QI 0 "nonimmediate_operand" "=dm,d")
	(truncate:QI
	 (match_operand:SI 1 "general_src_operand" "doJS,i")))]
  ""
{
  if (GET_CODE (operands[0]) == REG)
    {
      /* Must clear condition codes, since the move.l bases them on
	 the entire 32 bits, not just the desired 8 bits.  */
      CC_STATUS_INIT;
      return "move%.l %1,%0";
    }
  if (GET_CODE (operands[1]) == MEM)
    operands[1] = adjust_address (operands[1], QImode, 3);
  return "move%.b %1,%0";
})

(define_insn "trunchiqi2"
  [(set (match_operand:QI 0 "nonimmediate_operand" "=dm,d")
	(truncate:QI
	 (match_operand:HI 1 "general_src_operand" "doJS,i")))]
  ""
{
  if (GET_CODE (operands[0]) == REG
      && (GET_CODE (operands[1]) == MEM
	  || GET_CODE (operands[1]) == CONST_INT))
    {
      /* Must clear condition codes, since the move.w bases them on
	 the entire 16 bits, not just the desired 8 bits.  */
      CC_STATUS_INIT;
      return "move%.w %1,%0";
    }
  if (GET_CODE (operands[0]) == REG)
    {
      /* Must clear condition codes, since the move.l bases them on
	 the entire 32 bits, not just the desired 8 bits.  */
      CC_STATUS_INIT;
      return "move%.l %1,%0";
    }
  if (GET_CODE (operands[1]) == MEM)
    operands[1] = adjust_address (operands[1], QImode, 1);
  return "move%.b %1,%0";
})

(define_insn "truncsihi2"
  [(set (match_operand:HI 0 "nonimmediate_operand" "=dm,d")
	(truncate:HI
	 (match_operand:SI 1 "general_src_operand" "roJS,i")))]
  ""
{
  if (GET_CODE (operands[0]) == REG)
    {
      /* Must clear condition codes, since the move.l bases them on
	 the entire 32 bits, not just the desired 8 bits.  */
      CC_STATUS_INIT;
      return "move%.l %1,%0";
    }
  if (GET_CODE (operands[1]) == MEM)
    operands[1] = adjust_address (operands[1], QImode, 2);
  return "move%.w %1,%0";
})

;; zero extension instructions

;; two special patterns to match various post_inc/pre_dec patterns
(define_insn_and_split "*zero_extend_inc"
  [(set (match_operand 0 "post_inc_operand" "")
	(zero_extend (match_operand 1 "register_operand" "")))]
  "GET_MODE_CLASS (GET_MODE (operands[0])) == MODE_INT &&
   GET_MODE_CLASS (GET_MODE (operands[1])) == MODE_INT &&
   GET_MODE_SIZE (GET_MODE (operands[0])) == GET_MODE_SIZE (GET_MODE (operands[1])) * 2"
  "#"
  ""
  [(set (match_dup 0)
	(const_int 0))
   (set (match_dup 0)
	(match_dup 1))]
{
  operands[0] = adjust_address (operands[0], GET_MODE (operands[1]), 0);
})

(define_insn_and_split "*zero_extend_dec"
  [(set (match_operand 0 "pre_dec_operand" "")
	(zero_extend (match_operand 1 "register_operand" "")))]
  "(GET_MODE (operands[0]) != HImode || XEXP (XEXP (operands[0], 0), 0) != stack_pointer_rtx) &&
   GET_MODE_CLASS (GET_MODE (operands[0])) == MODE_INT &&
   GET_MODE_CLASS (GET_MODE (operands[1])) == MODE_INT &&
   GET_MODE_SIZE (GET_MODE (operands[0])) == GET_MODE_SIZE (GET_MODE (operands[1])) * 2"
  "#"
  ""
  [(set (match_dup 0)
	(match_dup 1))
   (set (match_dup 0)
	(const_int 0))]
{
  operands[0] = adjust_address (operands[0], GET_MODE (operands[1]), 0);
})

(define_insn_and_split "zero_extendqidi2"
  [(set (match_operand:DI 0 "register_operand" "")
	(zero_extend:DI (match_operand:QI 1 "nonimmediate_src_operand" "")))]
  ""
  "#"
  ""
  [(set (match_dup 2)
	(zero_extend:SI (match_dup 1)))
   (set (match_dup 3)
	(const_int 0))]
{
  operands[2] = gen_lowpart (SImode, operands[0]);
  operands[3] = gen_highpart (SImode, operands[0]);
})

(define_insn_and_split "zero_extendhidi2"
  [(set (match_operand:DI 0 "register_operand" "")
	(zero_extend:DI (match_operand:HI 1 "nonimmediate_src_operand" "")))]
  ""
  "#"
  ""
  [(set (match_dup 2)
	(zero_extend:SI (match_dup 1)))
   (set (match_dup 3)
	(const_int 0))]
{
  operands[2] = gen_lowpart (SImode, operands[0]);
  operands[3] = gen_highpart (SImode, operands[0]);
})

(define_expand "zero_extendsidi2"
  [(set (match_operand:DI 0 "nonimmediate_operand" "")
	(zero_extend:DI (match_operand:SI 1 "nonimmediate_src_operand" "")))]
  ""
{
  if (GET_CODE (operands[0]) == MEM
      && GET_CODE (operands[1]) == MEM)
    operands[1] = force_reg (SImode, operands[1]);
})

(define_insn_and_split "*zero_extendsidi2"
  [(set (match_operand:DI 0 "nonimmediate_operand" "")
	(zero_extend:DI (match_operand:SI 1 "nonimmediate_src_operand" "")))]
  "GET_CODE (operands[0]) != MEM || GET_CODE (operands[1]) != MEM"
  "#"
  ""
  [(set (match_dup 2)
	(match_dup 1))
   (set (match_dup 3)
	(const_int 0))]
{
  operands[2] = gen_lowpart (SImode, operands[0]);
  operands[3] = gen_highpart (SImode, operands[0]);
})

(define_insn "*zero_extendhisi2_cf"
  [(set (match_operand:SI 0 "register_operand" "=d")
	(zero_extend:SI (match_operand:HI 1 "nonimmediate_src_operand" "rmS")))]
  "ISA_HAS_MVS_MVZ"
  "mvz%.w %1,%0"
  [(set_attr "type" "mvsz")])

(define_insn "zero_extendhisi2"
  [(set (match_operand:SI 0 "register_operand" "=d")
	(zero_extend:SI (match_operand:HI 1 "nonimmediate_src_operand" "rmS")))]
  ""
  "#")

(define_expand "zero_extendqihi2"
  [(set (match_operand:HI 0 "register_operand" "")
	(zero_extend:HI (match_operand:QI 1 "nonimmediate_src_operand" "")))]
  "!TARGET_COLDFIRE"
  "")

(define_insn "*zero_extendqihi2"
  [(set (match_operand:HI 0 "register_operand" "=d")
	(zero_extend:HI (match_operand:QI 1 "nonimmediate_src_operand" "dmS")))]
  "!TARGET_COLDFIRE"
  "#")

(define_insn "*zero_extendqisi2_cfv4"
  [(set (match_operand:SI 0 "register_operand" "=d")
	(zero_extend:SI (match_operand:QI 1 "nonimmediate_src_operand" "dmS")))]
  "ISA_HAS_MVS_MVZ"
  "mvz%.b %1,%0"
  [(set_attr "type" "mvsz")])

(define_insn "zero_extendqisi2"
  [(set (match_operand:SI 0 "register_operand" "=d")
	(zero_extend:SI (match_operand:QI 1 "nonimmediate_src_operand" "dmS")))]
  ""
  "#")

;; these two pattern split everything else which isn't matched by
;; something else above
(define_split
  [(set (match_operand 0 "register_operand" "")
	(zero_extend (match_operand 1 "nonimmediate_src_operand" "")))]
  "!ISA_HAS_MVS_MVZ
   && reload_completed
   && reg_mentioned_p (operands[0], operands[1])"
  [(set (strict_low_part (match_dup 2))
	(match_dup 1))
   (set (match_dup 0)
	(match_op_dup 4 [(match_dup 0) (match_dup 3)]))]
{
  operands[2] = gen_lowpart (GET_MODE (operands[1]), operands[0]);
  operands[3] = GEN_INT (GET_MODE_MASK (GET_MODE (operands[1])));
  operands[4] = gen_rtx_AND (GET_MODE (operands[0]), operands[0], operands[3]);
})

(define_split
  [(set (match_operand 0 "register_operand" "")
	(zero_extend (match_operand 1 "nonimmediate_src_operand" "")))]
  "!ISA_HAS_MVS_MVZ && reload_completed"
  [(set (match_dup 0)
	(const_int 0))
   (set (strict_low_part (match_dup 2))
	(match_dup 1))]
{
  operands[2] = gen_lowpart (GET_MODE (operands[1]), operands[0]);
})

;; sign extension instructions

(define_insn "extendqidi2"
  [(set (match_operand:DI 0 "nonimmediate_operand" "=d")
        (sign_extend:DI (match_operand:QI 1 "general_src_operand" "rmS")))]
  ""
{
  CC_STATUS_INIT;
  operands[2] = gen_rtx_REG (SImode, REGNO (operands[0]) + 1);
  if (ISA_HAS_MVS_MVZ)
    return "mvs%.b %1,%2\;smi %0\;extb%.l %0";
  if (TARGET_68020 || TARGET_COLDFIRE)
    {
      if (ADDRESS_REG_P (operands[1]))
	return "move%.w %1,%2\;extb%.l %2\;smi %0\;extb%.l %0";
      else
	return "move%.b %1,%2\;extb%.l %2\;smi %0\;extb%.l %0";
    }
  else
    {
      if (ADDRESS_REG_P (operands[1]))
	return "move%.w %1,%2\;ext%.w %2\;ext%.l %2\;move%.l %2,%0\;smi %0";
      else
	return "move%.b %1,%2\;ext%.w %2\;ext%.l %2\;move%.l %2,%0\;smi %0";
    }
})

(define_insn "extendhidi2"
  [(set (match_operand:DI 0 "nonimmediate_operand" "=d")
	(sign_extend:DI
	 (match_operand:HI 1 "general_src_operand" "rmS")))]
  ""
{
  CC_STATUS_INIT;
  operands[2] = gen_rtx_REG (SImode, REGNO (operands[0]) + 1);
  if (ISA_HAS_MVS_MVZ)
    return "mvs%.w %1,%2\;smi %0\;extb%.l %0";
  if (TARGET_68020 || TARGET_COLDFIRE)
    return "move%.w %1,%2\;ext%.l %2\;smi %0\;extb%.l %0";
  else
    return "move%.w %1,%2\;ext%.l %2\;smi %0\;ext%.w %0\;ext%.l %0";
})

(define_insn "extendsidi2"
  [(set (match_operand:DI 0 "nonimmediate_operand" "=d,o,o,<")
	(sign_extend:DI
	 (match_operand:SI 1 "nonimmediate_src_operand" "rm,rm,r<Q>,rm")))
   (clobber (match_scratch:SI 2 "=X,d,d,d"))]
  ""
{
  CC_STATUS_INIT;

  if (which_alternative == 0)
    /* Handle alternative 0.  */
    {
      if (TARGET_68020 || TARGET_COLDFIRE)
        return "move%.l %1,%R0\;smi %0\;extb%.l %0";
      else
        return "move%.l %1,%R0\;smi %0\;ext%.w %0\;ext%.l %0";
    }

  /* Handle alternatives 1, 2 and 3.  We don't need to adjust address by 4
     in alternative 3 because autodecrement will do that for us.  */
  operands[3] = adjust_address (operands[0], SImode,
				which_alternative == 3 ? 0 : 4);
  operands[0] = adjust_address (operands[0], SImode, 0);

  if (TARGET_68020 || TARGET_COLDFIRE)
    return "move%.l %1,%3\;smi %2\;extb%.l %2\;move%.l %2,%0";
  else
    return "move%.l %1,%3\;smi %2\;ext%.w %2\;ext%.l %2\;move%.l %2,%0";
}
  [(set_attr "ok_for_coldfire" "yes,no,yes,yes")])

;; Special case when one can avoid register clobbering, copy and test
;; Maybe there is a way to make that the general case, by forcing the
;; result of the SI tree to be in the lower register of the DI target

(define_insn "extendplussidi"
  [(set (match_operand:DI 0 "register_operand" "=d")
    (sign_extend:DI (plus:SI (match_operand:SI 1 "general_operand" "%rmn")
            (match_operand:SI 2 "general_operand" "rmn"))))]
  ""
{
  CC_STATUS_INIT;
  operands[3] = gen_rtx_REG (SImode, REGNO (operands[0]) + 1);
  if (GET_CODE (operands[1]) == CONST_INT
  && (unsigned) INTVAL (operands[1]) > 8)
    {
      rtx tmp = operands[1];

      operands[1] = operands[2];
      operands[2] = tmp;
    }
  if (GET_CODE (operands[1]) == REG
      && REGNO (operands[1]) == REGNO (operands[3]))
    output_asm_insn ("add%.l %2,%3", operands);
  else
    output_asm_insn ("move%.l %2,%3\;add%.l %1,%3", operands);
  if (TARGET_68020 || TARGET_COLDFIRE)
    return "smi %0\;extb%.l %0";
  else
    return "smi %0\;ext%.w %0\;ext%.l %0";
})

(define_expand "extendhisi2"
  [(set (match_operand:SI 0 "nonimmediate_operand" "")
	(sign_extend:SI
	 (match_operand:HI 1 "nonimmediate_src_operand" "")))]
  ""
  "")

(define_insn "*cfv4_extendhisi2"
  [(set (match_operand:SI 0 "nonimmediate_operand" "=d")
	(sign_extend:SI
	 (match_operand:HI 1 "nonimmediate_src_operand" "rmS")))]
  "ISA_HAS_MVS_MVZ"
  "mvs%.w %1,%0"
  [(set_attr "type" "mvsz")])

(define_insn "*68k_extendhisi2"
  [(set (match_operand:SI 0 "nonimmediate_operand" "=*d,a")
	(sign_extend:SI
	 (match_operand:HI 1 "nonimmediate_src_operand" "0,rmS")))]
  "!ISA_HAS_MVS_MVZ"
  "@
   ext%.l %0
   move%.w %1,%0"
  [(set_attr "type" "ext,move")])

(define_insn "extendqihi2"
  [(set (match_operand:HI 0 "nonimmediate_operand" "=d")
	(sign_extend:HI (match_operand:QI 1 "nonimmediate_operand" "0")))]
  ""
  "ext%.w %0"
  [(set_attr "type" "ext")])

(define_expand "extendqisi2"
  [(set (match_operand:SI 0 "nonimmediate_operand" "")
	(sign_extend:SI (match_operand:QI 1 "nonimmediate_operand" "")))]
  "TARGET_68020 || TARGET_COLDFIRE"
  "")

(define_insn "*cfv4_extendqisi2"
  [(set (match_operand:SI 0 "nonimmediate_operand" "=d")
	(sign_extend:SI (match_operand:QI 1 "nonimmediate_operand" "rms")))]
  "ISA_HAS_MVS_MVZ"
  "mvs%.b %1,%0"
  [(set_attr "type" "mvsz")])

(define_insn "*68k_extendqisi2"
  [(set (match_operand:SI 0 "nonimmediate_operand" "=d")
	(sign_extend:SI (match_operand:QI 1 "nonimmediate_operand" "0")))]
  "TARGET_68020 || (TARGET_COLDFIRE && !ISA_HAS_MVS_MVZ)"
  "extb%.l %0"
  [(set_attr "type" "ext")])

;; Conversions between float and double.

(define_expand "extendsfdf2"
  [(set (match_operand:DF 0 "nonimmediate_operand" "")
	(float_extend:DF
	 (match_operand:SF 1 "general_operand" "")))]
  "TARGET_HARD_FLOAT"
  "")

(define_insn ""
  [(set (match_operand:DF 0 "nonimmediate_operand" "=*fdm,f")
	(float_extend:DF
	  (match_operand:SF 1 "general_operand" "f,dmF")))]
  "TARGET_68881"
{
  if (FP_REG_P (operands[0]) && FP_REG_P (operands[1]))
    {
      if (REGNO (operands[0]) == REGNO (operands[1]))
	{
	  /* Extending float to double in an fp-reg is a no-op.
	     NOTICE_UPDATE_CC has already assumed that the
	     cc will be set.  So cancel what it did.  */
	  cc_status = cc_prev_status;
	  return "";
	}
      return "f%&move%.x %1,%0";
    }
  if (FP_REG_P (operands[0]))
    return "f%&move%.s %f1,%0";
  if (DATA_REG_P (operands[0]) && FP_REG_P (operands[1]))
    {
      output_asm_insn ("fmove%.d %f1,%-\;move%.l %+,%0", operands);
      operands[0] = gen_rtx_REG (SImode, REGNO (operands[0]) + 1);
      return "move%.l %+,%0";
    }
  return "fmove%.d %f1,%0";
})

(define_insn "extendsfdf2_cf"
  [(set (match_operand:DF 0 "nonimmediate_operand" "=f,f")
	(float_extend:DF
	 (match_operand:SF 1 "general_operand" "f,<Q>U")))]
  "TARGET_COLDFIRE_FPU"
{
  if (FP_REG_P (operands[0]) && FP_REG_P (operands[1]))
    {
      if (REGNO (operands[0]) == REGNO (operands[1]))
	{
	  /* Extending float to double in an fp-reg is a no-op.
	     NOTICE_UPDATE_CC has already assumed that the
	     cc will be set.  So cancel what it did.  */
	  cc_status = cc_prev_status;
	  return "";
	}
      return "fdmove%.d %1,%0";
    }
  return "fdmove%.s %f1,%0";
})

;; This cannot output into an f-reg because there is no way to be
;; sure of truncating in that case.
(define_expand "truncdfsf2"
  [(set (match_operand:SF 0 "nonimmediate_operand" "")
	(float_truncate:SF
	  (match_operand:DF 1 "general_operand" "")))]
  "TARGET_HARD_FLOAT"
  "")

;; On the '040 we can truncate in a register accurately and easily.
(define_insn ""
  [(set (match_operand:SF 0 "nonimmediate_operand" "=f")
	(float_truncate:SF
	  (match_operand:DF 1 "general_operand" "fmG")))]
  "TARGET_68881 && TARGET_68040"
{
  if (FP_REG_P (operands[1]))
    return "f%$move%.x %1,%0";
  return "f%$move%.d %f1,%0";
})

(define_insn "truncdfsf2_cf"
  [(set (match_operand:SF 0 "nonimmediate_operand" "=f,d<Q>U")
	(float_truncate:SF
	  (match_operand:DF 1 "general_operand" "<Q>U,f")))]
  "TARGET_COLDFIRE_FPU"
  "@
  fsmove%.d %1,%0
  fmove%.s %1,%0"
  [(set_attr "type" "fmove")])

(define_insn "*truncdfsf2_68881"
  [(set (match_operand:SF 0 "nonimmediate_operand" "=dm")
	(float_truncate:SF
	  (match_operand:DF 1 "general_operand" "f")))]
  "TARGET_68881"
  "fmove%.s %f1,%0"
  [(set_attr "type" "fmove")])

;; Conversion between fixed point and floating point.
;; Note that among the fix-to-float insns
;; the ones that start with SImode come first.
;; That is so that an operand that is a CONST_INT
;; (and therefore lacks a specific machine mode).
;; will be recognized as SImode (which is always valid)
;; rather than as QImode or HImode.

(define_expand "floatsi<mode>2"
  [(set (match_operand:FP 0 "nonimmediate_operand" "")
	(float:FP (match_operand:SI 1 "general_operand" "")))]
  "TARGET_HARD_FLOAT"
  "")

(define_insn "floatsi<mode>2_68881"
  [(set (match_operand:FP 0 "nonimmediate_operand" "=f")
	(float:FP (match_operand:SI 1 "general_operand" "dmi")))]
  "TARGET_68881"
  "f<FP:round>move%.l %1,%0"
  [(set_attr "type" "fmove")])

(define_insn "floatsi<mode>2_cf"
  [(set (match_operand:FP 0 "nonimmediate_operand" "=f")
	(float:FP (match_operand:SI 1 "general_operand" "d<Q>U")))]
  "TARGET_COLDFIRE_FPU"
  "f<FP:prec>move%.l %1,%0"
  [(set_attr "type" "fmove")])


(define_expand "floathi<mode>2"
  [(set (match_operand:FP 0 "nonimmediate_operand" "")
	(float:FP (match_operand:HI 1 "general_operand" "")))]
  "TARGET_HARD_FLOAT"
  "")

(define_insn "floathi<mode>2_68881"
  [(set (match_operand:FP 0 "nonimmediate_operand" "=f")
	(float:FP (match_operand:HI 1 "general_operand" "dmn")))]
  "TARGET_68881"
  "fmove%.w %1,%0"
  [(set_attr "type" "fmove")])

(define_insn "floathi<mode>2_cf"
  [(set (match_operand:FP 0 "nonimmediate_operand" "=f")
        (float:FP (match_operand:HI 1 "general_operand" "d<Q>U")))]
  "TARGET_COLDFIRE_FPU"
  "fmove%.w %1,%0"
  [(set_attr "type" "fmove")])


(define_expand "floatqi<mode>2"
  [(set (match_operand:FP 0 "nonimmediate_operand" "")
	(float:FP (match_operand:QI 1 "general_operand" "")))]
  "TARGET_HARD_FLOAT"
  "")

(define_insn "floatqi<mode>2_68881"
  [(set (match_operand:FP 0 "nonimmediate_operand" "=f")
	(float:FP (match_operand:QI 1 "general_operand" "dmn")))]
  "TARGET_68881"
  "fmove%.b %1,%0"
  [(set_attr "type" "fmove")])

(define_insn "floatqi<mode>2_cf"
  [(set (match_operand:FP 0 "nonimmediate_operand" "=f")
	(float:FP (match_operand:QI 1 "general_operand" "d<Q>U")))]
  "TARGET_COLDFIRE_FPU"
  "fmove%.b %1,%0"
  [(set_attr "type" "fmove")])


;; New routines to convert floating-point values to integers
;; to be used on the '040.  These should be faster than trapping
;; into the kernel to emulate fintrz.  They should also be faster
;; than calling the subroutines fixsfsi or fixdfsi.

(define_insn "fix_truncdfsi2"
  [(set (match_operand:SI 0 "nonimmediate_operand" "=dm")
	(fix:SI (fix:DF (match_operand:DF 1 "register_operand" "f"))))
   (clobber (match_scratch:SI 2 "=d"))
   (clobber (match_scratch:SI 3 "=d"))]
  "TARGET_68881 && TUNE_68040"
{
  CC_STATUS_INIT;
  return "fmovem%.l %!,%2\;moveq #16,%3\;or%.l %2,%3\;and%.w #-33,%3\;fmovem%.l %3,%!\;fmove%.l %1,%0\;fmovem%.l %2,%!";
})

(define_insn "fix_truncdfhi2"
  [(set (match_operand:HI 0 "nonimmediate_operand" "=dm")
	(fix:HI (fix:DF (match_operand:DF 1 "register_operand" "f"))))
   (clobber (match_scratch:SI 2 "=d"))
   (clobber (match_scratch:SI 3 "=d"))]
  "TARGET_68881 && TUNE_68040"
{
  CC_STATUS_INIT;
  return "fmovem%.l %!,%2\;moveq #16,%3\;or%.l %2,%3\;and%.w #-33,%3\;fmovem%.l %3,%!\;fmove%.w %1,%0\;fmovem%.l %2,%!";
})

(define_insn "fix_truncdfqi2"
  [(set (match_operand:QI 0 "nonimmediate_operand" "=dm")
	(fix:QI (fix:DF (match_operand:DF 1 "register_operand" "f"))))
   (clobber (match_scratch:SI 2 "=d"))
   (clobber (match_scratch:SI 3 "=d"))]
  "TARGET_68881 && TUNE_68040"
{
  CC_STATUS_INIT;
  return "fmovem%.l %!,%2\;moveq #16,%3\;or%.l %2,%3\;and%.w #-33,%3\;fmovem%.l %3,%!\;fmove%.b %1,%0\;fmovem%.l %2,%!";
})

;; Convert a float to a float whose value is an integer.
;; This is the first stage of converting it to an integer type.

(define_expand "ftrunc<mode>2"
  [(set (match_operand:FP 0 "nonimmediate_operand" "")
	(fix:FP (match_operand:FP 1 "general_operand" "")))]
  "TARGET_HARD_FLOAT && !TUNE_68040"
  "")

(define_insn "ftrunc<mode>2_68881"
  [(set (match_operand:FP 0 "nonimmediate_operand" "=f")
	(fix:FP (match_operand:FP 1 "general_operand" "f<FP:dreg>m")))]
  "TARGET_68881 && !TUNE_68040"
{
  if (FP_REG_P (operands[1]))
    return "fintrz%.x %f1,%0";
  return "fintrz%.<FP:prec> %f1,%0";
}
  [(set_attr "type" "falu")])

(define_insn "ftrunc<mode>2_cf"
  [(set (match_operand:FP 0 "nonimmediate_operand" "=f")
        (fix:FP (match_operand:FP 1 "general_operand" "f<FP:dreg><Q>U")))]
  "TARGET_COLDFIRE_FPU"
{
  if (FP_REG_P (operands[1]))
    return "fintrz%.d %f1,%0";
  return "fintrz%.<FP:prec> %f1,%0";
}
  [(set_attr "type" "falu")])

;; Convert a float whose value is an integer
;; to an actual integer.  Second stage of converting float to integer type.
(define_expand "fix<mode>qi2"
  [(set (match_operand:QI 0 "nonimmediate_operand" "")
	(fix:QI (match_operand:FP 1 "general_operand" "")))]
  "TARGET_HARD_FLOAT"
  "")

(define_insn "fix<mode>qi2_68881"
  [(set (match_operand:QI 0 "nonimmediate_operand" "=dm")
	(fix:QI (match_operand:FP 1 "general_operand" "f")))]
  "TARGET_68881"
  "fmove%.b %1,%0"
  [(set_attr "type" "fmove")])

(define_insn "fix<mode>qi2_cf"
  [(set (match_operand:QI 0 "nonimmediate_operand" "=d<Q>U")
	(fix:QI (match_operand:FP 1 "general_operand" "f")))]
  "TARGET_COLDFIRE_FPU"
  "fmove%.b %1,%0"
  [(set_attr "type" "fmove")])

(define_expand "fix<mode>hi2"
  [(set (match_operand:HI 0 "nonimmediate_operand" "")
	(fix:HI (match_operand:FP 1 "general_operand" "")))]
  "TARGET_HARD_FLOAT"
  "")

(define_insn "fix<mode>hi2_68881"
  [(set (match_operand:HI 0 "nonimmediate_operand" "=dm")
	(fix:HI (match_operand:FP 1 "general_operand" "f")))]
  "TARGET_68881"
  "fmove%.w %1,%0"
  [(set_attr "type" "fmove")])

(define_insn "fix<mode>hi2_cf"
  [(set (match_operand:HI 0 "nonimmediate_operand" "=d<Q>U")
	(fix:HI (match_operand:FP 1 "general_operand" "f")))]
  "TARGET_COLDFIRE_FPU"
  "fmove%.w %1,%0"
  [(set_attr "type" "fmove")])

(define_expand "fix<mode>si2"
  [(set (match_operand:SI 0 "nonimmediate_operand" "")
	(fix:SI (match_operand:FP 1 "general_operand" "")))]
  "TARGET_HARD_FLOAT"
  "")

(define_insn "fix<mode>si2_68881"
  [(set (match_operand:SI 0 "nonimmediate_operand" "=dm")
	(fix:SI (match_operand:FP 1 "general_operand" "f")))]
  "TARGET_68881"
  "fmove%.l %1,%0"
  [(set_attr "type" "fmove")])

(define_insn "fix<mode>si2_cf"
  [(set (match_operand:SI 0 "nonimmediate_operand" "=d<Q>U")
	(fix:SI (match_operand:FP 1 "general_operand" "f")))]
  "TARGET_COLDFIRE_FPU"
  "fmove%.l %1,%0"
  [(set_attr "type" "fmove")])


;; add instructions

(define_insn "adddi_lshrdi_63"
  [(set (match_operand:DI 0 "nonimmediate_operand" "=d")
    (plus:DI (lshiftrt:DI (match_operand:DI 1 "general_operand" "rm")
            (const_int 63))
        (match_dup 1)))
   (clobber (match_scratch:SI 2 "=d"))]
  ""
{
  operands[3] = gen_rtx_REG (SImode, REGNO (operands[0]) + 1);
  if (REG_P (operands[1]) && REGNO (operands[1]) == REGNO (operands[0]))
    return
    "move%.l %1,%2\;add%.l %2,%2\;subx%.l %2,%2\;sub%.l %2,%3\;subx%.l %2,%0";
  if (GET_CODE (operands[1]) == REG)
    operands[4] = gen_rtx_REG (SImode, REGNO (operands[1]) + 1);
  else if (GET_CODE (XEXP (operands[1], 0)) == POST_INC
        || GET_CODE (XEXP (operands[1], 0)) == PRE_DEC)
    operands[4] = operands[1];
  else
    operands[4] = adjust_address (operands[1], SImode, 4);
  if (GET_CODE (operands[1]) == MEM
   && GET_CODE (XEXP (operands[1], 0)) == PRE_DEC)
    output_asm_insn ("move%.l %4,%3", operands);
  output_asm_insn ("move%.l %1,%0\;smi %2", operands);
  if (TARGET_68020 || TARGET_COLDFIRE)
    output_asm_insn ("extb%.l %2", operands);
  else
    output_asm_insn ("ext%.w %2\;ext%.l %2", operands);
  if (GET_CODE (operands[1]) != MEM
   || GET_CODE (XEXP (operands[1], 0)) != PRE_DEC)
    output_asm_insn ("move%.l %4,%3", operands);
  return "sub%.l %2,%3\;subx%.l %2,%0";
})

(define_insn "adddi_sexthishl32"
  [(set (match_operand:DI 0 "nonimmediate_operand" "=o,a,*d,*d")
    (plus:DI (ashift:DI (sign_extend:DI
          (match_operand:HI 1 "general_operand" "rm,rm,rm,rm"))
            (const_int 32))
        (match_operand:DI 2 "general_operand" "0,0,0,0")))
   (clobber (match_scratch:SI 3 "=&d,X,a,?d"))]
  "!TARGET_COLDFIRE"
{
  CC_STATUS_INIT;
  if (ADDRESS_REG_P (operands[0]))
    return "add%.w %1,%0";
  else if (ADDRESS_REG_P (operands[3]))
    return "move%.w %1,%3\;add%.l %3,%0";
  else
    return "move%.w %1,%3\;ext%.l %3\;add%.l %3,%0";
})

(define_insn "*adddi_dilshr32"
  [(set (match_operand:DI 0 "nonimmediate_operand" "=d,o")
	(plus:DI (lshiftrt:DI (match_operand:DI 1 "general_operand" "ro,d")
			      (const_int 32))
		 (match_operand:DI 2 "general_operand" "0,0")))]
  "!TARGET_COLDFIRE"
{
  CC_STATUS_INIT;
  if (GET_CODE (operands[0]) == REG)
    operands[2] = gen_rtx_REG (SImode, REGNO (operands[0]) + 1);
  else
    operands[2] = adjust_address (operands[0], SImode, 4);
  return "add%.l %1,%2\;negx%.l %0\;neg%.l %0";
})

(define_insn "*adddi_dilshr32_cf"
  [(set (match_operand:DI 0 "register_operand" "=d")
	(plus:DI (lshiftrt:DI (match_operand:DI 1 "nonimmediate_operand" "ro")
			      (const_int 32))
		 (match_operand:DI 2 "register_operand" "0")))]
  "TARGET_COLDFIRE"
{
  CC_STATUS_INIT;
  return "add%.l %1,%R0\;negx%.l %0\;neg%.l %0";
})

(define_insn "adddi_dishl32"
  [(set (match_operand:DI 0 "nonimmediate_operand" "=r,o")
;;    (plus:DI (match_operand:DI 2 "general_operand" "%0")
;;	(ashift:DI (match_operand:DI 1 "general_operand" "ro")
;;            (const_int 32))))]
    (plus:DI (ashift:DI (match_operand:DI 1 "general_operand" "ro,d")
            (const_int 32))
        (match_operand:DI 2 "general_operand" "0,0")))]
  ""
{
  CC_STATUS_INIT;
  if (GET_CODE (operands[1]) == REG)
    operands[1] = gen_rtx_REG (SImode, REGNO (operands[1]) + 1);
  else
    operands[1] = adjust_address (operands[1], SImode, 4);
  return "add%.l %1,%0";
}
  [(set_attr "type" "alu_l")])

(define_insn "adddi3"
  [(set (match_operand:DI 0 "nonimmediate_operand" "=o<>,d,d,d")
	(plus:DI (match_operand:DI 1 "general_operand" "%0,0,0,0")
		 (match_operand:DI 2 "general_operand" "d,no>,d,a")))
   (clobber (match_scratch:SI 3 "=&d,&d,X,&d"))]
  ""
{
  if (DATA_REG_P (operands[0]))
    {
      if (DATA_REG_P (operands[2]))
	return "add%.l %R2,%R0\;addx%.l %2,%0";
      else if (GET_CODE (operands[2]) == MEM
	  && GET_CODE (XEXP (operands[2], 0)) == POST_INC)
	return "move%.l %2,%3\;add%.l %2,%R0\;addx%.l %3,%0";
      else
	{
	  rtx high, low;
	  rtx xoperands[2];

	  if (GET_CODE (operands[2]) == REG)
	    {
	      low = gen_rtx_REG (SImode, REGNO (operands[2]) + 1);
	      high = operands[2];
	    }
	  else if (CONSTANT_P (operands[2]))
	    split_double (operands[2], &high, &low);
	  else
	    {
	      low = adjust_address (operands[2], SImode, 4);
	      high = operands[2];
	    }

	  operands[1] = low, operands[2] = high;
	  xoperands[0] = operands[3];
	  if (GET_CODE (operands[1]) == CONST_INT
	      && INTVAL (operands[1]) >= -8 && INTVAL (operands[1]) < 0)
	    xoperands[1] = GEN_INT (-INTVAL (operands[2]) - 1);
	  else
	    xoperands[1] = operands[2];

	  output_asm_insn (output_move_simode (xoperands), xoperands);
	  if (GET_CODE (operands[1]) == CONST_INT)
	    {
	      if (INTVAL (operands[1]) > 0 && INTVAL (operands[1]) <= 8)
		return "addq%.l %1,%R0\;addx%.l %3,%0";
	      else if (INTVAL (operands[1]) >= -8 && INTVAL (operands[1]) < 0)
		{
		  operands[1] = GEN_INT (-INTVAL (operands[1]));
		  return "subq%.l %1,%R0\;subx%.l %3,%0";
		}
	    }
	  return "add%.l %1,%R0\;addx%.l %3,%0";
	}
    }
  else
    {
      gcc_assert (GET_CODE (operands[0]) == MEM);
      CC_STATUS_INIT;
      if (GET_CODE (XEXP (operands[0], 0)) == POST_INC)
	{
	  operands[1] = gen_rtx_MEM (SImode,
				     plus_constant (Pmode,
						    XEXP(operands[0], 0), -8));
	  return "move%.l %0,%3\;add%.l %R2,%0\;addx%.l %2,%3\;move%.l %3,%1";
	}
      else if (GET_CODE (XEXP (operands[0], 0)) == PRE_DEC)
	{
	  operands[1] = XEXP(operands[0], 0);
	  return "add%.l %R2,%0\;move%.l %0,%3\;addx%.l %2,%3\;move%.l %3,%1";
	}
      else
	{
	  operands[1] = adjust_address (operands[0], SImode, 4);
	  return "add%.l %R2,%1\;move%.l %0,%3\;addx%.l %2,%3\;move%.l %3,%0";
	}
    }
})

(define_insn "addsi_lshrsi_31"
  [(set (match_operand:SI 0 "nonimmediate_operand" "=dm,dm,d<Q>")
    (plus:SI (lshiftrt:SI (match_operand:SI 1 "general_operand" "rm,r<Q>,rm")
            (const_int 31))
        (match_dup 1)))]
  ""
{
  operands[2] = operands[0];
  operands[3] = gen_label_rtx();
  if (GET_CODE (operands[0]) == MEM)
    {
      if (GET_CODE (XEXP (operands[0], 0)) == POST_INC)
        operands[0] = gen_rtx_MEM (SImode, XEXP (XEXP (operands[0], 0), 0));
      else if (GET_CODE (XEXP (operands[0], 0)) == PRE_DEC)
        operands[2] = gen_rtx_MEM (SImode, XEXP (XEXP (operands[0], 0), 0));
    }
  output_asm_insn ("move%.l %1,%0", operands);
  output_asm_insn ("jpl %l3", operands);
  output_asm_insn ("addq%.l #1,%2", operands);
  (*targetm.asm_out.internal_label) (asm_out_file, "L",
				CODE_LABEL_NUMBER (operands[3]));
  return "";
}
  [(set_attr "ok_for_coldfire" "no,yes,yes")])

(define_expand "addsi3"
  [(set (match_operand:SI 0 "nonimmediate_operand" "")
	(plus:SI (match_operand:SI 1 "general_operand" "")
		 (match_operand:SI 2 "general_src_operand" "")))]
  ""
  "")

;; Note that the middle two alternatives are near-duplicates
;; in order to handle insns generated by reload.
;; This is needed since they are not themselves reloaded,
;; so commutativity won't apply to them.
(define_insn "*addsi3_internal"
  [(set (match_operand:SI 0 "nonimmediate_operand" "=m,?a,?a,d,a")
        (plus:SI (match_operand:SI 1 "general_operand" "%0,a,rJK,0,0")
                 (match_operand:SI 2 "general_src_operand" "dIKLT,rJK,a,mSrIKLT,mSrIKLs")))]


  "! TARGET_COLDFIRE"
  "* return output_addsi3 (operands);")

(define_insn_and_split "*addsi3_5200"
  [(set (match_operand:SI 0 "nonimmediate_operand"         "=mr,mr,a,  m,r,  ?a, ?a,?a,?a")
	(plus:SI (match_operand:SI 1 "general_operand"     "%0, 0, 0,  0,0,   a,  a, r, a")
		 (match_operand:SI 2 "general_src_operand" " I, L, JCu,d,mrKi,Cj, r, a, JCu")))]
  "TARGET_COLDFIRE"
{
  switch (which_alternative)
    {
    case 0:
      return "addq%.l %2,%0";

    case 1:
      operands[2] = GEN_INT (- INTVAL (operands[2]));
      return "subq%.l %2,%0";

    case 3:
    case 4:
      return "add%.l %2,%0";

    case 5:
      /* move%.l %2,%0\n\tadd%.l %1,%0 */
      return "#";

    case 6:
      return MOTOROLA ? "lea (%1,%2.l),%0" : "lea %1@(0,%2:l),%0";

    case 7:
      return MOTOROLA ? "lea (%2,%1.l),%0" : "lea %2@(0,%1:l),%0";

    case 2:
    case 8:
      return MOTOROLA ? "lea (%c2,%1),%0" : "lea %1@(%c2),%0";

    default:
      gcc_unreachable ();
      return "";
    }
}
  "&& reload_completed && (extract_constrain_insn_cached (insn), which_alternative == 5) && !operands_match_p (operands[0], operands[1])"
  [(set (match_dup 0)
	(match_dup 2))
   (set (match_dup 0)
	(plus:SI (match_dup 0)
		 (match_dup 1)))]
  ""
  [(set_attr "type"     "aluq_l,aluq_l,lea, alu_l,alu_l,*,lea, lea, lea")
   (set_attr "opy"      "2,     2,     *,   2,    2,    *,*,   *,   *")
   (set_attr "opy_type" "*,     *,     mem5,*,    *,    *,mem6,mem6,mem5")])

(define_insn ""
  [(set (match_operand:SI 0 "nonimmediate_operand" "=a")
	(plus:SI (match_operand:SI 1 "general_operand" "0")
		 (sign_extend:SI
		  (match_operand:HI 2 "nonimmediate_src_operand" "rmS"))))]
  "!TARGET_COLDFIRE"
  "add%.w %2,%0")

(define_insn "addhi3"
  [(set (match_operand:HI 0 "nonimmediate_operand" "=m,r")
	(plus:HI (match_operand:HI 1 "general_operand" "%0,0")
		 (match_operand:HI 2 "general_src_operand" "dn,rmSn")))]
  "!TARGET_COLDFIRE"
{
  if (GET_CODE (operands[2]) == CONST_INT)
    {
      /* If the constant would be a negative number when interpreted as
	 HImode, make it negative.  This is usually, but not always, done
	 elsewhere in the compiler.  First check for constants out of range,
	 which could confuse us.  */

      if (INTVAL (operands[2]) >= 32768)
	operands[2] = GEN_INT (INTVAL (operands[2]) - 65536);

      if (INTVAL (operands[2]) > 0
	  && INTVAL (operands[2]) <= 8)
	return "addq%.w %2,%0";
      if (INTVAL (operands[2]) < 0
	  && INTVAL (operands[2]) >= -8)
	{
	  operands[2] = GEN_INT (- INTVAL (operands[2]));
	  return "subq%.w %2,%0";
	}
      /* On the CPU32 it is faster to use two addqw instructions to
	 add a small integer (8 < N <= 16) to a register.  
	 Likewise for subqw.  */
      if (TUNE_CPU32 && REG_P (operands[0]))
	{
	  if (INTVAL (operands[2]) > 8
	      && INTVAL (operands[2]) <= 16)
	    {
	      operands[2] = GEN_INT (INTVAL (operands[2]) - 8);
	      return "addq%.w #8,%0\;addq%.w %2,%0";
	    }
	  if (INTVAL (operands[2]) < -8
	      && INTVAL (operands[2]) >= -16)
	    {
	      operands[2] = GEN_INT (- INTVAL (operands[2]) - 8);
	      return "subq%.w #8,%0\;subq%.w %2,%0";
	    }
	}
      if (ADDRESS_REG_P (operands[0]) && !TUNE_68040)
	return MOTOROLA ? "lea (%c2,%0),%0" : "lea %0@(%c2),%0";
    }
  return "add%.w %2,%0";
})

;; These insns must use MATCH_DUP instead of the more expected
;; use of a matching constraint because the "output" here is also
;; an input, so you can't use the matching constraint.  That also means
;; that you can't use the "%", so you need patterns with the matched
;; operand in both positions.

(define_insn ""
  [(set (strict_low_part (match_operand:HI 0 "nonimmediate_operand" "+m,d"))
	(plus:HI (match_dup 0)
		 (match_operand:HI 1 "general_src_operand" "dn,rmSn")))]
  "!TARGET_COLDFIRE"
{
  if (GET_CODE (operands[1]) == CONST_INT)
    {
      /* If the constant would be a negative number when interpreted as
	 HImode, make it negative.  This is usually, but not always, done
	 elsewhere in the compiler.  First check for constants out of range,
	 which could confuse us.  */

      if (INTVAL (operands[1]) >= 32768)
	operands[1] = GEN_INT (INTVAL (operands[1]) - 65536);

      if (INTVAL (operands[1]) > 0
	  && INTVAL (operands[1]) <= 8)
	return "addq%.w %1,%0";
      if (INTVAL (operands[1]) < 0
	  && INTVAL (operands[1]) >= -8)
	{
	  operands[1] = GEN_INT (- INTVAL (operands[1]));
	  return "subq%.w %1,%0";
	}
      /* On the CPU32 it is faster to use two addqw instructions to
	 add a small integer (8 < N <= 16) to a register. 
	 Likewise for subqw.  */
      if (TUNE_CPU32 && REG_P (operands[0]))
	{
	  if (INTVAL (operands[1]) > 8
	      && INTVAL (operands[1]) <= 16)
	    {
	      operands[1] = GEN_INT (INTVAL (operands[1]) - 8);
	      return "addq%.w #8,%0\;addq%.w %1,%0";
	    }
	  if (INTVAL (operands[1]) < -8
	      && INTVAL (operands[1]) >= -16)
	    {
	      operands[1] = GEN_INT (- INTVAL (operands[1]) - 8);
	      return "subq%.w #8,%0\;subq%.w %1,%0";
	    }
	}
      if (ADDRESS_REG_P (operands[0]) && !TUNE_68040)
	return MOTOROLA ? "lea (%c1,%0),%0" : "lea %0@(%c1),%0";
    }
  return "add%.w %1,%0";
})

(define_insn ""
  [(set (strict_low_part (match_operand:HI 0 "nonimmediate_operand" "+m,d"))
	(plus:HI (match_operand:HI 1 "general_src_operand" "dn,rmSn")
		 (match_dup 0)))]
  "!TARGET_COLDFIRE"
{
  if (GET_CODE (operands[1]) == CONST_INT)
    {
      /* If the constant would be a negative number when interpreted as
	 HImode, make it negative.  This is usually, but not always, done
	 elsewhere in the compiler.  First check for constants out of range,
	 which could confuse us.  */

      if (INTVAL (operands[1]) >= 32768)
	operands[1] = GEN_INT (INTVAL (operands[1]) - 65536);

      if (INTVAL (operands[1]) > 0
	  && INTVAL (operands[1]) <= 8)
	return "addq%.w %1,%0";
      if (INTVAL (operands[1]) < 0
	  && INTVAL (operands[1]) >= -8)
	{
	  operands[1] = GEN_INT (- INTVAL (operands[1]));
	  return "subq%.w %1,%0";
	}
      /* On the CPU32 it is faster to use two addqw instructions to
	 add a small integer (8 < N <= 16) to a register.
	 Likewise for subqw.  */
      if (TUNE_CPU32 && REG_P (operands[0]))
	{
	  if (INTVAL (operands[1]) > 8
	      && INTVAL (operands[1]) <= 16)
	    {
	      operands[1] = GEN_INT (INTVAL (operands[1]) - 8);
	      return "addq%.w #8,%0\;addq%.w %1,%0";
	    }
	  if (INTVAL (operands[1]) < -8
	      && INTVAL (operands[1]) >= -16)
	    {
	      operands[1] = GEN_INT (- INTVAL (operands[1]) - 8);
	      return "subq%.w #8,%0\;subq%.w %1,%0";
	    }
	}
      if (ADDRESS_REG_P (operands[0]) && !TUNE_68040)
	return MOTOROLA ? "lea (%c1,%0),%0" : "lea %0@(%c1),%0";
    }
  return "add%.w %1,%0";
})

(define_insn "addqi3"
  [(set (match_operand:QI 0 "nonimmediate_operand" "=m,d")
	(plus:QI (match_operand:QI 1 "general_operand" "%0,0")
		 (match_operand:QI 2 "general_src_operand" "dn,dmSn")))]
  "!TARGET_COLDFIRE"
{
  if (GET_CODE (operands[2]) == CONST_INT)
    {
      if (INTVAL (operands[2]) >= 128)
	operands[2] = GEN_INT (INTVAL (operands[2]) - 256);

      if (INTVAL (operands[2]) > 0
	  && INTVAL (operands[2]) <= 8)
	return "addq%.b %2,%0";
      if (INTVAL (operands[2]) < 0 && INTVAL (operands[2]) >= -8)
       {
	 operands[2] = GEN_INT (- INTVAL (operands[2]));
	 return "subq%.b %2,%0";
       }
    }
  return "add%.b %2,%0";
})

(define_insn ""
  [(set (strict_low_part (match_operand:QI 0 "nonimmediate_operand" "+m,d"))
	(plus:QI (match_dup 0)
		 (match_operand:QI 1 "general_src_operand" "dn,dmSn")))]
  "!TARGET_COLDFIRE"
{
  if (GET_CODE (operands[1]) == CONST_INT)
    {
      if (INTVAL (operands[1]) >= 128)
	operands[1] = GEN_INT (INTVAL (operands[1]) - 256);

      if (INTVAL (operands[1]) > 0
	  && INTVAL (operands[1]) <= 8)
	return "addq%.b %1,%0";
      if (INTVAL (operands[1]) < 0 && INTVAL (operands[1]) >= -8)
       {
	 operands[1] = GEN_INT (- INTVAL (operands[1]));
	 return "subq%.b %1,%0";
       }
    }
  return "add%.b %1,%0";
})

(define_insn ""
  [(set (strict_low_part (match_operand:QI 0 "nonimmediate_operand" "+m,d"))
	(plus:QI (match_operand:QI 1 "general_src_operand" "dn,dmSn")
		 (match_dup 0)))]
  "!TARGET_COLDFIRE"
{
  if (GET_CODE (operands[1]) == CONST_INT)
    {
      if (INTVAL (operands[1]) >= 128)
	operands[1] = GEN_INT (INTVAL (operands[1]) - 256);

      if (INTVAL (operands[1]) > 0
	  && INTVAL (operands[1]) <= 8)
	return "addq%.b %1,%0";
      if (INTVAL (operands[1]) < 0 && INTVAL (operands[1]) >= -8)
       {
	 operands[1] = GEN_INT (- INTVAL (operands[1]));
	 return "subq%.b %1,%0";
       }
    }
  return "add%.b %1,%0";
})

(define_expand "add<mode>3"
  [(set (match_operand:FP 0 "nonimmediate_operand" "")
	(plus:FP (match_operand:FP 1 "general_operand" "")
		 (match_operand:FP 2 "general_operand" "")))]
  "TARGET_HARD_FLOAT"
  "")

(define_insn "add<mode>3_floatsi_68881"
  [(set (match_operand:FP 0 "nonimmediate_operand" "=f")
	(plus:FP (float:FP (match_operand:SI 2 "general_operand" "dmi"))
		 (match_operand:FP 1 "general_operand" "0")))]
  "TARGET_68881"
  "f<FP:round>add%.l %2,%0"
  [(set_attr "type" "falu")
   (set_attr "opy" "2")])

(define_insn "add<mode>3_floathi_68881"
  [(set (match_operand:FP 0 "nonimmediate_operand" "=f")
	(plus:FP (float:FP (match_operand:HI 2 "general_operand" "dmn"))
		 (match_operand:FP 1 "general_operand" "0")))]
  "TARGET_68881"
  "f<FP:round>add%.w %2,%0"
  [(set_attr "type" "falu")
   (set_attr "opy" "2")])

(define_insn "add<mode>3_floatqi_68881"
  [(set (match_operand:FP 0 "nonimmediate_operand" "=f")
	(plus:FP (float:FP (match_operand:QI 2 "general_operand" "dmn"))
		 (match_operand:FP 1 "general_operand" "0")))]
  "TARGET_68881"
  "f<FP:round>add%.b %2,%0"
  [(set_attr "type" "falu")
   (set_attr "opy" "2")])

(define_insn "add<mode>3_68881"
  [(set (match_operand:FP 0 "nonimmediate_operand" "=f")
	(plus:FP (match_operand:FP 1 "general_operand" "%0")
		 (match_operand:FP 2 "general_operand" "f<FP:dreg>m<FP:const>")))]
  "TARGET_68881"
{
  if (FP_REG_P (operands[2]))
    return "f<FP:round>add%.x %2,%0";
  return "f<FP:round>add%.<FP:prec> %f2,%0";
}
  [(set_attr "type" "falu")
   (set_attr "opy" "2")])

(define_insn "add<mode>3_cf"
  [(set (match_operand:FP 0 "nonimmediate_operand" "=f")
	(plus:FP (match_operand:FP 1 "general_operand" "%0")
		 (match_operand:FP 2 "general_operand" "f<FP:dreg><Q>U")))]
  "TARGET_COLDFIRE_FPU"
{
  if (FP_REG_P (operands[2]))
    return "f<FP:prec>add%.d %2,%0";
  return "f<FP:prec>add%.<FP:prec> %2,%0";
}
  [(set_attr "type" "falu")
   (set_attr "opy" "2")])

;; subtract instructions

(define_insn "subdi_sexthishl32"
  [(set (match_operand:DI 0 "nonimmediate_operand" "=o,a,*d,*d")
    (minus:DI (match_operand:DI 1 "general_operand" "0,0,0,0")
        (ashift:DI (sign_extend:DI (match_operand:HI 2 "general_operand" "rm,rm,rm,rm"))
            (const_int 32))))
   (clobber (match_scratch:SI 3 "=&d,X,a,?d"))]
  "!TARGET_COLDFIRE"
{
  CC_STATUS_INIT;
  if (ADDRESS_REG_P (operands[0]))
    return "sub%.w %2,%0";
  else if (ADDRESS_REG_P (operands[3]))
    return "move%.w %2,%3\;sub%.l %3,%0";
  else
    return "move%.w %2,%3\;ext%.l %3\;sub%.l %3,%0";
})

(define_insn "subdi_dishl32"
  [(set (match_operand:DI 0 "nonimmediate_operand" "+ro")
    (minus:DI (match_dup 0)
        (ashift:DI (match_operand:DI 1 "general_operand" "ro")
            (const_int 32))))]
  ""
{
  CC_STATUS_INIT;
  if (GET_CODE (operands[1]) == REG)
    operands[1] = gen_rtx_REG (SImode, REGNO (operands[1]) + 1);
  else
    operands[1] = adjust_address (operands[1], SImode, 4);
  return "sub%.l %1,%0";
}
  [(set_attr "type" "alu_l")])

(define_insn "subdi3"
  [(set (match_operand:DI 0 "nonimmediate_operand" "=o<>,d,d,d")
	(minus:DI (match_operand:DI 1 "general_operand" "0,0,0,0")
		 (match_operand:DI 2 "general_operand" "d,no>,d,a")))
   (clobber (match_scratch:SI 3 "=&d,&d,X,&d"))]
  ""
{
  if (DATA_REG_P (operands[0]))
    {
      if (DATA_REG_P (operands[2]))
	return "sub%.l %R2,%R0\;subx%.l %2,%0";
      else if (GET_CODE (operands[2]) == MEM
	  && GET_CODE (XEXP (operands[2], 0)) == POST_INC)
	{
	  return "move%.l %2,%3\;sub%.l %2,%R0\;subx%.l %3,%0";
	}
      else
	{
	  rtx high, low;
	  rtx xoperands[2];

	  if (GET_CODE (operands[2]) == REG)
	    {
	      low = gen_rtx_REG (SImode, REGNO (operands[2]) + 1);
	      high = operands[2];
	    }
	  else if (CONSTANT_P (operands[2]))
	    split_double (operands[2], &high, &low);
	  else
	    {
	      low = adjust_address (operands[2], SImode, 4);
	      high = operands[2];
	    }

	  operands[1] = low, operands[2] = high;
	  xoperands[0] = operands[3];
	  if (GET_CODE (operands[1]) == CONST_INT
	      && INTVAL (operands[1]) >= -8 && INTVAL (operands[1]) < 0)
	    xoperands[1] = GEN_INT (-INTVAL (operands[2]) - 1);
	  else
	    xoperands[1] = operands[2];

	  output_asm_insn (output_move_simode (xoperands), xoperands);
	  if (GET_CODE (operands[1]) == CONST_INT)
	    {
	      if (INTVAL (operands[1]) > 0 && INTVAL (operands[1]) <= 8)
		return "subq%.l %1,%R0\;subx%.l %3,%0";
	      else if (INTVAL (operands[1]) >= -8 && INTVAL (operands[1]) < 0)
		{
		  operands[1] = GEN_INT (-INTVAL (operands[1]));
		  return "addq%.l %1,%R0\;addx%.l %3,%0";
		}
	    }
	  return "sub%.l %1,%R0\;subx%.l %3,%0";
	}
    }
  else
    {
      gcc_assert (GET_CODE (operands[0]) == MEM);
      CC_STATUS_INIT;
      if (GET_CODE (XEXP (operands[0], 0)) == POST_INC)
	{
	  operands[1]
	    = gen_rtx_MEM (SImode, plus_constant (Pmode,
						  XEXP (operands[0], 0), -8));
	  return "move%.l %0,%3\;sub%.l %R2,%0\;subx%.l %2,%3\;move%.l %3,%1";
	}
      else if (GET_CODE (XEXP (operands[0], 0)) == PRE_DEC)
	{
	  operands[1] = XEXP(operands[0], 0);
	  return "sub%.l %R2,%0\;move%.l %0,%3\;subx%.l %2,%3\;move%.l %3,%1";
	}
      else
	{
	  operands[1] = adjust_address (operands[0], SImode, 4);
	  return "sub%.l %R2,%1\;move%.l %0,%3\;subx%.l %2,%3\;move%.l %3,%0";
	}
    }
})

(define_insn "subsi3"
  [(set (match_operand:SI 0 "nonimmediate_operand" "=mda,m,d,a")
	(minus:SI (match_operand:SI 1 "general_operand" "0,0,0,0")
		  (match_operand:SI 2 "general_src_operand" "I,dT,mSrT,mSrs")))]
  ""
  "@
   subq%.l %2, %0
   sub%.l %2,%0
   sub%.l %2,%0
   sub%.l %2,%0"
  [(set_attr "type" "aluq_l,alu_l,alu_l,alu_l")
   (set_attr "opy" "2")])

(define_insn ""
  [(set (match_operand:SI 0 "nonimmediate_operand" "=a")
	(minus:SI (match_operand:SI 1 "general_operand" "0")
		  (sign_extend:SI
		   (match_operand:HI 2 "nonimmediate_src_operand" "rmS"))))]
  "!TARGET_COLDFIRE"
  "sub%.w %2,%0")

(define_insn "subhi3"
  [(set (match_operand:HI 0 "nonimmediate_operand" "=m,r")
	(minus:HI (match_operand:HI 1 "general_operand" "0,0")
		  (match_operand:HI 2 "general_src_operand" "dn,rmSn")))]
  "!TARGET_COLDFIRE"
  "sub%.w %2,%0")

(define_insn ""
  [(set (strict_low_part (match_operand:HI 0 "nonimmediate_operand" "+m,d"))
	(minus:HI (match_dup 0)
		  (match_operand:HI 1 "general_src_operand" "dn,rmSn")))]
  "!TARGET_COLDFIRE"
  "sub%.w %1,%0")

(define_insn "subqi3"
  [(set (match_operand:QI 0 "nonimmediate_operand" "=m,d")
	(minus:QI (match_operand:QI 1 "general_operand" "0,0")
		  (match_operand:QI 2 "general_src_operand" "dn,dmSn")))]
  "!TARGET_COLDFIRE"
  "sub%.b %2,%0")

(define_insn ""
  [(set (strict_low_part (match_operand:QI 0 "nonimmediate_operand" "+m,d"))
	(minus:QI (match_dup 0)
		  (match_operand:QI 1 "general_src_operand" "dn,dmSn")))]
  "!TARGET_COLDFIRE"
  "sub%.b %1,%0")

(define_expand "sub<mode>3"
  [(set (match_operand:FP 0 "nonimmediate_operand" "")
	(minus:FP (match_operand:FP 1 "general_operand" "")
		  (match_operand:FP 2 "general_operand" "")))]
  "TARGET_HARD_FLOAT"
  "")

(define_insn "sub<mode>3_floatsi_68881"
  [(set (match_operand:FP 0 "nonimmediate_operand" "=f")
	(minus:FP (match_operand:FP 1 "general_operand" "0")
		  (float:FP (match_operand:SI 2 "general_operand" "dmi"))))]
  "TARGET_68881"
  "f<FP:round>sub%.l %2,%0"
  [(set_attr "type" "falu")
   (set_attr "opy" "2")])

(define_insn "sub<mode>3_floathi_68881"
  [(set (match_operand:FP 0 "nonimmediate_operand" "=f")
	(minus:FP (match_operand:FP 1 "general_operand" "0")
		  (float:FP (match_operand:HI 2 "general_operand" "dmn"))))]
  "TARGET_68881"
  "f<FP:round>sub%.w %2,%0"
  [(set_attr "type" "falu")
   (set_attr "opy" "2")])

(define_insn "sub<mode>3_floatqi_68881"
  [(set (match_operand:FP 0 "nonimmediate_operand" "=f")
	(minus:FP (match_operand:FP 1 "general_operand" "0")
		  (float:FP (match_operand:QI 2 "general_operand" "dmn"))))]
  "TARGET_68881"
  "f<FP:round>sub%.b %2,%0"
  [(set_attr "type" "falu")
   (set_attr "opy" "2")])

(define_insn "sub<mode>3_68881"
  [(set (match_operand:FP 0 "nonimmediate_operand" "=f")
	(minus:FP (match_operand:FP 1 "general_operand" "0")
		  (match_operand:FP 2 "general_operand" "f<FP:dreg>m<FP:const>")))]
  "TARGET_68881"
{
  if (FP_REG_P (operands[2]))
    return "f<FP:round>sub%.x %2,%0";
  return "f<FP:round>sub%.<FP:prec> %f2,%0";
}
  [(set_attr "type" "falu")
   (set_attr "opy" "2")])

(define_insn "sub<mode>3_cf"
  [(set (match_operand:FP 0 "nonimmediate_operand" "=f")
        (minus:FP (match_operand:FP 1 "general_operand" "0")
                  (match_operand:FP 2 "general_operand" "f<FP:dreg><Q>U")))]
  "TARGET_COLDFIRE_FPU"
{
  if (FP_REG_P (operands[2]))
    return "f<FP:prec>sub%.d %2,%0";
  return "f<FP:prec>sub%.<FP:prec> %2,%0";
}
  [(set_attr "type" "falu")
   (set_attr "opy" "2")])

;; multiply instructions

(define_insn "mulhi3"
  [(set (match_operand:HI 0 "nonimmediate_operand" "=d")
	(mult:HI (match_operand:HI 1 "general_operand" "%0")
		 (match_operand:HI 2 "general_src_operand" "dmSn")))]
  ""
{
  return MOTOROLA ? "muls%.w %2,%0" : "muls %2,%0";
}
  [(set_attr "type" "mul_w")
   (set_attr "opy" "2")])

(define_insn "mulhisi3"
  [(set (match_operand:SI 0 "nonimmediate_operand" "=d")
	(mult:SI (sign_extend:SI
		  (match_operand:HI 1 "nonimmediate_operand" "%0"))
		 (sign_extend:SI
		  (match_operand:HI 2 "nonimmediate_src_operand" "dmS"))))]
  ""
{
  return MOTOROLA ? "muls%.w %2,%0" : "muls %2,%0";
}
  [(set_attr "type" "mul_w")
   (set_attr "opy" "2")])

(define_insn "*mulhisisi3_s"
  [(set (match_operand:SI 0 "nonimmediate_operand" "=d")
	(mult:SI (sign_extend:SI
		  (match_operand:HI 1 "nonimmediate_operand" "%0"))
		 (match_operand:SI 2 "const_int_operand" "n")))]
  "INTVAL (operands[2]) >= -0x8000 && INTVAL (operands[2]) <= 0x7fff"
{
  return MOTOROLA ? "muls%.w %2,%0" : "muls %2,%0";
}
  [(set_attr "type" "mul_w")
   (set_attr "opy" "2")])

(define_expand "mulsi3"
  [(set (match_operand:SI 0 "nonimmediate_operand" "")
	(mult:SI (match_operand:SI 1 "general_operand" "")
		 (match_operand:SI 2 "general_operand" "")))]
  "TARGET_68020 || TARGET_COLDFIRE"
  "")

(define_insn "*mulsi3_68020"
  [(set (match_operand:SI 0 "nonimmediate_operand" "=d")
	(mult:SI (match_operand:SI 1 "general_operand" "%0")
                 (match_operand:SI 2 "general_src_operand" "dmSTK")))]

  "TARGET_68020"
  "muls%.l %2,%0"
  [(set_attr "type" "mul_l")
   (set_attr "opy" "2")])

(define_insn "*mulsi3_cf"
  [(set (match_operand:SI 0 "nonimmediate_operand" "=d")
	(mult:SI (match_operand:SI 1 "general_operand" "%0")
		 (match_operand:SI 2 "general_operand" "d<Q>")))]
  "TARGET_COLDFIRE"
  "muls%.l %2,%0"
  [(set_attr "type" "mul_l")
   (set_attr "opy" "2")])

(define_insn "umulhisi3"
  [(set (match_operand:SI 0 "nonimmediate_operand" "=d")
	(mult:SI (zero_extend:SI
		  (match_operand:HI 1 "nonimmediate_operand" "%0"))
		 (zero_extend:SI
		  (match_operand:HI 2 "nonimmediate_src_operand" "dmS"))))]
  ""
{
  return MOTOROLA ? "mulu%.w %2,%0" : "mulu %2,%0";
}
  [(set_attr "type" "mul_w")
   (set_attr "opy" "2")])

(define_insn "*mulhisisi3_z"
  [(set (match_operand:SI 0 "nonimmediate_operand" "=d")
	(mult:SI (zero_extend:SI
		  (match_operand:HI 1 "nonimmediate_operand" "%0"))
		 (match_operand:SI 2 "const_int_operand" "n")))]
  "INTVAL (operands[2]) >= 0 && INTVAL (operands[2]) <= 0xffff"
{
  return MOTOROLA ? "mulu%.w %2,%0" : "mulu %2,%0";
}
  [(set_attr "type" "mul_w")
   (set_attr "opy" "2")])

;; We need a separate DEFINE_EXPAND for u?mulsidi3 to be able to use the
;; proper matching constraint.  This is because the matching is between
;; the high-numbered word of the DImode operand[0] and operand[1].
(define_expand "umulsidi3"
  [(parallel
    [(set (subreg:SI (match_operand:DI 0 "register_operand" "") 4)
	  (mult:SI (match_operand:SI 1 "register_operand" "")
		   (match_operand:SI 2 "register_operand" "")))
     (set (subreg:SI (match_dup 0) 0)
	  (truncate:SI (lshiftrt:DI (mult:DI (zero_extend:DI (match_dup 1))
					     (zero_extend:DI (match_dup 2)))
				    (const_int 32))))])]
  "TARGET_68020 && !TUNE_68060 && !TARGET_COLDFIRE"
  "")

(define_insn ""
  [(set (match_operand:SI 0 "register_operand" "=d")
	(mult:SI (match_operand:SI 1 "register_operand" "%0")
		  (match_operand:SI 2 "nonimmediate_operand" "dm")))
   (set (match_operand:SI 3 "register_operand" "=d")
	(truncate:SI (lshiftrt:DI (mult:DI (zero_extend:DI (match_dup 1))
					   (zero_extend:DI (match_dup 2)))
				  (const_int 32))))]
  "TARGET_68020 && !TUNE_68060 && !TARGET_COLDFIRE"
  "mulu%.l %2,%3:%0")

; Match immediate case.  For 2.4 only match things < 2^31.
; It's tricky with larger values in these patterns since we need to match
; values between the two parallel multiplies, between a CONST_DOUBLE and
; a CONST_INT.
(define_insn ""
  [(set (match_operand:SI 0 "register_operand" "=d")
	(mult:SI (match_operand:SI 1 "register_operand" "%0")
		 (match_operand:SI 2 "const_int_operand" "n")))
   (set (match_operand:SI 3 "register_operand" "=d")
	(truncate:SI (lshiftrt:DI (mult:DI (zero_extend:DI (match_dup 1))
					   (match_dup 2))
				  (const_int 32))))]
  "TARGET_68020 && !TUNE_68060 && !TARGET_COLDFIRE
   && (unsigned) INTVAL (operands[2]) <= 0x7fffffff"
  "mulu%.l %2,%3:%0")

(define_expand "mulsidi3"
  [(parallel
    [(set (subreg:SI (match_operand:DI 0 "register_operand" "") 4)
	  (mult:SI (match_operand:SI 1 "register_operand" "")
		   (match_operand:SI 2 "register_operand" "")))
     (set (subreg:SI (match_dup 0) 0)
	  (truncate:SI (lshiftrt:DI (mult:DI (sign_extend:DI (match_dup 1))
					     (sign_extend:DI (match_dup 2)))
				    (const_int 32))))])]
  "TARGET_68020 && !TUNE_68060 && !TARGET_COLDFIRE"
  "")

(define_insn ""
  [(set (match_operand:SI 0 "register_operand" "=d")
	(mult:SI (match_operand:SI 1 "register_operand" "%0")
		 (match_operand:SI 2 "nonimmediate_operand" "dm")))
   (set (match_operand:SI 3 "register_operand" "=d")
	(truncate:SI (lshiftrt:DI (mult:DI (sign_extend:DI (match_dup 1))
					   (sign_extend:DI (match_dup 2)))
				  (const_int 32))))]
  "TARGET_68020 && !TUNE_68060 && !TARGET_COLDFIRE"
  "muls%.l %2,%3:%0")

(define_insn ""
  [(set (match_operand:SI 0 "register_operand" "=d")
	(mult:SI (match_operand:SI 1 "register_operand" "%0")
		 (match_operand:SI 2 "const_int_operand" "n")))
   (set (match_operand:SI 3 "register_operand" "=d")
	(truncate:SI (lshiftrt:DI (mult:DI (sign_extend:DI (match_dup 1))
					   (match_dup 2))
				  (const_int 32))))]
  "TARGET_68020 && !TUNE_68060 && !TARGET_COLDFIRE"
  "muls%.l %2,%3:%0")

(define_expand "umulsi3_highpart"
  [(parallel
    [(set (match_operand:SI 0 "register_operand" "")
	  (truncate:SI
	   (lshiftrt:DI
	    (mult:DI (zero_extend:DI (match_operand:SI 1 "register_operand" ""))
		     (zero_extend:DI (match_operand:SI 2 "general_operand" "")))
	    (const_int 32))))
     (clobber (match_dup 3))])]
  "TARGET_68020 && !TUNE_68060 && !TARGET_COLDFIRE"
{
  operands[3] = gen_reg_rtx (SImode);

  if (GET_CODE (operands[2]) == CONST_INT)
    {
      operands[2] = immed_double_const (INTVAL (operands[2]) & 0xffffffff,
					0, DImode);

      /* We have to adjust the operand order for the matching constraints.  */
      emit_insn (gen_const_umulsi3_highpart (operands[0], operands[3],
					     operands[1], operands[2]));
      DONE;
    }
})

(define_insn ""
  [(set (match_operand:SI 0 "register_operand" "=d")
	(truncate:SI
	 (lshiftrt:DI
	  (mult:DI (zero_extend:DI (match_operand:SI 2 "register_operand" "%1"))
		   (zero_extend:DI (match_operand:SI 3 "nonimmediate_operand" "dm")))
	  (const_int 32))))
   (clobber (match_operand:SI 1 "register_operand" "=d"))]
  "TARGET_68020 && !TUNE_68060 && !TARGET_COLDFIRE"
  "mulu%.l %3,%0:%1")

(define_insn "const_umulsi3_highpart"
  [(set (match_operand:SI 0 "register_operand" "=d")
	(truncate:SI
	 (lshiftrt:DI
	  (mult:DI (zero_extend:DI (match_operand:SI 2 "register_operand" "1"))
		   (match_operand:DI 3 "const_uint32_operand" "n"))
	  (const_int 32))))
   (clobber (match_operand:SI 1 "register_operand" "=d"))]
  "TARGET_68020 && !TUNE_68060 && !TARGET_COLDFIRE"
  "mulu%.l %3,%0:%1")

(define_expand "smulsi3_highpart"
  [(parallel
    [(set (match_operand:SI 0 "register_operand" "")
	  (truncate:SI
	   (lshiftrt:DI
	    (mult:DI (sign_extend:DI (match_operand:SI 1 "register_operand" ""))
		     (sign_extend:DI (match_operand:SI 2 "general_operand" "")))
	    (const_int 32))))
     (clobber (match_dup 3))])]
  "TARGET_68020 && !TUNE_68060 && !TARGET_COLDFIRE"
{
  operands[3] = gen_reg_rtx (SImode);
  if (GET_CODE (operands[2]) == CONST_INT)
    {
      /* We have to adjust the operand order for the matching constraints.  */
      emit_insn (gen_const_smulsi3_highpart (operands[0], operands[3],
					     operands[1], operands[2]));
      DONE;
    }
})

(define_insn ""
  [(set (match_operand:SI 0 "register_operand" "=d")
	(truncate:SI
	 (lshiftrt:DI
	  (mult:DI (sign_extend:DI (match_operand:SI 2 "register_operand" "%1"))
		   (sign_extend:DI (match_operand:SI 3 "nonimmediate_operand" "dm")))
	  (const_int 32))))
   (clobber (match_operand:SI 1 "register_operand" "=d"))]
  "TARGET_68020 && !TUNE_68060 && !TARGET_COLDFIRE"
  "muls%.l %3,%0:%1")

(define_insn "const_smulsi3_highpart"
  [(set (match_operand:SI 0 "register_operand" "=d")
	(truncate:SI
	 (lshiftrt:DI
	  (mult:DI (sign_extend:DI (match_operand:SI 2 "register_operand" "1"))
		   (match_operand:DI 3 "const_sint32_operand" "n"))
	  (const_int 32))))
   (clobber (match_operand:SI 1 "register_operand" "=d"))]
  "TARGET_68020 && !TUNE_68060 && !TARGET_COLDFIRE"
  "muls%.l %3,%0:%1")

(define_expand "mul<mode>3"
  [(set (match_operand:FP 0 "nonimmediate_operand" "")
	(mult:FP (match_operand:FP 1 "general_operand" "")
		 (match_operand:FP 2 "general_operand" "")))]
  "TARGET_HARD_FLOAT"
  "")

(define_insn "mul<mode>3_floatsi_68881"
  [(set (match_operand:FP 0 "nonimmediate_operand" "=f")
	(mult:FP (float:FP (match_operand:SI 2 "general_operand" "dmi"))
		 (match_operand:FP 1 "general_operand" "0")))]
  "TARGET_68881"
{
  return TARGET_68040
	 ? "f<FP:round>mul%.l %2,%0"
	 : "f<FP:round_mul>mul%.l %2,%0";
}
  [(set_attr "type" "fmul")
   (set_attr "opy" "2")])

(define_insn "mul<mode>3_floathi_68881"
  [(set (match_operand:FP 0 "nonimmediate_operand" "=f")
	(mult:FP (float:FP (match_operand:HI 2 "general_operand" "dmn"))
		 (match_operand:FP 1 "general_operand" "0")))]
  "TARGET_68881"
{
  return TARGET_68040
	 ? "f<FP:round>mul%.w %2,%0"
	 : "f<FP:round_mul>mul%.w %2,%0";
}
  [(set_attr "type" "fmul")
   (set_attr "opy" "2")])

(define_insn "mul<mode>3_floatqi_68881"
  [(set (match_operand:FP 0 "nonimmediate_operand" "=f")
	(mult:FP (float:FP (match_operand:QI 2 "general_operand" "dmn"))
		 (match_operand:FP 1 "general_operand" "0")))]
  "TARGET_68881"
{
  return TARGET_68040
	 ? "f<FP:round>mul%.b %2,%0"
	 : "f<FP:round_mul>mul%.b %2,%0";
}
  [(set_attr "type" "fmul")
   (set_attr "opy" "2")])

(define_insn "muldf_68881"
  [(set (match_operand:DF 0 "nonimmediate_operand" "=f")
	(mult:DF (match_operand:DF 1 "general_operand" "%0")
		 (match_operand:DF 2 "general_operand" "fmG")))]
  "TARGET_68881"
{
  if (GET_CODE (operands[2]) == CONST_DOUBLE
      && floating_exact_log2 (operands[2]) && !TUNE_68040_60)
    {
      int i = floating_exact_log2 (operands[2]);
      operands[2] = GEN_INT (i);
      return "fscale%.l %2,%0";
    }
  if (REG_P (operands[2]))
    return "f%&mul%.x %2,%0";
  return "f%&mul%.d %f2,%0";
})

(define_insn "mulsf_68881"
  [(set (match_operand:SF 0 "nonimmediate_operand" "=f")
	(mult:SF (match_operand:SF 1 "general_operand" "%0")
		 (match_operand:SF 2 "general_operand" "fdmF")))]
  "TARGET_68881"
{
  if (FP_REG_P (operands[2]))
    return (TARGET_68040
	    ? "fsmul%.x %2,%0"
	    : "fsglmul%.x %2,%0");
  return (TARGET_68040
	  ? "fsmul%.s %f2,%0"
	  : "fsglmul%.s %f2,%0");
})

(define_insn "mulxf3_68881"
  [(set (match_operand:XF 0 "nonimmediate_operand" "=f")
	(mult:XF (match_operand:XF 1 "nonimmediate_operand" "%0")
		 (match_operand:XF 2 "nonimmediate_operand" "fm")))]
  "TARGET_68881"
{
  return "fmul%.x %f2,%0";
})

(define_insn "fmul<mode>3_cf"
  [(set (match_operand:FP 0 "nonimmediate_operand" "=f")
	(mult:FP (match_operand:FP 1 "general_operand" "%0")
		 (match_operand:FP 2 "general_operand" "f<Q>U<FP:dreg>")))]
  "TARGET_COLDFIRE_FPU"
{
  if (FP_REG_P (operands[2]))
    return "f<FP:prec>mul%.d %2,%0";
  return "f<FP:prec>mul%.<FP:prec> %2,%0";
}
  [(set_attr "type" "fmul")
   (set_attr "opy" "2")])

;; divide instructions

(define_expand "div<mode>3"
  [(set (match_operand:FP 0 "nonimmediate_operand" "")
	(div:FP (match_operand:FP 1 "general_operand" "")
		(match_operand:FP 2 "general_operand" "")))]
  "TARGET_HARD_FLOAT"
  "")

(define_insn "div<mode>3_floatsi_68881"
  [(set (match_operand:FP 0 "nonimmediate_operand" "=f")
	(div:FP (match_operand:FP 1 "general_operand" "0")
		(float:FP (match_operand:SI 2 "general_operand" "dmi"))))]
  "TARGET_68881"
{
  return TARGET_68040
	 ? "f<FP:round>div%.l %2,%0"
	 : "f<FP:round_mul>div%.l %2,%0";
})

(define_insn "div<mode>3_floathi_68881"
  [(set (match_operand:FP 0 "nonimmediate_operand" "=f")
	(div:FP (match_operand:FP 1 "general_operand" "0")
		(float:FP (match_operand:HI 2 "general_operand" "dmn"))))]
  "TARGET_68881"
{
  return TARGET_68040
	 ? "f<FP:round>div%.w %2,%0"
	 : "f<FP:round_mul>div%.w %2,%0";
})

(define_insn "div<mode>3_floatqi_68881"
  [(set (match_operand:FP 0 "nonimmediate_operand" "=f")
	(div:FP (match_operand:FP 1 "general_operand" "0")
		(float:FP (match_operand:QI 2 "general_operand" "dmn"))))]
  "TARGET_68881"
{
  return TARGET_68040
	 ? "f<FP:round>div%.b %2,%0"
	 : "f<FP:round_mul>div%.b %2,%0";
})

(define_insn "div<mode>3_68881"
  [(set (match_operand:FP 0 "nonimmediate_operand" "=f")
	(div:FP (match_operand:FP 1 "general_operand" "0")
		(match_operand:FP 2 "general_operand" "f<FP:dreg>m<FP:const>")))]
  "TARGET_68881"
{
  if (FP_REG_P (operands[2]))
    return (TARGET_68040
	    ? "f<FP:round>div%.x %2,%0"
	    : "f<FP:round_mul>div%.x %2,%0");
  return (TARGET_68040
	  ? "f<FP:round>div%.<FP:prec> %f2,%0"
	  : "f<FP:round_mul>div%.<FP:prec> %f2,%0");
})

(define_insn "div<mode>3_cf"
  [(set (match_operand:FP 0 "nonimmediate_operand" "=f")
	(div:FP (match_operand:FP 1 "general_operand" "0")
		(match_operand:FP 2 "general_operand" "f<Q>U<FP:dreg>")))]
  "TARGET_COLDFIRE_FPU"
{
  if (FP_REG_P (operands[2]))
    return "f<FP:prec>div%.d %2,%0";
  return "f<FP:prec>div%.<FP:prec> %2,%0";
}
  [(set_attr "type" "fdiv")
   (set_attr "opy" "2")])

;; Remainder instructions.

(define_expand "divmodsi4"
  [(parallel
    [(set (match_operand:SI 0 "nonimmediate_operand" "")
          (div:SI (match_operand:SI 1 "general_operand" "")
                  (match_operand:SI 2 "general_src_operand" "")))
     (set (match_operand:SI 3 "nonimmediate_operand" "")
          (mod:SI (match_dup 1) (match_dup 2)))])]
  "TARGET_68020 || TARGET_CF_HWDIV"
  "")

(define_insn ""
  [(set (match_operand:SI 0 "nonimmediate_operand" "=d")
	(div:SI (match_operand:SI 1 "general_operand" "0")
		(match_operand:SI 2 "general_src_operand" "d<Q>U")))
   (set (match_operand:SI 3 "nonimmediate_operand" "=&d")
	(mod:SI (match_dup 1) (match_dup 2)))]
  "TARGET_CF_HWDIV"
{
  if (find_reg_note (insn, REG_UNUSED, operands[3]))
    return "divs%.l %2,%0";
  else if (find_reg_note (insn, REG_UNUSED, operands[0]))
    return "rems%.l %2,%3:%0";
  else
    return "rems%.l %2,%3:%0\;divs%.l %2,%0";
}
  [(set_attr "type" "div_l")
   (set_attr "opy" "2")])

(define_insn ""
  [(set (match_operand:SI 0 "nonimmediate_operand" "=d")
	(div:SI (match_operand:SI 1 "general_operand" "0")
		(match_operand:SI 2 "general_src_operand" "dmSTK")))
   (set (match_operand:SI 3 "nonimmediate_operand" "=d")
	(mod:SI (match_dup 1) (match_dup 2)))]
  "TARGET_68020"
{
  if (find_reg_note (insn, REG_UNUSED, operands[3]))
    return "divs%.l %2,%0";
  else
    return "divsl%.l %2,%3:%0";
})

(define_expand "udivmodsi4"
  [(parallel
    [(set (match_operand:SI 0 "nonimmediate_operand" "=d")
          (udiv:SI (match_operand:SI 1 "general_operand" "0")
                   (match_operand:SI 2 "general_src_operand" "dmSTK")))
     (set (match_operand:SI 3 "nonimmediate_operand" "=d")
          (umod:SI (match_dup 1) (match_dup 2)))])]
  "TARGET_68020 || TARGET_CF_HWDIV"
  "")

(define_insn ""
  [(set (match_operand:SI 0 "nonimmediate_operand" "=d")
	(udiv:SI (match_operand:SI 1 "general_operand" "0")
		 (match_operand:SI 2 "general_src_operand" "d<Q>U")))
   (set (match_operand:SI 3 "nonimmediate_operand" "=&d")
	(umod:SI (match_dup 1) (match_dup 2)))]
  "TARGET_CF_HWDIV"
{
  if (find_reg_note (insn, REG_UNUSED, operands[3]))
    return "divu%.l %2,%0";
  else if (find_reg_note (insn, REG_UNUSED, operands[0]))
    return "remu%.l %2,%3:%0";
  else
    return "remu%.l %2,%3:%0\;divu%.l %2,%0";
}
  [(set_attr "type" "div_l")
   (set_attr "opy" "2")])

(define_insn ""
  [(set (match_operand:SI 0 "nonimmediate_operand" "=d")
	(udiv:SI (match_operand:SI 1 "general_operand" "0")
		 (match_operand:SI 2 "general_src_operand" "dmSTK")))
   (set (match_operand:SI 3 "nonimmediate_operand" "=d")
	(umod:SI (match_dup 1) (match_dup 2)))]
  "TARGET_68020 && !TARGET_COLDFIRE"
{
  if (find_reg_note (insn, REG_UNUSED, operands[3]))
    return "divu%.l %2,%0";
  else
    return "divul%.l %2,%3:%0";
})

(define_insn "divmodhi4"
  [(set (match_operand:HI 0 "nonimmediate_operand" "=d")
	(div:HI (match_operand:HI 1 "general_operand" "0")
		(match_operand:HI 2 "general_src_operand" "dmSKT")))
   (set (match_operand:HI 3 "nonimmediate_operand" "=d")
	(mod:HI (match_dup 1) (match_dup 2)))]
  "!TARGET_COLDFIRE || TARGET_CF_HWDIV"
{
  output_asm_insn (MOTOROLA ?
    "ext%.l %0\;divs%.w %2,%0" :
    "extl %0\;divs %2,%0",
    operands);
  if (!find_reg_note(insn, REG_UNUSED, operands[3]))
    {
      CC_STATUS_INIT;
      return "move%.l %0,%3\;swap %3";
    }
  else
    return "";
})

(define_insn "udivmodhi4"
  [(set (match_operand:HI 0 "nonimmediate_operand" "=d")
	(udiv:HI (match_operand:HI 1 "general_operand" "0")
		 (match_operand:HI 2 "general_src_operand" "dmSKT")))
   (set (match_operand:HI 3 "nonimmediate_operand" "=d")
	(umod:HI (match_dup 1) (match_dup 2)))]
  "!TARGET_COLDFIRE || TARGET_CF_HWDIV"
{
  if (ISA_HAS_MVS_MVZ)
    output_asm_insn (MOTOROLA ?
      "mvz%.w %0,%0\;divu%.w %2,%0" :
      "mvz%.w %0,%0\;divu %2,%0",
      operands);
  else
    output_asm_insn (MOTOROLA ?
      "and%.l #0xFFFF,%0\;divu%.w %2,%0" :
      "and%.l #0xFFFF,%0\;divu %2,%0",
      operands);

  if (!find_reg_note(insn, REG_UNUSED, operands[3]))
    {
      CC_STATUS_INIT;
      return "move%.l %0,%3\;swap %3";
    }
  else
    return "";
})

;; logical-and instructions

;; Prevent AND from being made with sp.  This doesn't exist in the machine
;; and reload will cause inefficient code.  Since sp is a FIXED_REG, we
;; can't allocate pseudos into it.

(define_expand "andsi3"
  [(set (match_operand:SI 0 "not_sp_operand" "")
	(and:SI (match_operand:SI 1 "general_operand" "")
		(match_operand:SI 2 "general_src_operand" "")))]
  ""
  "")

;; produced by split operations after reload finished
(define_insn "*andsi3_split"
  [(set (match_operand:SI 0 "register_operand" "=d")
	(and:SI (match_operand:SI 1 "register_operand" "0")
		(match_operand:SI 2 "const_int_operand" "i")))]
  "reload_completed && !TARGET_COLDFIRE"
{
  return output_andsi3 (operands);
})

(define_insn "andsi3_internal"
  [(set (match_operand:SI 0 "not_sp_operand" "=m,d")
	(and:SI (match_operand:SI 1 "general_operand" "%0,0")
		(match_operand:SI 2 "general_src_operand" "dKT,dmSM")))]
  "!TARGET_COLDFIRE"
{
  return output_andsi3 (operands);
})

(define_insn "andsi3_5200"
  [(set (match_operand:SI 0 "not_sp_operand" "=m,d")
	(and:SI (match_operand:SI 1 "general_operand" "%0,0")
		(match_operand:SI 2 "general_src_operand" "d,dmsK")))]
  "TARGET_COLDFIRE"
{
  if (ISA_HAS_MVS_MVZ
      && DATA_REG_P (operands[0])
      && GET_CODE (operands[2]) == CONST_INT)
    {
      if (INTVAL (operands[2]) == 0x000000ff)
        return "mvz%.b %0,%0";
      else if (INTVAL (operands[2]) == 0x0000ffff)
        return "mvz%.w %0,%0";
    }
  return output_andsi3 (operands);
})

(define_insn "andhi3"
  [(set (match_operand:HI 0 "nonimmediate_operand" "=m,d")
	(and:HI (match_operand:HI 1 "general_operand" "%0,0")
		(match_operand:HI 2 "general_src_operand" "dn,dmSn")))]
  "!TARGET_COLDFIRE"
  "and%.w %2,%0")

(define_insn ""
  [(set (strict_low_part (match_operand:HI 0 "nonimmediate_operand" "+m,d"))
	(and:HI (match_dup 0)
		(match_operand:HI 1 "general_src_operand" "dn,dmSn")))]
  "!TARGET_COLDFIRE"
  "and%.w %1,%0")

(define_insn ""
  [(set (strict_low_part (match_operand:HI 0 "nonimmediate_operand" "+m,d"))
	(and:HI (match_operand:HI 1 "general_src_operand" "dn,dmSn")
		(match_dup 0)))]
  "!TARGET_COLDFIRE"
  "and%.w %1,%0")

(define_insn "andqi3"
  [(set (match_operand:QI 0 "nonimmediate_operand" "=m,d")
	(and:QI (match_operand:QI 1 "general_operand" "%0,0")
		(match_operand:QI 2 "general_src_operand" "dn,dmSn")))]
  "!TARGET_COLDFIRE"
  "and%.b %2,%0")

(define_insn ""
  [(set (strict_low_part (match_operand:QI 0 "nonimmediate_operand" "+m,d"))
	(and:QI (match_dup 0)
		(match_operand:QI 1 "general_src_operand" "dn,dmSn")))]
  "!TARGET_COLDFIRE"
  "and%.b %1,%0")

(define_insn ""
  [(set (strict_low_part (match_operand:QI 0 "nonimmediate_operand" "+m,d"))
	(and:QI (match_operand:QI 1 "general_src_operand" "dn,dmSn")
		(match_dup 0)))]
  "!TARGET_COLDFIRE"
  "and%.b %1,%0")

;; inclusive-or instructions

(define_insn "iordi_zext"
  [(set (match_operand:DI 0 "nonimmediate_operand" "=o,d")
    (ior:DI (zero_extend:DI (match_operand 1 "general_operand" "dn,dmn"))
        (match_operand:DI 2 "general_operand" "0,0")))]
  "!TARGET_COLDFIRE"
{
  int byte_mode;

  CC_STATUS_INIT;
  if (GET_CODE (operands[0]) == REG)
    operands[0] = gen_rtx_REG (SImode, REGNO (operands[0]) + 1);
  else
    operands[0] = adjust_address (operands[0], SImode, 4);
  if (GET_MODE (operands[1]) == SImode)
    return "or%.l %1,%0";
  byte_mode = (GET_MODE (operands[1]) == QImode);
  if (GET_CODE (operands[0]) == MEM)
    operands[0] = adjust_address (operands[0], byte_mode ? QImode : HImode,
				  byte_mode ? 3 : 2);
  if (byte_mode)
    return "or%.b %1,%0";
  else
    return "or%.w %1,%0";
})

(define_expand "iorsi3"
  [(set (match_operand:SI 0 "nonimmediate_operand" "")
	(ior:SI (match_operand:SI 1 "general_operand" "")
		(match_operand:SI 2 "general_src_operand" "")))]
  ""
  "")

(define_insn "iorsi3_internal"
  [(set (match_operand:SI 0 "nonimmediate_operand" "=m,d")
	(ior:SI (match_operand:SI 1 "general_operand" "%0,0")
                (match_operand:SI 2 "general_src_operand" "dKT,dmSMT")))]
  "! TARGET_COLDFIRE"
{
  return output_iorsi3 (operands);
})

(define_insn "iorsi3_5200"
  [(set (match_operand:SI 0 "nonimmediate_operand" "=m,d")
	(ior:SI (match_operand:SI 1 "general_operand" "%0,0")
		(match_operand:SI 2 "general_src_operand" "d,dmsK")))]
  "TARGET_COLDFIRE"
{
  return output_iorsi3 (operands);
})

(define_insn "iorhi3"
  [(set (match_operand:HI 0 "nonimmediate_operand" "=m,d")
	(ior:HI (match_operand:HI 1 "general_operand" "%0,0")
		(match_operand:HI 2 "general_src_operand" "dn,dmSn")))]
  "!TARGET_COLDFIRE"
  "or%.w %2,%0")

(define_insn ""
  [(set (strict_low_part (match_operand:HI 0 "nonimmediate_operand" "+m,d"))
	(ior:HI (match_dup 0)
		(match_operand:HI 1 "general_src_operand" "dn,dmSn")))]
  "!TARGET_COLDFIRE"
  "or%.w %1,%0")

(define_insn ""
  [(set (strict_low_part (match_operand:HI 0 "nonimmediate_operand" "+m,d"))
	(ior:HI (match_operand:HI 1 "general_src_operand" "dn,dmSn")
		(match_dup 0)))]
  "!TARGET_COLDFIRE"
  "or%.w %1,%0")

(define_insn "iorqi3"
  [(set (match_operand:QI 0 "nonimmediate_operand" "=m,d")
	(ior:QI (match_operand:QI 1 "general_operand" "%0,0")
                (match_operand:QI 2 "general_src_operand" "dn,dmSn")))]
  "!TARGET_COLDFIRE"
  "or%.b %2,%0")

(define_insn ""
  [(set (strict_low_part (match_operand:QI 0 "nonimmediate_operand" "+m,d"))
	(ior:QI (match_dup 0)
                (match_operand:QI 1 "general_src_operand" "dn,dmSn")))]
  "!TARGET_COLDFIRE"
  "or%.b %1,%0")

(define_insn ""
  [(set (strict_low_part (match_operand:QI 0 "nonimmediate_operand" "+m,d"))
        (ior:QI (match_operand:QI 1 "general_src_operand" "dn,dmSn")
		(match_dup 0)))]
  "!TARGET_COLDFIRE"
  "or%.b %1,%0")

;; On all 68k models, this makes faster code in a special case.
;; See also ashlsi_16, ashrsi_16 and lshrsi_16.

(define_insn "iorsi_zexthi_ashl16"
  [(set (match_operand:SI 0 "nonimmediate_operand" "=&d")
    (ior:SI (zero_extend:SI (match_operand:HI 1 "general_operand" "rmn"))
        (ashift:SI (match_operand:SI 2 "general_operand" "or")
            (const_int 16))))]
  ""
{
  CC_STATUS_INIT;
  if (GET_CODE (operands[2]) != REG)
      operands[2] = adjust_address (operands[2], HImode, 2);
  if (GET_CODE (operands[2]) != REG
  || REGNO (operands[2]) != REGNO (operands[0]))
    output_asm_insn ("move%.w %2,%0", operands);
  return "swap %0\;mov%.w %1,%0";
})

(define_insn "iorsi_zext"
  [(set (match_operand:SI 0 "nonimmediate_operand" "=o,d")
    (ior:SI (zero_extend:SI (match_operand 1 "general_operand" "dn,dmn"))
        (match_operand:SI 2 "general_operand" "0,0")))]
  "!TARGET_COLDFIRE"
{
  int byte_mode;

  CC_STATUS_INIT;
  byte_mode = (GET_MODE (operands[1]) == QImode);
  if (GET_CODE (operands[0]) == MEM)
    operands[0] = adjust_address (operands[0], byte_mode ? QImode : HImode,
				  byte_mode ? 3 : 2);
  if (byte_mode)
    return "or%.b %1,%0";
  else
    return "or%.w %1,%0";
})

;; xor instructions

(define_expand "xorsi3"
  [(set (match_operand:SI 0 "nonimmediate_operand" "")
	(xor:SI (match_operand:SI 1 "general_operand" "")
		(match_operand:SI 2 "general_operand" "")))]
  ""
  "")

(define_insn "xorsi3_internal"
  [(set (match_operand:SI 0 "nonimmediate_operand" "=do,m")
	(xor:SI (match_operand:SI 1 "general_operand" "%0,0")
                (match_operand:SI 2 "general_operand" "di,dKT")))]

  "!TARGET_COLDFIRE"
{
  return output_xorsi3 (operands);
})

(define_insn "xorsi3_5200"
  [(set (match_operand:SI 0 "nonimmediate_operand" "=dm,d")
	(xor:SI (match_operand:SI 1 "general_operand" "%0,0")
		(match_operand:SI 2 "general_operand" "d,Ks")))]
  "TARGET_COLDFIRE"
{
  return output_xorsi3 (operands);
})

(define_insn "xorhi3"
  [(set (match_operand:HI 0 "nonimmediate_operand" "=dm")
	(xor:HI (match_operand:HI 1 "general_operand" "%0")
		(match_operand:HI 2 "general_operand" "dn")))]
  "!TARGET_COLDFIRE"
  "eor%.w %2,%0")

(define_insn ""
  [(set (strict_low_part (match_operand:HI 0 "nonimmediate_operand" "+dm"))
	(xor:HI (match_dup 0)
		(match_operand:HI 1 "general_operand" "dn")))]
  "!TARGET_COLDFIRE"
  "eor%.w %1,%0")

(define_insn ""
  [(set (strict_low_part (match_operand:HI 0 "nonimmediate_operand" "+dm"))
	(xor:HI (match_operand:HI 1 "general_operand" "dn")
		(match_dup 0)))]
  "!TARGET_COLDFIRE"
  "eor%.w %1,%0")

(define_insn "xorqi3"
  [(set (match_operand:QI 0 "nonimmediate_operand" "=dm")
	(xor:QI (match_operand:QI 1 "general_operand" "%0")
		(match_operand:QI 2 "general_operand" "dn")))]
  "!TARGET_COLDFIRE"
  "eor%.b %2,%0")

(define_insn ""
  [(set (strict_low_part (match_operand:QI 0 "nonimmediate_operand" "+dm"))
	(xor:QI (match_dup 0)
		(match_operand:QI 1 "general_operand" "dn")))]
  "!TARGET_COLDFIRE"
  "eor%.b %1,%0")

(define_insn ""
  [(set (strict_low_part (match_operand:QI 0 "nonimmediate_operand" "+dm"))
	(xor:QI (match_operand:QI 1 "general_operand" "dn")
		(match_dup 0)))]
  "!TARGET_COLDFIRE"
  "eor%.b %1,%0")

;; negation instructions

(define_expand "negdi2"
  [(set (match_operand:DI 0 "nonimmediate_operand" "")
	(neg:DI (match_operand:DI 1 "general_operand" "")))]
  ""
{
  if (TARGET_COLDFIRE)
    emit_insn (gen_negdi2_5200 (operands[0], operands[1]));
  else
    emit_insn (gen_negdi2_internal (operands[0], operands[1]));
  DONE;
})

(define_insn "negdi2_internal"
  [(set (match_operand:DI 0 "nonimmediate_operand" "=<,do,!*a")
	(neg:DI (match_operand:DI 1 "general_operand" "0,0,0")))]
  "!TARGET_COLDFIRE"
{
  if (which_alternative == 0)
    return "neg%.l %0\;negx%.l %0";
  if (GET_CODE (operands[0]) == REG)
    operands[1] = gen_rtx_REG (SImode, REGNO (operands[0]) + 1);
  else
    operands[1] = adjust_address (operands[0], SImode, 4);
  if (ADDRESS_REG_P (operands[0]))
    return "exg %/d0,%1\;neg%.l %/d0\;exg %/d0,%1\;exg %/d0,%0\;negx%.l %/d0\;exg %/d0,%0";
  else
    return "neg%.l %1\;negx%.l %0";
})

(define_insn "negdi2_5200"
  [(set (match_operand:DI 0 "nonimmediate_operand" "=d")
	(neg:DI (match_operand:DI 1 "general_operand" "0")))]
  "TARGET_COLDFIRE"
{
  operands[1] = gen_rtx_REG (SImode, REGNO (operands[0]) + 1);
  return "neg%.l %1\;negx%.l %0";
})

(define_expand "negsi2"
  [(set (match_operand:SI 0 "nonimmediate_operand" "")
	(neg:SI (match_operand:SI 1 "general_operand" "")))]
  ""
{
  if (TARGET_COLDFIRE)
    emit_insn (gen_negsi2_5200 (operands[0], operands[1]));
  else
    emit_insn (gen_negsi2_internal (operands[0], operands[1]));
  DONE;
})

(define_insn "negsi2_internal"
  [(set (match_operand:SI 0 "nonimmediate_operand" "=dm")
	(neg:SI (match_operand:SI 1 "general_operand" "0")))]
  "!TARGET_COLDFIRE"
  "neg%.l %0"
  [(set_attr "type" "neg_l")])

(define_insn "negsi2_5200"
  [(set (match_operand:SI 0 "nonimmediate_operand" "=d")
	(neg:SI (match_operand:SI 1 "general_operand" "0")))]
  "TARGET_COLDFIRE"
  "neg%.l %0"
  [(set_attr "type" "neg_l")])

(define_insn "neghi2"
  [(set (match_operand:HI 0 "nonimmediate_operand" "=dm")
	(neg:HI (match_operand:HI 1 "general_operand" "0")))]
  "!TARGET_COLDFIRE"
  "neg%.w %0")

(define_insn ""
  [(set (strict_low_part (match_operand:HI 0 "nonimmediate_operand" "+dm"))
	(neg:HI (match_dup 0)))]
  "!TARGET_COLDFIRE"
  "neg%.w %0")

(define_insn "negqi2"
  [(set (match_operand:QI 0 "nonimmediate_operand" "=dm")
	(neg:QI (match_operand:QI 1 "general_operand" "0")))]
  "!TARGET_COLDFIRE"
  "neg%.b %0")

(define_insn ""
  [(set (strict_low_part (match_operand:QI 0 "nonimmediate_operand" "+dm"))
	(neg:QI (match_dup 0)))]
  "!TARGET_COLDFIRE"
  "neg%.b %0")

;; If using software floating point, just flip the sign bit.

(define_expand "negsf2"
  [(set (match_operand:SF 0 "nonimmediate_operand" "")
	(neg:SF (match_operand:SF 1 "general_operand" "")))]
  ""
{
  if (!TARGET_HARD_FLOAT)
    {
      rtx result;
      rtx target;

      target = operand_subword_force (operands[0], 0, SFmode);
      result = expand_binop (SImode, xor_optab,
			     operand_subword_force (operands[1], 0, SFmode),
			     GEN_INT (-2147483647 - 1), target, 0, OPTAB_WIDEN);
      gcc_assert (result);

      if (result != target)
	emit_move_insn (result, target);

      /* Make a place for REG_EQUAL.  */
      emit_move_insn (operands[0], operands[0]);
      DONE;
    }
})

(define_expand "negdf2"
  [(set (match_operand:DF 0 "nonimmediate_operand" "")
	(neg:DF (match_operand:DF 1 "general_operand" "")))]
  ""
{
  if (!TARGET_HARD_FLOAT)
    {
      rtx result;
      rtx target;
      rtx insns;

      start_sequence ();
      target = operand_subword (operands[0], 0, 1, DFmode);
      result = expand_binop (SImode, xor_optab,
			     operand_subword_force (operands[1], 0, DFmode),
			     GEN_INT (-2147483647 - 1), target, 0, OPTAB_WIDEN);
      gcc_assert (result);

      if (result != target)
	emit_move_insn (result, target);

      emit_move_insn (operand_subword (operands[0], 1, 1, DFmode),
		      operand_subword_force (operands[1], 1, DFmode));

      insns = get_insns ();
      end_sequence ();

      emit_insn (insns);
      DONE;
    }
})

(define_expand "negxf2"
  [(set (match_operand:XF 0 "nonimmediate_operand" "")
	(neg:XF (match_operand:XF 1 "nonimmediate_operand" "")))]
  ""
{
  if (!TARGET_68881)
    {
      rtx result;
      rtx target;
      rtx insns;

      start_sequence ();
      target = operand_subword (operands[0], 0, 1, XFmode);
      result = expand_binop (SImode, xor_optab,
			     operand_subword_force (operands[1], 0, XFmode),
			     GEN_INT (-2147483647 - 1), target, 0, OPTAB_WIDEN);
      gcc_assert (result);

      if (result != target)
	emit_move_insn (result, target);

      emit_move_insn (operand_subword (operands[0], 1, 1, XFmode),
		      operand_subword_force (operands[1], 1, XFmode));
      emit_move_insn (operand_subword (operands[0], 2, 1, XFmode),
		      operand_subword_force (operands[1], 2, XFmode));

      insns = get_insns ();
      end_sequence ();

      emit_insn (insns);
      DONE;
    }
})

(define_insn "neg<mode>2_68881"
  [(set (match_operand:FP 0 "nonimmediate_operand" "=f,d")
	(neg:FP (match_operand:FP 1 "general_operand" "f<FP:dreg>m<FP:const>,0")))]
  "TARGET_68881"
{
  if (DATA_REG_P (operands[0]))
    {
      operands[1] = GEN_INT (31);
      return "bchg %1,%0";
    }
  if (FP_REG_P (operands[1]))
    return "f<FP:round>neg%.x %1,%0";
  return "f<FP:round>neg%.<FP:prec> %f1,%0";
})

(define_insn "neg<mode>2_cf"
  [(set (match_operand:FP 0 "nonimmediate_operand" "=f,d")
	(neg:FP (match_operand:FP 1 "general_operand" "f<FP:dreg><Q>U,0")))]
  "TARGET_COLDFIRE_FPU"
{
  if (DATA_REG_P (operands[0]))
    {
      operands[1] = GEN_INT (31);
      return "bchg %1,%0";
    }
  if (FP_REG_P (operands[1]))
    return "f<FP:prec>neg%.d %1,%0";
  return "f<FP:prec>neg%.<FP:prec> %1,%0";
})

;; Sqrt instruction for the 68881

(define_expand "sqrt<mode>2"
  [(set (match_operand:FP 0 "nonimmediate_operand" "")
	(sqrt:FP (match_operand:FP 1 "general_operand" "")))]
  "TARGET_HARD_FLOAT"
  "")

(define_insn "sqrt<mode>2_68881"
  [(set (match_operand:FP 0 "nonimmediate_operand" "=f")
	(sqrt:FP (match_operand:FP 1 "general_operand" "f<FP:dreg>m")))]
  "TARGET_68881"
{
  if (FP_REG_P (operands[1]))
    return "f<FP:round>sqrt%.x %1,%0";
  return "f<FP:round>sqrt%.<FP:prec> %1,%0";
}
  [(set_attr "type" "fsqrt")])

(define_insn "sqrt<mode>2_cf"
  [(set (match_operand:FP 0 "nonimmediate_operand" "=f")
	(sqrt:FP (match_operand:FP 1 "general_operand" "f<FP:dreg><Q>U")))]
  "TARGET_COLDFIRE_FPU"
{
  if (FP_REG_P (operands[1]))
    return "f<FP:prec>sqrt%.d %1,%0";
  return "f<FP:prec>sqrt%.<FP:prec> %1,%0";
}
  [(set_attr "type" "fsqrt")])
;; Absolute value instructions
;; If using software floating point, just zero the sign bit.

(define_expand "abssf2"
  [(set (match_operand:SF 0 "nonimmediate_operand" "")
	(abs:SF (match_operand:SF 1 "general_operand" "")))]
  ""
{
  if (!TARGET_HARD_FLOAT)
    {
      rtx result;
      rtx target;

      target = operand_subword_force (operands[0], 0, SFmode);
      result = expand_binop (SImode, and_optab,
			     operand_subword_force (operands[1], 0, SFmode),
			     GEN_INT (0x7fffffff), target, 0, OPTAB_WIDEN);
      gcc_assert (result);

      if (result != target)
	emit_move_insn (result, target);

      /* Make a place for REG_EQUAL.  */
      emit_move_insn (operands[0], operands[0]);
      DONE;
    }
})

(define_expand "absdf2"
  [(set (match_operand:DF 0 "nonimmediate_operand" "")
	(abs:DF (match_operand:DF 1 "general_operand" "")))]
  ""
{
  if (!TARGET_HARD_FLOAT)
    {
      rtx result;
      rtx target;
      rtx insns;

      start_sequence ();
      target = operand_subword (operands[0], 0, 1, DFmode);
      result = expand_binop (SImode, and_optab,
			     operand_subword_force (operands[1], 0, DFmode),
			     GEN_INT (0x7fffffff), target, 0, OPTAB_WIDEN);
      gcc_assert (result);

      if (result != target)
	emit_move_insn (result, target);

      emit_move_insn (operand_subword (operands[0], 1, 1, DFmode),
		      operand_subword_force (operands[1], 1, DFmode));

      insns = get_insns ();
      end_sequence ();

      emit_insn (insns);
      DONE;
    }
})

(define_expand "absxf2"
  [(set (match_operand:XF 0 "nonimmediate_operand" "")
	(abs:XF (match_operand:XF 1 "nonimmediate_operand" "")))]
  ""
{
  if (!TARGET_68881)
    {
      rtx result;
      rtx target;
      rtx insns;

      start_sequence ();
      target = operand_subword (operands[0], 0, 1, XFmode);
      result = expand_binop (SImode, and_optab,
			     operand_subword_force (operands[1], 0, XFmode),
			     GEN_INT (0x7fffffff), target, 0, OPTAB_WIDEN);
      gcc_assert (result);

      if (result != target)
	emit_move_insn (result, target);

      emit_move_insn (operand_subword (operands[0], 1, 1, XFmode),
		      operand_subword_force (operands[1], 1, XFmode));
      emit_move_insn (operand_subword (operands[0], 2, 1, XFmode),
		      operand_subword_force (operands[1], 2, XFmode));

      insns = get_insns ();
      end_sequence ();

      emit_insn (insns);
      DONE;
    }
})

(define_insn "abs<mode>2_68881"
  [(set (match_operand:FP 0 "nonimmediate_operand" "=f,d")
	(abs:FP (match_operand:FP 1 "general_operand" "f<FP:dreg>m<FP:const>,0")))]
  "TARGET_68881"
{
  if (DATA_REG_P (operands[0]))
    {
      operands[1] = GEN_INT (31);
      return "bclr %1,%0";
    }
  if (FP_REG_P (operands[1]))
    return "f<FP:round>abs%.x %1,%0";
  return "f<FP:round>abs%.<FP:prec> %f1,%0";
})

(define_insn "abs<mode>2_cf"
  [(set (match_operand:FP 0 "nonimmediate_operand" "=f,d")
	(abs:FP (match_operand:FP 1 "general_operand" "f<FP:dreg><Q>U,0")))]
  "TARGET_COLDFIRE_FPU"
{
  if (DATA_REG_P (operands[0]))
    {
      operands[1] = GEN_INT (31);
      return "bclr %1,%0";
    }
  if (FP_REG_P (operands[1]))
    return "f<FP:prec>abs%.d %1,%0";
  return "f<FP:prec>abs%.<FP:prec> %1,%0";
}
  [(set_attr "type" "bitrw,fneg")])

;; bit indexing instructions

(define_expand "clzsi2"
  [(set (match_operand:SI 0 "register_operand" "")
        (clz:SI (match_operand:SI 1 "general_operand" "")))]
  "ISA_HAS_FF1 || (TARGET_68020 && TARGET_BITFIELD)"
{
  if (ISA_HAS_FF1)
    operands[1] = force_reg (SImode, operands[1]);
})

(define_insn "*clzsi2_68k"
  [(set (match_operand:SI 0 "register_operand" "=d")
        (clz:SI (match_operand:SI 1 "general_operand" "do")))]
  "TARGET_68020 && TARGET_BITFIELD"
{
  CC_STATUS_INIT;
  return "bfffo %1{#0:#0},%0";
})

;; ColdFire ff1 instruction implements clz.
(define_insn "*clzsi2_cf"
  [(set (match_operand:SI 0 "register_operand" "=d")
 	(clz:SI (match_operand:SI 1 "register_operand" "0")))]
  "ISA_HAS_FF1"
{
  CC_STATUS_INIT;
  return "ff1 %0";
}
  [(set_attr "type" "ext")])

;; one complement instructions

(define_expand "one_cmplsi2"
  [(set (match_operand:SI 0 "nonimmediate_operand" "")
	(not:SI (match_operand:SI 1 "general_operand" "")))]
  ""
{
  if (TARGET_COLDFIRE)
    emit_insn (gen_one_cmplsi2_5200 (operands[0], operands[1]));
  else
    emit_insn (gen_one_cmplsi2_internal (operands[0], operands[1]));
  DONE;
})

(define_insn "one_cmplsi2_internal"
  [(set (match_operand:SI 0 "nonimmediate_operand" "=dm")
	(not:SI (match_operand:SI 1 "general_operand" "0")))]
  "!TARGET_COLDFIRE"
  "not%.l %0")

(define_insn "one_cmplsi2_5200"
  [(set (match_operand:SI 0 "nonimmediate_operand" "=d")
	(not:SI (match_operand:SI 1 "general_operand" "0")))]
  "TARGET_COLDFIRE"
  "not%.l %0"
  [(set_attr "type" "neg_l")])

(define_insn "one_cmplhi2"
  [(set (match_operand:HI 0 "nonimmediate_operand" "=dm")
	(not:HI (match_operand:HI 1 "general_operand" "0")))]
  "!TARGET_COLDFIRE"
  "not%.w %0")

(define_insn ""
  [(set (strict_low_part (match_operand:HI 0 "nonimmediate_operand" "+dm"))
	(not:HI (match_dup 0)))]
  "!TARGET_COLDFIRE"
  "not%.w %0")

(define_insn "one_cmplqi2"
  [(set (match_operand:QI 0 "nonimmediate_operand" "=dm")
	(not:QI (match_operand:QI 1 "general_operand" "0")))]
  "!TARGET_COLDFIRE"
  "not%.b %0")

(define_insn ""
  [(set (strict_low_part (match_operand:QI 0 "nonimmediate_operand" "+dm"))
	(not:QI (match_dup 0)))]
  "!TARGET_COLDFIRE"
  "not%.b %0")

;; arithmetic shift instructions
;; We don't need the shift memory by 1 bit instruction
(define_insn_and_split "ashldi_extsi"
  [(set (match_operand:DI 0 "nonimmediate_operand" "=ro")
    (ashift:DI
      (match_operator:DI 2 "extend_operator"
        [(match_operand:SI 1 "general_operand" "rm")])
      (const_int 32)))]
  ""
  "#"
  "&& reload_completed"
  [(set (match_dup 3) (match_dup 1))
   (set (match_dup 2) (const_int 0))]
  "split_di(operands, 1, operands + 2, operands + 3);")

(define_insn "ashldi_sexthi"
  [(set (match_operand:DI 0 "nonimmediate_operand" "=m,a*d")
    (ashift:DI (sign_extend:DI (match_operand:HI 1 "general_operand" "rm,rm"))
        (const_int 32)))
    (clobber (match_scratch:SI 2 "=a,X"))]
  ""
{
  CC_STATUS_INIT;
  if (GET_CODE (operands[0]) == MEM)
    {
    if (GET_CODE (XEXP (operands[0], 0)) == PRE_DEC)
      return "clr%.l %0\;move%.w %1,%2\;move%.l %2,%0";
    else if (GET_CODE (XEXP (operands[0], 0)) == POST_INC)
      return "move%.w %1,%2\;move%.l %2,%0\;clr%.l %0";
    else
      {
	operands[3] = adjust_address (operands[0], SImode, 4);
	return "move%.w %1,%2\;move%.l %2,%0\;clr%.l %3";
      }
    }
  else if (DATA_REG_P (operands[0]))
    return "move%.w %1,%0\;ext%.l %0\;clr%.l %R0";
  else
    return "move%.w %1,%0\;sub%.l %R0,%R0";
})

(define_insn "*ashldi3_const1"
  [(set (match_operand:DI 0 "register_operand" "=d")
	(ashift:DI (match_operand:DI 1 "register_operand" "0")
		   (const_int 1)))]
  "!TARGET_COLDFIRE"
  "add%.l %R0,%R0\;addx%.l %0,%0")

(define_split
  [(set (match_operand:DI 0 "register_operand" "")
	(ashift:DI (match_operand:DI 1 "register_operand" "")
		   (const_int 2)))]
  "reload_completed && !TARGET_COLDFIRE"
  [(set (match_dup 0)
	(ashift:DI (match_dup 1) (const_int 1)))
   (set (match_dup 0)
	(ashift:DI (match_dup 0) (const_int 1)))]
  "")

(define_split
  [(set (match_operand:DI 0 "register_operand" "")
	(ashift:DI (match_operand:DI 1 "register_operand" "")
		   (const_int 3)))]
  "reload_completed && !TARGET_COLDFIRE"
  [(set (match_dup 0)
	(ashift:DI (match_dup 1) (const_int 2)))
   (set (match_dup 0)
	(ashift:DI (match_dup 0) (const_int 1)))]
  "")

(define_split
  [(set (match_operand:DI 0 "register_operand" "")
	(ashift:DI (match_operand:DI 1 "register_operand" "")
		   (const_int 8)))]
  "reload_completed && !TARGET_COLDFIRE"
  [(set (match_dup 2)
	(rotate:SI (match_dup 2) (const_int 8)))
   (set (match_dup 3)
	(rotate:SI (match_dup 3) (const_int 8)))
   (set (strict_low_part (subreg:QI (match_dup 0) 3))
	(subreg:QI (match_dup 0) 7))
   (set (strict_low_part (subreg:QI (match_dup 0) 7))
	(const_int 0))]
{
  operands[2] = gen_highpart (SImode, operands[0]);
  operands[3] = gen_lowpart (SImode, operands[0]);
})

(define_split
  [(set (match_operand:DI 0 "register_operand" "")
	(ashift:DI (match_operand:DI 1 "register_operand" "")
		   (const_int 16)))]
  "reload_completed && !TARGET_COLDFIRE"
  [(set (match_dup 2)
	(rotate:SI (match_dup 2) (const_int 16)))
   (set (match_dup 3)
	(rotate:SI (match_dup 3) (const_int 16)))
   (set (strict_low_part (subreg:HI (match_dup 0) 2))
	(subreg:HI (match_dup 0) 6))
   (set (strict_low_part (subreg:HI (match_dup 0) 6))
	(const_int 0))]
{
  operands[2] = gen_highpart (SImode, operands[0]);
  operands[3] = gen_lowpart (SImode, operands[0]);
})

(define_split
  [(set (match_operand:DI 0 "pre_dec_operand" "")
	(ashift:DI (match_operand:DI 1 "nonimmediate_operand" "")
		   (const_int 32)))]
  "reload_completed"
  [(set (match_dup 0) (const_int 0))
   (set (match_dup 0) (match_dup 1))]
{
  operands[0] = adjust_address(operands[0], SImode, 0);
  operands[1] = gen_lowpart(SImode, operands[1]);
})

(define_split
  [(set (match_operand:DI 0 "post_inc_operand" "")
	(ashift:DI (match_operand:DI 1 "nonimmediate_operand" "")
		   (const_int 32)))]
  "reload_completed"
  [(set (match_dup 0) (match_dup 1))
   (set (match_dup 0) (const_int 0))]
{
  operands[0] = adjust_address(operands[0], SImode, 0);
  operands[1] = gen_lowpart(SImode, operands[1]);
})

(define_insn_and_split "*ashldi3_const32"
  [(set (match_operand:DI 0 "nonimmediate_operand" "=ro<>")
	(ashift:DI (match_operand:DI 1 "nonimmediate_operand" "ro")
		   (const_int 32)))]
  ""
  "#"
  "&& reload_completed"
  [(set (match_dup 4) (match_dup 3))
   (set (match_dup 2) (const_int 0))]
  "split_di(operands, 2, operands + 2, operands + 4);")

(define_split
  [(set (match_operand:DI 0 "register_operand" "")
	(ashift:DI (match_operand:DI 1 "register_operand" "")
		   (match_operand 2 "const_int_operand" "")))]
  "reload_completed && !TARGET_COLDFIRE
   && INTVAL (operands[2]) > 32 && INTVAL (operands[2]) <= 40"
  [(set (match_dup 4) (ashift:SI (match_dup 4) (match_dup 2)))
   (set (match_dup 3) (match_dup 4))
   (set (match_dup 4) (const_int 0))]
{
  operands[2] = GEN_INT (INTVAL (operands[2]) - 32);
  operands[3] = gen_highpart (SImode, operands[0]);
  operands[4] = gen_lowpart (SImode, operands[0]);
})

(define_split
  [(set (match_operand:DI 0 "register_operand" "")
	(ashift:DI (match_operand:DI 1 "register_operand" "")
		   (const_int 48)))]
  "reload_completed && !TARGET_COLDFIRE"
  [(set (match_dup 2) (match_dup 3))
   (set (match_dup 2)
	(rotate:SI (match_dup 2) (const_int 16)))
   (set (match_dup 3) (const_int 0))
   (set (strict_low_part (subreg:HI (match_dup 0) 2))
	(const_int 0))]
{
  operands[2] = gen_highpart (SImode, operands[0]);
  operands[3] = gen_lowpart (SImode, operands[0]);
})

(define_split
  [(set (match_operand:DI 0 "register_operand" "")
	(ashift:DI (match_operand:DI 1 "register_operand" "")
		   (match_operand 2 "const_int_operand" "")))]
  "reload_completed && !TARGET_COLDFIRE
   && INTVAL (operands[2]) > 40 && INTVAL (operands[2]) <= 63"
  [(set (match_dup 3) (match_dup 2))
   (set (match_dup 4) (ashift:SI (match_dup 4) (match_dup 3)))
   (set (match_dup 3) (match_dup 4))
   (set (match_dup 4) (const_int 0))]
{
  operands[2] = GEN_INT (INTVAL (operands[2]) - 32);
  operands[3] = gen_highpart (SImode, operands[0]);
  operands[4] = gen_lowpart (SImode, operands[0]);
})

(define_insn "*ashldi3"
  [(set (match_operand:DI 0 "register_operand" "=d")
	(ashift:DI (match_operand:DI 1 "register_operand" "0")
		   (match_operand 2 "const_int_operand" "n")))]
  "!TARGET_COLDFIRE
    && ((INTVAL (operands[2]) >= 1 && INTVAL (operands[2]) <= 3)
	|| INTVAL (operands[2]) == 8 || INTVAL (operands[2]) == 16
	|| (INTVAL (operands[2]) > 32 && INTVAL (operands[2]) <= 63))"
  "#")

(define_expand "ashldi3"
  [(set (match_operand:DI 0 "register_operand" "")
	(ashift:DI (match_operand:DI 1 "register_operand" "")
		   (match_operand 2 "const_int_operand" "")))]
  "!TARGET_COLDFIRE"
{
  /* ???  This is a named pattern like this is not allowed to FAIL based
     on its operands.  */
  if (GET_CODE (operands[2]) != CONST_INT
      || ((INTVAL (operands[2]) < 1 || INTVAL (operands[2]) > 3)
	  && INTVAL (operands[2]) != 8 && INTVAL (operands[2]) != 16
	  && (INTVAL (operands[2]) < 32 || INTVAL (operands[2]) > 63)))
    FAIL;
})

;; On most 68k models, this makes faster code in a special case.

(define_insn "ashlsi_16"
  [(set (match_operand:SI 0 "register_operand" "=d")
	(ashift:SI (match_operand:SI 1 "register_operand" "0")
		   (const_int 16)))]
  "!TUNE_68060"
{
  CC_STATUS_INIT;
  return "swap %0\;clr%.w %0";
})

;; ashift patterns : use lsl instead of asl, because lsl always clears the
;; overflow bit, so we must not set CC_NO_OVERFLOW.

;; On the 68000, this makes faster code in a special case.

(define_insn "ashlsi_17_24"
  [(set (match_operand:SI 0 "register_operand" "=d")
	(ashift:SI (match_operand:SI 1 "register_operand" "0")
		   (match_operand:SI 2 "const_int_operand" "n")))]
  "TUNE_68000_10
   && INTVAL (operands[2]) > 16
   && INTVAL (operands[2]) <= 24"
{
  CC_STATUS_INIT;

  operands[2] = GEN_INT (INTVAL (operands[2]) - 16);
  return "lsl%.w %2,%0\;swap %0\;clr%.w %0";
})

(define_insn "ashlsi3"
  [(set (match_operand:SI 0 "register_operand" "=d")
	(ashift:SI (match_operand:SI 1 "register_operand" "0")
		   (match_operand:SI 2 "general_operand" "dI")))]
  ""
{
  if (operands[2] == const1_rtx)
    {
      cc_status.flags = CC_NO_OVERFLOW;
      return "add%.l %0,%0";
    }
  return "lsl%.l %2,%0";
})

(define_insn "ashlhi3"
  [(set (match_operand:HI 0 "register_operand" "=d")
	(ashift:HI (match_operand:HI 1 "register_operand" "0")
		   (match_operand:HI 2 "general_operand" "dI")))]
  "!TARGET_COLDFIRE"
  "lsl%.w %2,%0")

(define_insn ""
  [(set (strict_low_part (match_operand:HI 0 "register_operand" "+d"))
	(ashift:HI (match_dup 0)
		   (match_operand:HI 1 "general_operand" "dI")))]
  "!TARGET_COLDFIRE"
  "lsl%.w %1,%0")

(define_insn "ashlqi3"
  [(set (match_operand:QI 0 "register_operand" "=d")
	(ashift:QI (match_operand:QI 1 "register_operand" "0")
		   (match_operand:QI 2 "general_operand" "dI")))]
  "!TARGET_COLDFIRE"
  "lsl%.b %2,%0")

(define_insn ""
  [(set (strict_low_part (match_operand:QI 0 "register_operand" "+d"))
	(ashift:QI (match_dup 0)
		   (match_operand:QI 1 "general_operand" "dI")))]
  "!TARGET_COLDFIRE"
  "lsl%.b %1,%0")

;; On most 68k models, this makes faster code in a special case.

(define_insn "ashrsi_16"
  [(set (match_operand:SI 0 "register_operand" "=d")
	(ashiftrt:SI (match_operand:SI 1 "register_operand" "0")
		     (const_int 16)))]
  "!TUNE_68060"
  "swap %0\;ext%.l %0")

;; On the 68000, this makes faster code in a special case.

(define_insn ""
  [(set (match_operand:SI 0 "register_operand" "=d")
	(ashiftrt:SI (match_operand:SI 1 "register_operand" "0")
		     (match_operand:SI 2 "const_int_operand" "n")))]
  "TUNE_68000_10
   && INTVAL (operands[2]) > 16
   && INTVAL (operands[2]) <= 24"
{
  operands[2] = GEN_INT (INTVAL (operands[2]) - 16);
  return "swap %0\;asr%.w %2,%0\;ext%.l %0";
})

(define_insn "subreghi1ashrdi_const32"
  [(set (match_operand:HI 0 "nonimmediate_operand" "=rm")
    (subreg:HI (ashiftrt:DI (match_operand:DI 1 "general_operand" "ro")
            (const_int 32)) 6))]
  ""
{
  if (GET_CODE (operands[1]) != REG)
    operands[1] = adjust_address (operands[1], HImode, 2);
  return "move%.w %1,%0";
}
  [(set_attr "type" "move")])

(define_insn "subregsi1ashrdi_const32"
  [(set (match_operand:SI 0 "nonimmediate_operand" "=rm")
    (subreg:SI (ashiftrt:DI (match_operand:DI 1 "general_operand" "ro")
            (const_int 32)) 4))]
  ""
{
  return "move%.l %1,%0";
}
  [(set_attr "type" "move_l")])

(define_insn "*ashrdi3_const1"
  [(set (match_operand:DI 0 "register_operand" "=d")
	(ashiftrt:DI (match_operand:DI 1 "register_operand" "0")
		     (const_int 1)))]
  "!TARGET_COLDFIRE"
{
  operands[1] = gen_rtx_REG (SImode, REGNO (operands[0]) + 1);
  return "asr%.l #1,%0\;roxr%.l #1,%1";
})

(define_split
  [(set (match_operand:DI 0 "register_operand" "")
	(ashiftrt:DI (match_operand:DI 1 "register_operand" "")
		     (const_int 2)))]
  "reload_completed && !TARGET_COLDFIRE"
  [(set (match_dup 0)
	(ashiftrt:DI (match_dup 1) (const_int 1)))
   (set (match_dup 0)
	(ashiftrt:DI (match_dup 0) (const_int 1)))]
  "")

(define_split
  [(set (match_operand:DI 0 "register_operand" "")
	(ashiftrt:DI (match_operand:DI 1 "register_operand" "")
		     (const_int 3)))]
  "reload_completed && !TARGET_COLDFIRE"
  [(set (match_dup 0)
	(ashiftrt:DI (match_dup 1) (const_int 2)))
   (set (match_dup 0)
	(ashiftrt:DI (match_dup 0) (const_int 1)))]
  "")

(define_split
  [(set (match_operand:DI 0 "register_operand" "")
	(ashiftrt:DI (match_operand:DI 1 "register_operand" "")
		     (const_int 8)))]
  "reload_completed && !TARGET_COLDFIRE"
  [(set (strict_low_part (subreg:QI (match_dup 0) 7))
	(subreg:QI (match_dup 0) 3))
   (set (match_dup 2)
	(ashiftrt:SI (match_dup 2) (const_int 8)))
   (set (match_dup 3)
	(rotatert:SI (match_dup 3) (const_int 8)))]
{
  operands[2] = gen_highpart (SImode, operands[0]);
  operands[3] = gen_lowpart (SImode, operands[0]);
})

(define_split
  [(set (match_operand:DI 0 "register_operand" "")
	(ashiftrt:DI (match_operand:DI 1 "register_operand" "")
		     (const_int 16)))]
  "reload_completed && !TARGET_COLDFIRE"
  [(set (strict_low_part (subreg:HI (match_dup 0) 6))
	(subreg:HI (match_dup 0) 2))
   (set (match_dup 2)
	(rotate:SI (match_dup 2) (const_int 16)))
   (set (match_dup 3)
	(rotate:SI (match_dup 3) (const_int 16)))
   (set (match_dup 2)
	(sign_extend:SI (subreg:HI (match_dup 2) 2)))]
{
  operands[2] = gen_highpart (SImode, operands[0]);
  operands[3] = gen_lowpart (SImode, operands[0]);
})

(define_insn "*ashrdi_const32"
  [(set (match_operand:DI 0 "register_operand" "=d")
	(ashiftrt:DI (match_operand:DI 1 "nonimmediate_src_operand" "ro")
		     (const_int 32)))]
  ""
{
  CC_STATUS_INIT;
  if (TARGET_68020)
    return "move%.l %1,%R0\;smi %0\;extb%.l %0";
  else
    return "move%.l %1,%R0\;smi %0\;ext%.w %0\;ext%.l %0";
})

(define_insn "*ashrdi_const32_mem"
  [(set (match_operand:DI 0 "memory_operand" "=o,<")
	(ashiftrt:DI (match_operand:DI 1 "nonimmediate_src_operand" "ro,ro")
		     (const_int 32)))
   (clobber (match_scratch:SI 2 "=d,d"))]
  ""
{
  CC_STATUS_INIT;
  operands[3] = adjust_address (operands[0], SImode,
				which_alternative == 0 ? 4 : 0);
  operands[0] = adjust_address (operands[0], SImode, 0);
  if (TARGET_68020 || TARGET_COLDFIRE)
    return "move%.l %1,%3\;smi %2\;extb%.l %2\;move%.l %2,%0";
  else
    return "move%.l %1,%3\;smi %2\;ext%.w %2\;ext%.l %2\;move%.l %2,%0";
})

(define_split
  [(set (match_operand:DI 0 "register_operand" "")
	(ashiftrt:DI (match_operand:DI 1 "register_operand" "")
		     (const_int 63)))]
  "reload_completed && !TARGET_COLDFIRE"
  [(set (match_dup 3)
	(ashiftrt:SI (match_dup 3) (const_int 31)))
   (set (match_dup 2)
	(match_dup 3))]
  "split_di(operands, 1, operands + 2, operands + 3);")

;; The predicate below must be general_operand, because ashrdi3 allows that
(define_insn "ashrdi_const"
  [(set (match_operand:DI 0 "register_operand" "=d")
	(ashiftrt:DI (match_operand:DI 1 "register_operand" "0")
		     (match_operand 2 "const_int_operand" "n")))]
  "!TARGET_COLDFIRE
    && ((INTVAL (operands[2]) >= 1 && INTVAL (operands[2]) <= 3)
	|| INTVAL (operands[2]) == 8 || INTVAL (operands[2]) == 16
	|| INTVAL (operands[2]) == 31
	|| (INTVAL (operands[2]) > 32 && INTVAL (operands[2]) <= 63))"
{
  operands[1] = gen_rtx_REG (SImode, REGNO (operands[0]) + 1);
  CC_STATUS_INIT;
  if (INTVAL (operands[2]) == 48)
    return "swap %0\;ext%.l %0\;move%.l %0,%1\;smi %0\;ext%.w %0";
  if (INTVAL (operands[2]) == 31)
    return "add%.l %1,%1\;addx%.l %0,%0\;move%.l %0,%1\;subx%.l %0,%0";
  if (INTVAL (operands[2]) > 32 && INTVAL (operands[2]) <= 63)
    {
      operands[2] = GEN_INT (INTVAL (operands[2]) - 32);
      output_asm_insn (INTVAL (operands[2]) <= 8 ? "asr%.l %2,%0" :
			"moveq %2,%1\;asr%.l %1,%0", operands);
      output_asm_insn ("mov%.l %0,%1\;smi %0", operands);
      return INTVAL (operands[2]) >= 15 ? "ext%.w %d0" :
	     TARGET_68020 ? "extb%.l %0" : "ext%.w %0\;ext%.l %0";
    }
  return "#";
})

(define_expand "ashrdi3"
  [(set (match_operand:DI 0 "register_operand" "")
	(ashiftrt:DI (match_operand:DI 1 "register_operand" "")
		     (match_operand 2 "const_int_operand" "")))]
  "!TARGET_COLDFIRE"
{
  /* ???  This is a named pattern like this is not allowed to FAIL based
     on its operands.  */
  if (GET_CODE (operands[2]) != CONST_INT
      || ((INTVAL (operands[2]) < 1 || INTVAL (operands[2]) > 3)
	  && INTVAL (operands[2]) != 8 && INTVAL (operands[2]) != 16
	  && (INTVAL (operands[2]) < 31 || INTVAL (operands[2]) > 63)))
    FAIL;
})

;; On all 68k models, this makes faster code in a special case.

(define_insn "ashrsi_31"
  [(set (match_operand:SI 0 "register_operand" "=d")
	(ashiftrt:SI (match_operand:SI 1 "register_operand" "0")
		     (const_int 31)))]
  ""
{
  return "add%.l %0,%0\;subx%.l %0,%0";
})

(define_insn "ashrsi3"
  [(set (match_operand:SI 0 "register_operand" "=d")
	(ashiftrt:SI (match_operand:SI 1 "register_operand" "0")
		     (match_operand:SI 2 "general_operand" "dI")))]
  ""
  "asr%.l %2,%0"
  [(set_attr "type" "shift")
   (set_attr "opy" "2")])

(define_insn "ashrhi3"
  [(set (match_operand:HI 0 "register_operand" "=d")
	(ashiftrt:HI (match_operand:HI 1 "register_operand" "0")
		     (match_operand:HI 2 "general_operand" "dI")))]
  "!TARGET_COLDFIRE"
  "asr%.w %2,%0")

(define_insn ""
  [(set (strict_low_part (match_operand:HI 0 "register_operand" "+d"))
	(ashiftrt:HI (match_dup 0)
		     (match_operand:HI 1 "general_operand" "dI")))]
  "!TARGET_COLDFIRE"
  "asr%.w %1,%0")

(define_insn "ashrqi3"
  [(set (match_operand:QI 0 "register_operand" "=d")
	(ashiftrt:QI (match_operand:QI 1 "register_operand" "0")
		     (match_operand:QI 2 "general_operand" "dI")))]
  "!TARGET_COLDFIRE"
  "asr%.b %2,%0")

(define_insn ""
  [(set (strict_low_part (match_operand:QI 0 "register_operand" "+d"))
	(ashiftrt:QI (match_dup 0)
		     (match_operand:QI 1 "general_operand" "dI")))]
  "!TARGET_COLDFIRE"
  "asr%.b %1,%0")

;; logical shift instructions

;; commented out because of reload problems in 950612-1.c
;;(define_insn ""
;;        [(set (cc0)
;;            (subreg:SI (lshiftrt:DI (match_operand:DI 0 "general_operand" "ro")
;;                    (const_int 32)) 4))
;;        (set (match_operand:SI 1 "nonimmediate_operand" "=dm")
;;            (subreg:SI (lshiftrt:DI (match_dup 0)
;;                    (const_int 32)) 4))]
;;  ""
;;{
;;  return "move%.l %0,%1";
;;})
;;
;;(define_insn ""
;;        [(set (cc0)
;;            (subreg:SI (lshiftrt:DI (match_operand:DI 0 "general_operand" "ro")
;;                    (const_int 32)) 0))
;;        (set (match_operand:DI 1 "nonimmediate_operand" "=do")
;;            (lshiftrt:DI (match_dup 0)
;;                (const_int 32)))]
;;  ""
;;{
;;  if (GET_CODE (operands[1]) == REG)
;;    operands[2] = gen_rtx_REG (SImode, REGNO (operands[1]) + 1);
;;  else
;;    operands[2] = adjust_address (operands[1], SImode, 4);
;;  return "move%.l %0,%2\;clr%.l %1";
;;})

(define_insn "subreg1lshrdi_const32"
  [(set (match_operand:SI 0 "nonimmediate_operand" "=rm")
    (subreg:SI (lshiftrt:DI (match_operand:DI 1 "general_operand" "ro")
            (const_int 32)) 4))]
  ""
  "move%.l %1,%0"
  [(set_attr "type" "move_l")])

(define_insn "*lshrdi3_const1"
  [(set (match_operand:DI 0 "register_operand" "=d")
	(lshiftrt:DI (match_operand:DI 1 "register_operand" "0")
		     (const_int 1)))]
  "!TARGET_COLDFIRE"
  "lsr%.l #1,%0\;roxr%.l #1,%R0")

(define_split
  [(set (match_operand:DI 0 "register_operand" "")
	(lshiftrt:DI (match_operand:DI 1 "register_operand" "")
		     (const_int 2)))]
  "reload_completed && !TARGET_COLDFIRE"
  [(set (match_dup 0)
	(lshiftrt:DI (match_dup 1) (const_int 1)))
   (set (match_dup 0)
	(lshiftrt:DI (match_dup 0) (const_int 1)))]
  "")

(define_split
  [(set (match_operand:DI 0 "register_operand" "")
	(lshiftrt:DI (match_operand:DI 1 "register_operand" "")
		     (const_int 3)))]
  "reload_completed && !TARGET_COLDFIRE"
  [(set (match_dup 0)
	(lshiftrt:DI (match_dup 1) (const_int 2)))
   (set (match_dup 0)
	(lshiftrt:DI (match_dup 0) (const_int 1)))]
  "")

(define_split
  [(set (match_operand:DI 0 "register_operand" "")
	(lshiftrt:DI (match_operand:DI 1 "register_operand" "")
		     (const_int 8)))]
  "reload_completed && !TARGET_COLDFIRE"
  [(set (strict_low_part (subreg:QI (match_dup 0) 7))
	(subreg:QI (match_dup 0) 3))
   (set (match_dup 2)
	(lshiftrt:SI (match_dup 2) (const_int 8)))
   (set (match_dup 3)
	(rotatert:SI (match_dup 3) (const_int 8)))]
{
  operands[2] = gen_highpart (SImode, operands[0]);
  operands[3] = gen_lowpart (SImode, operands[0]);
})

(define_split
  [(set (match_operand:DI 0 "register_operand" "")
	(lshiftrt:DI (match_operand:DI 1 "register_operand" "")
		     (const_int 16)))]
  "reload_completed && !TARGET_COLDFIRE"
  [(set (strict_low_part (subreg:HI (match_dup 0) 6))
	(subreg:HI (match_dup 0) 2))
   (set (strict_low_part (subreg:HI (match_dup 0) 2))
	(const_int 0))
   (set (match_dup 3)
	(rotate:SI (match_dup 3) (const_int 16)))
   (set (match_dup 2)
	(rotate:SI (match_dup 2) (const_int 16)))]
{
  operands[2] = gen_highpart (SImode, operands[0]);
  operands[3] = gen_lowpart (SImode, operands[0]);
})

(define_split
  [(set (match_operand:DI 0 "pre_dec_operand" "")
	(lshiftrt:DI (match_operand:DI 1 "nonimmediate_operand" "")
		     (const_int 32)))]
  "reload_completed"
  [(set (match_dup 0) (match_dup 1))
   (set (match_dup 0) (const_int 0))]
{
  operands[0] = adjust_address(operands[0], SImode, 0);
  operands[1] = gen_highpart(SImode, operands[1]);
})

(define_split
  [(set (match_operand:DI 0 "post_inc_operand" "")
	(lshiftrt:DI (match_operand:DI 1 "nonimmediate_operand" "")
		     (const_int 32)))]
  "reload_completed"
  [(set (match_dup 0) (const_int 0))
   (set (match_dup 0) (match_dup 1))]
{
  operands[0] = adjust_address(operands[0], SImode, 0);
  operands[1] = gen_highpart(SImode, operands[1]);
})

(define_split
  [(set (match_operand:DI 0 "nonimmediate_operand" "")
	(lshiftrt:DI (match_operand:DI 1 "nonimmediate_operand" "")
		     (const_int 32)))]
  "reload_completed"
  [(set (match_dup 2) (match_dup 5))
   (set (match_dup 4) (const_int 0))]
  "split_di(operands, 2, operands + 2, operands + 4);")

(define_insn "*lshrdi_const32"
  [(set (match_operand:DI 0 "nonimmediate_operand" "=ro<>")
	(lshiftrt:DI (match_operand:DI 1 "general_operand" "ro")
		     (const_int 32)))]
  ""
  "#")

(define_split
  [(set (match_operand:DI 0 "register_operand" "")
	(lshiftrt:DI (match_operand:DI 1 "register_operand" "")
		     (match_operand 2 "const_int_operand" "")))]
  "reload_completed && !TARGET_COLDFIRE
   && INTVAL (operands[2]) > 32 && INTVAL (operands[2]) <= 40"
  [(set (match_dup 3) (lshiftrt:SI (match_dup 3) (match_dup 2)))
   (set (match_dup 4) (match_dup 3))
   (set (match_dup 3) (const_int 0))]
{
  operands[2] = GEN_INT (INTVAL (operands[2]) - 32);
  operands[3] = gen_highpart (SImode, operands[0]);
  operands[4] = gen_lowpart (SImode, operands[0]);
})

(define_split
  [(set (match_operand:DI 0 "register_operand" "")
	(lshiftrt:DI (match_operand:DI 1 "register_operand" "")
		     (const_int 48)))]
  "reload_completed"
  [(set (match_dup 3) (match_dup 2))
   (set (strict_low_part (subreg:HI (match_dup 0) 6))
	(const_int 0))
   (set (match_dup 2) (const_int 0))
   (set (match_dup 3)
	(rotate:SI (match_dup 3) (const_int 16)))]
{
  operands[2] = gen_highpart (SImode, operands[0]);
  operands[3] = gen_lowpart (SImode, operands[0]);
})

(define_split
  [(set (match_operand:DI 0 "register_operand" "")
	(lshiftrt:DI (match_operand:DI 1 "register_operand" "")
		     (match_operand 2 "const_int_operand" "")))]
  "reload_completed && !TARGET_COLDFIRE
   && INTVAL (operands[2]) > 40 && INTVAL (operands[2]) <= 62"
  [(set (match_dup 4) (match_dup 2))
   (set (match_dup 3) (lshiftrt:SI (match_dup 3) (match_dup 4)))
   (set (match_dup 4) (match_dup 3))
   (set (match_dup 3) (const_int 0))]
{
  operands[2] = GEN_INT (INTVAL (operands[2]) - 32);
  operands[3] = gen_highpart (SImode, operands[0]);
  operands[4] = gen_lowpart (SImode, operands[0]);
})

(define_insn "*lshrdi_const63"
  [(set (match_operand:DI 0 "register_operand" "=d")
	(lshiftrt:DI (match_operand:DI 1 "register_operand" "0")
		     (const_int 63)))]
  ""
  "add%.l %0,%0\;clr%.l %0\;clr%.l %R1\;addx%.l %R1,%R1")

(define_insn "*lshrdi3_const"
  [(set (match_operand:DI 0 "register_operand" "=d")
	(lshiftrt:DI (match_operand:DI 1 "register_operand" "0")
		     (match_operand 2 "const_int_operand" "n")))]
  "(!TARGET_COLDFIRE
    && ((INTVAL (operands[2]) >= 2 && INTVAL (operands[2]) <= 3)
	 || INTVAL (operands[2]) == 8 || INTVAL (operands[2]) == 16
	 || (INTVAL (operands[2]) > 32 && INTVAL (operands[2]) <= 63)))"
  "#")

(define_expand "lshrdi3"
  [(set (match_operand:DI 0 "register_operand" "")
	(lshiftrt:DI (match_operand:DI 1 "register_operand" "")
		     (match_operand 2 "const_int_operand" "")))]
  "!TARGET_COLDFIRE"
{
  /* ???  This is a named pattern like this is not allowed to FAIL based
     on its operands.  */
  if (GET_CODE (operands[2]) != CONST_INT
      || ((INTVAL (operands[2]) < 1 || INTVAL (operands[2]) > 3)
	  && INTVAL (operands[2]) != 8 && INTVAL (operands[2]) != 16
	  && (INTVAL (operands[2]) < 32 || INTVAL (operands[2]) > 63)))
    FAIL;
})

;; On all 68k models, this makes faster code in a special case.

(define_insn "lshrsi_31"
  [(set (match_operand:SI 0 "register_operand" "=d")
	(lshiftrt:SI (match_operand:SI 1 "register_operand" "0")
		     (const_int 31)))]
  ""
{
  return "add%.l %0,%0\;subx%.l %0,%0\;neg%.l %0";
})

;; On most 68k models, this makes faster code in a special case.

(define_insn "lshrsi_16"
  [(set (match_operand:SI 0 "register_operand" "=d")
	(lshiftrt:SI (match_operand:SI 1 "register_operand" "0")
		     (const_int 16)))]
  "!TUNE_68060"
{
  CC_STATUS_INIT;
  return "clr%.w %0\;swap %0";
})

;; On the 68000, this makes faster code in a special case.

(define_insn "lshrsi_17_24"
  [(set (match_operand:SI 0 "register_operand" "=d")
	(lshiftrt:SI (match_operand:SI 1 "register_operand" "0")
		     (match_operand:SI 2 "const_int_operand" "n")))]
  "TUNE_68000_10
   && INTVAL (operands[2]) > 16
   && INTVAL (operands[2]) <= 24"
{
  /* I think lsr%.w sets the CC properly.  */
  operands[2] = GEN_INT (INTVAL (operands[2]) - 16);
  return "clr%.w %0\;swap %0\;lsr%.w %2,%0";
})

(define_insn "lshrsi3"
  [(set (match_operand:SI 0 "register_operand" "=d")
	(lshiftrt:SI (match_operand:SI 1 "register_operand" "0")
		     (match_operand:SI 2 "general_operand" "dI")))]
  ""
  "lsr%.l %2,%0"
  [(set_attr "type" "shift")
   (set_attr "opy" "2")])

(define_insn "lshrhi3"
  [(set (match_operand:HI 0 "register_operand" "=d")
	(lshiftrt:HI (match_operand:HI 1 "register_operand" "0")
		     (match_operand:HI 2 "general_operand" "dI")))]
  "!TARGET_COLDFIRE"
  "lsr%.w %2,%0")

(define_insn ""
  [(set (strict_low_part (match_operand:HI 0 "register_operand" "+d"))
	(lshiftrt:HI (match_dup 0)
		     (match_operand:HI 1 "general_operand" "dI")))]
  "!TARGET_COLDFIRE"
  "lsr%.w %1,%0")

(define_insn "lshrqi3"
  [(set (match_operand:QI 0 "register_operand" "=d")
	(lshiftrt:QI (match_operand:QI 1 "register_operand" "0")
		     (match_operand:QI 2 "general_operand" "dI")))]
  "!TARGET_COLDFIRE"
  "lsr%.b %2,%0")

(define_insn ""
  [(set (strict_low_part (match_operand:QI 0 "register_operand" "+d"))
	(lshiftrt:QI (match_dup 0)
		     (match_operand:QI 1 "general_operand" "dI")))]
  "!TARGET_COLDFIRE"
  "lsr%.b %1,%0")

;; rotate instructions

(define_insn "rotlsi_16"
  [(set (match_operand:SI 0 "register_operand" "=d")
	(rotate:SI (match_operand:SI 1 "register_operand" "0")
		   (const_int 16)))]
  ""
  "swap %0"
  [(set_attr "type" "shift")])

(define_insn "rotlsi3"
  [(set (match_operand:SI 0 "register_operand" "=d")
	(rotate:SI (match_operand:SI 1 "register_operand" "0")
		   (match_operand:SI 2 "general_operand" "dINO")))]
  "!TARGET_COLDFIRE"
{
  if (GET_CODE (operands[2]) == CONST_INT && INTVAL (operands[2]) == 16)
    return "swap %0";
  else if (GET_CODE (operands[2]) == CONST_INT && INTVAL (operands[2]) >= 16)
    {
      operands[2] = GEN_INT (32 - INTVAL (operands[2]));
      return "ror%.l %2,%0";
    }
  else
    return "rol%.l %2,%0";
})

(define_insn "rotlhi3"
  [(set (match_operand:HI 0 "register_operand" "=d")
	(rotate:HI (match_operand:HI 1 "register_operand" "0")
		   (match_operand:HI 2 "general_operand" "dIP")))]
  "!TARGET_COLDFIRE"
{
  if (GET_CODE (operands[2]) == CONST_INT && INTVAL (operands[2]) >= 8)
    {
      operands[2] = GEN_INT (16 - INTVAL (operands[2]));
      return "ror%.w %2,%0";
    }
  else
    return "rol%.w %2,%0";
})

(define_insn "*rotlhi3_lowpart"
  [(set (strict_low_part (match_operand:HI 0 "register_operand" "+d"))
	(rotate:HI (match_dup 0)
		   (match_operand:HI 1 "general_operand" "dIP")))]
  "!TARGET_COLDFIRE"
{
  if (GET_CODE (operands[1]) == CONST_INT && INTVAL (operands[1]) >= 8)
    {
      operands[1] = GEN_INT (16 - INTVAL (operands[1]));
      return "ror%.w %1,%0";
    }
  else
    return "rol%.w %1,%0";
})

(define_insn "rotlqi3"
  [(set (match_operand:QI 0 "register_operand" "=d")
	(rotate:QI (match_operand:QI 1 "register_operand" "0")
		   (match_operand:QI 2 "general_operand" "dI")))]
  "!TARGET_COLDFIRE"
{
  if (GET_CODE (operands[2]) == CONST_INT && INTVAL (operands[2]) >= 4)
    {
      operands[2] = GEN_INT (8 - INTVAL (operands[2]));
      return "ror%.b %2,%0";
    }
  else
    return "rol%.b %2,%0";
})

(define_insn "*rotlqi3_lowpart"
  [(set (strict_low_part (match_operand:QI 0 "register_operand" "+d"))
	(rotate:QI (match_dup 0)
		   (match_operand:QI 1 "general_operand" "dI")))]
  "!TARGET_COLDFIRE"
{
  if (GET_CODE (operands[1]) == CONST_INT && INTVAL (operands[1]) >= 4)
    {
      operands[1] = GEN_INT (8 - INTVAL (operands[1]));
      return "ror%.b %1,%0";
    }
  else
    return "rol%.b %1,%0";
})

(define_insn "rotrsi3"
  [(set (match_operand:SI 0 "register_operand" "=d")
	(rotatert:SI (match_operand:SI 1 "register_operand" "0")
		     (match_operand:SI 2 "general_operand" "dI")))]
  "!TARGET_COLDFIRE"
  "ror%.l %2,%0")

(define_insn "rotrhi3"
  [(set (match_operand:HI 0 "register_operand" "=d")
	(rotatert:HI (match_operand:HI 1 "register_operand" "0")
		     (match_operand:HI 2 "general_operand" "dI")))]
  "!TARGET_COLDFIRE"
  "ror%.w %2,%0")

(define_insn "rotrhi_lowpart"
  [(set (strict_low_part (match_operand:HI 0 "register_operand" "+d"))
	(rotatert:HI (match_dup 0)
		     (match_operand:HI 1 "general_operand" "dI")))]
  "!TARGET_COLDFIRE"
  "ror%.w %1,%0")

(define_insn "rotrqi3"
  [(set (match_operand:QI 0 "register_operand" "=d")
	(rotatert:QI (match_operand:QI 1 "register_operand" "0")
		     (match_operand:QI 2 "general_operand" "dI")))]
  "!TARGET_COLDFIRE"
  "ror%.b %2,%0")

(define_insn ""
  [(set (strict_low_part (match_operand:QI 0 "register_operand" "+d"))
	(rotatert:QI (match_dup 0)
		     (match_operand:QI 1 "general_operand" "dI")))]
  "!TARGET_COLDFIRE"
  "ror%.b %1,%0")

(define_expand "bswapsi2"
  [(set (match_operand:SI 0 "register_operand")
	(bswap:SI (match_operand:SI 1 "register_operand")))]
  "!TARGET_COLDFIRE"
{
  rtx x = operands[0];
  emit_move_insn (x, operands[1]);
  emit_insn (gen_rotrhi_lowpart (gen_lowpart (HImode, x), GEN_INT (8)));
  emit_insn (gen_rotlsi3 (x, x, GEN_INT (16)));
  emit_insn (gen_rotrhi_lowpart (gen_lowpart (HImode, x), GEN_INT (8)));
  DONE;
})


;; Bit set/clear in memory byte.

;; set bit, bit number is int
(define_insn "bsetmemqi"
  [(set (match_operand:QI 0 "memory_operand" "+m")
	(ior:QI (subreg:QI (ashift:SI (const_int 1)
		(match_operand:SI 1 "general_operand" "d")) 3)
	(match_dup 0)))]
  ""
{
  CC_STATUS_INIT;
  return "bset %1,%0";
}
  [(set_attr "type" "bitrw")])

;; set bit, bit number is (sign/zero)_extended from HImode/QImode
(define_insn "*bsetmemqi_ext"
  [(set (match_operand:QI 0 "memory_operand" "+m")
	(ior:QI (subreg:QI (ashift:SI (const_int 1)
	    (match_operator:SI 2 "extend_operator"
		[(match_operand 1 "general_operand" "d")])) 3)
	(match_dup 0)))]
  ""
{
  CC_STATUS_INIT;
  return "bset %1,%0";
}
  [(set_attr "type" "bitrw")])

;; clear bit, bit number is int
(define_insn "bclrmemqi"
  [(set (zero_extract:SI (match_operand:QI 0 "memory_operand" "+m")
	(const_int 1)
	(minus:SI (const_int 7)
	    (match_operand:SI 1 "general_operand" "d")))
    (const_int 0))]
  ""
{
  CC_STATUS_INIT;
  return "bclr %1,%0";
}
  [(set_attr "type" "bitrw")])

;; clear bit, bit number is (sign/zero)_extended from HImode/QImode
(define_insn "*bclrmemqi_ext"
  [(set (zero_extract:SI (match_operand:QI 0 "memory_operand" "+m")
	(const_int 1)
	(minus:SI (const_int 7)
	    (match_operator:SI 2 "extend_operator"
		[(match_operand 1 "general_operand" "d")])))
    (const_int 0))]
  ""
{
  CC_STATUS_INIT;
  return "bclr %1,%0";
}
  [(set_attr "type" "bitrw")])

;; Special cases of bit-field insns which we should
;; recognize in preference to the general case.
;; These handle aligned 8-bit and 16-bit fields,
;; which can usually be done with move instructions.

;
; Special case for 32-bit field in memory.  This only occurs when 32-bit
; alignment of structure members is specified.
;
; The move is allowed to be odd byte aligned, because that's still faster
; than an odd byte aligned bit-field instruction.
;
(define_insn "*insv_32_mem"
  [(set (zero_extract:SI (match_operand:QI 0 "memory_operand" "+o")
			 (const_int 32)
			 (match_operand:SI 1 "const_int_operand" "n"))
	(match_operand:SI 2 "general_src_operand" "rmSi"))]
  "TARGET_68020 && TARGET_BITFIELD
   && (INTVAL (operands[1]) % 8) == 0
   && ! mode_dependent_address_p (XEXP (operands[0], 0),
                                  MEM_ADDR_SPACE (operands[0]))"
{
  operands[0]
    = adjust_address (operands[0], SImode, INTVAL (operands[1]) / 8);

  return "move%.l %2,%0";
})

(define_insn "*insv_8_16_reg"
  [(set (zero_extract:SI (match_operand:SI 0 "register_operand" "+d")
			 (match_operand:SI 1 "const_int_operand" "n")
			 (match_operand:SI 2 "const_int_operand" "n"))
	(match_operand:SI 3 "register_operand" "d"))]
  "TARGET_68020 && TARGET_BITFIELD
   && (INTVAL (operands[1]) == 8 || INTVAL (operands[1]) == 16)
   && INTVAL (operands[2]) % INTVAL (operands[1]) == 0"
{
  if (INTVAL (operands[1]) + INTVAL (operands[2]) != 32)
    return "bfins %3,%0{%b2:%b1}";

  if (INTVAL (operands[1]) == 8)
    return "move%.b %3,%0";
  return "move%.w %3,%0";
})


;
; Special case for 32-bit field in memory.  This only occurs when 32-bit
; alignment of structure members is specified.
;
; The move is allowed to be odd byte aligned, because that's still faster
; than an odd byte aligned bit-field instruction.
;
(define_insn "*extzv_32_mem"
  [(set (match_operand:SI 0 "nonimmediate_operand" "=rm")
	(zero_extract:SI (match_operand:QI 1 "memory_src_operand" "oS")
			 (const_int 32)
			 (match_operand:SI 2 "const_int_operand" "n")))]
  "TARGET_68020 && TARGET_BITFIELD
   && (INTVAL (operands[2]) % 8) == 0
   && ! mode_dependent_address_p (XEXP (operands[1], 0),
                                  MEM_ADDR_SPACE (operands[1]))"
{
  operands[1]
    = adjust_address (operands[1], SImode, INTVAL (operands[2]) / 8);

  return "move%.l %1,%0";
})

(define_insn "*extzv_8_16_reg"
  [(set (match_operand:SI 0 "nonimmediate_operand" "=&d")
	(zero_extract:SI (match_operand:SI 1 "register_operand" "d")
			 (match_operand:SI 2 "const_int_operand" "n")
			 (match_operand:SI 3 "const_int_operand" "n")))]
  "TARGET_68020 && TARGET_BITFIELD
   && (INTVAL (operands[2]) == 8 || INTVAL (operands[2]) == 16)
   && INTVAL (operands[3]) % INTVAL (operands[2]) == 0"
{
  cc_status.flags |= CC_NOT_NEGATIVE;
  if (INTVAL (operands[2]) + INTVAL (operands[3]) != 32)
    return "bfextu %1{%b3:%b2},%0";

  output_asm_insn ("clr%.l %0", operands);
  if (INTVAL (operands[2]) == 8)
    return "move%.b %1,%0";
  return "move%.w %1,%0";
})

;
; Special case for 32-bit field in memory.  This only occurs when 32-bit
; alignment of structure members is specified.
;
; The move is allowed to be odd byte aligned, because that's still faster
; than an odd byte aligned bit-field instruction.
;
(define_insn "*extv_32_mem"
  [(set (match_operand:SI 0 "nonimmediate_operand" "=rm")
	(sign_extract:SI (match_operand:QI 1 "memory_src_operand" "oS")
			 (const_int 32)
			 (match_operand:SI 2 "const_int_operand" "n")))]
  "TARGET_68020 && TARGET_BITFIELD
   && (INTVAL (operands[2]) % 8) == 0
   && ! mode_dependent_address_p (XEXP (operands[1], 0),
                                  MEM_ADDR_SPACE (operands[1]))"
{
  operands[1]
    = adjust_address (operands[1], SImode, INTVAL (operands[2]) / 8);

  return "move%.l %1,%0";
})

(define_insn "*extv_8_16_reg"
  [(set (match_operand:SI 0 "nonimmediate_operand" "=d")
	(sign_extract:SI (match_operand:SI 1 "register_operand" "d")
			 (match_operand:SI 2 "const_int_operand" "n")
			 (match_operand:SI 3 "const_int_operand" "n")))]
  "TARGET_68020 && TARGET_BITFIELD
   && (INTVAL (operands[2]) == 8 || INTVAL (operands[2]) == 16)
   && INTVAL (operands[3]) % INTVAL (operands[2]) == 0"
{
  if (INTVAL (operands[2]) + INTVAL (operands[3]) != 32)
    return "bfexts %1{%b3:%b2},%0";

  if (INTVAL (operands[2]) == 8)
    return "move%.b %1,%0\;extb%.l %0";
  return "move%.w %1,%0\;ext%.l %0";
})

;; Bit-field instructions, general cases.
;; "o,d" constraint causes a nonoffsettable memref to match the "o"
;; so that its address is reloaded.

(define_expand "extv"
  [(set (match_operand:SI 0 "register_operand" "")
	(sign_extract:SI (match_operand:SI 1 "general_operand" "")
			 (match_operand:SI 2 "const_int_operand" "")
			 (match_operand:SI 3 "const_int_operand" "")))]
  "TARGET_68020 && TARGET_BITFIELD"
  "")

(define_insn "*extv_bfexts_mem"
  [(set (match_operand:SI 0 "register_operand" "=d")
	(sign_extract:SI (match_operand:QI 1 "memory_operand" "o")
			 (match_operand:SI 2 "nonmemory_operand" "dn")
			 (match_operand:SI 3 "nonmemory_operand" "dn")))]
  "TARGET_68020 && TARGET_BITFIELD"
  "bfexts %1{%b3:%b2},%0")

(define_expand "extzv"
  [(set (match_operand:SI 0 "register_operand" "")
	(zero_extract:SI (match_operand:SI 1 "general_operand" "")
			 (match_operand:SI 2 "const_int_operand" "")
			 (match_operand:SI 3 "const_int_operand" "")))]
  "TARGET_68020 && TARGET_BITFIELD"
  "")

(define_insn "*extzv_bfextu_mem"
  [(set (match_operand:SI 0 "register_operand" "=d")
	(zero_extract:SI (match_operand:QI 1 "memory_operand" "o")
			 (match_operand:SI 2 "nonmemory_operand" "dn")
			 (match_operand:SI 3 "nonmemory_operand" "dn")))]
  "TARGET_68020 && TARGET_BITFIELD"
{
  if (GET_CODE (operands[2]) == CONST_INT)
    {
      if (INTVAL (operands[2]) != 32)
	cc_status.flags |= CC_NOT_NEGATIVE;
    }
  else
    {
      CC_STATUS_INIT;
    }
  return "bfextu %1{%b3:%b2},%0";
})

(define_insn "*insv_bfchg_mem"
  [(set (zero_extract:SI (match_operand:QI 0 "memory_operand" "+o")
			 (match_operand:SI 1 "nonmemory_operand" "dn")
			 (match_operand:SI 2 "nonmemory_operand" "dn"))
        (xor:SI (zero_extract:SI (match_dup 0) (match_dup 1) (match_dup 2))
		(match_operand 3 "const_int_operand" "n")))]
  "TARGET_68020 && TARGET_BITFIELD
   && (INTVAL (operands[3]) == -1
       || (GET_CODE (operands[1]) == CONST_INT
           && (~ INTVAL (operands[3]) & ((1 << INTVAL (operands[1]))- 1)) == 0))"
{
  CC_STATUS_INIT;
  return "bfchg %0{%b2:%b1}";
})

(define_insn "*insv_bfclr_mem"
  [(set (zero_extract:SI (match_operand:QI 0 "memory_operand" "+o")
			 (match_operand:SI 1 "nonmemory_operand" "dn")
			 (match_operand:SI 2 "nonmemory_operand" "dn"))
	(const_int 0))]
  "TARGET_68020 && TARGET_BITFIELD"
{
  CC_STATUS_INIT;
  return "bfclr %0{%b2:%b1}";
})

(define_insn "*insv_bfset_mem"
  [(set (zero_extract:SI (match_operand:QI 0 "memory_operand" "+o")
			 (match_operand:SI 1 "general_operand" "dn")
			 (match_operand:SI 2 "general_operand" "dn"))
	(const_int -1))]
  "TARGET_68020 && TARGET_BITFIELD"
{
  CC_STATUS_INIT;
  return "bfset %0{%b2:%b1}";
})

(define_expand "insv"
  [(set (zero_extract:SI (match_operand:SI 0 "nonimmediate_operand" "")
			 (match_operand:SI 1 "const_int_operand" "")
			 (match_operand:SI 2 "const_int_operand" ""))
	(match_operand:SI 3 "register_operand" ""))]
  "TARGET_68020 && TARGET_BITFIELD"
  "")

(define_insn "*insv_bfins_mem"
  [(set (zero_extract:SI (match_operand:QI 0 "memory_operand" "+o")
			 (match_operand:SI 1 "nonmemory_operand" "dn")
			 (match_operand:SI 2 "nonmemory_operand" "dn"))
	(match_operand:SI 3 "register_operand" "d"))]
  "TARGET_68020 && TARGET_BITFIELD"
  "bfins %3,%0{%b2:%b1}")

;; Now recognize bit-field insns that operate on registers
;; (or at least were intended to do so).

(define_insn "*extv_bfexts_reg"
  [(set (match_operand:SI 0 "nonimmediate_operand" "=d")
	(sign_extract:SI (match_operand:SI 1 "register_operand" "d")
			 (match_operand:SI 2 "const_int_operand" "n")
			 (match_operand:SI 3 "const_int_operand" "n")))]
  "TARGET_68020 && TARGET_BITFIELD"
  "bfexts %1{%b3:%b2},%0")

(define_insn "*extv_bfextu_reg"
  [(set (match_operand:SI 0 "nonimmediate_operand" "=d")
	(zero_extract:SI (match_operand:SI 1 "register_operand" "d")
			 (match_operand:SI 2 "const_int_operand" "n")
			 (match_operand:SI 3 "const_int_operand" "n")))]
  "TARGET_68020 && TARGET_BITFIELD"
{
  if (GET_CODE (operands[2]) == CONST_INT)
    {
      if (INTVAL (operands[2]) != 32)
	cc_status.flags |= CC_NOT_NEGATIVE;
    }
  else
    {
      CC_STATUS_INIT;
    }
  return "bfextu %1{%b3:%b2},%0";
})

(define_insn "*insv_bfclr_reg"
  [(set (zero_extract:SI (match_operand:SI 0 "register_operand" "+d")
			 (match_operand:SI 1 "const_int_operand" "n")
			 (match_operand:SI 2 "const_int_operand" "n"))
	(const_int 0))]
  "TARGET_68020 && TARGET_BITFIELD"
{
  CC_STATUS_INIT;
  return "bfclr %0{%b2:%b1}";
})

(define_insn "*insv_bfset_reg"
  [(set (zero_extract:SI (match_operand:SI 0 "register_operand" "+d")
			 (match_operand:SI 1 "const_int_operand" "n")
			 (match_operand:SI 2 "const_int_operand" "n"))
	(const_int -1))]
  "TARGET_68020 && TARGET_BITFIELD"
{
  CC_STATUS_INIT;
  return "bfset %0{%b2:%b1}";
})

(define_insn "*insv_bfins_reg"
  [(set (zero_extract:SI (match_operand:SI 0 "register_operand" "+d")
			 (match_operand:SI 1 "const_int_operand" "n")
			 (match_operand:SI 2 "const_int_operand" "n"))
	(match_operand:SI 3 "register_operand" "d"))]
  "TARGET_68020 && TARGET_BITFIELD"
{
#if 0
  /* These special cases are now recognized by a specific pattern.  */
  if (GET_CODE (operands[1]) == CONST_INT && GET_CODE (operands[2]) == CONST_INT
      && INTVAL (operands[1]) == 16 && INTVAL (operands[2]) == 16)
    return "move%.w %3,%0";
  if (GET_CODE (operands[1]) == CONST_INT && GET_CODE (operands[2]) == CONST_INT
      && INTVAL (operands[1]) == 24 && INTVAL (operands[2]) == 8)
    return "move%.b %3,%0";
#endif
  return "bfins %3,%0{%b2:%b1}";
})

;; Special patterns for optimizing bit-field instructions.

(define_insn "*tst_bftst_mem"
  [(set (cc0)
	(compare (zero_extract:SI (match_operand:QI 0 "memory_operand" "o")
				  (match_operand:SI 1 "const_int_operand" "n")
				  (match_operand:SI 2 "general_operand" "dn"))
	         (const_int 0)))]
  "TARGET_68020 && TARGET_BITFIELD"
{
  if (operands[1] == const1_rtx
      && GET_CODE (operands[2]) == CONST_INT)
    {
      int width = GET_CODE (operands[0]) == REG ? 31 : 7;
      return output_btst (operands,
			  GEN_INT (width - INTVAL (operands[2])),
			  operands[0], insn, 1000);
      /* Pass 1000 as SIGNPOS argument so that btst will
         not think we are testing the sign bit for an `and'
	 and assume that nonzero implies a negative result.  */
    }
  if (INTVAL (operands[1]) != 32)
    cc_status.flags = CC_NOT_NEGATIVE;
  return "bftst %0{%b2:%b1}";
})


;;; now handle the register cases
(define_insn "*tst_bftst_reg"
  [(set (cc0)
	(compare (zero_extract:SI (match_operand:SI 0 "register_operand" "d")
				  (match_operand:SI 1 "const_int_operand" "n")
			 	  (match_operand:SI 2 "general_operand" "dn"))
		 (const_int 0)))]
  "TARGET_68020 && TARGET_BITFIELD"
{
  if (operands[1] == const1_rtx
      && GET_CODE (operands[2]) == CONST_INT)
    {
      int width = GET_CODE (operands[0]) == REG ? 31 : 7;
      return output_btst (operands, GEN_INT (width - INTVAL (operands[2])),
			  operands[0], insn, 1000);
      /* Pass 1000 as SIGNPOS argument so that btst will
         not think we are testing the sign bit for an `and'
	 and assume that nonzero implies a negative result.  */
    }
  if (INTVAL (operands[1]) != 32)
    cc_status.flags = CC_NOT_NEGATIVE;
  return "bftst %0{%b2:%b1}";
})

(define_insn "scc0_di"
  [(set (match_operand:QI 0 "nonimmediate_operand" "=dm")
    (match_operator 1 "ordered_comparison_operator"
      [(match_operand:DI 2 "general_operand" "ro") (const_int 0)]))]
  "! TARGET_COLDFIRE"
{
  return output_scc_di (operands[1], operands[2], const0_rtx, operands[0]);
})

(define_insn "scc0_di_5200"
  [(set (match_operand:QI 0 "nonimmediate_operand" "=d")
    (match_operator 1 "ordered_comparison_operator"
      [(match_operand:DI 2 "general_operand" "ro") (const_int 0)]))]
  "TARGET_COLDFIRE"
{
  return output_scc_di (operands[1], operands[2], const0_rtx, operands[0]);
})

(define_insn "scc_di"
  [(set (match_operand:QI 0 "nonimmediate_operand" "=dm,dm")
    (match_operator 1 "ordered_comparison_operator"
      [(match_operand:DI 2 "general_operand" "ro,r")
       (match_operand:DI 3 "general_operand" "r,ro")]))]
  "! TARGET_COLDFIRE"
{
  return output_scc_di (operands[1], operands[2], operands[3], operands[0]);
})

(define_insn "scc_di_5200"
  [(set (match_operand:QI 0 "nonimmediate_operand" "=d,d")
    (match_operator 1 "ordered_comparison_operator"
      [(match_operand:DI 2 "general_operand" "ro,r")
       (match_operand:DI 3 "general_operand" "r,ro")]))]
  "TARGET_COLDFIRE"
{
  return output_scc_di (operands[1], operands[2], operands[3], operands[0]);
})

;; Note that operand 0 of an SCC insn is supported in the hardware as
;; memory, but we cannot allow it to be in memory in case the address
;; needs to be reloaded.

(define_insn ""
  [(set (match_operand:QI 0 "register_operand" "=d")
	(eq:QI (cc0) (const_int 0)))]
  ""
{
  cc_status = cc_prev_status;
  OUTPUT_JUMP ("seq %0", "fseq %0", "seq %0");
})

(define_insn ""
  [(set (match_operand:QI 0 "register_operand" "=d")
	(ne:QI (cc0) (const_int 0)))]
  ""
{
  cc_status = cc_prev_status;
  OUTPUT_JUMP ("sne %0", "fsne %0", "sne %0");
})

(define_insn ""
  [(set (match_operand:QI 0 "register_operand" "=d")
	(gt:QI (cc0) (const_int 0)))]
  ""
{
  cc_status = cc_prev_status;
  OUTPUT_JUMP ("sgt %0", "fsgt %0", 0);
})

(define_insn ""
  [(set (match_operand:QI 0 "register_operand" "=d")
	(gtu:QI (cc0) (const_int 0)))]
  ""
{
  cc_status = cc_prev_status;
  return "shi %0";
})

(define_insn ""
  [(set (match_operand:QI 0 "register_operand" "=d")
	(lt:QI (cc0) (const_int 0)))]
  ""
{
   cc_status = cc_prev_status;
   OUTPUT_JUMP ("slt %0", "fslt %0", "smi %0");
})

(define_insn ""
  [(set (match_operand:QI 0 "register_operand" "=d")
	(ltu:QI (cc0) (const_int 0)))]
  ""
{
   cc_status = cc_prev_status;
   return "scs %0";
})

(define_insn ""
  [(set (match_operand:QI 0 "register_operand" "=d")
	(ge:QI (cc0) (const_int 0)))]
  ""
{
   cc_status = cc_prev_status;
   OUTPUT_JUMP ("sge %0", "fsge %0", "spl %0");
})

(define_insn "*scc"
  [(set (match_operand:QI 0 "register_operand" "=d")
	(geu:QI (cc0) (const_int 0)))]
  ""
{
   cc_status = cc_prev_status;
   return "scc %0";
}
  [(set_attr "type" "scc")])

(define_insn ""
  [(set (match_operand:QI 0 "register_operand" "=d")
	(le:QI (cc0) (const_int 0)))]
  ""
{
  cc_status = cc_prev_status;
  OUTPUT_JUMP ("sle %0", "fsle %0", 0);
})

(define_insn "*sls"
  [(set (match_operand:QI 0 "register_operand" "=d")
	(leu:QI (cc0) (const_int 0)))]
  ""
{
   cc_status = cc_prev_status;
   return "sls %0";
}
  [(set_attr "type" "scc")])

(define_insn "*sordered_1"
  [(set (match_operand:QI 0 "register_operand" "=d")
	(ordered:QI (cc0) (const_int 0)))]
  "TARGET_68881 && !TUNE_68060"
{
  cc_status = cc_prev_status;
  return "fsor %0";
})

(define_insn "*sunordered_1"
  [(set (match_operand:QI 0 "register_operand" "=d")
	(unordered:QI (cc0) (const_int 0)))]
  "TARGET_68881 && !TUNE_68060"
{
  cc_status = cc_prev_status;
  return "fsun %0";
})

(define_insn "*suneq_1"
  [(set (match_operand:QI 0 "register_operand" "=d")
	(uneq:QI (cc0) (const_int 0)))]
  "TARGET_68881 && !TUNE_68060"
{
  cc_status = cc_prev_status;
  return "fsueq %0";
})

(define_insn "*sunge_1"
  [(set (match_operand:QI 0 "register_operand" "=d")
	(unge:QI (cc0) (const_int 0)))]
  "TARGET_68881 && !TUNE_68060"
{
  cc_status = cc_prev_status;
  return "fsuge %0";
})

(define_insn "*sungt_1"
  [(set (match_operand:QI 0 "register_operand" "=d")
	(ungt:QI (cc0) (const_int 0)))]
  "TARGET_68881 && !TUNE_68060"
{
  cc_status = cc_prev_status;
  return "fsugt %0";
})

(define_insn "*sunle_1"
  [(set (match_operand:QI 0 "register_operand" "=d")
	(unle:QI (cc0) (const_int 0)))]
  "TARGET_68881 && !TUNE_68060"
{
  cc_status = cc_prev_status;
  return "fsule %0";
})

(define_insn "*sunlt_1"
  [(set (match_operand:QI 0 "register_operand" "=d")
	(unlt:QI (cc0) (const_int 0)))]
  "TARGET_68881 && !TUNE_68060"
{
  cc_status = cc_prev_status;
  return "fsult %0";
})

(define_insn "*sltgt_1"
  [(set (match_operand:QI 0 "register_operand" "=d")
	(ltgt:QI (cc0) (const_int 0)))]
  "TARGET_68881 && !TUNE_68060"
{
  cc_status = cc_prev_status;
  return "fsogl %0";
})

(define_insn "*fsogt_1"
  [(set (match_operand:QI 0 "register_operand" "=d")
	(not:QI (unle:QI (cc0) (const_int 0))))]
  "TARGET_68881 && !TUNE_68060"
{
  cc_status = cc_prev_status;
  return "fsogt %0";
})

(define_insn "*fsoge_1"
  [(set (match_operand:QI 0 "register_operand" "=d")
	(not:QI (unlt:QI (cc0) (const_int 0))))]
  "TARGET_68881 && !TUNE_68060"
{
  cc_status = cc_prev_status;
  return "fsoge %0";
})

(define_insn "*fsolt_1"
  [(set (match_operand:QI 0 "register_operand" "=d")
	(not:QI (unge:QI (cc0) (const_int 0))))]
  "TARGET_68881 && !TUNE_68060"
{
  cc_status = cc_prev_status;
  return "fsolt %0";
})

(define_insn "*fsole_1"
  [(set (match_operand:QI 0 "register_operand" "=d")
	(not:QI (ungt:QI (cc0) (const_int 0))))]
  "TARGET_68881 && !TUNE_68060"
{
  cc_status = cc_prev_status;
  return "fsole %0";
})

;; Basic conditional jump instructions.

(define_insn "beq0_di"
  [(set (pc)
    (if_then_else (eq (match_operand:DI 0 "general_operand" "d*ao,<>")
            (const_int 0))
        (label_ref (match_operand 1 "" ","))
        (pc)))
   (clobber (match_scratch:SI 2 "=d,d"))]
  ""
{
  CC_STATUS_INIT;
  if (which_alternative == 1)
    return "move%.l %0,%2\;or%.l %0,%2\;jeq %l1";
  if ((cc_prev_status.value1
      && rtx_equal_p (cc_prev_status.value1, operands[0]))
    || (cc_prev_status.value2
      && rtx_equal_p (cc_prev_status.value2, operands[0])))
    {
      cc_status = cc_prev_status;
      return "jeq %l1";
    }
  if (GET_CODE (operands[0]) == REG)
    operands[3] = gen_rtx_REG (SImode, REGNO (operands[0]) + 1);
  else
    operands[3] = adjust_address (operands[0], SImode, 4);
  if (! ADDRESS_REG_P (operands[0]))
    {
      if (reg_overlap_mentioned_p (operands[2], operands[0]))
	{
	  if (reg_overlap_mentioned_p (operands[2], operands[3]))
	    return "or%.l %0,%2\;jeq %l1";
	  else
	    return "or%.l %3,%2\;jeq %l1";
	}
      return "move%.l %0,%2\;or%.l %3,%2\;jeq %l1";
    }
  operands[4] = gen_label_rtx();
  if (TARGET_68020 || TARGET_COLDFIRE)
    output_asm_insn ("tst%.l %0\;jne %l4\;tst%.l %3\;jeq %l1", operands);
  else
    output_asm_insn ("cmp%.w #0,%0\;jne %l4\;cmp%.w #0,%3\;jeq %l1", operands);
  (*targetm.asm_out.internal_label) (asm_out_file, "L",
				CODE_LABEL_NUMBER (operands[4]));
  return "";
})

(define_insn "bne0_di"
  [(set (pc)
    (if_then_else (ne (match_operand:DI 0 "general_operand" "do,*a")
            (const_int 0))
        (label_ref (match_operand 1 "" ","))
        (pc)))
   (clobber (match_scratch:SI 2 "=d,X"))]
  ""
{
  if ((cc_prev_status.value1
      && rtx_equal_p (cc_prev_status.value1, operands[0]))
    || (cc_prev_status.value2
      && rtx_equal_p (cc_prev_status.value2, operands[0])))
    {
      cc_status = cc_prev_status;
      return "jne %l1";
    }
  CC_STATUS_INIT;
  if (GET_CODE (operands[0]) == REG)
    operands[3] = gen_rtx_REG (SImode, REGNO (operands[0]) + 1);
  else
    operands[3] = adjust_address (operands[0], SImode, 4);
  if (!ADDRESS_REG_P (operands[0]))
    {
      if (reg_overlap_mentioned_p (operands[2], operands[0]))
	{
	  if (reg_overlap_mentioned_p (operands[2], operands[3]))
	    return "or%.l %0,%2\;jne %l1";
	  else
	    return "or%.l %3,%2\;jne %l1";
	}
      return "move%.l %0,%2\;or%.l %3,%2\;jne %l1";
    }
  if (TARGET_68020 || TARGET_COLDFIRE)
    return "tst%.l %0\;jne %l1\;tst%.l %3\;jne %l1";
  else
    return "cmp%.w #0,%0\;jne %l1\;cmp%.w #0,%3\;jne %l1";
})

(define_insn "bge0_di"
  [(set (pc)
    (if_then_else (ge (match_operand:DI 0 "general_operand" "ro")
            (const_int 0))
        (label_ref (match_operand 1 "" ""))
        (pc)))]
  ""
{
  if ((cc_prev_status.value1
      && rtx_equal_p (cc_prev_status.value1, operands[0]))
    || (cc_prev_status.value2
      && rtx_equal_p (cc_prev_status.value2, operands[0])))
    {
      cc_status = cc_prev_status;
      return cc_status.flags & CC_REVERSED ? "jle %l1" : "jpl %l1";
    }
  CC_STATUS_INIT;
  if (TARGET_68020 || TARGET_COLDFIRE || ! ADDRESS_REG_P (operands[0]))
    output_asm_insn("tst%.l %0", operands);
  else
    {
      /* On an address reg, cmpw may replace cmpl.  */
      output_asm_insn("cmp%.w #0,%0", operands);
    }
  return "jpl %l1";
})

(define_insn "blt0_di"
  [(set (pc)
    (if_then_else (lt (match_operand:DI 0 "general_operand" "ro")
            (const_int 0))
        (label_ref (match_operand 1 "" ""))
        (pc)))]
  ""
{
  if ((cc_prev_status.value1
      && rtx_equal_p (cc_prev_status.value1, operands[0]))
    || (cc_prev_status.value2
      && rtx_equal_p (cc_prev_status.value2, operands[0])))
    {
      cc_status = cc_prev_status;
      return cc_status.flags & CC_REVERSED ? "jgt %l1" : "jmi %l1";
    }
  CC_STATUS_INIT;
  if (TARGET_68020 || TARGET_COLDFIRE || ! ADDRESS_REG_P (operands[0]))
    output_asm_insn("tst%.l %0", operands);
  else
    {
      /* On an address reg, cmpw may replace cmpl.  */
      output_asm_insn("cmp%.w #0,%0", operands);
    }
  return "jmi %l1";
})

(define_insn "beq"
  [(set (pc)
	(if_then_else (eq (cc0)
			  (const_int 0))
		      (label_ref (match_operand 0 "" ""))
		      (pc)))]
  ""
{
  OUTPUT_JUMP ("jeq %l0", "fjeq %l0", "jeq %l0");
}
  [(set_attr "type" "bcc")])

(define_insn "bne"
  [(set (pc)
	(if_then_else (ne (cc0)
			  (const_int 0))
		      (label_ref (match_operand 0 "" ""))
		      (pc)))]
  ""
{
  OUTPUT_JUMP ("jne %l0", "fjne %l0", "jne %l0");
}
  [(set_attr "type" "bcc")])

(define_insn "bgt"
  [(set (pc)
	(if_then_else (gt (cc0)
			  (const_int 0))
		      (label_ref (match_operand 0 "" ""))
		      (pc)))]
  ""
{
  if ((cc_status.flags & CC_OVERFLOW_UNUSABLE) != 0)
    {
      cc_status.flags &= ~CC_OVERFLOW_UNUSABLE;
      return 0;
    }

  OUTPUT_JUMP ("jgt %l0", "fjgt %l0", 0);
}
  [(set_attr "type" "bcc")])

(define_insn "bgtu"
  [(set (pc)
	(if_then_else (gtu (cc0)
			   (const_int 0))
		      (label_ref (match_operand 0 "" ""))
		      (pc)))]
  ""
{
  if ((cc_status.flags & CC_OVERFLOW_UNUSABLE) != 0)
    {
      cc_status.flags &= ~CC_OVERFLOW_UNUSABLE;
      return 0;
    }

  return "jhi %l0";
}
  [(set_attr "type" "bcc")])

(define_insn "blt"
  [(set (pc)
	(if_then_else (lt (cc0)
			  (const_int 0))
		      (label_ref (match_operand 0 "" ""))
		      (pc)))]
  ""
{
  if ((cc_status.flags & CC_OVERFLOW_UNUSABLE) != 0)
    {
      cc_status.flags &= ~CC_OVERFLOW_UNUSABLE;
      return 0;
    }

  OUTPUT_JUMP ("jlt %l0", "fjlt %l0", "jmi %l0");
}
  [(set_attr "type" "bcc")])

(define_insn "bltu"
  [(set (pc)
	(if_then_else (ltu (cc0)
			   (const_int 0))
		      (label_ref (match_operand 0 "" ""))
		      (pc)))]
  ""
{
  if ((cc_status.flags & CC_OVERFLOW_UNUSABLE) != 0)
    {
      cc_status.flags &= ~CC_OVERFLOW_UNUSABLE;
      return 0;
    }

  return "jcs %l0";
}
  [(set_attr "type" "bcc")])

(define_insn "bge"
  [(set (pc)
	(if_then_else (ge (cc0)
			  (const_int 0))
		      (label_ref (match_operand 0 "" ""))
		      (pc)))]
  ""
{
  if ((cc_status.flags & CC_OVERFLOW_UNUSABLE) != 0)
    {
      cc_status.flags &= ~CC_OVERFLOW_UNUSABLE;
      return 0;
    }

  OUTPUT_JUMP ("jge %l0", "fjge %l0", "jpl %l0");
})

(define_insn "bgeu"
  [(set (pc)
	(if_then_else (geu (cc0)
			   (const_int 0))
		      (label_ref (match_operand 0 "" ""))
		      (pc)))]
  ""
{
  if ((cc_status.flags & CC_OVERFLOW_UNUSABLE) != 0)
    {
      cc_status.flags &= ~CC_OVERFLOW_UNUSABLE;
      return 0;
    }

  return "jcc %l0";
}
  [(set_attr "type" "bcc")])

(define_insn "ble"
  [(set (pc)
	(if_then_else (le (cc0)
			  (const_int 0))
		      (label_ref (match_operand 0 "" ""))
		      (pc)))]
  ""
{
  if ((cc_status.flags & CC_OVERFLOW_UNUSABLE) != 0)
    {
      cc_status.flags &= ~CC_OVERFLOW_UNUSABLE;
      return 0;
    }

  OUTPUT_JUMP ("jle %l0", "fjle %l0", 0);
}
  [(set_attr "type" "bcc")])

(define_insn "bleu"
  [(set (pc)
	(if_then_else (leu (cc0)
			   (const_int 0))
		      (label_ref (match_operand 0 "" ""))
		      (pc)))]
  ""
{
  if ((cc_status.flags & CC_OVERFLOW_UNUSABLE) != 0)
    {
      cc_status.flags &= ~CC_OVERFLOW_UNUSABLE;
      return 0;
    }

  return "jls %l0";
}
  [(set_attr "type" "bcc")])

(define_insn "bordered"
  [(set (pc)
	(if_then_else (ordered (cc0) (const_int 0))
		      (label_ref (match_operand 0 "" ""))
		      (pc)))]
  "TARGET_HARD_FLOAT"
{
  gcc_assert (cc_prev_status.flags & CC_IN_68881);
  return "fjor %l0";
}
  [(set_attr "type" "fbcc")])

(define_insn "bunordered"
  [(set (pc)
	(if_then_else (unordered (cc0) (const_int 0))
		      (label_ref (match_operand 0 "" ""))
		      (pc)))]
  "TARGET_HARD_FLOAT"
{
  gcc_assert (cc_prev_status.flags & CC_IN_68881);
  return "fjun %l0";
}
  [(set_attr "type" "fbcc")])

(define_insn "buneq"
  [(set (pc)
	(if_then_else (uneq (cc0) (const_int 0))
		      (label_ref (match_operand 0 "" ""))
		      (pc)))]
  "TARGET_HARD_FLOAT"
{
  gcc_assert (cc_prev_status.flags & CC_IN_68881);
  return "fjueq %l0";
}
  [(set_attr "type" "fbcc")])

(define_insn "bunge"
  [(set (pc)
	(if_then_else (unge (cc0) (const_int 0))
		      (label_ref (match_operand 0 "" ""))
		      (pc)))]
  "TARGET_HARD_FLOAT"
{
  gcc_assert (cc_prev_status.flags & CC_IN_68881);
  return "fjuge %l0";
}
  [(set_attr "type" "fbcc")])

(define_insn "bungt"
  [(set (pc)
	(if_then_else (ungt (cc0) (const_int 0))
		      (label_ref (match_operand 0 "" ""))
		      (pc)))]
  "TARGET_HARD_FLOAT"
{
  gcc_assert (cc_prev_status.flags & CC_IN_68881);
  return "fjugt %l0";
}
  [(set_attr "type" "fbcc")])

(define_insn "bunle"
  [(set (pc)
	(if_then_else (unle (cc0) (const_int 0))
		      (label_ref (match_operand 0 "" ""))
		      (pc)))]
  "TARGET_HARD_FLOAT"
{
  gcc_assert (cc_prev_status.flags & CC_IN_68881);
  return "fjule %l0";
}
  [(set_attr "type" "fbcc")])

(define_insn "bunlt"
  [(set (pc)
	(if_then_else (unlt (cc0) (const_int 0))
		      (label_ref (match_operand 0 "" ""))
		      (pc)))]
  "TARGET_HARD_FLOAT"
{
  gcc_assert (cc_prev_status.flags & CC_IN_68881);
  return "fjult %l0";
}
  [(set_attr "type" "fbcc")])

(define_insn "bltgt"
  [(set (pc)
	(if_then_else (ltgt (cc0) (const_int 0))
		      (label_ref (match_operand 0 "" ""))
		      (pc)))]
  "TARGET_HARD_FLOAT"
{
  gcc_assert (cc_prev_status.flags & CC_IN_68881);
  return "fjogl %l0";
}
  [(set_attr "type" "fbcc")])

;; Negated conditional jump instructions.

(define_insn "*beq_rev"
  [(set (pc)
	(if_then_else (eq (cc0)
			  (const_int 0))
		      (pc)
		      (label_ref (match_operand 0 "" ""))))]
  ""
{
  OUTPUT_JUMP ("jne %l0", "fjne %l0", "jne %l0");
}
  [(set_attr "type" "bcc")])

(define_insn "*bne_rev"
  [(set (pc)
	(if_then_else (ne (cc0)
			  (const_int 0))
		      (pc)
		      (label_ref (match_operand 0 "" ""))))]
  ""
{
  OUTPUT_JUMP ("jeq %l0", "fjeq %l0", "jeq %l0");
}
  [(set_attr "type" "bcc")])

(define_insn "*bgt_rev"
  [(set (pc)
	(if_then_else (gt (cc0)
			  (const_int 0))
		      (pc)
		      (label_ref (match_operand 0 "" ""))))]
  ""
{
  if ((cc_status.flags & CC_OVERFLOW_UNUSABLE) != 0)
    {
      cc_status.flags &= ~CC_OVERFLOW_UNUSABLE;
      return 0;
    }

  OUTPUT_JUMP ("jle %l0", "fjngt %l0", 0);
}
  [(set_attr "type" "bcc")])

(define_insn "*bgtu_rev"
  [(set (pc)
	(if_then_else (gtu (cc0)
			   (const_int 0))
		      (pc)
		      (label_ref (match_operand 0 "" ""))))]
  ""
{
  if ((cc_status.flags & CC_OVERFLOW_UNUSABLE) != 0)
    {
      cc_status.flags &= ~CC_OVERFLOW_UNUSABLE;
      return 0;
    }

  return "jls %l0";
}
  [(set_attr "type" "bcc")])

(define_insn "*blt_rev"
  [(set (pc)
	(if_then_else (lt (cc0)
			  (const_int 0))
		      (pc)
		      (label_ref (match_operand 0 "" ""))))]
  ""
{
  if ((cc_status.flags & CC_OVERFLOW_UNUSABLE) != 0)
    {
      cc_status.flags &= ~CC_OVERFLOW_UNUSABLE;
      return 0;
    }

  OUTPUT_JUMP ("jge %l0", "fjnlt %l0", "jpl %l0");
}
  [(set_attr "type" "bcc")])

(define_insn "*bltu_rev"
  [(set (pc)
	(if_then_else (ltu (cc0)
			   (const_int 0))
		      (pc)
		      (label_ref (match_operand 0 "" ""))))]
  ""
{
  if ((cc_status.flags & CC_OVERFLOW_UNUSABLE) != 0)
    {
      cc_status.flags &= ~CC_OVERFLOW_UNUSABLE;
      return 0;
    }

  return "jcc %l0";
}
  [(set_attr "type" "bcc")])

(define_insn "*bge_rev"
  [(set (pc)
	(if_then_else (ge (cc0)
			  (const_int 0))
		      (pc)
		      (label_ref (match_operand 0 "" ""))))]
  ""
{
  if ((cc_status.flags & CC_OVERFLOW_UNUSABLE) != 0)
    {
      cc_status.flags &= ~CC_OVERFLOW_UNUSABLE;
      return 0;
    }

  OUTPUT_JUMP ("jlt %l0", "fjnge %l0", "jmi %l0");
}
  [(set_attr "type" "bcc")])

(define_insn "*bgeu_rev"
  [(set (pc)
	(if_then_else (geu (cc0)
			   (const_int 0))
		      (pc)
		      (label_ref (match_operand 0 "" ""))))]
  ""
{
  if ((cc_status.flags & CC_OVERFLOW_UNUSABLE) != 0)
    {
      cc_status.flags &= ~CC_OVERFLOW_UNUSABLE;
      return 0;
    }

  return "jcs %l0";
}
  [(set_attr "type" "bcc")])

(define_insn "*ble_rev"
  [(set (pc)
	(if_then_else (le (cc0)
			  (const_int 0))
		      (pc)
		      (label_ref (match_operand 0 "" ""))))]
  ""
{
  if ((cc_status.flags & CC_OVERFLOW_UNUSABLE) != 0)
    {
      cc_status.flags &= ~CC_OVERFLOW_UNUSABLE;
      return 0;
    }

  OUTPUT_JUMP ("jgt %l0", "fjnle %l0", 0);
}
  [(set_attr "type" "bcc")])

(define_insn "*bleu_rev"
  [(set (pc)
	(if_then_else (leu (cc0)
			   (const_int 0))
		      (pc)
		      (label_ref (match_operand 0 "" ""))))]
  ""
{
  if ((cc_status.flags & CC_OVERFLOW_UNUSABLE) != 0)
    {
      cc_status.flags &= ~CC_OVERFLOW_UNUSABLE;
      return 0;
    }

  return "jhi %l0";
}
  [(set_attr "type" "bcc")])

(define_insn "*bordered_rev"
  [(set (pc)
	(if_then_else (ordered (cc0) (const_int 0))
		      (pc)
		      (label_ref (match_operand 0 "" ""))))]
  "TARGET_HARD_FLOAT"
{
  gcc_assert (cc_prev_status.flags & CC_IN_68881);
  return "fjun %l0";
}
  [(set_attr "type" "fbcc")])

(define_insn "*bunordered_rev"
  [(set (pc)
	(if_then_else (unordered (cc0) (const_int 0))
		      (pc)
		      (label_ref (match_operand 0 "" ""))))]
  "TARGET_HARD_FLOAT"
{
  gcc_assert (cc_prev_status.flags & CC_IN_68881);
  return "fjor %l0";
}
  [(set_attr "type" "fbcc")])

(define_insn "*buneq_rev"
  [(set (pc)
	(if_then_else (uneq (cc0) (const_int 0))
		      (pc)
		      (label_ref (match_operand 0 "" ""))))]
  "TARGET_HARD_FLOAT"
{
  gcc_assert (cc_prev_status.flags & CC_IN_68881);
  return "fjogl %l0";
}
  [(set_attr "type" "fbcc")])

(define_insn "*bunge_rev"
  [(set (pc)
	(if_then_else (unge (cc0) (const_int 0))
		      (pc)
		      (label_ref (match_operand 0 "" ""))))]
  "TARGET_HARD_FLOAT"
{
  gcc_assert (cc_prev_status.flags & CC_IN_68881);
  return "fjolt %l0";
}
  [(set_attr "type" "fbcc")])

(define_insn "*bungt_rev"
  [(set (pc)
	(if_then_else (ungt (cc0) (const_int 0))
		      (pc)
		      (label_ref (match_operand 0 "" ""))))]
  "TARGET_HARD_FLOAT"
{
  gcc_assert (cc_prev_status.flags & CC_IN_68881);
  return "fjole %l0";
}
  [(set_attr "type" "fbcc")])

(define_insn "*bunle_rev"
  [(set (pc)
	(if_then_else (unle (cc0) (const_int 0))
		      (pc)
		      (label_ref (match_operand 0 "" ""))))]
  "TARGET_HARD_FLOAT"
{
  gcc_assert (cc_prev_status.flags & CC_IN_68881);
  return "fjogt %l0";
}
  [(set_attr "type" "fbcc")])

(define_insn "*bunlt_rev"
  [(set (pc)
	(if_then_else (unlt (cc0) (const_int 0))
		      (pc)
		      (label_ref (match_operand 0 "" ""))))]
  "TARGET_HARD_FLOAT"
{
  gcc_assert (cc_prev_status.flags & CC_IN_68881);
  return "fjoge %l0";
}
  [(set_attr "type" "fbcc")])

(define_insn "*bltgt_rev"
  [(set (pc)
	(if_then_else (ltgt (cc0) (const_int 0))
		      (pc)
		      (label_ref (match_operand 0 "" ""))))]
  "TARGET_HARD_FLOAT"
{
  gcc_assert (cc_prev_status.flags & CC_IN_68881);
  return "fjueq %l0";
}
  [(set_attr "type" "fbcc")])

;; Unconditional and other jump instructions
(define_insn "jump"
  [(set (pc)
	(label_ref (match_operand 0 "" "")))]
  ""
  "jra %l0"
  [(set_attr "type" "bra")])

(define_expand "tablejump"
  [(parallel [(set (pc) (match_operand 0 "" ""))
	      (use (label_ref (match_operand 1 "" "")))])]
  ""
{
#if CASE_VECTOR_PC_RELATIVE
    operands[0] = gen_rtx_PLUS (SImode, pc_rtx,
				gen_rtx_SIGN_EXTEND (SImode, operands[0]));
#endif
})

;; Jump to variable address from dispatch table of absolute addresses.
(define_insn "*tablejump_internal"
  [(set (pc) (match_operand:SI 0 "register_operand" "a"))
   (use (label_ref (match_operand 1 "" "")))]
  ""
{
  return MOTOROLA ? "jmp (%0)" : "jmp %0@";
}
  [(set_attr "type" "jmp")])

;; Jump to variable address from dispatch table of relative addresses.
(define_insn ""
  [(set (pc)
	(plus:SI (pc)
		 (sign_extend:SI (match_operand:HI 0 "register_operand" "r"))))
   (use (label_ref (match_operand 1 "" "")))]
  ""
{
#ifdef ASM_RETURN_CASE_JUMP
  ASM_RETURN_CASE_JUMP;
#else
  if (TARGET_COLDFIRE)
    {
      if (ADDRESS_REG_P (operands[0]))
	return MOTOROLA ? "jmp (2,pc,%0.l)" : "jmp pc@(2,%0:l)";
      else if (MOTOROLA)
	return "ext%.l %0\;jmp (2,pc,%0.l)";
      else
	return "extl %0\;jmp pc@(2,%0:l)";
    }
  else
    return MOTOROLA ? "jmp (2,pc,%0.w)" : "jmp pc@(2,%0:w)";
#endif
})

;; Decrement-and-branch insns.
(define_insn "*dbne_hi"
  [(set (pc)
	(if_then_else
	 (ne (match_operand:HI 0 "nonimmediate_operand" "+d*g")
	     (const_int 0))
	 (label_ref (match_operand 1 "" ""))
	 (pc)))
   (set (match_dup 0)
	(plus:HI (match_dup 0)
		 (const_int -1)))]
  "!TARGET_COLDFIRE"
{
  CC_STATUS_INIT;
  if (DATA_REG_P (operands[0]))
    return "dbra %0,%l1";
  if (GET_CODE (operands[0]) == MEM)
    return "subq%.w #1,%0\;jcc %l1";
  return "subq%.w #1,%0\;cmp%.w #-1,%0\;jne %l1";
})

(define_insn "*dbne_si"
  [(set (pc)
	(if_then_else
	 (ne (match_operand:SI 0 "nonimmediate_operand" "+d*g")
	     (const_int 0))
	 (label_ref (match_operand 1 "" ""))
	 (pc)))
   (set (match_dup 0)
	(plus:SI (match_dup 0)
		 (const_int -1)))]
  "!TARGET_COLDFIRE"
{
  CC_STATUS_INIT;
  if (DATA_REG_P (operands[0]))
    return "dbra %0,%l1\;clr%.w %0\;subq%.l #1,%0\;jcc %l1";
  if (GET_CODE (operands[0]) == MEM)
    return "subq%.l #1,%0\;jcc %l1";
  return "subq%.l #1,%0\;cmp%.l #-1,%0\;jne %l1";
})

;; Two dbra patterns that use REG_NOTES info generated by strength_reduce.

(define_insn "*dbge_hi"
  [(set (pc)
	(if_then_else
	  (ge (plus:HI (match_operand:HI 0 "nonimmediate_operand" "+d*am")
		       (const_int -1))
	      (const_int 0))
	  (label_ref (match_operand 1 "" ""))
	  (pc)))
   (set (match_dup 0)
	(plus:HI (match_dup 0)
		 (const_int -1)))]
  "!TARGET_COLDFIRE && find_reg_note (insn, REG_NONNEG, 0)"
{
  CC_STATUS_INIT;
  if (DATA_REG_P (operands[0]))
    return "dbra %0,%l1";
  if (GET_CODE (operands[0]) == MEM)
    return "subq%.w #1,%0\;jcc %l1";
  return "subq%.w #1,%0\;cmp%.w #-1,%0\;jne %l1";
})

(define_expand "decrement_and_branch_until_zero"
  [(parallel [(set (pc)
		   (if_then_else
		    (ge (plus:SI (match_operand:SI 0 "nonimmediate_operand" "")
				 (const_int -1))
			(const_int 0))
		    (label_ref (match_operand 1 "" ""))
		    (pc)))
	      (set (match_dup 0)
		   (plus:SI (match_dup 0)
			    (const_int -1)))])]
  ""
  "")

(define_insn "*dbge_si"
  [(set (pc)
	(if_then_else
	  (ge (plus:SI (match_operand:SI 0 "nonimmediate_operand" "+d*am")
		       (const_int -1))
	      (const_int 0))
	  (label_ref (match_operand 1 "" ""))
	  (pc)))
   (set (match_dup 0)
	(plus:SI (match_dup 0)
		 (const_int -1)))]
  "!TARGET_COLDFIRE && find_reg_note (insn, REG_NONNEG, 0)"
{
  CC_STATUS_INIT;
  if (DATA_REG_P (operands[0]))
    return "dbra %0,%l1\;clr%.w %0\;subq%.l #1,%0\;jcc %l1";
  if (GET_CODE (operands[0]) == MEM)
    return "subq%.l #1,%0\;jcc %l1";
  return "subq%.l #1,%0\;cmp%.l #-1,%0\;jne %l1";
})

(define_expand "sibcall"
  [(call (match_operand:QI 0 "memory_operand" "")
	 (match_operand:SI 1 "general_operand" ""))]
  ""
{
  operands[0] = m68k_legitimize_sibcall_address (operands[0]);
})

(define_insn "*sibcall"
  [(call (mem:QI (match_operand:SI 0 "sibcall_operand" ""))
	 (match_operand:SI 1 "general_operand" ""))]
  "SIBLING_CALL_P (insn)"
{
  return output_sibcall (operands[0]);
})

(define_expand "sibcall_value"
  [(set (match_operand 0 "" "")
	(call (match_operand:QI 1 "memory_operand" "")
	      (match_operand:SI 2 "general_operand" "")))]
  ""
{
  operands[1] = m68k_legitimize_sibcall_address (operands[1]);
})

(define_insn "*sibcall_value"
  [(set (match_operand 0 "" "=rf,rf")
	(call (mem:QI (match_operand:SI 1 "sibcall_operand" ""))
	      (match_operand:SI 2 "general_operand" "")))]
  "SIBLING_CALL_P (insn)"
{
  operands[0] = operands[1];
  return output_sibcall (operands[0]);
})

;; Call subroutine with no return value.
(define_expand "call"
  [(call (match_operand:QI 0 "memory_operand" "")
	 (match_operand:SI 1 "general_operand" ""))]
  ;; Operand 1 not really used on the m68000.
  ""
{
  operands[0] = m68k_legitimize_call_address (operands[0]);
})

(define_insn "*call"
  [(call (mem:QI (match_operand:SI 0 "call_operand" "a,W"))
	 (match_operand:SI 1 "general_operand" "g,g"))]
  ;; Operand 1 not really used on the m68000.
  "!SIBLING_CALL_P (insn)"
{
  return output_call (operands[0]);
}
  [(set_attr "type" "jsr")])

;; Call subroutine, returning value in operand 0
;; (which must be a hard register).
(define_expand "call_value"
  [(set (match_operand 0 "" "")
	(call (match_operand:QI 1 "memory_operand" "")
	      (match_operand:SI 2 "general_operand" "")))]
  ;; Operand 2 not really used on the m68000.
  ""
{
  operands[1] = m68k_legitimize_call_address (operands[1]);
})

(define_insn "*non_symbolic_call_value"
  [(set (match_operand 0 "" "=rf,rf")
	(call (mem:QI (match_operand:SI 1 "non_symbolic_call_operand" "a,W"))
	      (match_operand:SI 2 "general_operand" "g,g")))]
  ;; Operand 2 not really used on the m68000.
  "!SIBLING_CALL_P (insn)"
  "jsr %a1"
  [(set_attr "type" "jsr")
   (set_attr "opx" "1")])

(define_insn "*symbolic_call_value_jsr"
  [(set (match_operand 0 "" "=rf,rf")
	(call (mem:QI (match_operand:SI 1 "symbolic_operand" "a,W"))
	      (match_operand:SI 2 "general_operand" "g,g")))]
  ;; Operand 2 not really used on the m68000.
  "!SIBLING_CALL_P (insn) && m68k_symbolic_call_var == M68K_SYMBOLIC_CALL_JSR"
{
  operands[0] = operands[1];
  return m68k_symbolic_call;
}
  [(set_attr "type" "jsr")
   (set_attr "opx" "1")])

(define_insn "*symbolic_call_value_bsr"
  [(set (match_operand 0 "" "=rf,rf")
	(call (mem:QI (match_operand:SI 1 "symbolic_operand" "a,W"))
	      (match_operand:SI 2 "general_operand" "g,g")))]
  ;; Operand 2 not really used on the m68000.
  "!SIBLING_CALL_P (insn)
   && (m68k_symbolic_call_var == M68K_SYMBOLIC_CALL_BSR_C
       || m68k_symbolic_call_var == M68K_SYMBOLIC_CALL_BSR_P)"
{
  operands[0] = operands[1];
  return m68k_symbolic_call;
}
  [(set_attr "type" "bsr")
   (set_attr "opx" "1")])

;; Call subroutine returning any type.

(define_expand "untyped_call"
  [(parallel [(call (match_operand 0 "" "")
		    (const_int 0))
	      (match_operand 1 "" "")
	      (match_operand 2 "" "")])]
  "NEEDS_UNTYPED_CALL"
{
  int i;

  emit_call_insn (GEN_CALL (operands[0], const0_rtx, NULL, const0_rtx));

  for (i = 0; i < XVECLEN (operands[2], 0); i++)
    {
      rtx set = XVECEXP (operands[2], 0, i);
      emit_move_insn (SET_DEST (set), SET_SRC (set));
    }

  /* The optimizer does not know that the call sets the function value
     registers we stored in the result block.  We avoid problems by
     claiming that all hard registers are used and clobbered at this
     point.  */
  emit_insn (gen_blockage ());

  DONE;
})

;; UNSPEC_VOLATILE is considered to use and clobber all hard registers and
;; all of memory.  This blocks insns from being moved across this point.

(define_insn "blockage"
  [(unspec_volatile [(const_int 0)] UNSPECV_BLOCKAGE)]
  ""
  "")

(define_insn "nop"
  [(const_int 0)]
  ""
  "nop"
  [(set_attr "type" "nop")])

(define_expand "prologue"
  [(const_int 0)]
  ""
{
  m68k_expand_prologue ();
  DONE;
})

(define_expand "epilogue"
  [(return)]
  ""
{
  m68k_expand_epilogue (false);
  DONE;
})

(define_expand "sibcall_epilogue"
  [(return)]
  ""
{
  m68k_expand_epilogue (true);
  DONE;
})

;; Used for frameless functions which save no regs and allocate no locals.
(define_expand "return"
  [(return)]
  "m68k_use_return_insn ()"
  "")

(define_insn "*return"
  [(return)]
  ""
{
  switch (m68k_get_function_kind (current_function_decl))
    {
    case m68k_fk_interrupt_handler:
      return "rte";

    case m68k_fk_interrupt_thread:
      return "sleep";

    default:
      if (crtl->args.pops_args)
	{
	  operands[0] = GEN_INT (crtl->args.pops_args);
	  return "rtd %0";
	}
      else
	return "rts";
    }
}
  [(set_attr "type" "rts")])

(define_insn "*m68k_store_multiple"
  [(match_parallel 0 "" [(match_operand 1 "")])]
  "m68k_movem_pattern_p (operands[0], NULL, 0, true)"
{
  return m68k_output_movem (operands, operands[0], 0, true);
})

(define_insn "*m68k_store_multiple_automod"
  [(match_parallel 0 ""
     [(set (match_operand:SI 1 "register_operand" "=a")
	   (plus:SI (match_operand:SI 2 "register_operand" "1")
		    (match_operand:SI 3 "const_int_operand")))])]
  "m68k_movem_pattern_p (operands[0], operands[1], INTVAL (operands[3]), true)"
{
  return m68k_output_movem (operands, operands[0], INTVAL (operands[3]), true);
})

(define_insn "*m68k_load_multiple"
  [(match_parallel 0 "" [(match_operand 1 "")])]
  "m68k_movem_pattern_p (operands[0], NULL, 0, false)"
{
  return m68k_output_movem (operands, operands[0], 0, false);
})

(define_insn "*m68k_load_multiple_automod"
  [(match_parallel 0 ""
     [(set (match_operand:SI 1 "register_operand" "=a")
	   (plus:SI (match_operand:SI 2 "register_operand" "1")
		    (match_operand:SI 3 "const_int_operand")))])]
  "m68k_movem_pattern_p (operands[0], operands[1],
			 INTVAL (operands[3]), false)"
{
  return m68k_output_movem (operands, operands[0],
			    INTVAL (operands[3]), false);
})

(define_expand "link"
  [(parallel
       [(set (match_operand:SI 0 "register_operand")
	     (plus:SI (reg:SI SP_REG) (const_int -4)))
	(set (match_dup 2)
	     (match_dup 0))
	(set (reg:SI SP_REG)
	     (plus:SI (reg:SI SP_REG)
		      (match_operand:SI 1 "const_int_operand")))])]
  "TARGET_68020 || INTVAL (operands[1]) >= -0x8004"
{
  operands[2] = gen_frame_mem (SImode,
			       plus_constant (Pmode, stack_pointer_rtx, -4));
})

(define_insn "*link"
  [(set (match_operand:SI 0 "register_operand" "+r")
	(plus:SI (reg:SI SP_REG) (const_int -4)))
   (set (mem:SI (plus:SI (reg:SI SP_REG) (const_int -4)))
	(match_dup 0))
   (set (reg:SI SP_REG)
	(plus:SI (reg:SI SP_REG)
		 (match_operand:SI 1 "const_int_operand")))]
  "TARGET_68020 || INTVAL (operands[1]) >= -0x8004"
{
  operands[1] = GEN_INT (INTVAL (operands[1]) + 4);
  if (!MOTOROLA)
    return "link %0,%1";
  else if (INTVAL (operands[1]) >= -0x8000)
    return "link.w %0,%1";
  else
    return "link.l %0,%1";
}
  [(set_attr "type" "link")])

(define_expand "unlink"
  [(parallel
      [(set (match_operand:SI 0 "register_operand")
	    (match_dup 1))
       (set (reg:SI SP_REG)
	    (plus:SI (match_dup 0)
		     (const_int 4)))])]
  ""
{
  operands[1] = gen_frame_mem (SImode, copy_rtx (operands[0]));
})

(define_insn "*unlink"
  [(set (match_operand:SI 0 "register_operand" "+r")
	(mem:SI (match_dup 0)))
   (set (reg:SI SP_REG)
	(plus:SI (match_dup 0)
		 (const_int 4)))]
  ""
  "unlk %0"
  [(set_attr "type" "unlk")])

(define_insn "load_got"
  [(set (match_operand:SI 0 "register_operand" "=a")
	(unspec:SI [(const_int 0)] UNSPEC_GOT))]
  ""
{
  if (TARGET_ID_SHARED_LIBRARY)
    {
      operands[1] = gen_rtx_REG (Pmode, PIC_REG);
      return MOTOROLA ? "move.l %?(%1),%0" : "movel %1@(%?), %0";
    }
  else if (MOTOROLA)
    {
      if (TARGET_COLDFIRE)
	/* Load the full 32-bit PC-relative offset of
	   _GLOBAL_OFFSET_TABLE_ into the PIC register, then use it to
	   calculate the absolute value.  The offset and "lea"
	   operation word together occupy 6 bytes.  */
	return ("move.l #_GLOBAL_OFFSET_TABLE_@GOTPC, %0\n\t"
		"lea (-6, %%pc, %0), %0");
      else
	return "lea (%%pc, _GLOBAL_OFFSET_TABLE_@GOTPC), %0";
    }
  else
    return ("movel #_GLOBAL_OFFSET_TABLE_, %0\n\t"
	    "lea %%pc@(0,%0:l),%0");
})

(define_insn "indirect_jump"
  [(set (pc) (match_operand:SI 0 "address_operand" "p"))]
  ""
  "jmp %a0"
  [(set_attr "type" "jmp")])

;; This should not be used unless the add/sub insns can't be.

(define_insn "*lea"
  [(set (match_operand:SI 0 "nonimmediate_operand" "=a")
	(match_operand:QI 1 "address_operand" "p"))]
  ""
  "lea %a1,%0")

;; This is the first machine-dependent peephole optimization.
;; It is useful when a floating value is returned from a function call
;; and then is moved into an FP register.
;; But it is mainly intended to test the support for these optimizations.

(define_peephole2
  [(set (reg:SI SP_REG) (plus:SI (reg:SI SP_REG) (const_int 4)))
   (set (match_operand:DF 0 "register_operand" "")
	(match_operand:DF 1 "register_operand" ""))]
  "FP_REG_P (operands[0]) && !FP_REG_P (operands[1])"
  [(set (mem:SI (reg:SI SP_REG)) (match_dup 1))
   (set (mem:SI (pre_dec:SI (reg:SI SP_REG))) (match_dup 2))
   (set (match_dup 0) (mem:DF (post_inc:SI (reg:SI SP_REG))))]
  "split_di(operands + 1, 1, operands + 1, operands + 2);")

;; Optimize a stack-adjust followed by a push of an argument.
;; This is said to happen frequently with -msoft-float
;; when there are consecutive library calls.

(define_peephole2
  [(set (reg:SI SP_REG) (plus:SI (reg:SI SP_REG) (const_int 4)))
   (set (match_operand:SF 0 "push_operand" "")
	(match_operand:SF 1 "general_operand" ""))]
  "!reg_mentioned_p (stack_pointer_rtx, operands[0])"
  [(set (match_dup 0) (match_dup 1))]
  "operands[0] = replace_equiv_address (operands[0], stack_pointer_rtx);")

(define_peephole2
  [(set (reg:SI SP_REG) (plus:SI (reg:SI SP_REG)
				 (match_operand:SI 0 "const_int_operand" "")))
   (set (match_operand:SF 1 "push_operand" "")
	(match_operand:SF 2 "general_operand" ""))]
  "INTVAL (operands[0]) > 4
   && !reg_mentioned_p (stack_pointer_rtx, operands[2])"
  [(set (reg:SI SP_REG) (plus:SI (reg:SI SP_REG) (match_dup 0)))
   (set (match_dup 1) (match_dup 2))]
{
  operands[0] = GEN_INT (INTVAL (operands[0]) - 4);
  operands[1] = replace_equiv_address (operands[1], stack_pointer_rtx);
})

;; Speed up stack adjust followed by a fullword fixedpoint push.
;; Constant operands need special care, as replacing a "pea X.w" with
;; "move.l #X,(%sp)" is often not a win.

;; Already done by the previous csa pass, left as reference.
(define_peephole2
  [(set (reg:SI SP_REG) (plus:SI (reg:SI SP_REG) (const_int 4)))
   (set (match_operand:SI 0 "push_operand" "")
	(match_operand:SI 1 "general_operand" ""))]
  "!reg_mentioned_p (stack_pointer_rtx, operands[1])"
  [(set (match_dup 0) (match_dup 1))]
  "operands[0] = replace_equiv_address (operands[0], stack_pointer_rtx);")

;; Try to use moveq, after stack push has been changed into a simple move.
(define_peephole2
  [(match_scratch:SI 2 "d")
   (set (match_operand:SI 0 "memory_operand" "")
	(match_operand:SI 1 "const_int_operand" ""))]
  "GET_CODE (XEXP (operands[0], 0)) != PRE_DEC
   && INTVAL (operands[1]) != 0
   && IN_RANGE (INTVAL (operands[1]), -0x80, 0x7f)
   && !valid_mov3q_const (INTVAL (operands[1]))"
  [(set (match_dup 2) (match_dup 1))
   (set (match_dup 0) (match_dup 2))])

;; This sequence adds an instruction, but is two bytes shorter.
(define_peephole2
  [(match_scratch:SI 2 "d")
   (set (reg:SI SP_REG) (plus:SI (reg:SI SP_REG) (const_int 12)))
   (set (match_operand:SI 0 "push_operand" "")
	(match_operand:SI 1 "const_int_operand" ""))]
  "INTVAL (operands[1]) != 0
   && IN_RANGE (INTVAL (operands[1]), -0x80, 0x7f)
   && !valid_mov3q_const (INTVAL (operands[1]))"
  [(set (reg:SI SP_REG) (plus:SI (reg:SI SP_REG) (const_int 8)))
   (set (match_dup 2) (match_dup 1))
   (set (match_dup 0) (match_dup 2))]
  "operands[0] = replace_equiv_address (operands[0], stack_pointer_rtx);")

;; Changing pea X.w into a move.l is no real win here.
(define_peephole2
  [(set (reg:SI SP_REG) (plus:SI (reg:SI SP_REG)
				 (match_operand:SI 0 "const_int_operand" "")))
   (set (match_operand:SI 1 "push_operand" "")
	(match_operand:SI 2 "general_operand" ""))]
  "INTVAL (operands[0]) > 4
   && !reg_mentioned_p (stack_pointer_rtx, operands[2])
   && !(CONST_INT_P (operands[2]) && INTVAL (operands[2]) != 0
	&& IN_RANGE (INTVAL (operands[2]), -0x8000, 0x7fff)
	&& !valid_mov3q_const (INTVAL (operands[2])))"
  [(set (reg:SI SP_REG) (plus:SI (reg:SI SP_REG) (match_dup 0)))
   (set (match_dup 1) (match_dup 2))]
{
  operands[0] = GEN_INT (INTVAL (operands[0]) - 4);
  operands[1] = replace_equiv_address (operands[1], stack_pointer_rtx);
})

;; Speed up pushing a single byte/two bytes but leaving four bytes of space
;; (which differs slightly between m680x0 and ColdFire).

(define_peephole2
  [(set (reg:SI SP_REG) (plus:SI (reg:SI SP_REG) (const_int -4)))
   (set (match_operand:QI 0 "memory_operand" "")
	(match_operand:QI 1 "register_operand" ""))]
  "!reg_mentioned_p (stack_pointer_rtx, operands[1])
   && GET_CODE (XEXP (operands[0], 0)) == PLUS
   && rtx_equal_p (XEXP (XEXP (operands[0], 0), 0), stack_pointer_rtx)
   && CONST_INT_P (XEXP (XEXP (operands[0], 0), 1))
   && INTVAL (XEXP (XEXP (operands[0], 0), 1)) == 3"
  [(set (match_dup 0) (match_dup 1))]
{
  rtx addr = gen_rtx_PRE_DEC (Pmode, stack_pointer_rtx);
  operands[0] = adjust_automodify_address (operands[0], SImode, addr, -3);
  operands[1] = simplify_gen_subreg (SImode, operands[1], QImode, 0);
})

(define_peephole2
  [(set (match_operand:QI 0 "push_operand" "")
	(match_operand:QI 1 "register_operand" ""))
   (set (reg:SI SP_REG) (plus:SI (reg:SI SP_REG) (const_int -3)))]
  "!reg_mentioned_p (stack_pointer_rtx, operands[1])"
  [(set (match_dup 0) (match_dup 1))]
{
  operands[0] = adjust_automodify_address (operands[0], SImode,
					   XEXP (operands[0], 0), -3);
  operands[1] = simplify_gen_subreg (SImode, operands[1], QImode, 0);
})

(define_peephole2
  [(set (match_operand:HI 0 "push_operand" "")
	(match_operand:HI 1 "register_operand" ""))
   (set (reg:SI SP_REG) (plus:SI (reg:SI SP_REG) (const_int -2)))]
  "!reg_mentioned_p (stack_pointer_rtx, operands[1])"
  [(set (match_dup 0) (match_dup 1))]
{
  operands[0] = adjust_automodify_address (operands[0], SImode,
					   XEXP (operands[0], 0), -2);
  operands[1] = simplify_gen_subreg (SImode, operands[1], HImode, 0);
})

;; Optimize a series of strict_low_part assignments

(define_peephole2
  [(set (match_operand:SI 0 "register_operand" "")
	(const_int 0))
   (set (strict_low_part (match_operand:HI 1 "register_operand" ""))
	(match_operand:HI 2 "general_operand" ""))]
  "REGNO (operands[0]) == REGNO (operands[1])
   && strict_low_part_peephole_ok (HImode, insn, operands[0])"
  [(set (strict_low_part (match_dup 1)) (match_dup 2))]
  "")

(define_peephole2
  [(set (match_operand:SI 0 "register_operand" "")
	(const_int 0))
   (set (strict_low_part (match_operand:QI 1 "register_operand" ""))
	(match_operand:QI 2 "general_operand" ""))]
  "REGNO (operands[0]) == REGNO (operands[1])
   && strict_low_part_peephole_ok (QImode, insn, operands[0])"
  [(set (strict_low_part (match_dup 1)) (match_dup 2))]
  "")

;; dbCC peepholes
;;
;; Turns
;;   loop:
;;           [ ... ]
;;           jCC label		; abnormal loop termination
;;           dbra dN, loop	; normal loop termination
;;
;; Into
;;   loop:
;;           [ ... ]
;;           dbCC dN, loop
;;           jCC label
;;
;; Which moves the jCC condition outside the inner loop for free.
;;

(define_peephole
  [(set (pc) (if_then_else (match_operator 3 "valid_dbcc_comparison_p"
                             [(cc0) (const_int 0)])
                           (label_ref (match_operand 2 "" ""))
                           (pc)))
   (parallel
    [(set (pc)
	  (if_then_else
	    (ne (match_operand:HI 0 "register_operand" "")
	        (const_int 0))
	    (label_ref (match_operand 1 "" ""))
	    (pc)))
     (set (match_dup 0)
	  (plus:HI (match_dup 0)
		   (const_int -1)))])]
  "!TARGET_COLDFIRE && DATA_REG_P (operands[0]) && ! flags_in_68881 ()"
{
  CC_STATUS_INIT;
  output_dbcc_and_branch (operands);
  return "";
})

(define_peephole
  [(set (pc) (if_then_else (match_operator 3 "valid_dbcc_comparison_p"
                             [(cc0) (const_int 0)])
                           (label_ref (match_operand 2 "" ""))
                           (pc)))
   (parallel
    [(set (pc)
	  (if_then_else
	    (ne (match_operand:SI 0 "register_operand" "")
	        (const_int 0))
	    (label_ref (match_operand 1 "" ""))
	    (pc)))
     (set (match_dup 0)
	  (plus:SI (match_dup 0)
		   (const_int -1)))])]
  "!TARGET_COLDFIRE && DATA_REG_P (operands[0]) && ! flags_in_68881 ()"
{
  CC_STATUS_INIT;
  output_dbcc_and_branch (operands);
  return "";
})

(define_peephole
  [(set (pc) (if_then_else (match_operator 3 "valid_dbcc_comparison_p"
                             [(cc0) (const_int 0)])
                           (label_ref (match_operand 2 "" ""))
                           (pc)))
   (parallel
    [(set (pc)
	  (if_then_else
	    (ge (plus:HI (match_operand:HI 0 "register_operand" "")
		         (const_int -1))
	        (const_int 0))
	    (label_ref (match_operand 1 "" ""))
	    (pc)))
     (set (match_dup 0)
	  (plus:HI (match_dup 0)
		   (const_int -1)))])]
  "!TARGET_COLDFIRE && DATA_REG_P (operands[0]) && ! flags_in_68881 ()"
{
  CC_STATUS_INIT;
  output_dbcc_and_branch (operands);
  return "";
})

(define_peephole
  [(set (pc) (if_then_else (match_operator 3 "valid_dbcc_comparison_p"
                             [(cc0) (const_int 0)])
                           (label_ref (match_operand 2 "" ""))
                           (pc)))
   (parallel
    [(set (pc)
	  (if_then_else
	    (ge (plus:SI (match_operand:SI 0 "register_operand" "")
		         (const_int -1))
	        (const_int 0))
	    (label_ref (match_operand 1 "" ""))
	    (pc)))
     (set (match_dup 0)
	  (plus:SI (match_dup 0)
		   (const_int -1)))])]
  "!TARGET_COLDFIRE && DATA_REG_P (operands[0]) && ! flags_in_68881 ()"
{
  CC_STATUS_INIT;
  output_dbcc_and_branch (operands);
  return "";
})


(define_insn "extendsfxf2"
  [(set (match_operand:XF 0 "nonimmediate_operand" "=fm,f")
	(float_extend:XF (match_operand:SF 1 "general_operand" "f,rmF")))]
  "TARGET_68881"
{
  if (FP_REG_P (operands[0]) && FP_REG_P (operands[1]))
    {
      if (REGNO (operands[0]) == REGNO (operands[1]))
	{
	  /* Extending float to double in an fp-reg is a no-op.
	     NOTICE_UPDATE_CC has already assumed that the
	     cc will be set.  So cancel what it did.  */
	  cc_status = cc_prev_status;
	  return "";
	}
      return "f%$move%.x %1,%0";
    }
  if (FP_REG_P (operands[0]))
    {
      if (FP_REG_P (operands[1]))
	return "f%$move%.x %1,%0";
      else if (ADDRESS_REG_P (operands[1]))
	return "move%.l %1,%-\;f%$move%.s %+,%0";
      else if (GET_CODE (operands[1]) == CONST_DOUBLE)
	return output_move_const_single (operands);
      return "f%$move%.s %f1,%0";
    }
  return "fmove%.x %f1,%0";
})


(define_insn "extenddfxf2"
  [(set (match_operand:XF 0 "nonimmediate_operand" "=fm,f")
	(float_extend:XF
          (match_operand:DF 1 "general_operand" "f,rmE")))]
  "TARGET_68881"
{
  if (FP_REG_P (operands[0]) && FP_REG_P (operands[1]))
    {
      if (REGNO (operands[0]) == REGNO (operands[1]))
	{
	  /* Extending float to double in an fp-reg is a no-op.
	     NOTICE_UPDATE_CC has already assumed that the
	     cc will be set.  So cancel what it did.  */
	  cc_status = cc_prev_status;
	  return "";
	}
      return "fmove%.x %1,%0";
    }
  if (FP_REG_P (operands[0]))
    {
      if (REG_P (operands[1]))
	{
	  rtx xoperands[2];
	  xoperands[1] = gen_rtx_REG (SImode, REGNO (operands[1]) + 1);
	  output_asm_insn ("move%.l %1,%-", xoperands);
	  output_asm_insn ("move%.l %1,%-", operands);
	  return "f%&move%.d %+,%0";
	}
      if (GET_CODE (operands[1]) == CONST_DOUBLE)
	return output_move_const_double (operands);
      return "f%&move%.d %f1,%0";
    }
  return "fmove%.x %f1,%0";
})

(define_insn "truncxfdf2"
  [(set (match_operand:DF 0 "nonimmediate_operand" "=m,!r")
	(float_truncate:DF
          (match_operand:XF 1 "general_operand" "f,f")))]
  "TARGET_68881"
{
  if (REG_P (operands[0]))
    {
      output_asm_insn ("fmove%.d %f1,%-\;move%.l %+,%0", operands);
      operands[0] = gen_rtx_REG (SImode, REGNO (operands[0]) + 1);
      return "move%.l %+,%0";
    }
  return "fmove%.d %f1,%0";
})

(define_insn "truncxfsf2"
  [(set (match_operand:SF 0 "nonimmediate_operand" "=dm")
	(float_truncate:SF
	  (match_operand:XF 1 "general_operand" "f")))]
  "TARGET_68881"
  "fmove%.s %f1,%0")

(define_insn "sin<mode>2"
  [(set (match_operand:FP 0 "nonimmediate_operand" "=f")
	(unspec:FP
	  [(match_operand:FP 1 "general_operand" "f<FP:dreg>m")] UNSPEC_SIN))]
  "TARGET_68881 && flag_unsafe_math_optimizations"
{
  if (FP_REG_P (operands[1]))
    return "fsin%.x %1,%0";
  else
    return "fsin%.<FP:prec> %1,%0";
})

(define_insn "cos<mode>2"
  [(set (match_operand:FP 0 "nonimmediate_operand" "=f")
	(unspec:FP
	  [(match_operand:FP 1 "general_operand" "f<FP:dreg>m")] UNSPEC_COS))]
  "TARGET_68881 && flag_unsafe_math_optimizations"
{
  if (FP_REG_P (operands[1]))
    return "fcos%.x %1,%0";
  else
    return "fcos%.<FP:prec> %1,%0";
})

;; Unconditional traps are assumed to have (const_int 1) for the condition.
(define_insn "trap"
  [(trap_if (const_int 1) (const_int 7))]
  ""
  "trap #7"
  [(set_attr "type" "trap")])

(define_expand "ctrapdi4"
  [(trap_if (match_operator 0 "ordered_comparison_operator"
			    [(cc0) (const_int 0)])
	    (match_operand:SI 3 "const1_operand" ""))]
  "TARGET_68020"
{
  if (operands[2] == const0_rtx)
    emit_insn (gen_tstdi (operands[1]));
  else
    emit_insn (gen_cmpdi (operands[1], operands[2]));
  operands[1] = cc0_rtx;
  operands[2] = const0_rtx;
})

(define_expand "ctrapsi4"
  [(set (cc0)
	(compare (match_operand:SI 1 "nonimmediate_operand" "")
		 (match_operand:SI 2 "general_operand" "")))
   (trap_if (match_operator 0 "ordered_comparison_operator"
			    [(cc0) (const_int 0)])
	    (match_operand:SI 3 "const1_operand" ""))]
  "TARGET_68020"
  "")

(define_expand "ctraphi4"
  [(set (cc0)
	(compare (match_operand:HI 1 "nonimmediate_src_operand" "")
		 (match_operand:HI 2 "general_src_operand" "")))
   (trap_if (match_operator 0 "ordered_comparison_operator"
			    [(cc0) (const_int 0)])
	    (match_operand:SI 3 "const1_operand" ""))]
  "TARGET_68020"
  "")

(define_expand "ctrapqi4"
  [(set (cc0)
	(compare (match_operand:QI 1 "nonimmediate_src_operand" "")
		 (match_operand:QI 2 "general_src_operand" "")))
   (trap_if (match_operator 0 "ordered_comparison_operator"
			    [(cc0) (const_int 0)])
	    (match_operand:SI 3 "const1_operand" ""))]
  "TARGET_68020"
  "")

(define_insn "*conditional_trap"
  [(trap_if (match_operator 0 "ordered_comparison_operator"
			    [(cc0) (const_int 0)])
	    (match_operand:SI 1 "const1_operand" "I"))]
  "TARGET_68020 && ! flags_in_68881 ()"
{
  switch (GET_CODE (operands[0]))
  {
  case EQ:  return "trapeq";
  case NE:  return "trapne";
  case GT:  return "trapgt";
  case GTU: return "traphi";
  case LT:  return "traplt";
  case LTU: return "trapcs";
  case GE:  return "trapge";
  case GEU: return "trapcc";
  case LE:  return "traple";
  case LEU: return "trapls";
  default: gcc_unreachable ();
  }
})

;; These are to prevent the scheduler from moving stores to the frame
;; before the stack adjustment.
(define_insn "stack_tie"
  [(set (mem:BLK (scratch))
	(unspec:BLK [(match_operand:SI 0 "register_operand" "r")
		     (match_operand:SI 1 "register_operand" "r")]
		    UNSPEC_TIE))]
  ""
  ""
  [(set_attr "type" "ignore")])

;; Instruction that subscribes one word in ColdFire instruction buffer.
;; This instruction is used within scheduler only and should not appear
;; in the instruction stream.
(define_insn "ib"
  [(unspec [(const_int 0)] UNSPEC_IB)]
  ""
  "#"
  [(set_attr "type" "ib")])

(include "cf.md")
(include "sync.md")
