@c Copyright (C) 2006-2014 Free Software Foundation, Inc.
@c This is part of the GCC manual.
@c For copying conditions, see the file gcc.texi.

@subsubsection Addition

@itemize @bullet
@item uint32x2_t vadd_u32 (uint32x2_t, uint32x2_t)
@*@emph{Form of expected instruction(s):} @code{vadd.i32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint16x4_t vadd_u16 (uint16x4_t, uint16x4_t)
@*@emph{Form of expected instruction(s):} @code{vadd.i16 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint8x8_t vadd_u8 (uint8x8_t, uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vadd.i8 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int32x2_t vadd_s32 (int32x2_t, int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vadd.i32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int16x4_t vadd_s16 (int16x4_t, int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vadd.i16 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int8x8_t vadd_s8 (int8x8_t, int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vadd.i8 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item float32x2_t vadd_f32 (float32x2_t, float32x2_t)
@*@emph{Form of expected instruction(s):} @code{vadd.f32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint64x1_t vadd_u64 (uint64x1_t, uint64x1_t)
@end itemize


@itemize @bullet
@item int64x1_t vadd_s64 (int64x1_t, int64x1_t)
@end itemize


@itemize @bullet
@item uint32x4_t vaddq_u32 (uint32x4_t, uint32x4_t)
@*@emph{Form of expected instruction(s):} @code{vadd.i32 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint16x8_t vaddq_u16 (uint16x8_t, uint16x8_t)
@*@emph{Form of expected instruction(s):} @code{vadd.i16 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint8x16_t vaddq_u8 (uint8x16_t, uint8x16_t)
@*@emph{Form of expected instruction(s):} @code{vadd.i8 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int32x4_t vaddq_s32 (int32x4_t, int32x4_t)
@*@emph{Form of expected instruction(s):} @code{vadd.i32 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int16x8_t vaddq_s16 (int16x8_t, int16x8_t)
@*@emph{Form of expected instruction(s):} @code{vadd.i16 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int8x16_t vaddq_s8 (int8x16_t, int8x16_t)
@*@emph{Form of expected instruction(s):} @code{vadd.i8 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint64x2_t vaddq_u64 (uint64x2_t, uint64x2_t)
@*@emph{Form of expected instruction(s):} @code{vadd.i64 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int64x2_t vaddq_s64 (int64x2_t, int64x2_t)
@*@emph{Form of expected instruction(s):} @code{vadd.i64 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item float32x4_t vaddq_f32 (float32x4_t, float32x4_t)
@*@emph{Form of expected instruction(s):} @code{vadd.f32 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint64x2_t vaddl_u32 (uint32x2_t, uint32x2_t)
@*@emph{Form of expected instruction(s):} @code{vaddl.u32 @var{q0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint32x4_t vaddl_u16 (uint16x4_t, uint16x4_t)
@*@emph{Form of expected instruction(s):} @code{vaddl.u16 @var{q0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint16x8_t vaddl_u8 (uint8x8_t, uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vaddl.u8 @var{q0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int64x2_t vaddl_s32 (int32x2_t, int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vaddl.s32 @var{q0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int32x4_t vaddl_s16 (int16x4_t, int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vaddl.s16 @var{q0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int16x8_t vaddl_s8 (int8x8_t, int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vaddl.s8 @var{q0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint64x2_t vaddw_u32 (uint64x2_t, uint32x2_t)
@*@emph{Form of expected instruction(s):} @code{vaddw.u32 @var{q0}, @var{q0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint32x4_t vaddw_u16 (uint32x4_t, uint16x4_t)
@*@emph{Form of expected instruction(s):} @code{vaddw.u16 @var{q0}, @var{q0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint16x8_t vaddw_u8 (uint16x8_t, uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vaddw.u8 @var{q0}, @var{q0}, @var{d0}}
@end itemize


@itemize @bullet
@item int64x2_t vaddw_s32 (int64x2_t, int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vaddw.s32 @var{q0}, @var{q0}, @var{d0}}
@end itemize


@itemize @bullet
@item int32x4_t vaddw_s16 (int32x4_t, int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vaddw.s16 @var{q0}, @var{q0}, @var{d0}}
@end itemize


@itemize @bullet
@item int16x8_t vaddw_s8 (int16x8_t, int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vaddw.s8 @var{q0}, @var{q0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint32x2_t vhadd_u32 (uint32x2_t, uint32x2_t)
@*@emph{Form of expected instruction(s):} @code{vhadd.u32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint16x4_t vhadd_u16 (uint16x4_t, uint16x4_t)
@*@emph{Form of expected instruction(s):} @code{vhadd.u16 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint8x8_t vhadd_u8 (uint8x8_t, uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vhadd.u8 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int32x2_t vhadd_s32 (int32x2_t, int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vhadd.s32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int16x4_t vhadd_s16 (int16x4_t, int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vhadd.s16 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int8x8_t vhadd_s8 (int8x8_t, int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vhadd.s8 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint32x4_t vhaddq_u32 (uint32x4_t, uint32x4_t)
@*@emph{Form of expected instruction(s):} @code{vhadd.u32 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint16x8_t vhaddq_u16 (uint16x8_t, uint16x8_t)
@*@emph{Form of expected instruction(s):} @code{vhadd.u16 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint8x16_t vhaddq_u8 (uint8x16_t, uint8x16_t)
@*@emph{Form of expected instruction(s):} @code{vhadd.u8 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int32x4_t vhaddq_s32 (int32x4_t, int32x4_t)
@*@emph{Form of expected instruction(s):} @code{vhadd.s32 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int16x8_t vhaddq_s16 (int16x8_t, int16x8_t)
@*@emph{Form of expected instruction(s):} @code{vhadd.s16 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int8x16_t vhaddq_s8 (int8x16_t, int8x16_t)
@*@emph{Form of expected instruction(s):} @code{vhadd.s8 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint32x2_t vrhadd_u32 (uint32x2_t, uint32x2_t)
@*@emph{Form of expected instruction(s):} @code{vrhadd.u32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint16x4_t vrhadd_u16 (uint16x4_t, uint16x4_t)
@*@emph{Form of expected instruction(s):} @code{vrhadd.u16 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint8x8_t vrhadd_u8 (uint8x8_t, uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vrhadd.u8 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int32x2_t vrhadd_s32 (int32x2_t, int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vrhadd.s32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int16x4_t vrhadd_s16 (int16x4_t, int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vrhadd.s16 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int8x8_t vrhadd_s8 (int8x8_t, int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vrhadd.s8 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint32x4_t vrhaddq_u32 (uint32x4_t, uint32x4_t)
@*@emph{Form of expected instruction(s):} @code{vrhadd.u32 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint16x8_t vrhaddq_u16 (uint16x8_t, uint16x8_t)
@*@emph{Form of expected instruction(s):} @code{vrhadd.u16 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint8x16_t vrhaddq_u8 (uint8x16_t, uint8x16_t)
@*@emph{Form of expected instruction(s):} @code{vrhadd.u8 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int32x4_t vrhaddq_s32 (int32x4_t, int32x4_t)
@*@emph{Form of expected instruction(s):} @code{vrhadd.s32 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int16x8_t vrhaddq_s16 (int16x8_t, int16x8_t)
@*@emph{Form of expected instruction(s):} @code{vrhadd.s16 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int8x16_t vrhaddq_s8 (int8x16_t, int8x16_t)
@*@emph{Form of expected instruction(s):} @code{vrhadd.s8 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint32x2_t vqadd_u32 (uint32x2_t, uint32x2_t)
@*@emph{Form of expected instruction(s):} @code{vqadd.u32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint16x4_t vqadd_u16 (uint16x4_t, uint16x4_t)
@*@emph{Form of expected instruction(s):} @code{vqadd.u16 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint8x8_t vqadd_u8 (uint8x8_t, uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vqadd.u8 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int32x2_t vqadd_s32 (int32x2_t, int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vqadd.s32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int16x4_t vqadd_s16 (int16x4_t, int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vqadd.s16 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int8x8_t vqadd_s8 (int8x8_t, int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vqadd.s8 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint64x1_t vqadd_u64 (uint64x1_t, uint64x1_t)
@*@emph{Form of expected instruction(s):} @code{vqadd.u64 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int64x1_t vqadd_s64 (int64x1_t, int64x1_t)
@*@emph{Form of expected instruction(s):} @code{vqadd.s64 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint32x4_t vqaddq_u32 (uint32x4_t, uint32x4_t)
@*@emph{Form of expected instruction(s):} @code{vqadd.u32 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint16x8_t vqaddq_u16 (uint16x8_t, uint16x8_t)
@*@emph{Form of expected instruction(s):} @code{vqadd.u16 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint8x16_t vqaddq_u8 (uint8x16_t, uint8x16_t)
@*@emph{Form of expected instruction(s):} @code{vqadd.u8 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int32x4_t vqaddq_s32 (int32x4_t, int32x4_t)
@*@emph{Form of expected instruction(s):} @code{vqadd.s32 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int16x8_t vqaddq_s16 (int16x8_t, int16x8_t)
@*@emph{Form of expected instruction(s):} @code{vqadd.s16 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int8x16_t vqaddq_s8 (int8x16_t, int8x16_t)
@*@emph{Form of expected instruction(s):} @code{vqadd.s8 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint64x2_t vqaddq_u64 (uint64x2_t, uint64x2_t)
@*@emph{Form of expected instruction(s):} @code{vqadd.u64 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int64x2_t vqaddq_s64 (int64x2_t, int64x2_t)
@*@emph{Form of expected instruction(s):} @code{vqadd.s64 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint32x2_t vaddhn_u64 (uint64x2_t, uint64x2_t)
@*@emph{Form of expected instruction(s):} @code{vaddhn.i64 @var{d0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint16x4_t vaddhn_u32 (uint32x4_t, uint32x4_t)
@*@emph{Form of expected instruction(s):} @code{vaddhn.i32 @var{d0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint8x8_t vaddhn_u16 (uint16x8_t, uint16x8_t)
@*@emph{Form of expected instruction(s):} @code{vaddhn.i16 @var{d0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int32x2_t vaddhn_s64 (int64x2_t, int64x2_t)
@*@emph{Form of expected instruction(s):} @code{vaddhn.i64 @var{d0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int16x4_t vaddhn_s32 (int32x4_t, int32x4_t)
@*@emph{Form of expected instruction(s):} @code{vaddhn.i32 @var{d0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int8x8_t vaddhn_s16 (int16x8_t, int16x8_t)
@*@emph{Form of expected instruction(s):} @code{vaddhn.i16 @var{d0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint32x2_t vraddhn_u64 (uint64x2_t, uint64x2_t)
@*@emph{Form of expected instruction(s):} @code{vraddhn.i64 @var{d0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint16x4_t vraddhn_u32 (uint32x4_t, uint32x4_t)
@*@emph{Form of expected instruction(s):} @code{vraddhn.i32 @var{d0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint8x8_t vraddhn_u16 (uint16x8_t, uint16x8_t)
@*@emph{Form of expected instruction(s):} @code{vraddhn.i16 @var{d0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int32x2_t vraddhn_s64 (int64x2_t, int64x2_t)
@*@emph{Form of expected instruction(s):} @code{vraddhn.i64 @var{d0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int16x4_t vraddhn_s32 (int32x4_t, int32x4_t)
@*@emph{Form of expected instruction(s):} @code{vraddhn.i32 @var{d0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int8x8_t vraddhn_s16 (int16x8_t, int16x8_t)
@*@emph{Form of expected instruction(s):} @code{vraddhn.i16 @var{d0}, @var{q0}, @var{q0}}
@end itemize




@subsubsection Multiplication

@itemize @bullet
@item uint32x2_t vmul_u32 (uint32x2_t, uint32x2_t)
@*@emph{Form of expected instruction(s):} @code{vmul.i32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint16x4_t vmul_u16 (uint16x4_t, uint16x4_t)
@*@emph{Form of expected instruction(s):} @code{vmul.i16 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint8x8_t vmul_u8 (uint8x8_t, uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vmul.i8 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int32x2_t vmul_s32 (int32x2_t, int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vmul.i32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int16x4_t vmul_s16 (int16x4_t, int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vmul.i16 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int8x8_t vmul_s8 (int8x8_t, int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vmul.i8 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item float32x2_t vmul_f32 (float32x2_t, float32x2_t)
@*@emph{Form of expected instruction(s):} @code{vmul.f32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item poly8x8_t vmul_p8 (poly8x8_t, poly8x8_t)
@*@emph{Form of expected instruction(s):} @code{vmul.p8 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint32x4_t vmulq_u32 (uint32x4_t, uint32x4_t)
@*@emph{Form of expected instruction(s):} @code{vmul.i32 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint16x8_t vmulq_u16 (uint16x8_t, uint16x8_t)
@*@emph{Form of expected instruction(s):} @code{vmul.i16 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint8x16_t vmulq_u8 (uint8x16_t, uint8x16_t)
@*@emph{Form of expected instruction(s):} @code{vmul.i8 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int32x4_t vmulq_s32 (int32x4_t, int32x4_t)
@*@emph{Form of expected instruction(s):} @code{vmul.i32 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int16x8_t vmulq_s16 (int16x8_t, int16x8_t)
@*@emph{Form of expected instruction(s):} @code{vmul.i16 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int8x16_t vmulq_s8 (int8x16_t, int8x16_t)
@*@emph{Form of expected instruction(s):} @code{vmul.i8 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item float32x4_t vmulq_f32 (float32x4_t, float32x4_t)
@*@emph{Form of expected instruction(s):} @code{vmul.f32 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item poly8x16_t vmulq_p8 (poly8x16_t, poly8x16_t)
@*@emph{Form of expected instruction(s):} @code{vmul.p8 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int32x2_t vqdmulh_s32 (int32x2_t, int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vqdmulh.s32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int16x4_t vqdmulh_s16 (int16x4_t, int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vqdmulh.s16 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int32x4_t vqdmulhq_s32 (int32x4_t, int32x4_t)
@*@emph{Form of expected instruction(s):} @code{vqdmulh.s32 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int16x8_t vqdmulhq_s16 (int16x8_t, int16x8_t)
@*@emph{Form of expected instruction(s):} @code{vqdmulh.s16 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int32x2_t vqrdmulh_s32 (int32x2_t, int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vqrdmulh.s32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int16x4_t vqrdmulh_s16 (int16x4_t, int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vqrdmulh.s16 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int32x4_t vqrdmulhq_s32 (int32x4_t, int32x4_t)
@*@emph{Form of expected instruction(s):} @code{vqrdmulh.s32 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int16x8_t vqrdmulhq_s16 (int16x8_t, int16x8_t)
@*@emph{Form of expected instruction(s):} @code{vqrdmulh.s16 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint64x2_t vmull_u32 (uint32x2_t, uint32x2_t)
@*@emph{Form of expected instruction(s):} @code{vmull.u32 @var{q0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint32x4_t vmull_u16 (uint16x4_t, uint16x4_t)
@*@emph{Form of expected instruction(s):} @code{vmull.u16 @var{q0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint16x8_t vmull_u8 (uint8x8_t, uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vmull.u8 @var{q0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int64x2_t vmull_s32 (int32x2_t, int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vmull.s32 @var{q0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int32x4_t vmull_s16 (int16x4_t, int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vmull.s16 @var{q0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int16x8_t vmull_s8 (int8x8_t, int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vmull.s8 @var{q0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item poly16x8_t vmull_p8 (poly8x8_t, poly8x8_t)
@*@emph{Form of expected instruction(s):} @code{vmull.p8 @var{q0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int64x2_t vqdmull_s32 (int32x2_t, int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vqdmull.s32 @var{q0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int32x4_t vqdmull_s16 (int16x4_t, int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vqdmull.s16 @var{q0}, @var{d0}, @var{d0}}
@end itemize




@subsubsection Multiply-accumulate

@itemize @bullet
@item uint32x2_t vmla_u32 (uint32x2_t, uint32x2_t, uint32x2_t)
@*@emph{Form of expected instruction(s):} @code{vmla.i32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint16x4_t vmla_u16 (uint16x4_t, uint16x4_t, uint16x4_t)
@*@emph{Form of expected instruction(s):} @code{vmla.i16 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint8x8_t vmla_u8 (uint8x8_t, uint8x8_t, uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vmla.i8 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int32x2_t vmla_s32 (int32x2_t, int32x2_t, int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vmla.i32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int16x4_t vmla_s16 (int16x4_t, int16x4_t, int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vmla.i16 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int8x8_t vmla_s8 (int8x8_t, int8x8_t, int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vmla.i8 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item float32x2_t vmla_f32 (float32x2_t, float32x2_t, float32x2_t)
@*@emph{Form of expected instruction(s):} @code{vmla.f32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint32x4_t vmlaq_u32 (uint32x4_t, uint32x4_t, uint32x4_t)
@*@emph{Form of expected instruction(s):} @code{vmla.i32 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint16x8_t vmlaq_u16 (uint16x8_t, uint16x8_t, uint16x8_t)
@*@emph{Form of expected instruction(s):} @code{vmla.i16 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint8x16_t vmlaq_u8 (uint8x16_t, uint8x16_t, uint8x16_t)
@*@emph{Form of expected instruction(s):} @code{vmla.i8 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int32x4_t vmlaq_s32 (int32x4_t, int32x4_t, int32x4_t)
@*@emph{Form of expected instruction(s):} @code{vmla.i32 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int16x8_t vmlaq_s16 (int16x8_t, int16x8_t, int16x8_t)
@*@emph{Form of expected instruction(s):} @code{vmla.i16 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int8x16_t vmlaq_s8 (int8x16_t, int8x16_t, int8x16_t)
@*@emph{Form of expected instruction(s):} @code{vmla.i8 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item float32x4_t vmlaq_f32 (float32x4_t, float32x4_t, float32x4_t)
@*@emph{Form of expected instruction(s):} @code{vmla.f32 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint64x2_t vmlal_u32 (uint64x2_t, uint32x2_t, uint32x2_t)
@*@emph{Form of expected instruction(s):} @code{vmlal.u32 @var{q0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint32x4_t vmlal_u16 (uint32x4_t, uint16x4_t, uint16x4_t)
@*@emph{Form of expected instruction(s):} @code{vmlal.u16 @var{q0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint16x8_t vmlal_u8 (uint16x8_t, uint8x8_t, uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vmlal.u8 @var{q0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int64x2_t vmlal_s32 (int64x2_t, int32x2_t, int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vmlal.s32 @var{q0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int32x4_t vmlal_s16 (int32x4_t, int16x4_t, int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vmlal.s16 @var{q0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int16x8_t vmlal_s8 (int16x8_t, int8x8_t, int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vmlal.s8 @var{q0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int64x2_t vqdmlal_s32 (int64x2_t, int32x2_t, int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vqdmlal.s32 @var{q0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int32x4_t vqdmlal_s16 (int32x4_t, int16x4_t, int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vqdmlal.s16 @var{q0}, @var{d0}, @var{d0}}
@end itemize




@subsubsection Multiply-subtract

@itemize @bullet
@item uint32x2_t vmls_u32 (uint32x2_t, uint32x2_t, uint32x2_t)
@*@emph{Form of expected instruction(s):} @code{vmls.i32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint16x4_t vmls_u16 (uint16x4_t, uint16x4_t, uint16x4_t)
@*@emph{Form of expected instruction(s):} @code{vmls.i16 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint8x8_t vmls_u8 (uint8x8_t, uint8x8_t, uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vmls.i8 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int32x2_t vmls_s32 (int32x2_t, int32x2_t, int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vmls.i32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int16x4_t vmls_s16 (int16x4_t, int16x4_t, int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vmls.i16 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int8x8_t vmls_s8 (int8x8_t, int8x8_t, int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vmls.i8 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item float32x2_t vmls_f32 (float32x2_t, float32x2_t, float32x2_t)
@*@emph{Form of expected instruction(s):} @code{vmls.f32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint32x4_t vmlsq_u32 (uint32x4_t, uint32x4_t, uint32x4_t)
@*@emph{Form of expected instruction(s):} @code{vmls.i32 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint16x8_t vmlsq_u16 (uint16x8_t, uint16x8_t, uint16x8_t)
@*@emph{Form of expected instruction(s):} @code{vmls.i16 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint8x16_t vmlsq_u8 (uint8x16_t, uint8x16_t, uint8x16_t)
@*@emph{Form of expected instruction(s):} @code{vmls.i8 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int32x4_t vmlsq_s32 (int32x4_t, int32x4_t, int32x4_t)
@*@emph{Form of expected instruction(s):} @code{vmls.i32 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int16x8_t vmlsq_s16 (int16x8_t, int16x8_t, int16x8_t)
@*@emph{Form of expected instruction(s):} @code{vmls.i16 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int8x16_t vmlsq_s8 (int8x16_t, int8x16_t, int8x16_t)
@*@emph{Form of expected instruction(s):} @code{vmls.i8 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item float32x4_t vmlsq_f32 (float32x4_t, float32x4_t, float32x4_t)
@*@emph{Form of expected instruction(s):} @code{vmls.f32 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint64x2_t vmlsl_u32 (uint64x2_t, uint32x2_t, uint32x2_t)
@*@emph{Form of expected instruction(s):} @code{vmlsl.u32 @var{q0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint32x4_t vmlsl_u16 (uint32x4_t, uint16x4_t, uint16x4_t)
@*@emph{Form of expected instruction(s):} @code{vmlsl.u16 @var{q0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint16x8_t vmlsl_u8 (uint16x8_t, uint8x8_t, uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vmlsl.u8 @var{q0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int64x2_t vmlsl_s32 (int64x2_t, int32x2_t, int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vmlsl.s32 @var{q0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int32x4_t vmlsl_s16 (int32x4_t, int16x4_t, int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vmlsl.s16 @var{q0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int16x8_t vmlsl_s8 (int16x8_t, int8x8_t, int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vmlsl.s8 @var{q0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int64x2_t vqdmlsl_s32 (int64x2_t, int32x2_t, int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vqdmlsl.s32 @var{q0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int32x4_t vqdmlsl_s16 (int32x4_t, int16x4_t, int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vqdmlsl.s16 @var{q0}, @var{d0}, @var{d0}}
@end itemize




@subsubsection Fused-multiply-accumulate

@itemize @bullet
@item float32x2_t vfma_f32 (float32x2_t, float32x2_t, float32x2_t)
@*@emph{Form of expected instruction(s):} @code{vfma.f32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item float32x4_t vfmaq_f32 (float32x4_t, float32x4_t, float32x4_t)
@*@emph{Form of expected instruction(s):} @code{vfma.f32 @var{q0}, @var{q0}, @var{q0}}
@end itemize




@subsubsection Fused-multiply-subtract

@itemize @bullet
@item float32x2_t vfms_f32 (float32x2_t, float32x2_t, float32x2_t)
@*@emph{Form of expected instruction(s):} @code{vfms.f32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item float32x4_t vfmsq_f32 (float32x4_t, float32x4_t, float32x4_t)
@*@emph{Form of expected instruction(s):} @code{vfms.f32 @var{q0}, @var{q0}, @var{q0}}
@end itemize




@subsubsection Round to integral (to nearest, ties to even)

@itemize @bullet
@item float32x2_t vrndn_f32 (float32x2_t)
@*@emph{Form of expected instruction(s):} @code{vrintn.f32 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item float32x4_t vrndqn_f32 (float32x4_t)
@*@emph{Form of expected instruction(s):} @code{vrintn.f32 @var{q0}, @var{q0}}
@end itemize




@subsubsection Round to integral (to nearest, ties away from zero)

@itemize @bullet
@item float32x2_t vrnda_f32 (float32x2_t)
@*@emph{Form of expected instruction(s):} @code{vrinta.f32 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item float32x4_t vrndqa_f32 (float32x4_t)
@*@emph{Form of expected instruction(s):} @code{vrinta.f32 @var{q0}, @var{q0}}
@end itemize




@subsubsection Round to integral (towards +Inf)

@itemize @bullet
@item float32x2_t vrndp_f32 (float32x2_t)
@*@emph{Form of expected instruction(s):} @code{vrintp.f32 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item float32x4_t vrndqp_f32 (float32x4_t)
@*@emph{Form of expected instruction(s):} @code{vrintp.f32 @var{q0}, @var{q0}}
@end itemize




@subsubsection Round to integral (towards -Inf)

@itemize @bullet
@item float32x2_t vrndm_f32 (float32x2_t)
@*@emph{Form of expected instruction(s):} @code{vrintm.f32 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item float32x4_t vrndqm_f32 (float32x4_t)
@*@emph{Form of expected instruction(s):} @code{vrintm.f32 @var{q0}, @var{q0}}
@end itemize




@subsubsection Round to integral (towards 0)

@itemize @bullet
@item float32x2_t vrnd_f32 (float32x2_t)
@*@emph{Form of expected instruction(s):} @code{vrintz.f32 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item float32x4_t vrndq_f32 (float32x4_t)
@*@emph{Form of expected instruction(s):} @code{vrintz.f32 @var{q0}, @var{q0}}
@end itemize




@subsubsection Subtraction

@itemize @bullet
@item uint32x2_t vsub_u32 (uint32x2_t, uint32x2_t)
@*@emph{Form of expected instruction(s):} @code{vsub.i32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint16x4_t vsub_u16 (uint16x4_t, uint16x4_t)
@*@emph{Form of expected instruction(s):} @code{vsub.i16 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint8x8_t vsub_u8 (uint8x8_t, uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vsub.i8 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int32x2_t vsub_s32 (int32x2_t, int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vsub.i32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int16x4_t vsub_s16 (int16x4_t, int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vsub.i16 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int8x8_t vsub_s8 (int8x8_t, int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vsub.i8 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item float32x2_t vsub_f32 (float32x2_t, float32x2_t)
@*@emph{Form of expected instruction(s):} @code{vsub.f32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint64x1_t vsub_u64 (uint64x1_t, uint64x1_t)
@end itemize


@itemize @bullet
@item int64x1_t vsub_s64 (int64x1_t, int64x1_t)
@end itemize


@itemize @bullet
@item uint32x4_t vsubq_u32 (uint32x4_t, uint32x4_t)
@*@emph{Form of expected instruction(s):} @code{vsub.i32 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint16x8_t vsubq_u16 (uint16x8_t, uint16x8_t)
@*@emph{Form of expected instruction(s):} @code{vsub.i16 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint8x16_t vsubq_u8 (uint8x16_t, uint8x16_t)
@*@emph{Form of expected instruction(s):} @code{vsub.i8 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int32x4_t vsubq_s32 (int32x4_t, int32x4_t)
@*@emph{Form of expected instruction(s):} @code{vsub.i32 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int16x8_t vsubq_s16 (int16x8_t, int16x8_t)
@*@emph{Form of expected instruction(s):} @code{vsub.i16 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int8x16_t vsubq_s8 (int8x16_t, int8x16_t)
@*@emph{Form of expected instruction(s):} @code{vsub.i8 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint64x2_t vsubq_u64 (uint64x2_t, uint64x2_t)
@*@emph{Form of expected instruction(s):} @code{vsub.i64 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int64x2_t vsubq_s64 (int64x2_t, int64x2_t)
@*@emph{Form of expected instruction(s):} @code{vsub.i64 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item float32x4_t vsubq_f32 (float32x4_t, float32x4_t)
@*@emph{Form of expected instruction(s):} @code{vsub.f32 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint64x2_t vsubl_u32 (uint32x2_t, uint32x2_t)
@*@emph{Form of expected instruction(s):} @code{vsubl.u32 @var{q0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint32x4_t vsubl_u16 (uint16x4_t, uint16x4_t)
@*@emph{Form of expected instruction(s):} @code{vsubl.u16 @var{q0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint16x8_t vsubl_u8 (uint8x8_t, uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vsubl.u8 @var{q0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int64x2_t vsubl_s32 (int32x2_t, int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vsubl.s32 @var{q0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int32x4_t vsubl_s16 (int16x4_t, int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vsubl.s16 @var{q0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int16x8_t vsubl_s8 (int8x8_t, int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vsubl.s8 @var{q0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint64x2_t vsubw_u32 (uint64x2_t, uint32x2_t)
@*@emph{Form of expected instruction(s):} @code{vsubw.u32 @var{q0}, @var{q0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint32x4_t vsubw_u16 (uint32x4_t, uint16x4_t)
@*@emph{Form of expected instruction(s):} @code{vsubw.u16 @var{q0}, @var{q0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint16x8_t vsubw_u8 (uint16x8_t, uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vsubw.u8 @var{q0}, @var{q0}, @var{d0}}
@end itemize


@itemize @bullet
@item int64x2_t vsubw_s32 (int64x2_t, int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vsubw.s32 @var{q0}, @var{q0}, @var{d0}}
@end itemize


@itemize @bullet
@item int32x4_t vsubw_s16 (int32x4_t, int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vsubw.s16 @var{q0}, @var{q0}, @var{d0}}
@end itemize


@itemize @bullet
@item int16x8_t vsubw_s8 (int16x8_t, int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vsubw.s8 @var{q0}, @var{q0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint32x2_t vhsub_u32 (uint32x2_t, uint32x2_t)
@*@emph{Form of expected instruction(s):} @code{vhsub.u32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint16x4_t vhsub_u16 (uint16x4_t, uint16x4_t)
@*@emph{Form of expected instruction(s):} @code{vhsub.u16 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint8x8_t vhsub_u8 (uint8x8_t, uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vhsub.u8 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int32x2_t vhsub_s32 (int32x2_t, int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vhsub.s32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int16x4_t vhsub_s16 (int16x4_t, int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vhsub.s16 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int8x8_t vhsub_s8 (int8x8_t, int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vhsub.s8 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint32x4_t vhsubq_u32 (uint32x4_t, uint32x4_t)
@*@emph{Form of expected instruction(s):} @code{vhsub.u32 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint16x8_t vhsubq_u16 (uint16x8_t, uint16x8_t)
@*@emph{Form of expected instruction(s):} @code{vhsub.u16 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint8x16_t vhsubq_u8 (uint8x16_t, uint8x16_t)
@*@emph{Form of expected instruction(s):} @code{vhsub.u8 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int32x4_t vhsubq_s32 (int32x4_t, int32x4_t)
@*@emph{Form of expected instruction(s):} @code{vhsub.s32 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int16x8_t vhsubq_s16 (int16x8_t, int16x8_t)
@*@emph{Form of expected instruction(s):} @code{vhsub.s16 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int8x16_t vhsubq_s8 (int8x16_t, int8x16_t)
@*@emph{Form of expected instruction(s):} @code{vhsub.s8 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint32x2_t vqsub_u32 (uint32x2_t, uint32x2_t)
@*@emph{Form of expected instruction(s):} @code{vqsub.u32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint16x4_t vqsub_u16 (uint16x4_t, uint16x4_t)
@*@emph{Form of expected instruction(s):} @code{vqsub.u16 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint8x8_t vqsub_u8 (uint8x8_t, uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vqsub.u8 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int32x2_t vqsub_s32 (int32x2_t, int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vqsub.s32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int16x4_t vqsub_s16 (int16x4_t, int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vqsub.s16 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int8x8_t vqsub_s8 (int8x8_t, int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vqsub.s8 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint64x1_t vqsub_u64 (uint64x1_t, uint64x1_t)
@*@emph{Form of expected instruction(s):} @code{vqsub.u64 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int64x1_t vqsub_s64 (int64x1_t, int64x1_t)
@*@emph{Form of expected instruction(s):} @code{vqsub.s64 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint32x4_t vqsubq_u32 (uint32x4_t, uint32x4_t)
@*@emph{Form of expected instruction(s):} @code{vqsub.u32 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint16x8_t vqsubq_u16 (uint16x8_t, uint16x8_t)
@*@emph{Form of expected instruction(s):} @code{vqsub.u16 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint8x16_t vqsubq_u8 (uint8x16_t, uint8x16_t)
@*@emph{Form of expected instruction(s):} @code{vqsub.u8 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int32x4_t vqsubq_s32 (int32x4_t, int32x4_t)
@*@emph{Form of expected instruction(s):} @code{vqsub.s32 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int16x8_t vqsubq_s16 (int16x8_t, int16x8_t)
@*@emph{Form of expected instruction(s):} @code{vqsub.s16 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int8x16_t vqsubq_s8 (int8x16_t, int8x16_t)
@*@emph{Form of expected instruction(s):} @code{vqsub.s8 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint64x2_t vqsubq_u64 (uint64x2_t, uint64x2_t)
@*@emph{Form of expected instruction(s):} @code{vqsub.u64 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int64x2_t vqsubq_s64 (int64x2_t, int64x2_t)
@*@emph{Form of expected instruction(s):} @code{vqsub.s64 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint32x2_t vsubhn_u64 (uint64x2_t, uint64x2_t)
@*@emph{Form of expected instruction(s):} @code{vsubhn.i64 @var{d0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint16x4_t vsubhn_u32 (uint32x4_t, uint32x4_t)
@*@emph{Form of expected instruction(s):} @code{vsubhn.i32 @var{d0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint8x8_t vsubhn_u16 (uint16x8_t, uint16x8_t)
@*@emph{Form of expected instruction(s):} @code{vsubhn.i16 @var{d0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int32x2_t vsubhn_s64 (int64x2_t, int64x2_t)
@*@emph{Form of expected instruction(s):} @code{vsubhn.i64 @var{d0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int16x4_t vsubhn_s32 (int32x4_t, int32x4_t)
@*@emph{Form of expected instruction(s):} @code{vsubhn.i32 @var{d0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int8x8_t vsubhn_s16 (int16x8_t, int16x8_t)
@*@emph{Form of expected instruction(s):} @code{vsubhn.i16 @var{d0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint32x2_t vrsubhn_u64 (uint64x2_t, uint64x2_t)
@*@emph{Form of expected instruction(s):} @code{vrsubhn.i64 @var{d0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint16x4_t vrsubhn_u32 (uint32x4_t, uint32x4_t)
@*@emph{Form of expected instruction(s):} @code{vrsubhn.i32 @var{d0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint8x8_t vrsubhn_u16 (uint16x8_t, uint16x8_t)
@*@emph{Form of expected instruction(s):} @code{vrsubhn.i16 @var{d0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int32x2_t vrsubhn_s64 (int64x2_t, int64x2_t)
@*@emph{Form of expected instruction(s):} @code{vrsubhn.i64 @var{d0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int16x4_t vrsubhn_s32 (int32x4_t, int32x4_t)
@*@emph{Form of expected instruction(s):} @code{vrsubhn.i32 @var{d0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int8x8_t vrsubhn_s16 (int16x8_t, int16x8_t)
@*@emph{Form of expected instruction(s):} @code{vrsubhn.i16 @var{d0}, @var{q0}, @var{q0}}
@end itemize




@subsubsection Comparison (equal-to)

@itemize @bullet
@item uint32x2_t vceq_u32 (uint32x2_t, uint32x2_t)
@*@emph{Form of expected instruction(s):} @code{vceq.i32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint16x4_t vceq_u16 (uint16x4_t, uint16x4_t)
@*@emph{Form of expected instruction(s):} @code{vceq.i16 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint8x8_t vceq_u8 (uint8x8_t, uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vceq.i8 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint32x2_t vceq_s32 (int32x2_t, int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vceq.i32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint16x4_t vceq_s16 (int16x4_t, int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vceq.i16 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint8x8_t vceq_s8 (int8x8_t, int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vceq.i8 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint32x2_t vceq_f32 (float32x2_t, float32x2_t)
@*@emph{Form of expected instruction(s):} @code{vceq.f32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint8x8_t vceq_p8 (poly8x8_t, poly8x8_t)
@*@emph{Form of expected instruction(s):} @code{vceq.i8 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint32x4_t vceqq_u32 (uint32x4_t, uint32x4_t)
@*@emph{Form of expected instruction(s):} @code{vceq.i32 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint16x8_t vceqq_u16 (uint16x8_t, uint16x8_t)
@*@emph{Form of expected instruction(s):} @code{vceq.i16 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint8x16_t vceqq_u8 (uint8x16_t, uint8x16_t)
@*@emph{Form of expected instruction(s):} @code{vceq.i8 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint32x4_t vceqq_s32 (int32x4_t, int32x4_t)
@*@emph{Form of expected instruction(s):} @code{vceq.i32 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint16x8_t vceqq_s16 (int16x8_t, int16x8_t)
@*@emph{Form of expected instruction(s):} @code{vceq.i16 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint8x16_t vceqq_s8 (int8x16_t, int8x16_t)
@*@emph{Form of expected instruction(s):} @code{vceq.i8 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint32x4_t vceqq_f32 (float32x4_t, float32x4_t)
@*@emph{Form of expected instruction(s):} @code{vceq.f32 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint8x16_t vceqq_p8 (poly8x16_t, poly8x16_t)
@*@emph{Form of expected instruction(s):} @code{vceq.i8 @var{q0}, @var{q0}, @var{q0}}
@end itemize




@subsubsection Comparison (greater-than-or-equal-to)

@itemize @bullet
@item uint32x2_t vcge_s32 (int32x2_t, int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vcge.s32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint16x4_t vcge_s16 (int16x4_t, int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vcge.s16 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint8x8_t vcge_s8 (int8x8_t, int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vcge.s8 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint32x2_t vcge_f32 (float32x2_t, float32x2_t)
@*@emph{Form of expected instruction(s):} @code{vcge.f32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint32x2_t vcge_u32 (uint32x2_t, uint32x2_t)
@*@emph{Form of expected instruction(s):} @code{vcge.u32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint16x4_t vcge_u16 (uint16x4_t, uint16x4_t)
@*@emph{Form of expected instruction(s):} @code{vcge.u16 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint8x8_t vcge_u8 (uint8x8_t, uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vcge.u8 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint32x4_t vcgeq_s32 (int32x4_t, int32x4_t)
@*@emph{Form of expected instruction(s):} @code{vcge.s32 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint16x8_t vcgeq_s16 (int16x8_t, int16x8_t)
@*@emph{Form of expected instruction(s):} @code{vcge.s16 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint8x16_t vcgeq_s8 (int8x16_t, int8x16_t)
@*@emph{Form of expected instruction(s):} @code{vcge.s8 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint32x4_t vcgeq_f32 (float32x4_t, float32x4_t)
@*@emph{Form of expected instruction(s):} @code{vcge.f32 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint32x4_t vcgeq_u32 (uint32x4_t, uint32x4_t)
@*@emph{Form of expected instruction(s):} @code{vcge.u32 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint16x8_t vcgeq_u16 (uint16x8_t, uint16x8_t)
@*@emph{Form of expected instruction(s):} @code{vcge.u16 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint8x16_t vcgeq_u8 (uint8x16_t, uint8x16_t)
@*@emph{Form of expected instruction(s):} @code{vcge.u8 @var{q0}, @var{q0}, @var{q0}}
@end itemize




@subsubsection Comparison (less-than-or-equal-to)

@itemize @bullet
@item uint32x2_t vcle_s32 (int32x2_t, int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vcge.s32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint16x4_t vcle_s16 (int16x4_t, int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vcge.s16 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint8x8_t vcle_s8 (int8x8_t, int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vcge.s8 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint32x2_t vcle_f32 (float32x2_t, float32x2_t)
@*@emph{Form of expected instruction(s):} @code{vcge.f32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint32x2_t vcle_u32 (uint32x2_t, uint32x2_t)
@*@emph{Form of expected instruction(s):} @code{vcge.u32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint16x4_t vcle_u16 (uint16x4_t, uint16x4_t)
@*@emph{Form of expected instruction(s):} @code{vcge.u16 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint8x8_t vcle_u8 (uint8x8_t, uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vcge.u8 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint32x4_t vcleq_s32 (int32x4_t, int32x4_t)
@*@emph{Form of expected instruction(s):} @code{vcge.s32 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint16x8_t vcleq_s16 (int16x8_t, int16x8_t)
@*@emph{Form of expected instruction(s):} @code{vcge.s16 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint8x16_t vcleq_s8 (int8x16_t, int8x16_t)
@*@emph{Form of expected instruction(s):} @code{vcge.s8 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint32x4_t vcleq_f32 (float32x4_t, float32x4_t)
@*@emph{Form of expected instruction(s):} @code{vcge.f32 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint32x4_t vcleq_u32 (uint32x4_t, uint32x4_t)
@*@emph{Form of expected instruction(s):} @code{vcge.u32 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint16x8_t vcleq_u16 (uint16x8_t, uint16x8_t)
@*@emph{Form of expected instruction(s):} @code{vcge.u16 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint8x16_t vcleq_u8 (uint8x16_t, uint8x16_t)
@*@emph{Form of expected instruction(s):} @code{vcge.u8 @var{q0}, @var{q0}, @var{q0}}
@end itemize




@subsubsection Comparison (greater-than)

@itemize @bullet
@item uint32x2_t vcgt_s32 (int32x2_t, int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vcgt.s32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint16x4_t vcgt_s16 (int16x4_t, int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vcgt.s16 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint8x8_t vcgt_s8 (int8x8_t, int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vcgt.s8 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint32x2_t vcgt_f32 (float32x2_t, float32x2_t)
@*@emph{Form of expected instruction(s):} @code{vcgt.f32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint32x2_t vcgt_u32 (uint32x2_t, uint32x2_t)
@*@emph{Form of expected instruction(s):} @code{vcgt.u32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint16x4_t vcgt_u16 (uint16x4_t, uint16x4_t)
@*@emph{Form of expected instruction(s):} @code{vcgt.u16 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint8x8_t vcgt_u8 (uint8x8_t, uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vcgt.u8 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint32x4_t vcgtq_s32 (int32x4_t, int32x4_t)
@*@emph{Form of expected instruction(s):} @code{vcgt.s32 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint16x8_t vcgtq_s16 (int16x8_t, int16x8_t)
@*@emph{Form of expected instruction(s):} @code{vcgt.s16 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint8x16_t vcgtq_s8 (int8x16_t, int8x16_t)
@*@emph{Form of expected instruction(s):} @code{vcgt.s8 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint32x4_t vcgtq_f32 (float32x4_t, float32x4_t)
@*@emph{Form of expected instruction(s):} @code{vcgt.f32 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint32x4_t vcgtq_u32 (uint32x4_t, uint32x4_t)
@*@emph{Form of expected instruction(s):} @code{vcgt.u32 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint16x8_t vcgtq_u16 (uint16x8_t, uint16x8_t)
@*@emph{Form of expected instruction(s):} @code{vcgt.u16 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint8x16_t vcgtq_u8 (uint8x16_t, uint8x16_t)
@*@emph{Form of expected instruction(s):} @code{vcgt.u8 @var{q0}, @var{q0}, @var{q0}}
@end itemize




@subsubsection Comparison (less-than)

@itemize @bullet
@item uint32x2_t vclt_s32 (int32x2_t, int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vcgt.s32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint16x4_t vclt_s16 (int16x4_t, int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vcgt.s16 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint8x8_t vclt_s8 (int8x8_t, int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vcgt.s8 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint32x2_t vclt_f32 (float32x2_t, float32x2_t)
@*@emph{Form of expected instruction(s):} @code{vcgt.f32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint32x2_t vclt_u32 (uint32x2_t, uint32x2_t)
@*@emph{Form of expected instruction(s):} @code{vcgt.u32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint16x4_t vclt_u16 (uint16x4_t, uint16x4_t)
@*@emph{Form of expected instruction(s):} @code{vcgt.u16 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint8x8_t vclt_u8 (uint8x8_t, uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vcgt.u8 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint32x4_t vcltq_s32 (int32x4_t, int32x4_t)
@*@emph{Form of expected instruction(s):} @code{vcgt.s32 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint16x8_t vcltq_s16 (int16x8_t, int16x8_t)
@*@emph{Form of expected instruction(s):} @code{vcgt.s16 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint8x16_t vcltq_s8 (int8x16_t, int8x16_t)
@*@emph{Form of expected instruction(s):} @code{vcgt.s8 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint32x4_t vcltq_f32 (float32x4_t, float32x4_t)
@*@emph{Form of expected instruction(s):} @code{vcgt.f32 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint32x4_t vcltq_u32 (uint32x4_t, uint32x4_t)
@*@emph{Form of expected instruction(s):} @code{vcgt.u32 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint16x8_t vcltq_u16 (uint16x8_t, uint16x8_t)
@*@emph{Form of expected instruction(s):} @code{vcgt.u16 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint8x16_t vcltq_u8 (uint8x16_t, uint8x16_t)
@*@emph{Form of expected instruction(s):} @code{vcgt.u8 @var{q0}, @var{q0}, @var{q0}}
@end itemize




@subsubsection Comparison (absolute greater-than-or-equal-to)

@itemize @bullet
@item uint32x2_t vcage_f32 (float32x2_t, float32x2_t)
@*@emph{Form of expected instruction(s):} @code{vacge.f32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint32x4_t vcageq_f32 (float32x4_t, float32x4_t)
@*@emph{Form of expected instruction(s):} @code{vacge.f32 @var{q0}, @var{q0}, @var{q0}}
@end itemize




@subsubsection Comparison (absolute less-than-or-equal-to)

@itemize @bullet
@item uint32x2_t vcale_f32 (float32x2_t, float32x2_t)
@*@emph{Form of expected instruction(s):} @code{vacge.f32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint32x4_t vcaleq_f32 (float32x4_t, float32x4_t)
@*@emph{Form of expected instruction(s):} @code{vacge.f32 @var{q0}, @var{q0}, @var{q0}}
@end itemize




@subsubsection Comparison (absolute greater-than)

@itemize @bullet
@item uint32x2_t vcagt_f32 (float32x2_t, float32x2_t)
@*@emph{Form of expected instruction(s):} @code{vacgt.f32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint32x4_t vcagtq_f32 (float32x4_t, float32x4_t)
@*@emph{Form of expected instruction(s):} @code{vacgt.f32 @var{q0}, @var{q0}, @var{q0}}
@end itemize




@subsubsection Comparison (absolute less-than)

@itemize @bullet
@item uint32x2_t vcalt_f32 (float32x2_t, float32x2_t)
@*@emph{Form of expected instruction(s):} @code{vacgt.f32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint32x4_t vcaltq_f32 (float32x4_t, float32x4_t)
@*@emph{Form of expected instruction(s):} @code{vacgt.f32 @var{q0}, @var{q0}, @var{q0}}
@end itemize




@subsubsection Test bits

@itemize @bullet
@item uint32x2_t vtst_u32 (uint32x2_t, uint32x2_t)
@*@emph{Form of expected instruction(s):} @code{vtst.32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint16x4_t vtst_u16 (uint16x4_t, uint16x4_t)
@*@emph{Form of expected instruction(s):} @code{vtst.16 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint8x8_t vtst_u8 (uint8x8_t, uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vtst.8 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint32x2_t vtst_s32 (int32x2_t, int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vtst.32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint16x4_t vtst_s16 (int16x4_t, int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vtst.16 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint8x8_t vtst_s8 (int8x8_t, int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vtst.8 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint8x8_t vtst_p8 (poly8x8_t, poly8x8_t)
@*@emph{Form of expected instruction(s):} @code{vtst.8 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint32x4_t vtstq_u32 (uint32x4_t, uint32x4_t)
@*@emph{Form of expected instruction(s):} @code{vtst.32 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint16x8_t vtstq_u16 (uint16x8_t, uint16x8_t)
@*@emph{Form of expected instruction(s):} @code{vtst.16 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint8x16_t vtstq_u8 (uint8x16_t, uint8x16_t)
@*@emph{Form of expected instruction(s):} @code{vtst.8 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint32x4_t vtstq_s32 (int32x4_t, int32x4_t)
@*@emph{Form of expected instruction(s):} @code{vtst.32 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint16x8_t vtstq_s16 (int16x8_t, int16x8_t)
@*@emph{Form of expected instruction(s):} @code{vtst.16 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint8x16_t vtstq_s8 (int8x16_t, int8x16_t)
@*@emph{Form of expected instruction(s):} @code{vtst.8 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint8x16_t vtstq_p8 (poly8x16_t, poly8x16_t)
@*@emph{Form of expected instruction(s):} @code{vtst.8 @var{q0}, @var{q0}, @var{q0}}
@end itemize




@subsubsection Absolute difference

@itemize @bullet
@item uint32x2_t vabd_u32 (uint32x2_t, uint32x2_t)
@*@emph{Form of expected instruction(s):} @code{vabd.u32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint16x4_t vabd_u16 (uint16x4_t, uint16x4_t)
@*@emph{Form of expected instruction(s):} @code{vabd.u16 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint8x8_t vabd_u8 (uint8x8_t, uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vabd.u8 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int32x2_t vabd_s32 (int32x2_t, int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vabd.s32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int16x4_t vabd_s16 (int16x4_t, int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vabd.s16 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int8x8_t vabd_s8 (int8x8_t, int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vabd.s8 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item float32x2_t vabd_f32 (float32x2_t, float32x2_t)
@*@emph{Form of expected instruction(s):} @code{vabd.f32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint32x4_t vabdq_u32 (uint32x4_t, uint32x4_t)
@*@emph{Form of expected instruction(s):} @code{vabd.u32 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint16x8_t vabdq_u16 (uint16x8_t, uint16x8_t)
@*@emph{Form of expected instruction(s):} @code{vabd.u16 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint8x16_t vabdq_u8 (uint8x16_t, uint8x16_t)
@*@emph{Form of expected instruction(s):} @code{vabd.u8 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int32x4_t vabdq_s32 (int32x4_t, int32x4_t)
@*@emph{Form of expected instruction(s):} @code{vabd.s32 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int16x8_t vabdq_s16 (int16x8_t, int16x8_t)
@*@emph{Form of expected instruction(s):} @code{vabd.s16 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int8x16_t vabdq_s8 (int8x16_t, int8x16_t)
@*@emph{Form of expected instruction(s):} @code{vabd.s8 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item float32x4_t vabdq_f32 (float32x4_t, float32x4_t)
@*@emph{Form of expected instruction(s):} @code{vabd.f32 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint64x2_t vabdl_u32 (uint32x2_t, uint32x2_t)
@*@emph{Form of expected instruction(s):} @code{vabdl.u32 @var{q0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint32x4_t vabdl_u16 (uint16x4_t, uint16x4_t)
@*@emph{Form of expected instruction(s):} @code{vabdl.u16 @var{q0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint16x8_t vabdl_u8 (uint8x8_t, uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vabdl.u8 @var{q0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int64x2_t vabdl_s32 (int32x2_t, int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vabdl.s32 @var{q0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int32x4_t vabdl_s16 (int16x4_t, int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vabdl.s16 @var{q0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int16x8_t vabdl_s8 (int8x8_t, int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vabdl.s8 @var{q0}, @var{d0}, @var{d0}}
@end itemize




@subsubsection Absolute difference and accumulate

@itemize @bullet
@item uint32x2_t vaba_u32 (uint32x2_t, uint32x2_t, uint32x2_t)
@*@emph{Form of expected instruction(s):} @code{vaba.u32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint16x4_t vaba_u16 (uint16x4_t, uint16x4_t, uint16x4_t)
@*@emph{Form of expected instruction(s):} @code{vaba.u16 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint8x8_t vaba_u8 (uint8x8_t, uint8x8_t, uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vaba.u8 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int32x2_t vaba_s32 (int32x2_t, int32x2_t, int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vaba.s32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int16x4_t vaba_s16 (int16x4_t, int16x4_t, int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vaba.s16 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int8x8_t vaba_s8 (int8x8_t, int8x8_t, int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vaba.s8 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint32x4_t vabaq_u32 (uint32x4_t, uint32x4_t, uint32x4_t)
@*@emph{Form of expected instruction(s):} @code{vaba.u32 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint16x8_t vabaq_u16 (uint16x8_t, uint16x8_t, uint16x8_t)
@*@emph{Form of expected instruction(s):} @code{vaba.u16 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint8x16_t vabaq_u8 (uint8x16_t, uint8x16_t, uint8x16_t)
@*@emph{Form of expected instruction(s):} @code{vaba.u8 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int32x4_t vabaq_s32 (int32x4_t, int32x4_t, int32x4_t)
@*@emph{Form of expected instruction(s):} @code{vaba.s32 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int16x8_t vabaq_s16 (int16x8_t, int16x8_t, int16x8_t)
@*@emph{Form of expected instruction(s):} @code{vaba.s16 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int8x16_t vabaq_s8 (int8x16_t, int8x16_t, int8x16_t)
@*@emph{Form of expected instruction(s):} @code{vaba.s8 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint64x2_t vabal_u32 (uint64x2_t, uint32x2_t, uint32x2_t)
@*@emph{Form of expected instruction(s):} @code{vabal.u32 @var{q0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint32x4_t vabal_u16 (uint32x4_t, uint16x4_t, uint16x4_t)
@*@emph{Form of expected instruction(s):} @code{vabal.u16 @var{q0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint16x8_t vabal_u8 (uint16x8_t, uint8x8_t, uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vabal.u8 @var{q0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int64x2_t vabal_s32 (int64x2_t, int32x2_t, int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vabal.s32 @var{q0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int32x4_t vabal_s16 (int32x4_t, int16x4_t, int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vabal.s16 @var{q0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int16x8_t vabal_s8 (int16x8_t, int8x8_t, int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vabal.s8 @var{q0}, @var{d0}, @var{d0}}
@end itemize




@subsubsection Maximum

@itemize @bullet
@item uint32x2_t vmax_u32 (uint32x2_t, uint32x2_t)
@*@emph{Form of expected instruction(s):} @code{vmax.u32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint16x4_t vmax_u16 (uint16x4_t, uint16x4_t)
@*@emph{Form of expected instruction(s):} @code{vmax.u16 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint8x8_t vmax_u8 (uint8x8_t, uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vmax.u8 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int32x2_t vmax_s32 (int32x2_t, int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vmax.s32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int16x4_t vmax_s16 (int16x4_t, int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vmax.s16 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int8x8_t vmax_s8 (int8x8_t, int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vmax.s8 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item float32x2_t vmax_f32 (float32x2_t, float32x2_t)
@*@emph{Form of expected instruction(s):} @code{vmax.f32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint32x4_t vmaxq_u32 (uint32x4_t, uint32x4_t)
@*@emph{Form of expected instruction(s):} @code{vmax.u32 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint16x8_t vmaxq_u16 (uint16x8_t, uint16x8_t)
@*@emph{Form of expected instruction(s):} @code{vmax.u16 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint8x16_t vmaxq_u8 (uint8x16_t, uint8x16_t)
@*@emph{Form of expected instruction(s):} @code{vmax.u8 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int32x4_t vmaxq_s32 (int32x4_t, int32x4_t)
@*@emph{Form of expected instruction(s):} @code{vmax.s32 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int16x8_t vmaxq_s16 (int16x8_t, int16x8_t)
@*@emph{Form of expected instruction(s):} @code{vmax.s16 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int8x16_t vmaxq_s8 (int8x16_t, int8x16_t)
@*@emph{Form of expected instruction(s):} @code{vmax.s8 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item float32x4_t vmaxq_f32 (float32x4_t, float32x4_t)
@*@emph{Form of expected instruction(s):} @code{vmax.f32 @var{q0}, @var{q0}, @var{q0}}
@end itemize




@subsubsection Minimum

@itemize @bullet
@item uint32x2_t vmin_u32 (uint32x2_t, uint32x2_t)
@*@emph{Form of expected instruction(s):} @code{vmin.u32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint16x4_t vmin_u16 (uint16x4_t, uint16x4_t)
@*@emph{Form of expected instruction(s):} @code{vmin.u16 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint8x8_t vmin_u8 (uint8x8_t, uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vmin.u8 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int32x2_t vmin_s32 (int32x2_t, int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vmin.s32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int16x4_t vmin_s16 (int16x4_t, int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vmin.s16 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int8x8_t vmin_s8 (int8x8_t, int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vmin.s8 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item float32x2_t vmin_f32 (float32x2_t, float32x2_t)
@*@emph{Form of expected instruction(s):} @code{vmin.f32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint32x4_t vminq_u32 (uint32x4_t, uint32x4_t)
@*@emph{Form of expected instruction(s):} @code{vmin.u32 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint16x8_t vminq_u16 (uint16x8_t, uint16x8_t)
@*@emph{Form of expected instruction(s):} @code{vmin.u16 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint8x16_t vminq_u8 (uint8x16_t, uint8x16_t)
@*@emph{Form of expected instruction(s):} @code{vmin.u8 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int32x4_t vminq_s32 (int32x4_t, int32x4_t)
@*@emph{Form of expected instruction(s):} @code{vmin.s32 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int16x8_t vminq_s16 (int16x8_t, int16x8_t)
@*@emph{Form of expected instruction(s):} @code{vmin.s16 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int8x16_t vminq_s8 (int8x16_t, int8x16_t)
@*@emph{Form of expected instruction(s):} @code{vmin.s8 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item float32x4_t vminq_f32 (float32x4_t, float32x4_t)
@*@emph{Form of expected instruction(s):} @code{vmin.f32 @var{q0}, @var{q0}, @var{q0}}
@end itemize




@subsubsection Pairwise add

@itemize @bullet
@item uint32x2_t vpadd_u32 (uint32x2_t, uint32x2_t)
@*@emph{Form of expected instruction(s):} @code{vpadd.i32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint16x4_t vpadd_u16 (uint16x4_t, uint16x4_t)
@*@emph{Form of expected instruction(s):} @code{vpadd.i16 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint8x8_t vpadd_u8 (uint8x8_t, uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vpadd.i8 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int32x2_t vpadd_s32 (int32x2_t, int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vpadd.i32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int16x4_t vpadd_s16 (int16x4_t, int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vpadd.i16 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int8x8_t vpadd_s8 (int8x8_t, int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vpadd.i8 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item float32x2_t vpadd_f32 (float32x2_t, float32x2_t)
@*@emph{Form of expected instruction(s):} @code{vpadd.f32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint64x1_t vpaddl_u32 (uint32x2_t)
@*@emph{Form of expected instruction(s):} @code{vpaddl.u32 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint32x2_t vpaddl_u16 (uint16x4_t)
@*@emph{Form of expected instruction(s):} @code{vpaddl.u16 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint16x4_t vpaddl_u8 (uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vpaddl.u8 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int64x1_t vpaddl_s32 (int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vpaddl.s32 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int32x2_t vpaddl_s16 (int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vpaddl.s16 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int16x4_t vpaddl_s8 (int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vpaddl.s8 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint64x2_t vpaddlq_u32 (uint32x4_t)
@*@emph{Form of expected instruction(s):} @code{vpaddl.u32 @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint32x4_t vpaddlq_u16 (uint16x8_t)
@*@emph{Form of expected instruction(s):} @code{vpaddl.u16 @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint16x8_t vpaddlq_u8 (uint8x16_t)
@*@emph{Form of expected instruction(s):} @code{vpaddl.u8 @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int64x2_t vpaddlq_s32 (int32x4_t)
@*@emph{Form of expected instruction(s):} @code{vpaddl.s32 @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int32x4_t vpaddlq_s16 (int16x8_t)
@*@emph{Form of expected instruction(s):} @code{vpaddl.s16 @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int16x8_t vpaddlq_s8 (int8x16_t)
@*@emph{Form of expected instruction(s):} @code{vpaddl.s8 @var{q0}, @var{q0}}
@end itemize




@subsubsection Pairwise add, single_opcode widen and accumulate

@itemize @bullet
@item uint64x1_t vpadal_u32 (uint64x1_t, uint32x2_t)
@*@emph{Form of expected instruction(s):} @code{vpadal.u32 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint32x2_t vpadal_u16 (uint32x2_t, uint16x4_t)
@*@emph{Form of expected instruction(s):} @code{vpadal.u16 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint16x4_t vpadal_u8 (uint16x4_t, uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vpadal.u8 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int64x1_t vpadal_s32 (int64x1_t, int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vpadal.s32 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int32x2_t vpadal_s16 (int32x2_t, int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vpadal.s16 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int16x4_t vpadal_s8 (int16x4_t, int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vpadal.s8 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint64x2_t vpadalq_u32 (uint64x2_t, uint32x4_t)
@*@emph{Form of expected instruction(s):} @code{vpadal.u32 @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint32x4_t vpadalq_u16 (uint32x4_t, uint16x8_t)
@*@emph{Form of expected instruction(s):} @code{vpadal.u16 @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint16x8_t vpadalq_u8 (uint16x8_t, uint8x16_t)
@*@emph{Form of expected instruction(s):} @code{vpadal.u8 @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int64x2_t vpadalq_s32 (int64x2_t, int32x4_t)
@*@emph{Form of expected instruction(s):} @code{vpadal.s32 @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int32x4_t vpadalq_s16 (int32x4_t, int16x8_t)
@*@emph{Form of expected instruction(s):} @code{vpadal.s16 @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int16x8_t vpadalq_s8 (int16x8_t, int8x16_t)
@*@emph{Form of expected instruction(s):} @code{vpadal.s8 @var{q0}, @var{q0}}
@end itemize




@subsubsection Folding maximum

@itemize @bullet
@item uint32x2_t vpmax_u32 (uint32x2_t, uint32x2_t)
@*@emph{Form of expected instruction(s):} @code{vpmax.u32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint16x4_t vpmax_u16 (uint16x4_t, uint16x4_t)
@*@emph{Form of expected instruction(s):} @code{vpmax.u16 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint8x8_t vpmax_u8 (uint8x8_t, uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vpmax.u8 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int32x2_t vpmax_s32 (int32x2_t, int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vpmax.s32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int16x4_t vpmax_s16 (int16x4_t, int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vpmax.s16 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int8x8_t vpmax_s8 (int8x8_t, int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vpmax.s8 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item float32x2_t vpmax_f32 (float32x2_t, float32x2_t)
@*@emph{Form of expected instruction(s):} @code{vpmax.f32 @var{d0}, @var{d0}, @var{d0}}
@end itemize




@subsubsection Folding minimum

@itemize @bullet
@item uint32x2_t vpmin_u32 (uint32x2_t, uint32x2_t)
@*@emph{Form of expected instruction(s):} @code{vpmin.u32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint16x4_t vpmin_u16 (uint16x4_t, uint16x4_t)
@*@emph{Form of expected instruction(s):} @code{vpmin.u16 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint8x8_t vpmin_u8 (uint8x8_t, uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vpmin.u8 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int32x2_t vpmin_s32 (int32x2_t, int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vpmin.s32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int16x4_t vpmin_s16 (int16x4_t, int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vpmin.s16 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int8x8_t vpmin_s8 (int8x8_t, int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vpmin.s8 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item float32x2_t vpmin_f32 (float32x2_t, float32x2_t)
@*@emph{Form of expected instruction(s):} @code{vpmin.f32 @var{d0}, @var{d0}, @var{d0}}
@end itemize




@subsubsection Reciprocal step

@itemize @bullet
@item float32x2_t vrecps_f32 (float32x2_t, float32x2_t)
@*@emph{Form of expected instruction(s):} @code{vrecps.f32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item float32x4_t vrecpsq_f32 (float32x4_t, float32x4_t)
@*@emph{Form of expected instruction(s):} @code{vrecps.f32 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item float32x2_t vrsqrts_f32 (float32x2_t, float32x2_t)
@*@emph{Form of expected instruction(s):} @code{vrsqrts.f32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item float32x4_t vrsqrtsq_f32 (float32x4_t, float32x4_t)
@*@emph{Form of expected instruction(s):} @code{vrsqrts.f32 @var{q0}, @var{q0}, @var{q0}}
@end itemize




@subsubsection Vector shift left

@itemize @bullet
@item uint32x2_t vshl_u32 (uint32x2_t, int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vshl.u32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint16x4_t vshl_u16 (uint16x4_t, int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vshl.u16 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint8x8_t vshl_u8 (uint8x8_t, int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vshl.u8 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int32x2_t vshl_s32 (int32x2_t, int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vshl.s32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int16x4_t vshl_s16 (int16x4_t, int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vshl.s16 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int8x8_t vshl_s8 (int8x8_t, int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vshl.s8 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint64x1_t vshl_u64 (uint64x1_t, int64x1_t)
@*@emph{Form of expected instruction(s):} @code{vshl.u64 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int64x1_t vshl_s64 (int64x1_t, int64x1_t)
@*@emph{Form of expected instruction(s):} @code{vshl.s64 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint32x4_t vshlq_u32 (uint32x4_t, int32x4_t)
@*@emph{Form of expected instruction(s):} @code{vshl.u32 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint16x8_t vshlq_u16 (uint16x8_t, int16x8_t)
@*@emph{Form of expected instruction(s):} @code{vshl.u16 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint8x16_t vshlq_u8 (uint8x16_t, int8x16_t)
@*@emph{Form of expected instruction(s):} @code{vshl.u8 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int32x4_t vshlq_s32 (int32x4_t, int32x4_t)
@*@emph{Form of expected instruction(s):} @code{vshl.s32 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int16x8_t vshlq_s16 (int16x8_t, int16x8_t)
@*@emph{Form of expected instruction(s):} @code{vshl.s16 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int8x16_t vshlq_s8 (int8x16_t, int8x16_t)
@*@emph{Form of expected instruction(s):} @code{vshl.s8 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint64x2_t vshlq_u64 (uint64x2_t, int64x2_t)
@*@emph{Form of expected instruction(s):} @code{vshl.u64 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int64x2_t vshlq_s64 (int64x2_t, int64x2_t)
@*@emph{Form of expected instruction(s):} @code{vshl.s64 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint32x2_t vrshl_u32 (uint32x2_t, int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vrshl.u32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint16x4_t vrshl_u16 (uint16x4_t, int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vrshl.u16 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint8x8_t vrshl_u8 (uint8x8_t, int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vrshl.u8 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int32x2_t vrshl_s32 (int32x2_t, int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vrshl.s32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int16x4_t vrshl_s16 (int16x4_t, int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vrshl.s16 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int8x8_t vrshl_s8 (int8x8_t, int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vrshl.s8 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint64x1_t vrshl_u64 (uint64x1_t, int64x1_t)
@*@emph{Form of expected instruction(s):} @code{vrshl.u64 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int64x1_t vrshl_s64 (int64x1_t, int64x1_t)
@*@emph{Form of expected instruction(s):} @code{vrshl.s64 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint32x4_t vrshlq_u32 (uint32x4_t, int32x4_t)
@*@emph{Form of expected instruction(s):} @code{vrshl.u32 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint16x8_t vrshlq_u16 (uint16x8_t, int16x8_t)
@*@emph{Form of expected instruction(s):} @code{vrshl.u16 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint8x16_t vrshlq_u8 (uint8x16_t, int8x16_t)
@*@emph{Form of expected instruction(s):} @code{vrshl.u8 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int32x4_t vrshlq_s32 (int32x4_t, int32x4_t)
@*@emph{Form of expected instruction(s):} @code{vrshl.s32 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int16x8_t vrshlq_s16 (int16x8_t, int16x8_t)
@*@emph{Form of expected instruction(s):} @code{vrshl.s16 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int8x16_t vrshlq_s8 (int8x16_t, int8x16_t)
@*@emph{Form of expected instruction(s):} @code{vrshl.s8 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint64x2_t vrshlq_u64 (uint64x2_t, int64x2_t)
@*@emph{Form of expected instruction(s):} @code{vrshl.u64 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int64x2_t vrshlq_s64 (int64x2_t, int64x2_t)
@*@emph{Form of expected instruction(s):} @code{vrshl.s64 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint32x2_t vqshl_u32 (uint32x2_t, int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vqshl.u32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint16x4_t vqshl_u16 (uint16x4_t, int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vqshl.u16 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint8x8_t vqshl_u8 (uint8x8_t, int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vqshl.u8 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int32x2_t vqshl_s32 (int32x2_t, int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vqshl.s32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int16x4_t vqshl_s16 (int16x4_t, int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vqshl.s16 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int8x8_t vqshl_s8 (int8x8_t, int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vqshl.s8 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint64x1_t vqshl_u64 (uint64x1_t, int64x1_t)
@*@emph{Form of expected instruction(s):} @code{vqshl.u64 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int64x1_t vqshl_s64 (int64x1_t, int64x1_t)
@*@emph{Form of expected instruction(s):} @code{vqshl.s64 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint32x4_t vqshlq_u32 (uint32x4_t, int32x4_t)
@*@emph{Form of expected instruction(s):} @code{vqshl.u32 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint16x8_t vqshlq_u16 (uint16x8_t, int16x8_t)
@*@emph{Form of expected instruction(s):} @code{vqshl.u16 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint8x16_t vqshlq_u8 (uint8x16_t, int8x16_t)
@*@emph{Form of expected instruction(s):} @code{vqshl.u8 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int32x4_t vqshlq_s32 (int32x4_t, int32x4_t)
@*@emph{Form of expected instruction(s):} @code{vqshl.s32 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int16x8_t vqshlq_s16 (int16x8_t, int16x8_t)
@*@emph{Form of expected instruction(s):} @code{vqshl.s16 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int8x16_t vqshlq_s8 (int8x16_t, int8x16_t)
@*@emph{Form of expected instruction(s):} @code{vqshl.s8 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint64x2_t vqshlq_u64 (uint64x2_t, int64x2_t)
@*@emph{Form of expected instruction(s):} @code{vqshl.u64 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int64x2_t vqshlq_s64 (int64x2_t, int64x2_t)
@*@emph{Form of expected instruction(s):} @code{vqshl.s64 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint32x2_t vqrshl_u32 (uint32x2_t, int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vqrshl.u32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint16x4_t vqrshl_u16 (uint16x4_t, int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vqrshl.u16 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint8x8_t vqrshl_u8 (uint8x8_t, int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vqrshl.u8 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int32x2_t vqrshl_s32 (int32x2_t, int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vqrshl.s32 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int16x4_t vqrshl_s16 (int16x4_t, int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vqrshl.s16 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int8x8_t vqrshl_s8 (int8x8_t, int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vqrshl.s8 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint64x1_t vqrshl_u64 (uint64x1_t, int64x1_t)
@*@emph{Form of expected instruction(s):} @code{vqrshl.u64 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int64x1_t vqrshl_s64 (int64x1_t, int64x1_t)
@*@emph{Form of expected instruction(s):} @code{vqrshl.s64 @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint32x4_t vqrshlq_u32 (uint32x4_t, int32x4_t)
@*@emph{Form of expected instruction(s):} @code{vqrshl.u32 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint16x8_t vqrshlq_u16 (uint16x8_t, int16x8_t)
@*@emph{Form of expected instruction(s):} @code{vqrshl.u16 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint8x16_t vqrshlq_u8 (uint8x16_t, int8x16_t)
@*@emph{Form of expected instruction(s):} @code{vqrshl.u8 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int32x4_t vqrshlq_s32 (int32x4_t, int32x4_t)
@*@emph{Form of expected instruction(s):} @code{vqrshl.s32 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int16x8_t vqrshlq_s16 (int16x8_t, int16x8_t)
@*@emph{Form of expected instruction(s):} @code{vqrshl.s16 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int8x16_t vqrshlq_s8 (int8x16_t, int8x16_t)
@*@emph{Form of expected instruction(s):} @code{vqrshl.s8 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint64x2_t vqrshlq_u64 (uint64x2_t, int64x2_t)
@*@emph{Form of expected instruction(s):} @code{vqrshl.u64 @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int64x2_t vqrshlq_s64 (int64x2_t, int64x2_t)
@*@emph{Form of expected instruction(s):} @code{vqrshl.s64 @var{q0}, @var{q0}, @var{q0}}
@end itemize




@subsubsection Vector shift left by constant

@itemize @bullet
@item uint32x2_t vshl_n_u32 (uint32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vshl.i32 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint16x4_t vshl_n_u16 (uint16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vshl.i16 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint8x8_t vshl_n_u8 (uint8x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vshl.i8 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item int32x2_t vshl_n_s32 (int32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vshl.i32 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item int16x4_t vshl_n_s16 (int16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vshl.i16 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item int8x8_t vshl_n_s8 (int8x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vshl.i8 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint64x1_t vshl_n_u64 (uint64x1_t, const int)
@*@emph{Form of expected instruction(s):} @code{vshl.i64 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item int64x1_t vshl_n_s64 (int64x1_t, const int)
@*@emph{Form of expected instruction(s):} @code{vshl.i64 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint32x4_t vshlq_n_u32 (uint32x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vshl.i32 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint16x8_t vshlq_n_u16 (uint16x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vshl.i16 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint8x16_t vshlq_n_u8 (uint8x16_t, const int)
@*@emph{Form of expected instruction(s):} @code{vshl.i8 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item int32x4_t vshlq_n_s32 (int32x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vshl.i32 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item int16x8_t vshlq_n_s16 (int16x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vshl.i16 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item int8x16_t vshlq_n_s8 (int8x16_t, const int)
@*@emph{Form of expected instruction(s):} @code{vshl.i8 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint64x2_t vshlq_n_u64 (uint64x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vshl.i64 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item int64x2_t vshlq_n_s64 (int64x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vshl.i64 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint32x2_t vqshl_n_u32 (uint32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vqshl.u32 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint16x4_t vqshl_n_u16 (uint16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vqshl.u16 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint8x8_t vqshl_n_u8 (uint8x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vqshl.u8 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item int32x2_t vqshl_n_s32 (int32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vqshl.s32 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item int16x4_t vqshl_n_s16 (int16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vqshl.s16 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item int8x8_t vqshl_n_s8 (int8x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vqshl.s8 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint64x1_t vqshl_n_u64 (uint64x1_t, const int)
@*@emph{Form of expected instruction(s):} @code{vqshl.u64 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item int64x1_t vqshl_n_s64 (int64x1_t, const int)
@*@emph{Form of expected instruction(s):} @code{vqshl.s64 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint32x4_t vqshlq_n_u32 (uint32x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vqshl.u32 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint16x8_t vqshlq_n_u16 (uint16x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vqshl.u16 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint8x16_t vqshlq_n_u8 (uint8x16_t, const int)
@*@emph{Form of expected instruction(s):} @code{vqshl.u8 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item int32x4_t vqshlq_n_s32 (int32x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vqshl.s32 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item int16x8_t vqshlq_n_s16 (int16x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vqshl.s16 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item int8x16_t vqshlq_n_s8 (int8x16_t, const int)
@*@emph{Form of expected instruction(s):} @code{vqshl.s8 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint64x2_t vqshlq_n_u64 (uint64x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vqshl.u64 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item int64x2_t vqshlq_n_s64 (int64x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vqshl.s64 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint64x1_t vqshlu_n_s64 (int64x1_t, const int)
@*@emph{Form of expected instruction(s):} @code{vqshlu.s64 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint32x2_t vqshlu_n_s32 (int32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vqshlu.s32 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint16x4_t vqshlu_n_s16 (int16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vqshlu.s16 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint8x8_t vqshlu_n_s8 (int8x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vqshlu.s8 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint64x2_t vqshluq_n_s64 (int64x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vqshlu.s64 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint32x4_t vqshluq_n_s32 (int32x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vqshlu.s32 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint16x8_t vqshluq_n_s16 (int16x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vqshlu.s16 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint8x16_t vqshluq_n_s8 (int8x16_t, const int)
@*@emph{Form of expected instruction(s):} @code{vqshlu.s8 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint64x2_t vshll_n_u32 (uint32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vshll.u32 @var{q0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint32x4_t vshll_n_u16 (uint16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vshll.u16 @var{q0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint16x8_t vshll_n_u8 (uint8x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vshll.u8 @var{q0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item int64x2_t vshll_n_s32 (int32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vshll.s32 @var{q0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item int32x4_t vshll_n_s16 (int16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vshll.s16 @var{q0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item int16x8_t vshll_n_s8 (int8x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vshll.s8 @var{q0}, @var{d0}, #@var{0}}
@end itemize




@subsubsection Vector shift right by constant

@itemize @bullet
@item uint32x2_t vshr_n_u32 (uint32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vshr.u32 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint16x4_t vshr_n_u16 (uint16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vshr.u16 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint8x8_t vshr_n_u8 (uint8x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vshr.u8 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item int32x2_t vshr_n_s32 (int32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vshr.s32 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item int16x4_t vshr_n_s16 (int16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vshr.s16 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item int8x8_t vshr_n_s8 (int8x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vshr.s8 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint64x1_t vshr_n_u64 (uint64x1_t, const int)
@*@emph{Form of expected instruction(s):} @code{vshr.u64 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item int64x1_t vshr_n_s64 (int64x1_t, const int)
@*@emph{Form of expected instruction(s):} @code{vshr.s64 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint32x4_t vshrq_n_u32 (uint32x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vshr.u32 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint16x8_t vshrq_n_u16 (uint16x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vshr.u16 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint8x16_t vshrq_n_u8 (uint8x16_t, const int)
@*@emph{Form of expected instruction(s):} @code{vshr.u8 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item int32x4_t vshrq_n_s32 (int32x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vshr.s32 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item int16x8_t vshrq_n_s16 (int16x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vshr.s16 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item int8x16_t vshrq_n_s8 (int8x16_t, const int)
@*@emph{Form of expected instruction(s):} @code{vshr.s8 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint64x2_t vshrq_n_u64 (uint64x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vshr.u64 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item int64x2_t vshrq_n_s64 (int64x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vshr.s64 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint32x2_t vrshr_n_u32 (uint32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vrshr.u32 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint16x4_t vrshr_n_u16 (uint16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vrshr.u16 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint8x8_t vrshr_n_u8 (uint8x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vrshr.u8 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item int32x2_t vrshr_n_s32 (int32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vrshr.s32 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item int16x4_t vrshr_n_s16 (int16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vrshr.s16 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item int8x8_t vrshr_n_s8 (int8x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vrshr.s8 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint64x1_t vrshr_n_u64 (uint64x1_t, const int)
@*@emph{Form of expected instruction(s):} @code{vrshr.u64 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item int64x1_t vrshr_n_s64 (int64x1_t, const int)
@*@emph{Form of expected instruction(s):} @code{vrshr.s64 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint32x4_t vrshrq_n_u32 (uint32x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vrshr.u32 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint16x8_t vrshrq_n_u16 (uint16x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vrshr.u16 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint8x16_t vrshrq_n_u8 (uint8x16_t, const int)
@*@emph{Form of expected instruction(s):} @code{vrshr.u8 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item int32x4_t vrshrq_n_s32 (int32x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vrshr.s32 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item int16x8_t vrshrq_n_s16 (int16x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vrshr.s16 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item int8x16_t vrshrq_n_s8 (int8x16_t, const int)
@*@emph{Form of expected instruction(s):} @code{vrshr.s8 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint64x2_t vrshrq_n_u64 (uint64x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vrshr.u64 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item int64x2_t vrshrq_n_s64 (int64x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vrshr.s64 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint32x2_t vshrn_n_u64 (uint64x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vshrn.i64 @var{d0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint16x4_t vshrn_n_u32 (uint32x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vshrn.i32 @var{d0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint8x8_t vshrn_n_u16 (uint16x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vshrn.i16 @var{d0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item int32x2_t vshrn_n_s64 (int64x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vshrn.i64 @var{d0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item int16x4_t vshrn_n_s32 (int32x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vshrn.i32 @var{d0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item int8x8_t vshrn_n_s16 (int16x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vshrn.i16 @var{d0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint32x2_t vrshrn_n_u64 (uint64x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vrshrn.i64 @var{d0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint16x4_t vrshrn_n_u32 (uint32x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vrshrn.i32 @var{d0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint8x8_t vrshrn_n_u16 (uint16x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vrshrn.i16 @var{d0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item int32x2_t vrshrn_n_s64 (int64x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vrshrn.i64 @var{d0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item int16x4_t vrshrn_n_s32 (int32x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vrshrn.i32 @var{d0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item int8x8_t vrshrn_n_s16 (int16x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vrshrn.i16 @var{d0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint32x2_t vqshrn_n_u64 (uint64x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vqshrn.u64 @var{d0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint16x4_t vqshrn_n_u32 (uint32x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vqshrn.u32 @var{d0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint8x8_t vqshrn_n_u16 (uint16x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vqshrn.u16 @var{d0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item int32x2_t vqshrn_n_s64 (int64x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vqshrn.s64 @var{d0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item int16x4_t vqshrn_n_s32 (int32x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vqshrn.s32 @var{d0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item int8x8_t vqshrn_n_s16 (int16x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vqshrn.s16 @var{d0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint32x2_t vqrshrn_n_u64 (uint64x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vqrshrn.u64 @var{d0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint16x4_t vqrshrn_n_u32 (uint32x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vqrshrn.u32 @var{d0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint8x8_t vqrshrn_n_u16 (uint16x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vqrshrn.u16 @var{d0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item int32x2_t vqrshrn_n_s64 (int64x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vqrshrn.s64 @var{d0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item int16x4_t vqrshrn_n_s32 (int32x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vqrshrn.s32 @var{d0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item int8x8_t vqrshrn_n_s16 (int16x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vqrshrn.s16 @var{d0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint32x2_t vqshrun_n_s64 (int64x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vqshrun.s64 @var{d0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint16x4_t vqshrun_n_s32 (int32x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vqshrun.s32 @var{d0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint8x8_t vqshrun_n_s16 (int16x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vqshrun.s16 @var{d0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint32x2_t vqrshrun_n_s64 (int64x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vqrshrun.s64 @var{d0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint16x4_t vqrshrun_n_s32 (int32x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vqrshrun.s32 @var{d0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint8x8_t vqrshrun_n_s16 (int16x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vqrshrun.s16 @var{d0}, @var{q0}, #@var{0}}
@end itemize




@subsubsection Vector shift right by constant and accumulate

@itemize @bullet
@item uint32x2_t vsra_n_u32 (uint32x2_t, uint32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vsra.u32 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint16x4_t vsra_n_u16 (uint16x4_t, uint16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vsra.u16 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint8x8_t vsra_n_u8 (uint8x8_t, uint8x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vsra.u8 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item int32x2_t vsra_n_s32 (int32x2_t, int32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vsra.s32 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item int16x4_t vsra_n_s16 (int16x4_t, int16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vsra.s16 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item int8x8_t vsra_n_s8 (int8x8_t, int8x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vsra.s8 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint64x1_t vsra_n_u64 (uint64x1_t, uint64x1_t, const int)
@*@emph{Form of expected instruction(s):} @code{vsra.u64 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item int64x1_t vsra_n_s64 (int64x1_t, int64x1_t, const int)
@*@emph{Form of expected instruction(s):} @code{vsra.s64 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint32x4_t vsraq_n_u32 (uint32x4_t, uint32x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vsra.u32 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint16x8_t vsraq_n_u16 (uint16x8_t, uint16x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vsra.u16 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint8x16_t vsraq_n_u8 (uint8x16_t, uint8x16_t, const int)
@*@emph{Form of expected instruction(s):} @code{vsra.u8 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item int32x4_t vsraq_n_s32 (int32x4_t, int32x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vsra.s32 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item int16x8_t vsraq_n_s16 (int16x8_t, int16x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vsra.s16 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item int8x16_t vsraq_n_s8 (int8x16_t, int8x16_t, const int)
@*@emph{Form of expected instruction(s):} @code{vsra.s8 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint64x2_t vsraq_n_u64 (uint64x2_t, uint64x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vsra.u64 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item int64x2_t vsraq_n_s64 (int64x2_t, int64x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vsra.s64 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint32x2_t vrsra_n_u32 (uint32x2_t, uint32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vrsra.u32 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint16x4_t vrsra_n_u16 (uint16x4_t, uint16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vrsra.u16 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint8x8_t vrsra_n_u8 (uint8x8_t, uint8x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vrsra.u8 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item int32x2_t vrsra_n_s32 (int32x2_t, int32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vrsra.s32 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item int16x4_t vrsra_n_s16 (int16x4_t, int16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vrsra.s16 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item int8x8_t vrsra_n_s8 (int8x8_t, int8x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vrsra.s8 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint64x1_t vrsra_n_u64 (uint64x1_t, uint64x1_t, const int)
@*@emph{Form of expected instruction(s):} @code{vrsra.u64 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item int64x1_t vrsra_n_s64 (int64x1_t, int64x1_t, const int)
@*@emph{Form of expected instruction(s):} @code{vrsra.s64 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint32x4_t vrsraq_n_u32 (uint32x4_t, uint32x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vrsra.u32 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint16x8_t vrsraq_n_u16 (uint16x8_t, uint16x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vrsra.u16 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint8x16_t vrsraq_n_u8 (uint8x16_t, uint8x16_t, const int)
@*@emph{Form of expected instruction(s):} @code{vrsra.u8 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item int32x4_t vrsraq_n_s32 (int32x4_t, int32x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vrsra.s32 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item int16x8_t vrsraq_n_s16 (int16x8_t, int16x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vrsra.s16 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item int8x16_t vrsraq_n_s8 (int8x16_t, int8x16_t, const int)
@*@emph{Form of expected instruction(s):} @code{vrsra.s8 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint64x2_t vrsraq_n_u64 (uint64x2_t, uint64x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vrsra.u64 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item int64x2_t vrsraq_n_s64 (int64x2_t, int64x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vrsra.s64 @var{q0}, @var{q0}, #@var{0}}
@end itemize




@subsubsection Vector shift right and insert

@itemize @bullet
@item poly64x1_t vsri_n_p64 (poly64x1_t, poly64x1_t, const int)
@*@emph{Form of expected instruction(s):} @code{vsri.64 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint32x2_t vsri_n_u32 (uint32x2_t, uint32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vsri.32 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint16x4_t vsri_n_u16 (uint16x4_t, uint16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vsri.16 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint8x8_t vsri_n_u8 (uint8x8_t, uint8x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vsri.8 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item int32x2_t vsri_n_s32 (int32x2_t, int32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vsri.32 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item int16x4_t vsri_n_s16 (int16x4_t, int16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vsri.16 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item int8x8_t vsri_n_s8 (int8x8_t, int8x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vsri.8 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint64x1_t vsri_n_u64 (uint64x1_t, uint64x1_t, const int)
@*@emph{Form of expected instruction(s):} @code{vsri.64 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item int64x1_t vsri_n_s64 (int64x1_t, int64x1_t, const int)
@*@emph{Form of expected instruction(s):} @code{vsri.64 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item poly16x4_t vsri_n_p16 (poly16x4_t, poly16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vsri.16 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item poly8x8_t vsri_n_p8 (poly8x8_t, poly8x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vsri.8 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item poly64x2_t vsriq_n_p64 (poly64x2_t, poly64x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vsri.64 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint32x4_t vsriq_n_u32 (uint32x4_t, uint32x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vsri.32 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint16x8_t vsriq_n_u16 (uint16x8_t, uint16x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vsri.16 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint8x16_t vsriq_n_u8 (uint8x16_t, uint8x16_t, const int)
@*@emph{Form of expected instruction(s):} @code{vsri.8 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item int32x4_t vsriq_n_s32 (int32x4_t, int32x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vsri.32 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item int16x8_t vsriq_n_s16 (int16x8_t, int16x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vsri.16 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item int8x16_t vsriq_n_s8 (int8x16_t, int8x16_t, const int)
@*@emph{Form of expected instruction(s):} @code{vsri.8 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint64x2_t vsriq_n_u64 (uint64x2_t, uint64x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vsri.64 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item int64x2_t vsriq_n_s64 (int64x2_t, int64x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vsri.64 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item poly16x8_t vsriq_n_p16 (poly16x8_t, poly16x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vsri.16 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item poly8x16_t vsriq_n_p8 (poly8x16_t, poly8x16_t, const int)
@*@emph{Form of expected instruction(s):} @code{vsri.8 @var{q0}, @var{q0}, #@var{0}}
@end itemize




@subsubsection Vector shift left and insert

@itemize @bullet
@item poly64x1_t vsli_n_p64 (poly64x1_t, poly64x1_t, const int)
@*@emph{Form of expected instruction(s):} @code{vsli.64 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint32x2_t vsli_n_u32 (uint32x2_t, uint32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vsli.32 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint16x4_t vsli_n_u16 (uint16x4_t, uint16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vsli.16 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint8x8_t vsli_n_u8 (uint8x8_t, uint8x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vsli.8 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item int32x2_t vsli_n_s32 (int32x2_t, int32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vsli.32 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item int16x4_t vsli_n_s16 (int16x4_t, int16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vsli.16 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item int8x8_t vsli_n_s8 (int8x8_t, int8x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vsli.8 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint64x1_t vsli_n_u64 (uint64x1_t, uint64x1_t, const int)
@*@emph{Form of expected instruction(s):} @code{vsli.64 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item int64x1_t vsli_n_s64 (int64x1_t, int64x1_t, const int)
@*@emph{Form of expected instruction(s):} @code{vsli.64 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item poly16x4_t vsli_n_p16 (poly16x4_t, poly16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vsli.16 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item poly8x8_t vsli_n_p8 (poly8x8_t, poly8x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vsli.8 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item poly64x2_t vsliq_n_p64 (poly64x2_t, poly64x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vsli.64 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint32x4_t vsliq_n_u32 (uint32x4_t, uint32x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vsli.32 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint16x8_t vsliq_n_u16 (uint16x8_t, uint16x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vsli.16 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint8x16_t vsliq_n_u8 (uint8x16_t, uint8x16_t, const int)
@*@emph{Form of expected instruction(s):} @code{vsli.8 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item int32x4_t vsliq_n_s32 (int32x4_t, int32x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vsli.32 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item int16x8_t vsliq_n_s16 (int16x8_t, int16x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vsli.16 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item int8x16_t vsliq_n_s8 (int8x16_t, int8x16_t, const int)
@*@emph{Form of expected instruction(s):} @code{vsli.8 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint64x2_t vsliq_n_u64 (uint64x2_t, uint64x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vsli.64 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item int64x2_t vsliq_n_s64 (int64x2_t, int64x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vsli.64 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item poly16x8_t vsliq_n_p16 (poly16x8_t, poly16x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vsli.16 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item poly8x16_t vsliq_n_p8 (poly8x16_t, poly8x16_t, const int)
@*@emph{Form of expected instruction(s):} @code{vsli.8 @var{q0}, @var{q0}, #@var{0}}
@end itemize




@subsubsection Absolute value

@itemize @bullet
@item float32x2_t vabs_f32 (float32x2_t)
@*@emph{Form of expected instruction(s):} @code{vabs.f32 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int32x2_t vabs_s32 (int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vabs.s32 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int16x4_t vabs_s16 (int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vabs.s16 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int8x8_t vabs_s8 (int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vabs.s8 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item float32x4_t vabsq_f32 (float32x4_t)
@*@emph{Form of expected instruction(s):} @code{vabs.f32 @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int32x4_t vabsq_s32 (int32x4_t)
@*@emph{Form of expected instruction(s):} @code{vabs.s32 @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int16x8_t vabsq_s16 (int16x8_t)
@*@emph{Form of expected instruction(s):} @code{vabs.s16 @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int8x16_t vabsq_s8 (int8x16_t)
@*@emph{Form of expected instruction(s):} @code{vabs.s8 @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int32x2_t vqabs_s32 (int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vqabs.s32 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int16x4_t vqabs_s16 (int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vqabs.s16 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int8x8_t vqabs_s8 (int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vqabs.s8 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int32x4_t vqabsq_s32 (int32x4_t)
@*@emph{Form of expected instruction(s):} @code{vqabs.s32 @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int16x8_t vqabsq_s16 (int16x8_t)
@*@emph{Form of expected instruction(s):} @code{vqabs.s16 @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int8x16_t vqabsq_s8 (int8x16_t)
@*@emph{Form of expected instruction(s):} @code{vqabs.s8 @var{q0}, @var{q0}}
@end itemize




@subsubsection Negation

@itemize @bullet
@item float32x2_t vneg_f32 (float32x2_t)
@*@emph{Form of expected instruction(s):} @code{vneg.f32 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int32x2_t vneg_s32 (int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vneg.s32 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int16x4_t vneg_s16 (int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vneg.s16 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int8x8_t vneg_s8 (int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vneg.s8 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item float32x4_t vnegq_f32 (float32x4_t)
@*@emph{Form of expected instruction(s):} @code{vneg.f32 @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int32x4_t vnegq_s32 (int32x4_t)
@*@emph{Form of expected instruction(s):} @code{vneg.s32 @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int16x8_t vnegq_s16 (int16x8_t)
@*@emph{Form of expected instruction(s):} @code{vneg.s16 @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int8x16_t vnegq_s8 (int8x16_t)
@*@emph{Form of expected instruction(s):} @code{vneg.s8 @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int32x2_t vqneg_s32 (int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vqneg.s32 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int16x4_t vqneg_s16 (int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vqneg.s16 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int8x8_t vqneg_s8 (int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vqneg.s8 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int32x4_t vqnegq_s32 (int32x4_t)
@*@emph{Form of expected instruction(s):} @code{vqneg.s32 @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int16x8_t vqnegq_s16 (int16x8_t)
@*@emph{Form of expected instruction(s):} @code{vqneg.s16 @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int8x16_t vqnegq_s8 (int8x16_t)
@*@emph{Form of expected instruction(s):} @code{vqneg.s8 @var{q0}, @var{q0}}
@end itemize




@subsubsection Bitwise not

@itemize @bullet
@item uint32x2_t vmvn_u32 (uint32x2_t)
@*@emph{Form of expected instruction(s):} @code{vmvn @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint16x4_t vmvn_u16 (uint16x4_t)
@*@emph{Form of expected instruction(s):} @code{vmvn @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint8x8_t vmvn_u8 (uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vmvn @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int32x2_t vmvn_s32 (int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vmvn @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int16x4_t vmvn_s16 (int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vmvn @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int8x8_t vmvn_s8 (int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vmvn @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item poly8x8_t vmvn_p8 (poly8x8_t)
@*@emph{Form of expected instruction(s):} @code{vmvn @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint32x4_t vmvnq_u32 (uint32x4_t)
@*@emph{Form of expected instruction(s):} @code{vmvn @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint16x8_t vmvnq_u16 (uint16x8_t)
@*@emph{Form of expected instruction(s):} @code{vmvn @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint8x16_t vmvnq_u8 (uint8x16_t)
@*@emph{Form of expected instruction(s):} @code{vmvn @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int32x4_t vmvnq_s32 (int32x4_t)
@*@emph{Form of expected instruction(s):} @code{vmvn @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int16x8_t vmvnq_s16 (int16x8_t)
@*@emph{Form of expected instruction(s):} @code{vmvn @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int8x16_t vmvnq_s8 (int8x16_t)
@*@emph{Form of expected instruction(s):} @code{vmvn @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item poly8x16_t vmvnq_p8 (poly8x16_t)
@*@emph{Form of expected instruction(s):} @code{vmvn @var{q0}, @var{q0}}
@end itemize




@subsubsection Count leading sign bits

@itemize @bullet
@item int32x2_t vcls_s32 (int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vcls.s32 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int16x4_t vcls_s16 (int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vcls.s16 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int8x8_t vcls_s8 (int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vcls.s8 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int32x4_t vclsq_s32 (int32x4_t)
@*@emph{Form of expected instruction(s):} @code{vcls.s32 @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int16x8_t vclsq_s16 (int16x8_t)
@*@emph{Form of expected instruction(s):} @code{vcls.s16 @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int8x16_t vclsq_s8 (int8x16_t)
@*@emph{Form of expected instruction(s):} @code{vcls.s8 @var{q0}, @var{q0}}
@end itemize




@subsubsection Count leading zeros

@itemize @bullet
@item uint32x2_t vclz_u32 (uint32x2_t)
@*@emph{Form of expected instruction(s):} @code{vclz.i32 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint16x4_t vclz_u16 (uint16x4_t)
@*@emph{Form of expected instruction(s):} @code{vclz.i16 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint8x8_t vclz_u8 (uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vclz.i8 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int32x2_t vclz_s32 (int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vclz.i32 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int16x4_t vclz_s16 (int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vclz.i16 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int8x8_t vclz_s8 (int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vclz.i8 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint32x4_t vclzq_u32 (uint32x4_t)
@*@emph{Form of expected instruction(s):} @code{vclz.i32 @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint16x8_t vclzq_u16 (uint16x8_t)
@*@emph{Form of expected instruction(s):} @code{vclz.i16 @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint8x16_t vclzq_u8 (uint8x16_t)
@*@emph{Form of expected instruction(s):} @code{vclz.i8 @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int32x4_t vclzq_s32 (int32x4_t)
@*@emph{Form of expected instruction(s):} @code{vclz.i32 @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int16x8_t vclzq_s16 (int16x8_t)
@*@emph{Form of expected instruction(s):} @code{vclz.i16 @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int8x16_t vclzq_s8 (int8x16_t)
@*@emph{Form of expected instruction(s):} @code{vclz.i8 @var{q0}, @var{q0}}
@end itemize




@subsubsection Count number of set bits

@itemize @bullet
@item uint8x8_t vcnt_u8 (uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vcnt.8 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int8x8_t vcnt_s8 (int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vcnt.8 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item poly8x8_t vcnt_p8 (poly8x8_t)
@*@emph{Form of expected instruction(s):} @code{vcnt.8 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint8x16_t vcntq_u8 (uint8x16_t)
@*@emph{Form of expected instruction(s):} @code{vcnt.8 @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int8x16_t vcntq_s8 (int8x16_t)
@*@emph{Form of expected instruction(s):} @code{vcnt.8 @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item poly8x16_t vcntq_p8 (poly8x16_t)
@*@emph{Form of expected instruction(s):} @code{vcnt.8 @var{q0}, @var{q0}}
@end itemize




@subsubsection Reciprocal estimate

@itemize @bullet
@item float32x2_t vrecpe_f32 (float32x2_t)
@*@emph{Form of expected instruction(s):} @code{vrecpe.f32 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint32x2_t vrecpe_u32 (uint32x2_t)
@*@emph{Form of expected instruction(s):} @code{vrecpe.u32 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item float32x4_t vrecpeq_f32 (float32x4_t)
@*@emph{Form of expected instruction(s):} @code{vrecpe.f32 @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint32x4_t vrecpeq_u32 (uint32x4_t)
@*@emph{Form of expected instruction(s):} @code{vrecpe.u32 @var{q0}, @var{q0}}
@end itemize




@subsubsection Reciprocal square-root estimate

@itemize @bullet
@item float32x2_t vrsqrte_f32 (float32x2_t)
@*@emph{Form of expected instruction(s):} @code{vrsqrte.f32 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint32x2_t vrsqrte_u32 (uint32x2_t)
@*@emph{Form of expected instruction(s):} @code{vrsqrte.u32 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item float32x4_t vrsqrteq_f32 (float32x4_t)
@*@emph{Form of expected instruction(s):} @code{vrsqrte.f32 @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint32x4_t vrsqrteq_u32 (uint32x4_t)
@*@emph{Form of expected instruction(s):} @code{vrsqrte.u32 @var{q0}, @var{q0}}
@end itemize




@subsubsection Get lanes from a vector

@itemize @bullet
@item uint32_t vget_lane_u32 (uint32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmov.32 @var{r0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item uint16_t vget_lane_u16 (uint16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmov.u16 @var{r0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item uint8_t vget_lane_u8 (uint8x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmov.u8 @var{r0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int32_t vget_lane_s32 (int32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmov.32 @var{r0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int16_t vget_lane_s16 (int16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmov.s16 @var{r0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int8_t vget_lane_s8 (int8x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmov.s8 @var{r0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item float32_t vget_lane_f32 (float32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmov.32 @var{r0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item poly16_t vget_lane_p16 (poly16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmov.u16 @var{r0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item poly8_t vget_lane_p8 (poly8x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmov.u8 @var{r0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item uint64_t vget_lane_u64 (uint64x1_t, const int)
@end itemize


@itemize @bullet
@item int64_t vget_lane_s64 (int64x1_t, const int)
@end itemize


@itemize @bullet
@item uint32_t vgetq_lane_u32 (uint32x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmov.32 @var{r0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item uint16_t vgetq_lane_u16 (uint16x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmov.u16 @var{r0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item uint8_t vgetq_lane_u8 (uint8x16_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmov.u8 @var{r0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int32_t vgetq_lane_s32 (int32x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmov.32 @var{r0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int16_t vgetq_lane_s16 (int16x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmov.s16 @var{r0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int8_t vgetq_lane_s8 (int8x16_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmov.s8 @var{r0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item float32_t vgetq_lane_f32 (float32x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmov.32 @var{r0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item poly16_t vgetq_lane_p16 (poly16x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmov.u16 @var{r0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item poly8_t vgetq_lane_p8 (poly8x16_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmov.u8 @var{r0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item uint64_t vgetq_lane_u64 (uint64x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmov @var{r0}, @var{r0}, @var{d0}} @emph{or} @code{fmrrd @var{r0}, @var{r0}, @var{d0}}
@end itemize


@itemize @bullet
@item int64_t vgetq_lane_s64 (int64x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmov @var{r0}, @var{r0}, @var{d0}} @emph{or} @code{fmrrd @var{r0}, @var{r0}, @var{d0}}
@end itemize




@subsubsection Set lanes in a vector

@itemize @bullet
@item uint32x2_t vset_lane_u32 (uint32_t, uint32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmov.32 @var{d0}[@var{0}], @var{r0}}
@end itemize


@itemize @bullet
@item uint16x4_t vset_lane_u16 (uint16_t, uint16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmov.16 @var{d0}[@var{0}], @var{r0}}
@end itemize


@itemize @bullet
@item uint8x8_t vset_lane_u8 (uint8_t, uint8x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmov.8 @var{d0}[@var{0}], @var{r0}}
@end itemize


@itemize @bullet
@item int32x2_t vset_lane_s32 (int32_t, int32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmov.32 @var{d0}[@var{0}], @var{r0}}
@end itemize


@itemize @bullet
@item int16x4_t vset_lane_s16 (int16_t, int16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmov.16 @var{d0}[@var{0}], @var{r0}}
@end itemize


@itemize @bullet
@item int8x8_t vset_lane_s8 (int8_t, int8x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmov.8 @var{d0}[@var{0}], @var{r0}}
@end itemize


@itemize @bullet
@item float32x2_t vset_lane_f32 (float32_t, float32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmov.32 @var{d0}[@var{0}], @var{r0}}
@end itemize


@itemize @bullet
@item poly16x4_t vset_lane_p16 (poly16_t, poly16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmov.16 @var{d0}[@var{0}], @var{r0}}
@end itemize


@itemize @bullet
@item poly8x8_t vset_lane_p8 (poly8_t, poly8x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmov.8 @var{d0}[@var{0}], @var{r0}}
@end itemize


@itemize @bullet
@item uint64x1_t vset_lane_u64 (uint64_t, uint64x1_t, const int)
@end itemize


@itemize @bullet
@item int64x1_t vset_lane_s64 (int64_t, int64x1_t, const int)
@end itemize


@itemize @bullet
@item uint32x4_t vsetq_lane_u32 (uint32_t, uint32x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmov.32 @var{d0}[@var{0}], @var{r0}}
@end itemize


@itemize @bullet
@item uint16x8_t vsetq_lane_u16 (uint16_t, uint16x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmov.16 @var{d0}[@var{0}], @var{r0}}
@end itemize


@itemize @bullet
@item uint8x16_t vsetq_lane_u8 (uint8_t, uint8x16_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmov.8 @var{d0}[@var{0}], @var{r0}}
@end itemize


@itemize @bullet
@item int32x4_t vsetq_lane_s32 (int32_t, int32x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmov.32 @var{d0}[@var{0}], @var{r0}}
@end itemize


@itemize @bullet
@item int16x8_t vsetq_lane_s16 (int16_t, int16x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmov.16 @var{d0}[@var{0}], @var{r0}}
@end itemize


@itemize @bullet
@item int8x16_t vsetq_lane_s8 (int8_t, int8x16_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmov.8 @var{d0}[@var{0}], @var{r0}}
@end itemize


@itemize @bullet
@item float32x4_t vsetq_lane_f32 (float32_t, float32x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmov.32 @var{d0}[@var{0}], @var{r0}}
@end itemize


@itemize @bullet
@item poly16x8_t vsetq_lane_p16 (poly16_t, poly16x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmov.16 @var{d0}[@var{0}], @var{r0}}
@end itemize


@itemize @bullet
@item poly8x16_t vsetq_lane_p8 (poly8_t, poly8x16_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmov.8 @var{d0}[@var{0}], @var{r0}}
@end itemize


@itemize @bullet
@item uint64x2_t vsetq_lane_u64 (uint64_t, uint64x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmov @var{d0}, @var{r0}, @var{r0}}
@end itemize


@itemize @bullet
@item int64x2_t vsetq_lane_s64 (int64_t, int64x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmov @var{d0}, @var{r0}, @var{r0}}
@end itemize




@subsubsection Create vector from literal bit pattern

@itemize @bullet
@item poly64x1_t vcreate_p64 (uint64_t)
@end itemize


@itemize @bullet
@item uint32x2_t vcreate_u32 (uint64_t)
@end itemize


@itemize @bullet
@item uint16x4_t vcreate_u16 (uint64_t)
@end itemize


@itemize @bullet
@item uint8x8_t vcreate_u8 (uint64_t)
@end itemize


@itemize @bullet
@item int32x2_t vcreate_s32 (uint64_t)
@end itemize


@itemize @bullet
@item int16x4_t vcreate_s16 (uint64_t)
@end itemize


@itemize @bullet
@item int8x8_t vcreate_s8 (uint64_t)
@end itemize


@itemize @bullet
@item uint64x1_t vcreate_u64 (uint64_t)
@end itemize


@itemize @bullet
@item int64x1_t vcreate_s64 (uint64_t)
@end itemize


@itemize @bullet
@item float32x2_t vcreate_f32 (uint64_t)
@end itemize


@itemize @bullet
@item poly16x4_t vcreate_p16 (uint64_t)
@end itemize


@itemize @bullet
@item poly8x8_t vcreate_p8 (uint64_t)
@end itemize




@subsubsection Set all lanes to the same value

@itemize @bullet
@item uint32x2_t vdup_n_u32 (uint32_t)
@*@emph{Form of expected instruction(s):} @code{vdup.32 @var{d0}, @var{r0}}
@end itemize


@itemize @bullet
@item uint16x4_t vdup_n_u16 (uint16_t)
@*@emph{Form of expected instruction(s):} @code{vdup.16 @var{d0}, @var{r0}}
@end itemize


@itemize @bullet
@item uint8x8_t vdup_n_u8 (uint8_t)
@*@emph{Form of expected instruction(s):} @code{vdup.8 @var{d0}, @var{r0}}
@end itemize


@itemize @bullet
@item int32x2_t vdup_n_s32 (int32_t)
@*@emph{Form of expected instruction(s):} @code{vdup.32 @var{d0}, @var{r0}}
@end itemize


@itemize @bullet
@item int16x4_t vdup_n_s16 (int16_t)
@*@emph{Form of expected instruction(s):} @code{vdup.16 @var{d0}, @var{r0}}
@end itemize


@itemize @bullet
@item int8x8_t vdup_n_s8 (int8_t)
@*@emph{Form of expected instruction(s):} @code{vdup.8 @var{d0}, @var{r0}}
@end itemize


@itemize @bullet
@item float32x2_t vdup_n_f32 (float32_t)
@*@emph{Form of expected instruction(s):} @code{vdup.32 @var{d0}, @var{r0}}
@end itemize


@itemize @bullet
@item poly16x4_t vdup_n_p16 (poly16_t)
@*@emph{Form of expected instruction(s):} @code{vdup.16 @var{d0}, @var{r0}}
@end itemize


@itemize @bullet
@item poly8x8_t vdup_n_p8 (poly8_t)
@*@emph{Form of expected instruction(s):} @code{vdup.8 @var{d0}, @var{r0}}
@end itemize


@itemize @bullet
@item poly64x1_t vdup_n_p64 (poly64_t)
@end itemize


@itemize @bullet
@item uint64x1_t vdup_n_u64 (uint64_t)
@end itemize


@itemize @bullet
@item int64x1_t vdup_n_s64 (int64_t)
@end itemize


@itemize @bullet
@item poly64x2_t vdupq_n_p64 (poly64_t)
@end itemize


@itemize @bullet
@item uint32x4_t vdupq_n_u32 (uint32_t)
@*@emph{Form of expected instruction(s):} @code{vdup.32 @var{q0}, @var{r0}}
@end itemize


@itemize @bullet
@item uint16x8_t vdupq_n_u16 (uint16_t)
@*@emph{Form of expected instruction(s):} @code{vdup.16 @var{q0}, @var{r0}}
@end itemize


@itemize @bullet
@item uint8x16_t vdupq_n_u8 (uint8_t)
@*@emph{Form of expected instruction(s):} @code{vdup.8 @var{q0}, @var{r0}}
@end itemize


@itemize @bullet
@item int32x4_t vdupq_n_s32 (int32_t)
@*@emph{Form of expected instruction(s):} @code{vdup.32 @var{q0}, @var{r0}}
@end itemize


@itemize @bullet
@item int16x8_t vdupq_n_s16 (int16_t)
@*@emph{Form of expected instruction(s):} @code{vdup.16 @var{q0}, @var{r0}}
@end itemize


@itemize @bullet
@item int8x16_t vdupq_n_s8 (int8_t)
@*@emph{Form of expected instruction(s):} @code{vdup.8 @var{q0}, @var{r0}}
@end itemize


@itemize @bullet
@item float32x4_t vdupq_n_f32 (float32_t)
@*@emph{Form of expected instruction(s):} @code{vdup.32 @var{q0}, @var{r0}}
@end itemize


@itemize @bullet
@item poly16x8_t vdupq_n_p16 (poly16_t)
@*@emph{Form of expected instruction(s):} @code{vdup.16 @var{q0}, @var{r0}}
@end itemize


@itemize @bullet
@item poly8x16_t vdupq_n_p8 (poly8_t)
@*@emph{Form of expected instruction(s):} @code{vdup.8 @var{q0}, @var{r0}}
@end itemize


@itemize @bullet
@item uint64x2_t vdupq_n_u64 (uint64_t)
@end itemize


@itemize @bullet
@item int64x2_t vdupq_n_s64 (int64_t)
@end itemize


@itemize @bullet
@item uint32x2_t vmov_n_u32 (uint32_t)
@*@emph{Form of expected instruction(s):} @code{vdup.32 @var{d0}, @var{r0}}
@end itemize


@itemize @bullet
@item uint16x4_t vmov_n_u16 (uint16_t)
@*@emph{Form of expected instruction(s):} @code{vdup.16 @var{d0}, @var{r0}}
@end itemize


@itemize @bullet
@item uint8x8_t vmov_n_u8 (uint8_t)
@*@emph{Form of expected instruction(s):} @code{vdup.8 @var{d0}, @var{r0}}
@end itemize


@itemize @bullet
@item int32x2_t vmov_n_s32 (int32_t)
@*@emph{Form of expected instruction(s):} @code{vdup.32 @var{d0}, @var{r0}}
@end itemize


@itemize @bullet
@item int16x4_t vmov_n_s16 (int16_t)
@*@emph{Form of expected instruction(s):} @code{vdup.16 @var{d0}, @var{r0}}
@end itemize


@itemize @bullet
@item int8x8_t vmov_n_s8 (int8_t)
@*@emph{Form of expected instruction(s):} @code{vdup.8 @var{d0}, @var{r0}}
@end itemize


@itemize @bullet
@item float32x2_t vmov_n_f32 (float32_t)
@*@emph{Form of expected instruction(s):} @code{vdup.32 @var{d0}, @var{r0}}
@end itemize


@itemize @bullet
@item poly16x4_t vmov_n_p16 (poly16_t)
@*@emph{Form of expected instruction(s):} @code{vdup.16 @var{d0}, @var{r0}}
@end itemize


@itemize @bullet
@item poly8x8_t vmov_n_p8 (poly8_t)
@*@emph{Form of expected instruction(s):} @code{vdup.8 @var{d0}, @var{r0}}
@end itemize


@itemize @bullet
@item uint64x1_t vmov_n_u64 (uint64_t)
@end itemize


@itemize @bullet
@item int64x1_t vmov_n_s64 (int64_t)
@end itemize


@itemize @bullet
@item uint32x4_t vmovq_n_u32 (uint32_t)
@*@emph{Form of expected instruction(s):} @code{vdup.32 @var{q0}, @var{r0}}
@end itemize


@itemize @bullet
@item uint16x8_t vmovq_n_u16 (uint16_t)
@*@emph{Form of expected instruction(s):} @code{vdup.16 @var{q0}, @var{r0}}
@end itemize


@itemize @bullet
@item uint8x16_t vmovq_n_u8 (uint8_t)
@*@emph{Form of expected instruction(s):} @code{vdup.8 @var{q0}, @var{r0}}
@end itemize


@itemize @bullet
@item int32x4_t vmovq_n_s32 (int32_t)
@*@emph{Form of expected instruction(s):} @code{vdup.32 @var{q0}, @var{r0}}
@end itemize


@itemize @bullet
@item int16x8_t vmovq_n_s16 (int16_t)
@*@emph{Form of expected instruction(s):} @code{vdup.16 @var{q0}, @var{r0}}
@end itemize


@itemize @bullet
@item int8x16_t vmovq_n_s8 (int8_t)
@*@emph{Form of expected instruction(s):} @code{vdup.8 @var{q0}, @var{r0}}
@end itemize


@itemize @bullet
@item float32x4_t vmovq_n_f32 (float32_t)
@*@emph{Form of expected instruction(s):} @code{vdup.32 @var{q0}, @var{r0}}
@end itemize


@itemize @bullet
@item poly16x8_t vmovq_n_p16 (poly16_t)
@*@emph{Form of expected instruction(s):} @code{vdup.16 @var{q0}, @var{r0}}
@end itemize


@itemize @bullet
@item poly8x16_t vmovq_n_p8 (poly8_t)
@*@emph{Form of expected instruction(s):} @code{vdup.8 @var{q0}, @var{r0}}
@end itemize


@itemize @bullet
@item uint64x2_t vmovq_n_u64 (uint64_t)
@end itemize


@itemize @bullet
@item int64x2_t vmovq_n_s64 (int64_t)
@end itemize


@itemize @bullet
@item uint32x2_t vdup_lane_u32 (uint32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vdup.32 @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item uint16x4_t vdup_lane_u16 (uint16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vdup.16 @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item uint8x8_t vdup_lane_u8 (uint8x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vdup.8 @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int32x2_t vdup_lane_s32 (int32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vdup.32 @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int16x4_t vdup_lane_s16 (int16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vdup.16 @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int8x8_t vdup_lane_s8 (int8x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vdup.8 @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item float32x2_t vdup_lane_f32 (float32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vdup.32 @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item poly16x4_t vdup_lane_p16 (poly16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vdup.16 @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item poly8x8_t vdup_lane_p8 (poly8x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vdup.8 @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item poly64x1_t vdup_lane_p64 (poly64x1_t, const int)
@end itemize


@itemize @bullet
@item uint64x1_t vdup_lane_u64 (uint64x1_t, const int)
@end itemize


@itemize @bullet
@item int64x1_t vdup_lane_s64 (int64x1_t, const int)
@end itemize


@itemize @bullet
@item uint32x4_t vdupq_lane_u32 (uint32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vdup.32 @var{q0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item uint16x8_t vdupq_lane_u16 (uint16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vdup.16 @var{q0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item uint8x16_t vdupq_lane_u8 (uint8x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vdup.8 @var{q0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int32x4_t vdupq_lane_s32 (int32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vdup.32 @var{q0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int16x8_t vdupq_lane_s16 (int16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vdup.16 @var{q0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int8x16_t vdupq_lane_s8 (int8x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vdup.8 @var{q0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item float32x4_t vdupq_lane_f32 (float32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vdup.32 @var{q0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item poly16x8_t vdupq_lane_p16 (poly16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vdup.16 @var{q0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item poly8x16_t vdupq_lane_p8 (poly8x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vdup.8 @var{q0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item poly64x2_t vdupq_lane_p64 (poly64x1_t, const int)
@end itemize


@itemize @bullet
@item uint64x2_t vdupq_lane_u64 (uint64x1_t, const int)
@end itemize


@itemize @bullet
@item int64x2_t vdupq_lane_s64 (int64x1_t, const int)
@end itemize




@subsubsection Combining vectors

@itemize @bullet
@item poly64x2_t vcombine_p64 (poly64x1_t, poly64x1_t)
@end itemize


@itemize @bullet
@item uint32x4_t vcombine_u32 (uint32x2_t, uint32x2_t)
@end itemize


@itemize @bullet
@item uint16x8_t vcombine_u16 (uint16x4_t, uint16x4_t)
@end itemize


@itemize @bullet
@item uint8x16_t vcombine_u8 (uint8x8_t, uint8x8_t)
@end itemize


@itemize @bullet
@item int32x4_t vcombine_s32 (int32x2_t, int32x2_t)
@end itemize


@itemize @bullet
@item int16x8_t vcombine_s16 (int16x4_t, int16x4_t)
@end itemize


@itemize @bullet
@item int8x16_t vcombine_s8 (int8x8_t, int8x8_t)
@end itemize


@itemize @bullet
@item uint64x2_t vcombine_u64 (uint64x1_t, uint64x1_t)
@end itemize


@itemize @bullet
@item int64x2_t vcombine_s64 (int64x1_t, int64x1_t)
@end itemize


@itemize @bullet
@item float32x4_t vcombine_f32 (float32x2_t, float32x2_t)
@end itemize


@itemize @bullet
@item poly16x8_t vcombine_p16 (poly16x4_t, poly16x4_t)
@end itemize


@itemize @bullet
@item poly8x16_t vcombine_p8 (poly8x8_t, poly8x8_t)
@end itemize




@subsubsection Splitting vectors

@itemize @bullet
@item poly64x1_t vget_high_p64 (poly64x2_t)
@end itemize


@itemize @bullet
@item uint32x2_t vget_high_u32 (uint32x4_t)
@end itemize


@itemize @bullet
@item uint16x4_t vget_high_u16 (uint16x8_t)
@end itemize


@itemize @bullet
@item uint8x8_t vget_high_u8 (uint8x16_t)
@end itemize


@itemize @bullet
@item int32x2_t vget_high_s32 (int32x4_t)
@end itemize


@itemize @bullet
@item int16x4_t vget_high_s16 (int16x8_t)
@end itemize


@itemize @bullet
@item int8x8_t vget_high_s8 (int8x16_t)
@end itemize


@itemize @bullet
@item uint64x1_t vget_high_u64 (uint64x2_t)
@end itemize


@itemize @bullet
@item int64x1_t vget_high_s64 (int64x2_t)
@end itemize


@itemize @bullet
@item float32x2_t vget_high_f32 (float32x4_t)
@end itemize


@itemize @bullet
@item poly16x4_t vget_high_p16 (poly16x8_t)
@end itemize


@itemize @bullet
@item poly8x8_t vget_high_p8 (poly8x16_t)
@end itemize


@itemize @bullet
@item uint32x2_t vget_low_u32 (uint32x4_t)
@*@emph{Form of expected instruction(s):} @code{vmov @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint16x4_t vget_low_u16 (uint16x8_t)
@*@emph{Form of expected instruction(s):} @code{vmov @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint8x8_t vget_low_u8 (uint8x16_t)
@*@emph{Form of expected instruction(s):} @code{vmov @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int32x2_t vget_low_s32 (int32x4_t)
@*@emph{Form of expected instruction(s):} @code{vmov @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int16x4_t vget_low_s16 (int16x8_t)
@*@emph{Form of expected instruction(s):} @code{vmov @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int8x8_t vget_low_s8 (int8x16_t)
@*@emph{Form of expected instruction(s):} @code{vmov @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item float32x2_t vget_low_f32 (float32x4_t)
@*@emph{Form of expected instruction(s):} @code{vmov @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item poly16x4_t vget_low_p16 (poly16x8_t)
@*@emph{Form of expected instruction(s):} @code{vmov @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item poly8x8_t vget_low_p8 (poly8x16_t)
@*@emph{Form of expected instruction(s):} @code{vmov @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item poly64x1_t vget_low_p64 (poly64x2_t)
@end itemize


@itemize @bullet
@item uint64x1_t vget_low_u64 (uint64x2_t)
@end itemize


@itemize @bullet
@item int64x1_t vget_low_s64 (int64x2_t)
@end itemize




@subsubsection Conversions

@itemize @bullet
@item float32x2_t vcvt_f32_u32 (uint32x2_t)
@*@emph{Form of expected instruction(s):} @code{vcvt.f32.u32 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item float32x2_t vcvt_f32_s32 (int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vcvt.f32.s32 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint32x2_t vcvt_u32_f32 (float32x2_t)
@*@emph{Form of expected instruction(s):} @code{vcvt.u32.f32 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int32x2_t vcvt_s32_f32 (float32x2_t)
@*@emph{Form of expected instruction(s):} @code{vcvt.s32.f32 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item float32x4_t vcvtq_f32_u32 (uint32x4_t)
@*@emph{Form of expected instruction(s):} @code{vcvt.f32.u32 @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item float32x4_t vcvtq_f32_s32 (int32x4_t)
@*@emph{Form of expected instruction(s):} @code{vcvt.f32.s32 @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint32x4_t vcvtq_u32_f32 (float32x4_t)
@*@emph{Form of expected instruction(s):} @code{vcvt.u32.f32 @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int32x4_t vcvtq_s32_f32 (float32x4_t)
@*@emph{Form of expected instruction(s):} @code{vcvt.s32.f32 @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item float16x4_t vcvt_f16_f32 (float32x4_t)
@*@emph{Form of expected instruction(s):} @code{vcvt.f16.f32 @var{d0}, @var{q0}}
@end itemize


@itemize @bullet
@item float32x4_t vcvt_f32_f16 (float16x4_t)
@*@emph{Form of expected instruction(s):} @code{vcvt.f32.f16 @var{q0}, @var{d0}}
@end itemize


@itemize @bullet
@item float32x2_t vcvt_n_f32_u32 (uint32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vcvt.f32.u32 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item float32x2_t vcvt_n_f32_s32 (int32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vcvt.f32.s32 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint32x2_t vcvt_n_u32_f32 (float32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vcvt.u32.f32 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item int32x2_t vcvt_n_s32_f32 (float32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vcvt.s32.f32 @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item float32x4_t vcvtq_n_f32_u32 (uint32x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vcvt.f32.u32 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item float32x4_t vcvtq_n_f32_s32 (int32x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vcvt.f32.s32 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint32x4_t vcvtq_n_u32_f32 (float32x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vcvt.u32.f32 @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item int32x4_t vcvtq_n_s32_f32 (float32x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vcvt.s32.f32 @var{q0}, @var{q0}, #@var{0}}
@end itemize




@subsubsection Move, single_opcode narrowing

@itemize @bullet
@item uint32x2_t vmovn_u64 (uint64x2_t)
@*@emph{Form of expected instruction(s):} @code{vmovn.i64 @var{d0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint16x4_t vmovn_u32 (uint32x4_t)
@*@emph{Form of expected instruction(s):} @code{vmovn.i32 @var{d0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint8x8_t vmovn_u16 (uint16x8_t)
@*@emph{Form of expected instruction(s):} @code{vmovn.i16 @var{d0}, @var{q0}}
@end itemize


@itemize @bullet
@item int32x2_t vmovn_s64 (int64x2_t)
@*@emph{Form of expected instruction(s):} @code{vmovn.i64 @var{d0}, @var{q0}}
@end itemize


@itemize @bullet
@item int16x4_t vmovn_s32 (int32x4_t)
@*@emph{Form of expected instruction(s):} @code{vmovn.i32 @var{d0}, @var{q0}}
@end itemize


@itemize @bullet
@item int8x8_t vmovn_s16 (int16x8_t)
@*@emph{Form of expected instruction(s):} @code{vmovn.i16 @var{d0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint32x2_t vqmovn_u64 (uint64x2_t)
@*@emph{Form of expected instruction(s):} @code{vqmovn.u64 @var{d0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint16x4_t vqmovn_u32 (uint32x4_t)
@*@emph{Form of expected instruction(s):} @code{vqmovn.u32 @var{d0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint8x8_t vqmovn_u16 (uint16x8_t)
@*@emph{Form of expected instruction(s):} @code{vqmovn.u16 @var{d0}, @var{q0}}
@end itemize


@itemize @bullet
@item int32x2_t vqmovn_s64 (int64x2_t)
@*@emph{Form of expected instruction(s):} @code{vqmovn.s64 @var{d0}, @var{q0}}
@end itemize


@itemize @bullet
@item int16x4_t vqmovn_s32 (int32x4_t)
@*@emph{Form of expected instruction(s):} @code{vqmovn.s32 @var{d0}, @var{q0}}
@end itemize


@itemize @bullet
@item int8x8_t vqmovn_s16 (int16x8_t)
@*@emph{Form of expected instruction(s):} @code{vqmovn.s16 @var{d0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint32x2_t vqmovun_s64 (int64x2_t)
@*@emph{Form of expected instruction(s):} @code{vqmovun.s64 @var{d0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint16x4_t vqmovun_s32 (int32x4_t)
@*@emph{Form of expected instruction(s):} @code{vqmovun.s32 @var{d0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint8x8_t vqmovun_s16 (int16x8_t)
@*@emph{Form of expected instruction(s):} @code{vqmovun.s16 @var{d0}, @var{q0}}
@end itemize




@subsubsection Move, single_opcode long

@itemize @bullet
@item uint64x2_t vmovl_u32 (uint32x2_t)
@*@emph{Form of expected instruction(s):} @code{vmovl.u32 @var{q0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint32x4_t vmovl_u16 (uint16x4_t)
@*@emph{Form of expected instruction(s):} @code{vmovl.u16 @var{q0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint16x8_t vmovl_u8 (uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vmovl.u8 @var{q0}, @var{d0}}
@end itemize


@itemize @bullet
@item int64x2_t vmovl_s32 (int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vmovl.s32 @var{q0}, @var{d0}}
@end itemize


@itemize @bullet
@item int32x4_t vmovl_s16 (int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vmovl.s16 @var{q0}, @var{d0}}
@end itemize


@itemize @bullet
@item int16x8_t vmovl_s8 (int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vmovl.s8 @var{q0}, @var{d0}}
@end itemize




@subsubsection Table lookup

@itemize @bullet
@item poly8x8_t vtbl1_p8 (poly8x8_t, uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vtbl.8 @var{d0}, @{@var{d0}@}, @var{d0}}
@end itemize


@itemize @bullet
@item int8x8_t vtbl1_s8 (int8x8_t, int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vtbl.8 @var{d0}, @{@var{d0}@}, @var{d0}}
@end itemize


@itemize @bullet
@item uint8x8_t vtbl1_u8 (uint8x8_t, uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vtbl.8 @var{d0}, @{@var{d0}@}, @var{d0}}
@end itemize


@itemize @bullet
@item poly8x8_t vtbl2_p8 (poly8x8x2_t, uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vtbl.8 @var{d0}, @{@var{d0}, @var{d1}@}, @var{d0}}
@end itemize


@itemize @bullet
@item int8x8_t vtbl2_s8 (int8x8x2_t, int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vtbl.8 @var{d0}, @{@var{d0}, @var{d1}@}, @var{d0}}
@end itemize


@itemize @bullet
@item uint8x8_t vtbl2_u8 (uint8x8x2_t, uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vtbl.8 @var{d0}, @{@var{d0}, @var{d1}@}, @var{d0}}
@end itemize


@itemize @bullet
@item poly8x8_t vtbl3_p8 (poly8x8x3_t, uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vtbl.8 @var{d0}, @{@var{d0}, @var{d1}, @var{d2}@}, @var{d0}}
@end itemize


@itemize @bullet
@item int8x8_t vtbl3_s8 (int8x8x3_t, int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vtbl.8 @var{d0}, @{@var{d0}, @var{d1}, @var{d2}@}, @var{d0}}
@end itemize


@itemize @bullet
@item uint8x8_t vtbl3_u8 (uint8x8x3_t, uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vtbl.8 @var{d0}, @{@var{d0}, @var{d1}, @var{d2}@}, @var{d0}}
@end itemize


@itemize @bullet
@item poly8x8_t vtbl4_p8 (poly8x8x4_t, uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vtbl.8 @var{d0}, @{@var{d0}, @var{d1}, @var{d2}, @var{d3}@}, @var{d0}}
@end itemize


@itemize @bullet
@item int8x8_t vtbl4_s8 (int8x8x4_t, int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vtbl.8 @var{d0}, @{@var{d0}, @var{d1}, @var{d2}, @var{d3}@}, @var{d0}}
@end itemize


@itemize @bullet
@item uint8x8_t vtbl4_u8 (uint8x8x4_t, uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vtbl.8 @var{d0}, @{@var{d0}, @var{d1}, @var{d2}, @var{d3}@}, @var{d0}}
@end itemize




@subsubsection Extended table lookup

@itemize @bullet
@item poly8x8_t vtbx1_p8 (poly8x8_t, poly8x8_t, uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vtbx.8 @var{d0}, @{@var{d0}@}, @var{d0}}
@end itemize


@itemize @bullet
@item int8x8_t vtbx1_s8 (int8x8_t, int8x8_t, int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vtbx.8 @var{d0}, @{@var{d0}@}, @var{d0}}
@end itemize


@itemize @bullet
@item uint8x8_t vtbx1_u8 (uint8x8_t, uint8x8_t, uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vtbx.8 @var{d0}, @{@var{d0}@}, @var{d0}}
@end itemize


@itemize @bullet
@item poly8x8_t vtbx2_p8 (poly8x8_t, poly8x8x2_t, uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vtbx.8 @var{d0}, @{@var{d0}, @var{d1}@}, @var{d0}}
@end itemize


@itemize @bullet
@item int8x8_t vtbx2_s8 (int8x8_t, int8x8x2_t, int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vtbx.8 @var{d0}, @{@var{d0}, @var{d1}@}, @var{d0}}
@end itemize


@itemize @bullet
@item uint8x8_t vtbx2_u8 (uint8x8_t, uint8x8x2_t, uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vtbx.8 @var{d0}, @{@var{d0}, @var{d1}@}, @var{d0}}
@end itemize


@itemize @bullet
@item poly8x8_t vtbx3_p8 (poly8x8_t, poly8x8x3_t, uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vtbx.8 @var{d0}, @{@var{d0}, @var{d1}, @var{d2}@}, @var{d0}}
@end itemize


@itemize @bullet
@item int8x8_t vtbx3_s8 (int8x8_t, int8x8x3_t, int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vtbx.8 @var{d0}, @{@var{d0}, @var{d1}, @var{d2}@}, @var{d0}}
@end itemize


@itemize @bullet
@item uint8x8_t vtbx3_u8 (uint8x8_t, uint8x8x3_t, uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vtbx.8 @var{d0}, @{@var{d0}, @var{d1}, @var{d2}@}, @var{d0}}
@end itemize


@itemize @bullet
@item poly8x8_t vtbx4_p8 (poly8x8_t, poly8x8x4_t, uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vtbx.8 @var{d0}, @{@var{d0}, @var{d1}, @var{d2}, @var{d3}@}, @var{d0}}
@end itemize


@itemize @bullet
@item int8x8_t vtbx4_s8 (int8x8_t, int8x8x4_t, int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vtbx.8 @var{d0}, @{@var{d0}, @var{d1}, @var{d2}, @var{d3}@}, @var{d0}}
@end itemize


@itemize @bullet
@item uint8x8_t vtbx4_u8 (uint8x8_t, uint8x8x4_t, uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vtbx.8 @var{d0}, @{@var{d0}, @var{d1}, @var{d2}, @var{d3}@}, @var{d0}}
@end itemize




@subsubsection Multiply, lane

@itemize @bullet
@item float32x2_t vmul_lane_f32 (float32x2_t, float32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmul.f32 @var{d0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item uint32x2_t vmul_lane_u32 (uint32x2_t, uint32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmul.i32 @var{d0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item uint16x4_t vmul_lane_u16 (uint16x4_t, uint16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmul.i16 @var{d0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int32x2_t vmul_lane_s32 (int32x2_t, int32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmul.i32 @var{d0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int16x4_t vmul_lane_s16 (int16x4_t, int16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmul.i16 @var{d0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item float32x4_t vmulq_lane_f32 (float32x4_t, float32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmul.f32 @var{q0}, @var{q0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item uint32x4_t vmulq_lane_u32 (uint32x4_t, uint32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmul.i32 @var{q0}, @var{q0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item uint16x8_t vmulq_lane_u16 (uint16x8_t, uint16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmul.i16 @var{q0}, @var{q0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int32x4_t vmulq_lane_s32 (int32x4_t, int32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmul.i32 @var{q0}, @var{q0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int16x8_t vmulq_lane_s16 (int16x8_t, int16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmul.i16 @var{q0}, @var{q0}, @var{d0}[@var{0}]}
@end itemize




@subsubsection Long multiply, lane

@itemize @bullet
@item uint64x2_t vmull_lane_u32 (uint32x2_t, uint32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmull.u32 @var{q0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item uint32x4_t vmull_lane_u16 (uint16x4_t, uint16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmull.u16 @var{q0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int64x2_t vmull_lane_s32 (int32x2_t, int32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmull.s32 @var{q0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int32x4_t vmull_lane_s16 (int16x4_t, int16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmull.s16 @var{q0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize




@subsubsection Saturating doubling long multiply, lane

@itemize @bullet
@item int64x2_t vqdmull_lane_s32 (int32x2_t, int32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vqdmull.s32 @var{q0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int32x4_t vqdmull_lane_s16 (int16x4_t, int16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vqdmull.s16 @var{q0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize




@subsubsection Saturating doubling multiply high, lane

@itemize @bullet
@item int32x4_t vqdmulhq_lane_s32 (int32x4_t, int32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vqdmulh.s32 @var{q0}, @var{q0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int16x8_t vqdmulhq_lane_s16 (int16x8_t, int16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vqdmulh.s16 @var{q0}, @var{q0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int32x2_t vqdmulh_lane_s32 (int32x2_t, int32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vqdmulh.s32 @var{d0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int16x4_t vqdmulh_lane_s16 (int16x4_t, int16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vqdmulh.s16 @var{d0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int32x4_t vqrdmulhq_lane_s32 (int32x4_t, int32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vqrdmulh.s32 @var{q0}, @var{q0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int16x8_t vqrdmulhq_lane_s16 (int16x8_t, int16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vqrdmulh.s16 @var{q0}, @var{q0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int32x2_t vqrdmulh_lane_s32 (int32x2_t, int32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vqrdmulh.s32 @var{d0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int16x4_t vqrdmulh_lane_s16 (int16x4_t, int16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vqrdmulh.s16 @var{d0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize




@subsubsection Multiply-accumulate, lane

@itemize @bullet
@item float32x2_t vmla_lane_f32 (float32x2_t, float32x2_t, float32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmla.f32 @var{d0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item uint32x2_t vmla_lane_u32 (uint32x2_t, uint32x2_t, uint32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmla.i32 @var{d0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item uint16x4_t vmla_lane_u16 (uint16x4_t, uint16x4_t, uint16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmla.i16 @var{d0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int32x2_t vmla_lane_s32 (int32x2_t, int32x2_t, int32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmla.i32 @var{d0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int16x4_t vmla_lane_s16 (int16x4_t, int16x4_t, int16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmla.i16 @var{d0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item float32x4_t vmlaq_lane_f32 (float32x4_t, float32x4_t, float32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmla.f32 @var{q0}, @var{q0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item uint32x4_t vmlaq_lane_u32 (uint32x4_t, uint32x4_t, uint32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmla.i32 @var{q0}, @var{q0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item uint16x8_t vmlaq_lane_u16 (uint16x8_t, uint16x8_t, uint16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmla.i16 @var{q0}, @var{q0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int32x4_t vmlaq_lane_s32 (int32x4_t, int32x4_t, int32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmla.i32 @var{q0}, @var{q0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int16x8_t vmlaq_lane_s16 (int16x8_t, int16x8_t, int16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmla.i16 @var{q0}, @var{q0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item uint64x2_t vmlal_lane_u32 (uint64x2_t, uint32x2_t, uint32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmlal.u32 @var{q0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item uint32x4_t vmlal_lane_u16 (uint32x4_t, uint16x4_t, uint16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmlal.u16 @var{q0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int64x2_t vmlal_lane_s32 (int64x2_t, int32x2_t, int32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmlal.s32 @var{q0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int32x4_t vmlal_lane_s16 (int32x4_t, int16x4_t, int16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmlal.s16 @var{q0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int64x2_t vqdmlal_lane_s32 (int64x2_t, int32x2_t, int32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vqdmlal.s32 @var{q0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int32x4_t vqdmlal_lane_s16 (int32x4_t, int16x4_t, int16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vqdmlal.s16 @var{q0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize




@subsubsection Multiply-subtract, lane

@itemize @bullet
@item float32x2_t vmls_lane_f32 (float32x2_t, float32x2_t, float32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmls.f32 @var{d0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item uint32x2_t vmls_lane_u32 (uint32x2_t, uint32x2_t, uint32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmls.i32 @var{d0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item uint16x4_t vmls_lane_u16 (uint16x4_t, uint16x4_t, uint16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmls.i16 @var{d0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int32x2_t vmls_lane_s32 (int32x2_t, int32x2_t, int32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmls.i32 @var{d0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int16x4_t vmls_lane_s16 (int16x4_t, int16x4_t, int16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmls.i16 @var{d0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item float32x4_t vmlsq_lane_f32 (float32x4_t, float32x4_t, float32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmls.f32 @var{q0}, @var{q0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item uint32x4_t vmlsq_lane_u32 (uint32x4_t, uint32x4_t, uint32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmls.i32 @var{q0}, @var{q0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item uint16x8_t vmlsq_lane_u16 (uint16x8_t, uint16x8_t, uint16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmls.i16 @var{q0}, @var{q0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int32x4_t vmlsq_lane_s32 (int32x4_t, int32x4_t, int32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmls.i32 @var{q0}, @var{q0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int16x8_t vmlsq_lane_s16 (int16x8_t, int16x8_t, int16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmls.i16 @var{q0}, @var{q0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item uint64x2_t vmlsl_lane_u32 (uint64x2_t, uint32x2_t, uint32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmlsl.u32 @var{q0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item uint32x4_t vmlsl_lane_u16 (uint32x4_t, uint16x4_t, uint16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmlsl.u16 @var{q0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int64x2_t vmlsl_lane_s32 (int64x2_t, int32x2_t, int32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmlsl.s32 @var{q0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int32x4_t vmlsl_lane_s16 (int32x4_t, int16x4_t, int16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vmlsl.s16 @var{q0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int64x2_t vqdmlsl_lane_s32 (int64x2_t, int32x2_t, int32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vqdmlsl.s32 @var{q0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int32x4_t vqdmlsl_lane_s16 (int32x4_t, int16x4_t, int16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vqdmlsl.s16 @var{q0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize




@subsubsection Vector multiply by scalar

@itemize @bullet
@item float32x2_t vmul_n_f32 (float32x2_t, float32_t)
@*@emph{Form of expected instruction(s):} @code{vmul.f32 @var{d0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item uint32x2_t vmul_n_u32 (uint32x2_t, uint32_t)
@*@emph{Form of expected instruction(s):} @code{vmul.i32 @var{d0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item uint16x4_t vmul_n_u16 (uint16x4_t, uint16_t)
@*@emph{Form of expected instruction(s):} @code{vmul.i16 @var{d0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int32x2_t vmul_n_s32 (int32x2_t, int32_t)
@*@emph{Form of expected instruction(s):} @code{vmul.i32 @var{d0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int16x4_t vmul_n_s16 (int16x4_t, int16_t)
@*@emph{Form of expected instruction(s):} @code{vmul.i16 @var{d0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item float32x4_t vmulq_n_f32 (float32x4_t, float32_t)
@*@emph{Form of expected instruction(s):} @code{vmul.f32 @var{q0}, @var{q0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item uint32x4_t vmulq_n_u32 (uint32x4_t, uint32_t)
@*@emph{Form of expected instruction(s):} @code{vmul.i32 @var{q0}, @var{q0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item uint16x8_t vmulq_n_u16 (uint16x8_t, uint16_t)
@*@emph{Form of expected instruction(s):} @code{vmul.i16 @var{q0}, @var{q0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int32x4_t vmulq_n_s32 (int32x4_t, int32_t)
@*@emph{Form of expected instruction(s):} @code{vmul.i32 @var{q0}, @var{q0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int16x8_t vmulq_n_s16 (int16x8_t, int16_t)
@*@emph{Form of expected instruction(s):} @code{vmul.i16 @var{q0}, @var{q0}, @var{d0}[@var{0}]}
@end itemize




@subsubsection Vector long multiply by scalar

@itemize @bullet
@item uint64x2_t vmull_n_u32 (uint32x2_t, uint32_t)
@*@emph{Form of expected instruction(s):} @code{vmull.u32 @var{q0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item uint32x4_t vmull_n_u16 (uint16x4_t, uint16_t)
@*@emph{Form of expected instruction(s):} @code{vmull.u16 @var{q0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int64x2_t vmull_n_s32 (int32x2_t, int32_t)
@*@emph{Form of expected instruction(s):} @code{vmull.s32 @var{q0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int32x4_t vmull_n_s16 (int16x4_t, int16_t)
@*@emph{Form of expected instruction(s):} @code{vmull.s16 @var{q0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize




@subsubsection Vector saturating doubling long multiply by scalar

@itemize @bullet
@item int64x2_t vqdmull_n_s32 (int32x2_t, int32_t)
@*@emph{Form of expected instruction(s):} @code{vqdmull.s32 @var{q0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int32x4_t vqdmull_n_s16 (int16x4_t, int16_t)
@*@emph{Form of expected instruction(s):} @code{vqdmull.s16 @var{q0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize




@subsubsection Vector saturating doubling multiply high by scalar

@itemize @bullet
@item int32x4_t vqdmulhq_n_s32 (int32x4_t, int32_t)
@*@emph{Form of expected instruction(s):} @code{vqdmulh.s32 @var{q0}, @var{q0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int16x8_t vqdmulhq_n_s16 (int16x8_t, int16_t)
@*@emph{Form of expected instruction(s):} @code{vqdmulh.s16 @var{q0}, @var{q0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int32x2_t vqdmulh_n_s32 (int32x2_t, int32_t)
@*@emph{Form of expected instruction(s):} @code{vqdmulh.s32 @var{d0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int16x4_t vqdmulh_n_s16 (int16x4_t, int16_t)
@*@emph{Form of expected instruction(s):} @code{vqdmulh.s16 @var{d0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int32x4_t vqrdmulhq_n_s32 (int32x4_t, int32_t)
@*@emph{Form of expected instruction(s):} @code{vqrdmulh.s32 @var{q0}, @var{q0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int16x8_t vqrdmulhq_n_s16 (int16x8_t, int16_t)
@*@emph{Form of expected instruction(s):} @code{vqrdmulh.s16 @var{q0}, @var{q0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int32x2_t vqrdmulh_n_s32 (int32x2_t, int32_t)
@*@emph{Form of expected instruction(s):} @code{vqrdmulh.s32 @var{d0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int16x4_t vqrdmulh_n_s16 (int16x4_t, int16_t)
@*@emph{Form of expected instruction(s):} @code{vqrdmulh.s16 @var{d0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize




@subsubsection Vector multiply-accumulate by scalar

@itemize @bullet
@item float32x2_t vmla_n_f32 (float32x2_t, float32x2_t, float32_t)
@*@emph{Form of expected instruction(s):} @code{vmla.f32 @var{d0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item uint32x2_t vmla_n_u32 (uint32x2_t, uint32x2_t, uint32_t)
@*@emph{Form of expected instruction(s):} @code{vmla.i32 @var{d0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item uint16x4_t vmla_n_u16 (uint16x4_t, uint16x4_t, uint16_t)
@*@emph{Form of expected instruction(s):} @code{vmla.i16 @var{d0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int32x2_t vmla_n_s32 (int32x2_t, int32x2_t, int32_t)
@*@emph{Form of expected instruction(s):} @code{vmla.i32 @var{d0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int16x4_t vmla_n_s16 (int16x4_t, int16x4_t, int16_t)
@*@emph{Form of expected instruction(s):} @code{vmla.i16 @var{d0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item float32x4_t vmlaq_n_f32 (float32x4_t, float32x4_t, float32_t)
@*@emph{Form of expected instruction(s):} @code{vmla.f32 @var{q0}, @var{q0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item uint32x4_t vmlaq_n_u32 (uint32x4_t, uint32x4_t, uint32_t)
@*@emph{Form of expected instruction(s):} @code{vmla.i32 @var{q0}, @var{q0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item uint16x8_t vmlaq_n_u16 (uint16x8_t, uint16x8_t, uint16_t)
@*@emph{Form of expected instruction(s):} @code{vmla.i16 @var{q0}, @var{q0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int32x4_t vmlaq_n_s32 (int32x4_t, int32x4_t, int32_t)
@*@emph{Form of expected instruction(s):} @code{vmla.i32 @var{q0}, @var{q0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int16x8_t vmlaq_n_s16 (int16x8_t, int16x8_t, int16_t)
@*@emph{Form of expected instruction(s):} @code{vmla.i16 @var{q0}, @var{q0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item uint64x2_t vmlal_n_u32 (uint64x2_t, uint32x2_t, uint32_t)
@*@emph{Form of expected instruction(s):} @code{vmlal.u32 @var{q0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item uint32x4_t vmlal_n_u16 (uint32x4_t, uint16x4_t, uint16_t)
@*@emph{Form of expected instruction(s):} @code{vmlal.u16 @var{q0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int64x2_t vmlal_n_s32 (int64x2_t, int32x2_t, int32_t)
@*@emph{Form of expected instruction(s):} @code{vmlal.s32 @var{q0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int32x4_t vmlal_n_s16 (int32x4_t, int16x4_t, int16_t)
@*@emph{Form of expected instruction(s):} @code{vmlal.s16 @var{q0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int64x2_t vqdmlal_n_s32 (int64x2_t, int32x2_t, int32_t)
@*@emph{Form of expected instruction(s):} @code{vqdmlal.s32 @var{q0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int32x4_t vqdmlal_n_s16 (int32x4_t, int16x4_t, int16_t)
@*@emph{Form of expected instruction(s):} @code{vqdmlal.s16 @var{q0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize




@subsubsection Vector multiply-subtract by scalar

@itemize @bullet
@item float32x2_t vmls_n_f32 (float32x2_t, float32x2_t, float32_t)
@*@emph{Form of expected instruction(s):} @code{vmls.f32 @var{d0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item uint32x2_t vmls_n_u32 (uint32x2_t, uint32x2_t, uint32_t)
@*@emph{Form of expected instruction(s):} @code{vmls.i32 @var{d0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item uint16x4_t vmls_n_u16 (uint16x4_t, uint16x4_t, uint16_t)
@*@emph{Form of expected instruction(s):} @code{vmls.i16 @var{d0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int32x2_t vmls_n_s32 (int32x2_t, int32x2_t, int32_t)
@*@emph{Form of expected instruction(s):} @code{vmls.i32 @var{d0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int16x4_t vmls_n_s16 (int16x4_t, int16x4_t, int16_t)
@*@emph{Form of expected instruction(s):} @code{vmls.i16 @var{d0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item float32x4_t vmlsq_n_f32 (float32x4_t, float32x4_t, float32_t)
@*@emph{Form of expected instruction(s):} @code{vmls.f32 @var{q0}, @var{q0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item uint32x4_t vmlsq_n_u32 (uint32x4_t, uint32x4_t, uint32_t)
@*@emph{Form of expected instruction(s):} @code{vmls.i32 @var{q0}, @var{q0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item uint16x8_t vmlsq_n_u16 (uint16x8_t, uint16x8_t, uint16_t)
@*@emph{Form of expected instruction(s):} @code{vmls.i16 @var{q0}, @var{q0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int32x4_t vmlsq_n_s32 (int32x4_t, int32x4_t, int32_t)
@*@emph{Form of expected instruction(s):} @code{vmls.i32 @var{q0}, @var{q0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int16x8_t vmlsq_n_s16 (int16x8_t, int16x8_t, int16_t)
@*@emph{Form of expected instruction(s):} @code{vmls.i16 @var{q0}, @var{q0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item uint64x2_t vmlsl_n_u32 (uint64x2_t, uint32x2_t, uint32_t)
@*@emph{Form of expected instruction(s):} @code{vmlsl.u32 @var{q0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item uint32x4_t vmlsl_n_u16 (uint32x4_t, uint16x4_t, uint16_t)
@*@emph{Form of expected instruction(s):} @code{vmlsl.u16 @var{q0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int64x2_t vmlsl_n_s32 (int64x2_t, int32x2_t, int32_t)
@*@emph{Form of expected instruction(s):} @code{vmlsl.s32 @var{q0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int32x4_t vmlsl_n_s16 (int32x4_t, int16x4_t, int16_t)
@*@emph{Form of expected instruction(s):} @code{vmlsl.s16 @var{q0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int64x2_t vqdmlsl_n_s32 (int64x2_t, int32x2_t, int32_t)
@*@emph{Form of expected instruction(s):} @code{vqdmlsl.s32 @var{q0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize


@itemize @bullet
@item int32x4_t vqdmlsl_n_s16 (int32x4_t, int16x4_t, int16_t)
@*@emph{Form of expected instruction(s):} @code{vqdmlsl.s16 @var{q0}, @var{d0}, @var{d0}[@var{0}]}
@end itemize




@subsubsection Vector extract

@itemize @bullet
@item poly64x1_t vext_p64 (poly64x1_t, poly64x1_t, const int)
@*@emph{Form of expected instruction(s):} @code{vext.64 @var{d0}, @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint32x2_t vext_u32 (uint32x2_t, uint32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vext.32 @var{d0}, @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint16x4_t vext_u16 (uint16x4_t, uint16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vext.16 @var{d0}, @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint8x8_t vext_u8 (uint8x8_t, uint8x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vext.8 @var{d0}, @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item int32x2_t vext_s32 (int32x2_t, int32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vext.32 @var{d0}, @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item int16x4_t vext_s16 (int16x4_t, int16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vext.16 @var{d0}, @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item int8x8_t vext_s8 (int8x8_t, int8x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vext.8 @var{d0}, @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint64x1_t vext_u64 (uint64x1_t, uint64x1_t, const int)
@*@emph{Form of expected instruction(s):} @code{vext.64 @var{d0}, @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item int64x1_t vext_s64 (int64x1_t, int64x1_t, const int)
@*@emph{Form of expected instruction(s):} @code{vext.64 @var{d0}, @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item float32x2_t vext_f32 (float32x2_t, float32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vext.32 @var{d0}, @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item poly16x4_t vext_p16 (poly16x4_t, poly16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vext.16 @var{d0}, @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item poly8x8_t vext_p8 (poly8x8_t, poly8x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vext.8 @var{d0}, @var{d0}, @var{d0}, #@var{0}}
@end itemize


@itemize @bullet
@item poly64x2_t vextq_p64 (poly64x2_t, poly64x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vext.64 @var{q0}, @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint32x4_t vextq_u32 (uint32x4_t, uint32x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vext.32 @var{q0}, @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint16x8_t vextq_u16 (uint16x8_t, uint16x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vext.16 @var{q0}, @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint8x16_t vextq_u8 (uint8x16_t, uint8x16_t, const int)
@*@emph{Form of expected instruction(s):} @code{vext.8 @var{q0}, @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item int32x4_t vextq_s32 (int32x4_t, int32x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vext.32 @var{q0}, @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item int16x8_t vextq_s16 (int16x8_t, int16x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vext.16 @var{q0}, @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item int8x16_t vextq_s8 (int8x16_t, int8x16_t, const int)
@*@emph{Form of expected instruction(s):} @code{vext.8 @var{q0}, @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item uint64x2_t vextq_u64 (uint64x2_t, uint64x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vext.64 @var{q0}, @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item int64x2_t vextq_s64 (int64x2_t, int64x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vext.64 @var{q0}, @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item float32x4_t vextq_f32 (float32x4_t, float32x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vext.32 @var{q0}, @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item poly16x8_t vextq_p16 (poly16x8_t, poly16x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vext.16 @var{q0}, @var{q0}, @var{q0}, #@var{0}}
@end itemize


@itemize @bullet
@item poly8x16_t vextq_p8 (poly8x16_t, poly8x16_t, const int)
@*@emph{Form of expected instruction(s):} @code{vext.8 @var{q0}, @var{q0}, @var{q0}, #@var{0}}
@end itemize




@subsubsection Reverse elements

@itemize @bullet
@item uint32x2_t vrev64_u32 (uint32x2_t)
@*@emph{Form of expected instruction(s):} @code{vrev64.32 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint16x4_t vrev64_u16 (uint16x4_t)
@*@emph{Form of expected instruction(s):} @code{vrev64.16 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint8x8_t vrev64_u8 (uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vrev64.8 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int32x2_t vrev64_s32 (int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vrev64.32 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int16x4_t vrev64_s16 (int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vrev64.16 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int8x8_t vrev64_s8 (int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vrev64.8 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item float32x2_t vrev64_f32 (float32x2_t)
@*@emph{Form of expected instruction(s):} @code{vrev64.32 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item poly16x4_t vrev64_p16 (poly16x4_t)
@*@emph{Form of expected instruction(s):} @code{vrev64.16 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item poly8x8_t vrev64_p8 (poly8x8_t)
@*@emph{Form of expected instruction(s):} @code{vrev64.8 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint32x4_t vrev64q_u32 (uint32x4_t)
@*@emph{Form of expected instruction(s):} @code{vrev64.32 @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint16x8_t vrev64q_u16 (uint16x8_t)
@*@emph{Form of expected instruction(s):} @code{vrev64.16 @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint8x16_t vrev64q_u8 (uint8x16_t)
@*@emph{Form of expected instruction(s):} @code{vrev64.8 @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int32x4_t vrev64q_s32 (int32x4_t)
@*@emph{Form of expected instruction(s):} @code{vrev64.32 @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int16x8_t vrev64q_s16 (int16x8_t)
@*@emph{Form of expected instruction(s):} @code{vrev64.16 @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int8x16_t vrev64q_s8 (int8x16_t)
@*@emph{Form of expected instruction(s):} @code{vrev64.8 @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item float32x4_t vrev64q_f32 (float32x4_t)
@*@emph{Form of expected instruction(s):} @code{vrev64.32 @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item poly16x8_t vrev64q_p16 (poly16x8_t)
@*@emph{Form of expected instruction(s):} @code{vrev64.16 @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item poly8x16_t vrev64q_p8 (poly8x16_t)
@*@emph{Form of expected instruction(s):} @code{vrev64.8 @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint16x4_t vrev32_u16 (uint16x4_t)
@*@emph{Form of expected instruction(s):} @code{vrev32.16 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int16x4_t vrev32_s16 (int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vrev32.16 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint8x8_t vrev32_u8 (uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vrev32.8 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int8x8_t vrev32_s8 (int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vrev32.8 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item poly16x4_t vrev32_p16 (poly16x4_t)
@*@emph{Form of expected instruction(s):} @code{vrev32.16 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item poly8x8_t vrev32_p8 (poly8x8_t)
@*@emph{Form of expected instruction(s):} @code{vrev32.8 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint16x8_t vrev32q_u16 (uint16x8_t)
@*@emph{Form of expected instruction(s):} @code{vrev32.16 @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int16x8_t vrev32q_s16 (int16x8_t)
@*@emph{Form of expected instruction(s):} @code{vrev32.16 @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint8x16_t vrev32q_u8 (uint8x16_t)
@*@emph{Form of expected instruction(s):} @code{vrev32.8 @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int8x16_t vrev32q_s8 (int8x16_t)
@*@emph{Form of expected instruction(s):} @code{vrev32.8 @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item poly16x8_t vrev32q_p16 (poly16x8_t)
@*@emph{Form of expected instruction(s):} @code{vrev32.16 @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item poly8x16_t vrev32q_p8 (poly8x16_t)
@*@emph{Form of expected instruction(s):} @code{vrev32.8 @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint8x8_t vrev16_u8 (uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vrev16.8 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int8x8_t vrev16_s8 (int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vrev16.8 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item poly8x8_t vrev16_p8 (poly8x8_t)
@*@emph{Form of expected instruction(s):} @code{vrev16.8 @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint8x16_t vrev16q_u8 (uint8x16_t)
@*@emph{Form of expected instruction(s):} @code{vrev16.8 @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int8x16_t vrev16q_s8 (int8x16_t)
@*@emph{Form of expected instruction(s):} @code{vrev16.8 @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item poly8x16_t vrev16q_p8 (poly8x16_t)
@*@emph{Form of expected instruction(s):} @code{vrev16.8 @var{q0}, @var{q0}}
@end itemize




@subsubsection Bit selection

@itemize @bullet
@item poly64x1_t vbsl_p64 (uint64x1_t, poly64x1_t, poly64x1_t)
@*@emph{Form of expected instruction(s):} @code{vbsl @var{d0}, @var{d0}, @var{d0}} @emph{or} @code{vbit @var{d0}, @var{d0}, @var{d0}} @emph{or} @code{vbif @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint32x2_t vbsl_u32 (uint32x2_t, uint32x2_t, uint32x2_t)
@*@emph{Form of expected instruction(s):} @code{vbsl @var{d0}, @var{d0}, @var{d0}} @emph{or} @code{vbit @var{d0}, @var{d0}, @var{d0}} @emph{or} @code{vbif @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint16x4_t vbsl_u16 (uint16x4_t, uint16x4_t, uint16x4_t)
@*@emph{Form of expected instruction(s):} @code{vbsl @var{d0}, @var{d0}, @var{d0}} @emph{or} @code{vbit @var{d0}, @var{d0}, @var{d0}} @emph{or} @code{vbif @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint8x8_t vbsl_u8 (uint8x8_t, uint8x8_t, uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vbsl @var{d0}, @var{d0}, @var{d0}} @emph{or} @code{vbit @var{d0}, @var{d0}, @var{d0}} @emph{or} @code{vbif @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int32x2_t vbsl_s32 (uint32x2_t, int32x2_t, int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vbsl @var{d0}, @var{d0}, @var{d0}} @emph{or} @code{vbit @var{d0}, @var{d0}, @var{d0}} @emph{or} @code{vbif @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int16x4_t vbsl_s16 (uint16x4_t, int16x4_t, int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vbsl @var{d0}, @var{d0}, @var{d0}} @emph{or} @code{vbit @var{d0}, @var{d0}, @var{d0}} @emph{or} @code{vbif @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int8x8_t vbsl_s8 (uint8x8_t, int8x8_t, int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vbsl @var{d0}, @var{d0}, @var{d0}} @emph{or} @code{vbit @var{d0}, @var{d0}, @var{d0}} @emph{or} @code{vbif @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint64x1_t vbsl_u64 (uint64x1_t, uint64x1_t, uint64x1_t)
@*@emph{Form of expected instruction(s):} @code{vbsl @var{d0}, @var{d0}, @var{d0}} @emph{or} @code{vbit @var{d0}, @var{d0}, @var{d0}} @emph{or} @code{vbif @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int64x1_t vbsl_s64 (uint64x1_t, int64x1_t, int64x1_t)
@*@emph{Form of expected instruction(s):} @code{vbsl @var{d0}, @var{d0}, @var{d0}} @emph{or} @code{vbit @var{d0}, @var{d0}, @var{d0}} @emph{or} @code{vbif @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item float32x2_t vbsl_f32 (uint32x2_t, float32x2_t, float32x2_t)
@*@emph{Form of expected instruction(s):} @code{vbsl @var{d0}, @var{d0}, @var{d0}} @emph{or} @code{vbit @var{d0}, @var{d0}, @var{d0}} @emph{or} @code{vbif @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item poly16x4_t vbsl_p16 (uint16x4_t, poly16x4_t, poly16x4_t)
@*@emph{Form of expected instruction(s):} @code{vbsl @var{d0}, @var{d0}, @var{d0}} @emph{or} @code{vbit @var{d0}, @var{d0}, @var{d0}} @emph{or} @code{vbif @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item poly8x8_t vbsl_p8 (uint8x8_t, poly8x8_t, poly8x8_t)
@*@emph{Form of expected instruction(s):} @code{vbsl @var{d0}, @var{d0}, @var{d0}} @emph{or} @code{vbit @var{d0}, @var{d0}, @var{d0}} @emph{or} @code{vbif @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item poly64x2_t vbslq_p64 (uint64x2_t, poly64x2_t, poly64x2_t)
@*@emph{Form of expected instruction(s):} @code{vbsl @var{q0}, @var{q0}, @var{q0}} @emph{or} @code{vbit @var{q0}, @var{q0}, @var{q0}} @emph{or} @code{vbif @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint32x4_t vbslq_u32 (uint32x4_t, uint32x4_t, uint32x4_t)
@*@emph{Form of expected instruction(s):} @code{vbsl @var{q0}, @var{q0}, @var{q0}} @emph{or} @code{vbit @var{q0}, @var{q0}, @var{q0}} @emph{or} @code{vbif @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint16x8_t vbslq_u16 (uint16x8_t, uint16x8_t, uint16x8_t)
@*@emph{Form of expected instruction(s):} @code{vbsl @var{q0}, @var{q0}, @var{q0}} @emph{or} @code{vbit @var{q0}, @var{q0}, @var{q0}} @emph{or} @code{vbif @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint8x16_t vbslq_u8 (uint8x16_t, uint8x16_t, uint8x16_t)
@*@emph{Form of expected instruction(s):} @code{vbsl @var{q0}, @var{q0}, @var{q0}} @emph{or} @code{vbit @var{q0}, @var{q0}, @var{q0}} @emph{or} @code{vbif @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int32x4_t vbslq_s32 (uint32x4_t, int32x4_t, int32x4_t)
@*@emph{Form of expected instruction(s):} @code{vbsl @var{q0}, @var{q0}, @var{q0}} @emph{or} @code{vbit @var{q0}, @var{q0}, @var{q0}} @emph{or} @code{vbif @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int16x8_t vbslq_s16 (uint16x8_t, int16x8_t, int16x8_t)
@*@emph{Form of expected instruction(s):} @code{vbsl @var{q0}, @var{q0}, @var{q0}} @emph{or} @code{vbit @var{q0}, @var{q0}, @var{q0}} @emph{or} @code{vbif @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int8x16_t vbslq_s8 (uint8x16_t, int8x16_t, int8x16_t)
@*@emph{Form of expected instruction(s):} @code{vbsl @var{q0}, @var{q0}, @var{q0}} @emph{or} @code{vbit @var{q0}, @var{q0}, @var{q0}} @emph{or} @code{vbif @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint64x2_t vbslq_u64 (uint64x2_t, uint64x2_t, uint64x2_t)
@*@emph{Form of expected instruction(s):} @code{vbsl @var{q0}, @var{q0}, @var{q0}} @emph{or} @code{vbit @var{q0}, @var{q0}, @var{q0}} @emph{or} @code{vbif @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int64x2_t vbslq_s64 (uint64x2_t, int64x2_t, int64x2_t)
@*@emph{Form of expected instruction(s):} @code{vbsl @var{q0}, @var{q0}, @var{q0}} @emph{or} @code{vbit @var{q0}, @var{q0}, @var{q0}} @emph{or} @code{vbif @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item float32x4_t vbslq_f32 (uint32x4_t, float32x4_t, float32x4_t)
@*@emph{Form of expected instruction(s):} @code{vbsl @var{q0}, @var{q0}, @var{q0}} @emph{or} @code{vbit @var{q0}, @var{q0}, @var{q0}} @emph{or} @code{vbif @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item poly16x8_t vbslq_p16 (uint16x8_t, poly16x8_t, poly16x8_t)
@*@emph{Form of expected instruction(s):} @code{vbsl @var{q0}, @var{q0}, @var{q0}} @emph{or} @code{vbit @var{q0}, @var{q0}, @var{q0}} @emph{or} @code{vbif @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item poly8x16_t vbslq_p8 (uint8x16_t, poly8x16_t, poly8x16_t)
@*@emph{Form of expected instruction(s):} @code{vbsl @var{q0}, @var{q0}, @var{q0}} @emph{or} @code{vbit @var{q0}, @var{q0}, @var{q0}} @emph{or} @code{vbif @var{q0}, @var{q0}, @var{q0}}
@end itemize




@subsubsection Transpose elements

@itemize @bullet
@item uint16x4x2_t vtrn_u16 (uint16x4_t, uint16x4_t)
@*@emph{Form of expected instruction(s):} @code{vtrn.16 @var{d0}, @var{d1}}
@end itemize


@itemize @bullet
@item uint8x8x2_t vtrn_u8 (uint8x8_t, uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vtrn.8 @var{d0}, @var{d1}}
@end itemize


@itemize @bullet
@item int16x4x2_t vtrn_s16 (int16x4_t, int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vtrn.16 @var{d0}, @var{d1}}
@end itemize


@itemize @bullet
@item int8x8x2_t vtrn_s8 (int8x8_t, int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vtrn.8 @var{d0}, @var{d1}}
@end itemize


@itemize @bullet
@item poly16x4x2_t vtrn_p16 (poly16x4_t, poly16x4_t)
@*@emph{Form of expected instruction(s):} @code{vtrn.16 @var{d0}, @var{d1}}
@end itemize


@itemize @bullet
@item poly8x8x2_t vtrn_p8 (poly8x8_t, poly8x8_t)
@*@emph{Form of expected instruction(s):} @code{vtrn.8 @var{d0}, @var{d1}}
@end itemize


@itemize @bullet
@item float32x2x2_t vtrn_f32 (float32x2_t, float32x2_t)
@*@emph{Form of expected instruction(s):} @code{vuzp.32 @var{d0}, @var{d1}}
@end itemize


@itemize @bullet
@item uint32x2x2_t vtrn_u32 (uint32x2_t, uint32x2_t)
@*@emph{Form of expected instruction(s):} @code{vuzp.32 @var{d0}, @var{d1}}
@end itemize


@itemize @bullet
@item int32x2x2_t vtrn_s32 (int32x2_t, int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vuzp.32 @var{d0}, @var{d1}}
@end itemize


@itemize @bullet
@item uint32x4x2_t vtrnq_u32 (uint32x4_t, uint32x4_t)
@*@emph{Form of expected instruction(s):} @code{vtrn.32 @var{q0}, @var{q1}}
@end itemize


@itemize @bullet
@item uint16x8x2_t vtrnq_u16 (uint16x8_t, uint16x8_t)
@*@emph{Form of expected instruction(s):} @code{vtrn.16 @var{q0}, @var{q1}}
@end itemize


@itemize @bullet
@item uint8x16x2_t vtrnq_u8 (uint8x16_t, uint8x16_t)
@*@emph{Form of expected instruction(s):} @code{vtrn.8 @var{q0}, @var{q1}}
@end itemize


@itemize @bullet
@item int32x4x2_t vtrnq_s32 (int32x4_t, int32x4_t)
@*@emph{Form of expected instruction(s):} @code{vtrn.32 @var{q0}, @var{q1}}
@end itemize


@itemize @bullet
@item int16x8x2_t vtrnq_s16 (int16x8_t, int16x8_t)
@*@emph{Form of expected instruction(s):} @code{vtrn.16 @var{q0}, @var{q1}}
@end itemize


@itemize @bullet
@item int8x16x2_t vtrnq_s8 (int8x16_t, int8x16_t)
@*@emph{Form of expected instruction(s):} @code{vtrn.8 @var{q0}, @var{q1}}
@end itemize


@itemize @bullet
@item float32x4x2_t vtrnq_f32 (float32x4_t, float32x4_t)
@*@emph{Form of expected instruction(s):} @code{vtrn.32 @var{q0}, @var{q1}}
@end itemize


@itemize @bullet
@item poly16x8x2_t vtrnq_p16 (poly16x8_t, poly16x8_t)
@*@emph{Form of expected instruction(s):} @code{vtrn.16 @var{q0}, @var{q1}}
@end itemize


@itemize @bullet
@item poly8x16x2_t vtrnq_p8 (poly8x16_t, poly8x16_t)
@*@emph{Form of expected instruction(s):} @code{vtrn.8 @var{q0}, @var{q1}}
@end itemize




@subsubsection Zip elements

@itemize @bullet
@item uint16x4x2_t vzip_u16 (uint16x4_t, uint16x4_t)
@*@emph{Form of expected instruction(s):} @code{vzip.16 @var{d0}, @var{d1}}
@end itemize


@itemize @bullet
@item uint8x8x2_t vzip_u8 (uint8x8_t, uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vzip.8 @var{d0}, @var{d1}}
@end itemize


@itemize @bullet
@item int16x4x2_t vzip_s16 (int16x4_t, int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vzip.16 @var{d0}, @var{d1}}
@end itemize


@itemize @bullet
@item int8x8x2_t vzip_s8 (int8x8_t, int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vzip.8 @var{d0}, @var{d1}}
@end itemize


@itemize @bullet
@item poly16x4x2_t vzip_p16 (poly16x4_t, poly16x4_t)
@*@emph{Form of expected instruction(s):} @code{vzip.16 @var{d0}, @var{d1}}
@end itemize


@itemize @bullet
@item poly8x8x2_t vzip_p8 (poly8x8_t, poly8x8_t)
@*@emph{Form of expected instruction(s):} @code{vzip.8 @var{d0}, @var{d1}}
@end itemize


@itemize @bullet
@item float32x2x2_t vzip_f32 (float32x2_t, float32x2_t)
@*@emph{Form of expected instruction(s):} @code{vuzp.32 @var{d0}, @var{d1}}
@end itemize


@itemize @bullet
@item uint32x2x2_t vzip_u32 (uint32x2_t, uint32x2_t)
@*@emph{Form of expected instruction(s):} @code{vuzp.32 @var{d0}, @var{d1}}
@end itemize


@itemize @bullet
@item int32x2x2_t vzip_s32 (int32x2_t, int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vuzp.32 @var{d0}, @var{d1}}
@end itemize


@itemize @bullet
@item uint32x4x2_t vzipq_u32 (uint32x4_t, uint32x4_t)
@*@emph{Form of expected instruction(s):} @code{vzip.32 @var{q0}, @var{q1}}
@end itemize


@itemize @bullet
@item uint16x8x2_t vzipq_u16 (uint16x8_t, uint16x8_t)
@*@emph{Form of expected instruction(s):} @code{vzip.16 @var{q0}, @var{q1}}
@end itemize


@itemize @bullet
@item uint8x16x2_t vzipq_u8 (uint8x16_t, uint8x16_t)
@*@emph{Form of expected instruction(s):} @code{vzip.8 @var{q0}, @var{q1}}
@end itemize


@itemize @bullet
@item int32x4x2_t vzipq_s32 (int32x4_t, int32x4_t)
@*@emph{Form of expected instruction(s):} @code{vzip.32 @var{q0}, @var{q1}}
@end itemize


@itemize @bullet
@item int16x8x2_t vzipq_s16 (int16x8_t, int16x8_t)
@*@emph{Form of expected instruction(s):} @code{vzip.16 @var{q0}, @var{q1}}
@end itemize


@itemize @bullet
@item int8x16x2_t vzipq_s8 (int8x16_t, int8x16_t)
@*@emph{Form of expected instruction(s):} @code{vzip.8 @var{q0}, @var{q1}}
@end itemize


@itemize @bullet
@item float32x4x2_t vzipq_f32 (float32x4_t, float32x4_t)
@*@emph{Form of expected instruction(s):} @code{vzip.32 @var{q0}, @var{q1}}
@end itemize


@itemize @bullet
@item poly16x8x2_t vzipq_p16 (poly16x8_t, poly16x8_t)
@*@emph{Form of expected instruction(s):} @code{vzip.16 @var{q0}, @var{q1}}
@end itemize


@itemize @bullet
@item poly8x16x2_t vzipq_p8 (poly8x16_t, poly8x16_t)
@*@emph{Form of expected instruction(s):} @code{vzip.8 @var{q0}, @var{q1}}
@end itemize




@subsubsection Unzip elements

@itemize @bullet
@item uint32x2x2_t vuzp_u32 (uint32x2_t, uint32x2_t)
@*@emph{Form of expected instruction(s):} @code{vuzp.32 @var{d0}, @var{d1}}
@end itemize


@itemize @bullet
@item uint16x4x2_t vuzp_u16 (uint16x4_t, uint16x4_t)
@*@emph{Form of expected instruction(s):} @code{vuzp.16 @var{d0}, @var{d1}}
@end itemize


@itemize @bullet
@item uint8x8x2_t vuzp_u8 (uint8x8_t, uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vuzp.8 @var{d0}, @var{d1}}
@end itemize


@itemize @bullet
@item int32x2x2_t vuzp_s32 (int32x2_t, int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vuzp.32 @var{d0}, @var{d1}}
@end itemize


@itemize @bullet
@item int16x4x2_t vuzp_s16 (int16x4_t, int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vuzp.16 @var{d0}, @var{d1}}
@end itemize


@itemize @bullet
@item int8x8x2_t vuzp_s8 (int8x8_t, int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vuzp.8 @var{d0}, @var{d1}}
@end itemize


@itemize @bullet
@item float32x2x2_t vuzp_f32 (float32x2_t, float32x2_t)
@*@emph{Form of expected instruction(s):} @code{vuzp.32 @var{d0}, @var{d1}}
@end itemize


@itemize @bullet
@item poly16x4x2_t vuzp_p16 (poly16x4_t, poly16x4_t)
@*@emph{Form of expected instruction(s):} @code{vuzp.16 @var{d0}, @var{d1}}
@end itemize


@itemize @bullet
@item poly8x8x2_t vuzp_p8 (poly8x8_t, poly8x8_t)
@*@emph{Form of expected instruction(s):} @code{vuzp.8 @var{d0}, @var{d1}}
@end itemize


@itemize @bullet
@item uint32x4x2_t vuzpq_u32 (uint32x4_t, uint32x4_t)
@*@emph{Form of expected instruction(s):} @code{vuzp.32 @var{q0}, @var{q1}}
@end itemize


@itemize @bullet
@item uint16x8x2_t vuzpq_u16 (uint16x8_t, uint16x8_t)
@*@emph{Form of expected instruction(s):} @code{vuzp.16 @var{q0}, @var{q1}}
@end itemize


@itemize @bullet
@item uint8x16x2_t vuzpq_u8 (uint8x16_t, uint8x16_t)
@*@emph{Form of expected instruction(s):} @code{vuzp.8 @var{q0}, @var{q1}}
@end itemize


@itemize @bullet
@item int32x4x2_t vuzpq_s32 (int32x4_t, int32x4_t)
@*@emph{Form of expected instruction(s):} @code{vuzp.32 @var{q0}, @var{q1}}
@end itemize


@itemize @bullet
@item int16x8x2_t vuzpq_s16 (int16x8_t, int16x8_t)
@*@emph{Form of expected instruction(s):} @code{vuzp.16 @var{q0}, @var{q1}}
@end itemize


@itemize @bullet
@item int8x16x2_t vuzpq_s8 (int8x16_t, int8x16_t)
@*@emph{Form of expected instruction(s):} @code{vuzp.8 @var{q0}, @var{q1}}
@end itemize


@itemize @bullet
@item float32x4x2_t vuzpq_f32 (float32x4_t, float32x4_t)
@*@emph{Form of expected instruction(s):} @code{vuzp.32 @var{q0}, @var{q1}}
@end itemize


@itemize @bullet
@item poly16x8x2_t vuzpq_p16 (poly16x8_t, poly16x8_t)
@*@emph{Form of expected instruction(s):} @code{vuzp.16 @var{q0}, @var{q1}}
@end itemize


@itemize @bullet
@item poly8x16x2_t vuzpq_p8 (poly8x16_t, poly8x16_t)
@*@emph{Form of expected instruction(s):} @code{vuzp.8 @var{q0}, @var{q1}}
@end itemize




@subsubsection Element/structure loads, VLD1 variants

@itemize @bullet
@item poly64x1_t vld1_p64 (const poly64_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.64 @{@var{d0}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint32x2_t vld1_u32 (const uint32_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.32 @{@var{d0}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint16x4_t vld1_u16 (const uint16_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.16 @{@var{d0}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint8x8_t vld1_u8 (const uint8_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.8 @{@var{d0}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int32x2_t vld1_s32 (const int32_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.32 @{@var{d0}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int16x4_t vld1_s16 (const int16_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.16 @{@var{d0}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int8x8_t vld1_s8 (const int8_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.8 @{@var{d0}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint64x1_t vld1_u64 (const uint64_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.64 @{@var{d0}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int64x1_t vld1_s64 (const int64_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.64 @{@var{d0}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item float32x2_t vld1_f32 (const float32_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.32 @{@var{d0}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item poly16x4_t vld1_p16 (const poly16_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.16 @{@var{d0}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item poly8x8_t vld1_p8 (const poly8_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.8 @{@var{d0}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item poly64x2_t vld1q_p64 (const poly64_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.64 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint32x4_t vld1q_u32 (const uint32_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.32 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint16x8_t vld1q_u16 (const uint16_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.16 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint8x16_t vld1q_u8 (const uint8_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.8 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int32x4_t vld1q_s32 (const int32_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.32 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int16x8_t vld1q_s16 (const int16_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.16 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int8x16_t vld1q_s8 (const int8_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.8 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint64x2_t vld1q_u64 (const uint64_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.64 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int64x2_t vld1q_s64 (const int64_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.64 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item float32x4_t vld1q_f32 (const float32_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.32 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item poly16x8_t vld1q_p16 (const poly16_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.16 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item poly8x16_t vld1q_p8 (const poly8_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.8 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint32x2_t vld1_lane_u32 (const uint32_t *, uint32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld1.32 @{@var{d0}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint16x4_t vld1_lane_u16 (const uint16_t *, uint16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld1.16 @{@var{d0}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint8x8_t vld1_lane_u8 (const uint8_t *, uint8x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld1.8 @{@var{d0}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int32x2_t vld1_lane_s32 (const int32_t *, int32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld1.32 @{@var{d0}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int16x4_t vld1_lane_s16 (const int16_t *, int16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld1.16 @{@var{d0}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int8x8_t vld1_lane_s8 (const int8_t *, int8x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld1.8 @{@var{d0}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item float32x2_t vld1_lane_f32 (const float32_t *, float32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld1.32 @{@var{d0}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item poly16x4_t vld1_lane_p16 (const poly16_t *, poly16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld1.16 @{@var{d0}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item poly8x8_t vld1_lane_p8 (const poly8_t *, poly8x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld1.8 @{@var{d0}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item poly64x1_t vld1_lane_p64 (const poly64_t *, poly64x1_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld1.64 @{@var{d0}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint64x1_t vld1_lane_u64 (const uint64_t *, uint64x1_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld1.64 @{@var{d0}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int64x1_t vld1_lane_s64 (const int64_t *, int64x1_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld1.64 @{@var{d0}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint32x4_t vld1q_lane_u32 (const uint32_t *, uint32x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld1.32 @{@var{d0}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint16x8_t vld1q_lane_u16 (const uint16_t *, uint16x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld1.16 @{@var{d0}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint8x16_t vld1q_lane_u8 (const uint8_t *, uint8x16_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld1.8 @{@var{d0}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int32x4_t vld1q_lane_s32 (const int32_t *, int32x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld1.32 @{@var{d0}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int16x8_t vld1q_lane_s16 (const int16_t *, int16x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld1.16 @{@var{d0}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int8x16_t vld1q_lane_s8 (const int8_t *, int8x16_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld1.8 @{@var{d0}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item float32x4_t vld1q_lane_f32 (const float32_t *, float32x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld1.32 @{@var{d0}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item poly16x8_t vld1q_lane_p16 (const poly16_t *, poly16x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld1.16 @{@var{d0}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item poly8x16_t vld1q_lane_p8 (const poly8_t *, poly8x16_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld1.8 @{@var{d0}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item poly64x2_t vld1q_lane_p64 (const poly64_t *, poly64x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld1.64 @{@var{d0}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint64x2_t vld1q_lane_u64 (const uint64_t *, uint64x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld1.64 @{@var{d0}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int64x2_t vld1q_lane_s64 (const int64_t *, int64x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld1.64 @{@var{d0}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint32x2_t vld1_dup_u32 (const uint32_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.32 @{@var{d0}[]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint16x4_t vld1_dup_u16 (const uint16_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.16 @{@var{d0}[]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint8x8_t vld1_dup_u8 (const uint8_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.8 @{@var{d0}[]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int32x2_t vld1_dup_s32 (const int32_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.32 @{@var{d0}[]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int16x4_t vld1_dup_s16 (const int16_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.16 @{@var{d0}[]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int8x8_t vld1_dup_s8 (const int8_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.8 @{@var{d0}[]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item float32x2_t vld1_dup_f32 (const float32_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.32 @{@var{d0}[]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item poly16x4_t vld1_dup_p16 (const poly16_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.16 @{@var{d0}[]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item poly8x8_t vld1_dup_p8 (const poly8_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.8 @{@var{d0}[]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item poly64x1_t vld1_dup_p64 (const poly64_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.64 @{@var{d0}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint64x1_t vld1_dup_u64 (const uint64_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.64 @{@var{d0}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int64x1_t vld1_dup_s64 (const int64_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.64 @{@var{d0}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint32x4_t vld1q_dup_u32 (const uint32_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.32 @{@var{d0}[], @var{d1}[]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint16x8_t vld1q_dup_u16 (const uint16_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.16 @{@var{d0}[], @var{d1}[]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint8x16_t vld1q_dup_u8 (const uint8_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.8 @{@var{d0}[], @var{d1}[]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int32x4_t vld1q_dup_s32 (const int32_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.32 @{@var{d0}[], @var{d1}[]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int16x8_t vld1q_dup_s16 (const int16_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.16 @{@var{d0}[], @var{d1}[]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int8x16_t vld1q_dup_s8 (const int8_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.8 @{@var{d0}[], @var{d1}[]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item float32x4_t vld1q_dup_f32 (const float32_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.32 @{@var{d0}[], @var{d1}[]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item poly16x8_t vld1q_dup_p16 (const poly16_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.16 @{@var{d0}[], @var{d1}[]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item poly8x16_t vld1q_dup_p8 (const poly8_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.8 @{@var{d0}[], @var{d1}[]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item poly64x2_t vld1q_dup_p64 (const poly64_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.64 @{@var{d0}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint64x2_t vld1q_dup_u64 (const uint64_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.64 @{@var{d0}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int64x2_t vld1q_dup_s64 (const int64_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.64 @{@var{d0}@}, [@var{r0}]}
@end itemize




@subsubsection Element/structure stores, VST1 variants

@itemize @bullet
@item void vst1_p64 (poly64_t *, poly64x1_t)
@*@emph{Form of expected instruction(s):} @code{vst1.64 @{@var{d0}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst1_u32 (uint32_t *, uint32x2_t)
@*@emph{Form of expected instruction(s):} @code{vst1.32 @{@var{d0}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst1_u16 (uint16_t *, uint16x4_t)
@*@emph{Form of expected instruction(s):} @code{vst1.16 @{@var{d0}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst1_u8 (uint8_t *, uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vst1.8 @{@var{d0}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst1_s32 (int32_t *, int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vst1.32 @{@var{d0}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst1_s16 (int16_t *, int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vst1.16 @{@var{d0}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst1_s8 (int8_t *, int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vst1.8 @{@var{d0}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst1_u64 (uint64_t *, uint64x1_t)
@*@emph{Form of expected instruction(s):} @code{vst1.64 @{@var{d0}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst1_s64 (int64_t *, int64x1_t)
@*@emph{Form of expected instruction(s):} @code{vst1.64 @{@var{d0}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst1_f32 (float32_t *, float32x2_t)
@*@emph{Form of expected instruction(s):} @code{vst1.32 @{@var{d0}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst1_p16 (poly16_t *, poly16x4_t)
@*@emph{Form of expected instruction(s):} @code{vst1.16 @{@var{d0}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst1_p8 (poly8_t *, poly8x8_t)
@*@emph{Form of expected instruction(s):} @code{vst1.8 @{@var{d0}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst1q_p64 (poly64_t *, poly64x2_t)
@*@emph{Form of expected instruction(s):} @code{vst1.64 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst1q_u32 (uint32_t *, uint32x4_t)
@*@emph{Form of expected instruction(s):} @code{vst1.32 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst1q_u16 (uint16_t *, uint16x8_t)
@*@emph{Form of expected instruction(s):} @code{vst1.16 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst1q_u8 (uint8_t *, uint8x16_t)
@*@emph{Form of expected instruction(s):} @code{vst1.8 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst1q_s32 (int32_t *, int32x4_t)
@*@emph{Form of expected instruction(s):} @code{vst1.32 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst1q_s16 (int16_t *, int16x8_t)
@*@emph{Form of expected instruction(s):} @code{vst1.16 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst1q_s8 (int8_t *, int8x16_t)
@*@emph{Form of expected instruction(s):} @code{vst1.8 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst1q_u64 (uint64_t *, uint64x2_t)
@*@emph{Form of expected instruction(s):} @code{vst1.64 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst1q_s64 (int64_t *, int64x2_t)
@*@emph{Form of expected instruction(s):} @code{vst1.64 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst1q_f32 (float32_t *, float32x4_t)
@*@emph{Form of expected instruction(s):} @code{vst1.32 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst1q_p16 (poly16_t *, poly16x8_t)
@*@emph{Form of expected instruction(s):} @code{vst1.16 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst1q_p8 (poly8_t *, poly8x16_t)
@*@emph{Form of expected instruction(s):} @code{vst1.8 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst1_lane_u32 (uint32_t *, uint32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst1.32 @{@var{d0}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst1_lane_u16 (uint16_t *, uint16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst1.16 @{@var{d0}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst1_lane_u8 (uint8_t *, uint8x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst1.8 @{@var{d0}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst1_lane_s32 (int32_t *, int32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst1.32 @{@var{d0}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst1_lane_s16 (int16_t *, int16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst1.16 @{@var{d0}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst1_lane_s8 (int8_t *, int8x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst1.8 @{@var{d0}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst1_lane_f32 (float32_t *, float32x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst1.32 @{@var{d0}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst1_lane_p16 (poly16_t *, poly16x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst1.16 @{@var{d0}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst1_lane_p8 (poly8_t *, poly8x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst1.8 @{@var{d0}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst1_lane_p64 (poly64_t *, poly64x1_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst1.64 @{@var{d0}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst1_lane_s64 (int64_t *, int64x1_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst1.64 @{@var{d0}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst1_lane_u64 (uint64_t *, uint64x1_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst1.64 @{@var{d0}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst1q_lane_u32 (uint32_t *, uint32x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst1.32 @{@var{d0}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst1q_lane_u16 (uint16_t *, uint16x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst1.16 @{@var{d0}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst1q_lane_u8 (uint8_t *, uint8x16_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst1.8 @{@var{d0}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst1q_lane_s32 (int32_t *, int32x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst1.32 @{@var{d0}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst1q_lane_s16 (int16_t *, int16x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst1.16 @{@var{d0}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst1q_lane_s8 (int8_t *, int8x16_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst1.8 @{@var{d0}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst1q_lane_f32 (float32_t *, float32x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst1.32 @{@var{d0}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst1q_lane_p16 (poly16_t *, poly16x8_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst1.16 @{@var{d0}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst1q_lane_p8 (poly8_t *, poly8x16_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst1.8 @{@var{d0}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst1q_lane_p64 (poly64_t *, poly64x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst1.64 @{@var{d0}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst1q_lane_s64 (int64_t *, int64x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst1.64 @{@var{d0}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst1q_lane_u64 (uint64_t *, uint64x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst1.64 @{@var{d0}@}, [@var{r0}]}
@end itemize




@subsubsection Element/structure loads, VLD2 variants

@itemize @bullet
@item uint32x2x2_t vld2_u32 (const uint32_t *)
@*@emph{Form of expected instruction(s):} @code{vld2.32 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint16x4x2_t vld2_u16 (const uint16_t *)
@*@emph{Form of expected instruction(s):} @code{vld2.16 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint8x8x2_t vld2_u8 (const uint8_t *)
@*@emph{Form of expected instruction(s):} @code{vld2.8 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int32x2x2_t vld2_s32 (const int32_t *)
@*@emph{Form of expected instruction(s):} @code{vld2.32 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int16x4x2_t vld2_s16 (const int16_t *)
@*@emph{Form of expected instruction(s):} @code{vld2.16 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int8x8x2_t vld2_s8 (const int8_t *)
@*@emph{Form of expected instruction(s):} @code{vld2.8 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item float32x2x2_t vld2_f32 (const float32_t *)
@*@emph{Form of expected instruction(s):} @code{vld2.32 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item poly16x4x2_t vld2_p16 (const poly16_t *)
@*@emph{Form of expected instruction(s):} @code{vld2.16 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item poly8x8x2_t vld2_p8 (const poly8_t *)
@*@emph{Form of expected instruction(s):} @code{vld2.8 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item poly64x1x2_t vld2_p64 (const poly64_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.64 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint64x1x2_t vld2_u64 (const uint64_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.64 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int64x1x2_t vld2_s64 (const int64_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.64 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint32x4x2_t vld2q_u32 (const uint32_t *)
@*@emph{Form of expected instruction(s):} @code{vld2.32 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint16x8x2_t vld2q_u16 (const uint16_t *)
@*@emph{Form of expected instruction(s):} @code{vld2.16 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint8x16x2_t vld2q_u8 (const uint8_t *)
@*@emph{Form of expected instruction(s):} @code{vld2.8 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int32x4x2_t vld2q_s32 (const int32_t *)
@*@emph{Form of expected instruction(s):} @code{vld2.32 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int16x8x2_t vld2q_s16 (const int16_t *)
@*@emph{Form of expected instruction(s):} @code{vld2.16 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int8x16x2_t vld2q_s8 (const int8_t *)
@*@emph{Form of expected instruction(s):} @code{vld2.8 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item float32x4x2_t vld2q_f32 (const float32_t *)
@*@emph{Form of expected instruction(s):} @code{vld2.32 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item poly16x8x2_t vld2q_p16 (const poly16_t *)
@*@emph{Form of expected instruction(s):} @code{vld2.16 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item poly8x16x2_t vld2q_p8 (const poly8_t *)
@*@emph{Form of expected instruction(s):} @code{vld2.8 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint32x2x2_t vld2_lane_u32 (const uint32_t *, uint32x2x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld2.32 @{@var{d0}[@var{0}], @var{d1}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint16x4x2_t vld2_lane_u16 (const uint16_t *, uint16x4x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld2.16 @{@var{d0}[@var{0}], @var{d1}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint8x8x2_t vld2_lane_u8 (const uint8_t *, uint8x8x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld2.8 @{@var{d0}[@var{0}], @var{d1}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int32x2x2_t vld2_lane_s32 (const int32_t *, int32x2x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld2.32 @{@var{d0}[@var{0}], @var{d1}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int16x4x2_t vld2_lane_s16 (const int16_t *, int16x4x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld2.16 @{@var{d0}[@var{0}], @var{d1}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int8x8x2_t vld2_lane_s8 (const int8_t *, int8x8x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld2.8 @{@var{d0}[@var{0}], @var{d1}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item float32x2x2_t vld2_lane_f32 (const float32_t *, float32x2x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld2.32 @{@var{d0}[@var{0}], @var{d1}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item poly16x4x2_t vld2_lane_p16 (const poly16_t *, poly16x4x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld2.16 @{@var{d0}[@var{0}], @var{d1}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item poly8x8x2_t vld2_lane_p8 (const poly8_t *, poly8x8x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld2.8 @{@var{d0}[@var{0}], @var{d1}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int32x4x2_t vld2q_lane_s32 (const int32_t *, int32x4x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld2.32 @{@var{d0}[@var{0}], @var{d1}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int16x8x2_t vld2q_lane_s16 (const int16_t *, int16x8x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld2.16 @{@var{d0}[@var{0}], @var{d1}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint32x4x2_t vld2q_lane_u32 (const uint32_t *, uint32x4x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld2.32 @{@var{d0}[@var{0}], @var{d1}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint16x8x2_t vld2q_lane_u16 (const uint16_t *, uint16x8x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld2.16 @{@var{d0}[@var{0}], @var{d1}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item float32x4x2_t vld2q_lane_f32 (const float32_t *, float32x4x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld2.32 @{@var{d0}[@var{0}], @var{d1}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item poly16x8x2_t vld2q_lane_p16 (const poly16_t *, poly16x8x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld2.16 @{@var{d0}[@var{0}], @var{d1}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint32x2x2_t vld2_dup_u32 (const uint32_t *)
@*@emph{Form of expected instruction(s):} @code{vld2.32 @{@var{d0}[], @var{d1}[]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint16x4x2_t vld2_dup_u16 (const uint16_t *)
@*@emph{Form of expected instruction(s):} @code{vld2.16 @{@var{d0}[], @var{d1}[]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint8x8x2_t vld2_dup_u8 (const uint8_t *)
@*@emph{Form of expected instruction(s):} @code{vld2.8 @{@var{d0}[], @var{d1}[]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int32x2x2_t vld2_dup_s32 (const int32_t *)
@*@emph{Form of expected instruction(s):} @code{vld2.32 @{@var{d0}[], @var{d1}[]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int16x4x2_t vld2_dup_s16 (const int16_t *)
@*@emph{Form of expected instruction(s):} @code{vld2.16 @{@var{d0}[], @var{d1}[]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int8x8x2_t vld2_dup_s8 (const int8_t *)
@*@emph{Form of expected instruction(s):} @code{vld2.8 @{@var{d0}[], @var{d1}[]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item float32x2x2_t vld2_dup_f32 (const float32_t *)
@*@emph{Form of expected instruction(s):} @code{vld2.32 @{@var{d0}[], @var{d1}[]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item poly16x4x2_t vld2_dup_p16 (const poly16_t *)
@*@emph{Form of expected instruction(s):} @code{vld2.16 @{@var{d0}[], @var{d1}[]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item poly8x8x2_t vld2_dup_p8 (const poly8_t *)
@*@emph{Form of expected instruction(s):} @code{vld2.8 @{@var{d0}[], @var{d1}[]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item poly64x1x2_t vld2_dup_p64 (const poly64_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.64 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint64x1x2_t vld2_dup_u64 (const uint64_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.64 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int64x1x2_t vld2_dup_s64 (const int64_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.64 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize




@subsubsection Element/structure stores, VST2 variants

@itemize @bullet
@item void vst2_u32 (uint32_t *, uint32x2x2_t)
@*@emph{Form of expected instruction(s):} @code{vst2.32 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst2_u16 (uint16_t *, uint16x4x2_t)
@*@emph{Form of expected instruction(s):} @code{vst2.16 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst2_u8 (uint8_t *, uint8x8x2_t)
@*@emph{Form of expected instruction(s):} @code{vst2.8 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst2_s32 (int32_t *, int32x2x2_t)
@*@emph{Form of expected instruction(s):} @code{vst2.32 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst2_s16 (int16_t *, int16x4x2_t)
@*@emph{Form of expected instruction(s):} @code{vst2.16 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst2_s8 (int8_t *, int8x8x2_t)
@*@emph{Form of expected instruction(s):} @code{vst2.8 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst2_f32 (float32_t *, float32x2x2_t)
@*@emph{Form of expected instruction(s):} @code{vst2.32 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst2_p16 (poly16_t *, poly16x4x2_t)
@*@emph{Form of expected instruction(s):} @code{vst2.16 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst2_p8 (poly8_t *, poly8x8x2_t)
@*@emph{Form of expected instruction(s):} @code{vst2.8 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst2_p64 (poly64_t *, poly64x1x2_t)
@*@emph{Form of expected instruction(s):} @code{vst1.64 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst2_u64 (uint64_t *, uint64x1x2_t)
@*@emph{Form of expected instruction(s):} @code{vst1.64 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst2_s64 (int64_t *, int64x1x2_t)
@*@emph{Form of expected instruction(s):} @code{vst1.64 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst2q_u32 (uint32_t *, uint32x4x2_t)
@*@emph{Form of expected instruction(s):} @code{vst2.32 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst2q_u16 (uint16_t *, uint16x8x2_t)
@*@emph{Form of expected instruction(s):} @code{vst2.16 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst2q_u8 (uint8_t *, uint8x16x2_t)
@*@emph{Form of expected instruction(s):} @code{vst2.8 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst2q_s32 (int32_t *, int32x4x2_t)
@*@emph{Form of expected instruction(s):} @code{vst2.32 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst2q_s16 (int16_t *, int16x8x2_t)
@*@emph{Form of expected instruction(s):} @code{vst2.16 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst2q_s8 (int8_t *, int8x16x2_t)
@*@emph{Form of expected instruction(s):} @code{vst2.8 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst2q_f32 (float32_t *, float32x4x2_t)
@*@emph{Form of expected instruction(s):} @code{vst2.32 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst2q_p16 (poly16_t *, poly16x8x2_t)
@*@emph{Form of expected instruction(s):} @code{vst2.16 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst2q_p8 (poly8_t *, poly8x16x2_t)
@*@emph{Form of expected instruction(s):} @code{vst2.8 @{@var{d0}, @var{d1}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst2_lane_u32 (uint32_t *, uint32x2x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst2.32 @{@var{d0}[@var{0}], @var{d1}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst2_lane_u16 (uint16_t *, uint16x4x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst2.16 @{@var{d0}[@var{0}], @var{d1}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst2_lane_u8 (uint8_t *, uint8x8x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst2.8 @{@var{d0}[@var{0}], @var{d1}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst2_lane_s32 (int32_t *, int32x2x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst2.32 @{@var{d0}[@var{0}], @var{d1}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst2_lane_s16 (int16_t *, int16x4x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst2.16 @{@var{d0}[@var{0}], @var{d1}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst2_lane_s8 (int8_t *, int8x8x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst2.8 @{@var{d0}[@var{0}], @var{d1}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst2_lane_f32 (float32_t *, float32x2x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst2.32 @{@var{d0}[@var{0}], @var{d1}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst2_lane_p16 (poly16_t *, poly16x4x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst2.16 @{@var{d0}[@var{0}], @var{d1}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst2_lane_p8 (poly8_t *, poly8x8x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst2.8 @{@var{d0}[@var{0}], @var{d1}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst2q_lane_s32 (int32_t *, int32x4x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst2.32 @{@var{d0}[@var{0}], @var{d1}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst2q_lane_s16 (int16_t *, int16x8x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst2.16 @{@var{d0}[@var{0}], @var{d1}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst2q_lane_u32 (uint32_t *, uint32x4x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst2.32 @{@var{d0}[@var{0}], @var{d1}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst2q_lane_u16 (uint16_t *, uint16x8x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst2.16 @{@var{d0}[@var{0}], @var{d1}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst2q_lane_f32 (float32_t *, float32x4x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst2.32 @{@var{d0}[@var{0}], @var{d1}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst2q_lane_p16 (poly16_t *, poly16x8x2_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst2.16 @{@var{d0}[@var{0}], @var{d1}[@var{0}]@}, [@var{r0}]}
@end itemize




@subsubsection Element/structure loads, VLD3 variants

@itemize @bullet
@item uint32x2x3_t vld3_u32 (const uint32_t *)
@*@emph{Form of expected instruction(s):} @code{vld3.32 @{@var{d0}, @var{d1}, @var{d2}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint16x4x3_t vld3_u16 (const uint16_t *)
@*@emph{Form of expected instruction(s):} @code{vld3.16 @{@var{d0}, @var{d1}, @var{d2}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint8x8x3_t vld3_u8 (const uint8_t *)
@*@emph{Form of expected instruction(s):} @code{vld3.8 @{@var{d0}, @var{d1}, @var{d2}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int32x2x3_t vld3_s32 (const int32_t *)
@*@emph{Form of expected instruction(s):} @code{vld3.32 @{@var{d0}, @var{d1}, @var{d2}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int16x4x3_t vld3_s16 (const int16_t *)
@*@emph{Form of expected instruction(s):} @code{vld3.16 @{@var{d0}, @var{d1}, @var{d2}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int8x8x3_t vld3_s8 (const int8_t *)
@*@emph{Form of expected instruction(s):} @code{vld3.8 @{@var{d0}, @var{d1}, @var{d2}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item float32x2x3_t vld3_f32 (const float32_t *)
@*@emph{Form of expected instruction(s):} @code{vld3.32 @{@var{d0}, @var{d1}, @var{d2}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item poly16x4x3_t vld3_p16 (const poly16_t *)
@*@emph{Form of expected instruction(s):} @code{vld3.16 @{@var{d0}, @var{d1}, @var{d2}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item poly8x8x3_t vld3_p8 (const poly8_t *)
@*@emph{Form of expected instruction(s):} @code{vld3.8 @{@var{d0}, @var{d1}, @var{d2}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item poly64x1x3_t vld3_p64 (const poly64_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.64 @{@var{d0}, @var{d1}, @var{d2}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint64x1x3_t vld3_u64 (const uint64_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.64 @{@var{d0}, @var{d1}, @var{d2}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int64x1x3_t vld3_s64 (const int64_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.64 @{@var{d0}, @var{d1}, @var{d2}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint32x4x3_t vld3q_u32 (const uint32_t *)
@*@emph{Form of expected instruction(s):} @code{vld3.32 @{@var{d0}, @var{d1}, @var{d2}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint16x8x3_t vld3q_u16 (const uint16_t *)
@*@emph{Form of expected instruction(s):} @code{vld3.16 @{@var{d0}, @var{d1}, @var{d2}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint8x16x3_t vld3q_u8 (const uint8_t *)
@*@emph{Form of expected instruction(s):} @code{vld3.8 @{@var{d0}, @var{d1}, @var{d2}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int32x4x3_t vld3q_s32 (const int32_t *)
@*@emph{Form of expected instruction(s):} @code{vld3.32 @{@var{d0}, @var{d1}, @var{d2}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int16x8x3_t vld3q_s16 (const int16_t *)
@*@emph{Form of expected instruction(s):} @code{vld3.16 @{@var{d0}, @var{d1}, @var{d2}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int8x16x3_t vld3q_s8 (const int8_t *)
@*@emph{Form of expected instruction(s):} @code{vld3.8 @{@var{d0}, @var{d1}, @var{d2}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item float32x4x3_t vld3q_f32 (const float32_t *)
@*@emph{Form of expected instruction(s):} @code{vld3.32 @{@var{d0}, @var{d1}, @var{d2}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item poly16x8x3_t vld3q_p16 (const poly16_t *)
@*@emph{Form of expected instruction(s):} @code{vld3.16 @{@var{d0}, @var{d1}, @var{d2}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item poly8x16x3_t vld3q_p8 (const poly8_t *)
@*@emph{Form of expected instruction(s):} @code{vld3.8 @{@var{d0}, @var{d1}, @var{d2}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint32x2x3_t vld3_lane_u32 (const uint32_t *, uint32x2x3_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld3.32 @{@var{d0}[@var{0}], @var{d1}[@var{0}], @var{d2}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint16x4x3_t vld3_lane_u16 (const uint16_t *, uint16x4x3_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld3.16 @{@var{d0}[@var{0}], @var{d1}[@var{0}], @var{d2}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint8x8x3_t vld3_lane_u8 (const uint8_t *, uint8x8x3_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld3.8 @{@var{d0}[@var{0}], @var{d1}[@var{0}], @var{d2}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int32x2x3_t vld3_lane_s32 (const int32_t *, int32x2x3_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld3.32 @{@var{d0}[@var{0}], @var{d1}[@var{0}], @var{d2}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int16x4x3_t vld3_lane_s16 (const int16_t *, int16x4x3_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld3.16 @{@var{d0}[@var{0}], @var{d1}[@var{0}], @var{d2}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int8x8x3_t vld3_lane_s8 (const int8_t *, int8x8x3_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld3.8 @{@var{d0}[@var{0}], @var{d1}[@var{0}], @var{d2}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item float32x2x3_t vld3_lane_f32 (const float32_t *, float32x2x3_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld3.32 @{@var{d0}[@var{0}], @var{d1}[@var{0}], @var{d2}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item poly16x4x3_t vld3_lane_p16 (const poly16_t *, poly16x4x3_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld3.16 @{@var{d0}[@var{0}], @var{d1}[@var{0}], @var{d2}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item poly8x8x3_t vld3_lane_p8 (const poly8_t *, poly8x8x3_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld3.8 @{@var{d0}[@var{0}], @var{d1}[@var{0}], @var{d2}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int32x4x3_t vld3q_lane_s32 (const int32_t *, int32x4x3_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld3.32 @{@var{d0}[@var{0}], @var{d1}[@var{0}], @var{d2}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int16x8x3_t vld3q_lane_s16 (const int16_t *, int16x8x3_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld3.16 @{@var{d0}[@var{0}], @var{d1}[@var{0}], @var{d2}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint32x4x3_t vld3q_lane_u32 (const uint32_t *, uint32x4x3_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld3.32 @{@var{d0}[@var{0}], @var{d1}[@var{0}], @var{d2}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint16x8x3_t vld3q_lane_u16 (const uint16_t *, uint16x8x3_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld3.16 @{@var{d0}[@var{0}], @var{d1}[@var{0}], @var{d2}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item float32x4x3_t vld3q_lane_f32 (const float32_t *, float32x4x3_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld3.32 @{@var{d0}[@var{0}], @var{d1}[@var{0}], @var{d2}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item poly16x8x3_t vld3q_lane_p16 (const poly16_t *, poly16x8x3_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld3.16 @{@var{d0}[@var{0}], @var{d1}[@var{0}], @var{d2}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint32x2x3_t vld3_dup_u32 (const uint32_t *)
@*@emph{Form of expected instruction(s):} @code{vld3.32 @{@var{d0}[], @var{d1}[], @var{d2}[]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint16x4x3_t vld3_dup_u16 (const uint16_t *)
@*@emph{Form of expected instruction(s):} @code{vld3.16 @{@var{d0}[], @var{d1}[], @var{d2}[]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint8x8x3_t vld3_dup_u8 (const uint8_t *)
@*@emph{Form of expected instruction(s):} @code{vld3.8 @{@var{d0}[], @var{d1}[], @var{d2}[]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int32x2x3_t vld3_dup_s32 (const int32_t *)
@*@emph{Form of expected instruction(s):} @code{vld3.32 @{@var{d0}[], @var{d1}[], @var{d2}[]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int16x4x3_t vld3_dup_s16 (const int16_t *)
@*@emph{Form of expected instruction(s):} @code{vld3.16 @{@var{d0}[], @var{d1}[], @var{d2}[]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int8x8x3_t vld3_dup_s8 (const int8_t *)
@*@emph{Form of expected instruction(s):} @code{vld3.8 @{@var{d0}[], @var{d1}[], @var{d2}[]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item float32x2x3_t vld3_dup_f32 (const float32_t *)
@*@emph{Form of expected instruction(s):} @code{vld3.32 @{@var{d0}[], @var{d1}[], @var{d2}[]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item poly16x4x3_t vld3_dup_p16 (const poly16_t *)
@*@emph{Form of expected instruction(s):} @code{vld3.16 @{@var{d0}[], @var{d1}[], @var{d2}[]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item poly8x8x3_t vld3_dup_p8 (const poly8_t *)
@*@emph{Form of expected instruction(s):} @code{vld3.8 @{@var{d0}[], @var{d1}[], @var{d2}[]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item poly64x1x3_t vld3_dup_p64 (const poly64_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.64 @{@var{d0}, @var{d1}, @var{d2}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint64x1x3_t vld3_dup_u64 (const uint64_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.64 @{@var{d0}, @var{d1}, @var{d2}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int64x1x3_t vld3_dup_s64 (const int64_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.64 @{@var{d0}, @var{d1}, @var{d2}@}, [@var{r0}]}
@end itemize




@subsubsection Element/structure stores, VST3 variants

@itemize @bullet
@item void vst3_u32 (uint32_t *, uint32x2x3_t)
@*@emph{Form of expected instruction(s):} @code{vst3.32 @{@var{d0}, @var{d1}, @var{d2}, @var{d3}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst3_u16 (uint16_t *, uint16x4x3_t)
@*@emph{Form of expected instruction(s):} @code{vst3.16 @{@var{d0}, @var{d1}, @var{d2}, @var{d3}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst3_u8 (uint8_t *, uint8x8x3_t)
@*@emph{Form of expected instruction(s):} @code{vst3.8 @{@var{d0}, @var{d1}, @var{d2}, @var{d3}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst3_s32 (int32_t *, int32x2x3_t)
@*@emph{Form of expected instruction(s):} @code{vst3.32 @{@var{d0}, @var{d1}, @var{d2}, @var{d3}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst3_s16 (int16_t *, int16x4x3_t)
@*@emph{Form of expected instruction(s):} @code{vst3.16 @{@var{d0}, @var{d1}, @var{d2}, @var{d3}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst3_s8 (int8_t *, int8x8x3_t)
@*@emph{Form of expected instruction(s):} @code{vst3.8 @{@var{d0}, @var{d1}, @var{d2}, @var{d3}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst3_f32 (float32_t *, float32x2x3_t)
@*@emph{Form of expected instruction(s):} @code{vst3.32 @{@var{d0}, @var{d1}, @var{d2}, @var{d3}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst3_p16 (poly16_t *, poly16x4x3_t)
@*@emph{Form of expected instruction(s):} @code{vst3.16 @{@var{d0}, @var{d1}, @var{d2}, @var{d3}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst3_p8 (poly8_t *, poly8x8x3_t)
@*@emph{Form of expected instruction(s):} @code{vst3.8 @{@var{d0}, @var{d1}, @var{d2}, @var{d3}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst3_p64 (poly64_t *, poly64x1x3_t)
@*@emph{Form of expected instruction(s):} @code{vst1.64 @{@var{d0}, @var{d1}, @var{d2}, @var{d3}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst3_u64 (uint64_t *, uint64x1x3_t)
@*@emph{Form of expected instruction(s):} @code{vst1.64 @{@var{d0}, @var{d1}, @var{d2}, @var{d3}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst3_s64 (int64_t *, int64x1x3_t)
@*@emph{Form of expected instruction(s):} @code{vst1.64 @{@var{d0}, @var{d1}, @var{d2}, @var{d3}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst3q_u32 (uint32_t *, uint32x4x3_t)
@*@emph{Form of expected instruction(s):} @code{vst3.32 @{@var{d0}, @var{d1}, @var{d2}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst3q_u16 (uint16_t *, uint16x8x3_t)
@*@emph{Form of expected instruction(s):} @code{vst3.16 @{@var{d0}, @var{d1}, @var{d2}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst3q_u8 (uint8_t *, uint8x16x3_t)
@*@emph{Form of expected instruction(s):} @code{vst3.8 @{@var{d0}, @var{d1}, @var{d2}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst3q_s32 (int32_t *, int32x4x3_t)
@*@emph{Form of expected instruction(s):} @code{vst3.32 @{@var{d0}, @var{d1}, @var{d2}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst3q_s16 (int16_t *, int16x8x3_t)
@*@emph{Form of expected instruction(s):} @code{vst3.16 @{@var{d0}, @var{d1}, @var{d2}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst3q_s8 (int8_t *, int8x16x3_t)
@*@emph{Form of expected instruction(s):} @code{vst3.8 @{@var{d0}, @var{d1}, @var{d2}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst3q_f32 (float32_t *, float32x4x3_t)
@*@emph{Form of expected instruction(s):} @code{vst3.32 @{@var{d0}, @var{d1}, @var{d2}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst3q_p16 (poly16_t *, poly16x8x3_t)
@*@emph{Form of expected instruction(s):} @code{vst3.16 @{@var{d0}, @var{d1}, @var{d2}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst3q_p8 (poly8_t *, poly8x16x3_t)
@*@emph{Form of expected instruction(s):} @code{vst3.8 @{@var{d0}, @var{d1}, @var{d2}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst3_lane_u32 (uint32_t *, uint32x2x3_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst3.32 @{@var{d0}[@var{0}], @var{d1}[@var{0}], @var{d2}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst3_lane_u16 (uint16_t *, uint16x4x3_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst3.16 @{@var{d0}[@var{0}], @var{d1}[@var{0}], @var{d2}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst3_lane_u8 (uint8_t *, uint8x8x3_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst3.8 @{@var{d0}[@var{0}], @var{d1}[@var{0}], @var{d2}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst3_lane_s32 (int32_t *, int32x2x3_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst3.32 @{@var{d0}[@var{0}], @var{d1}[@var{0}], @var{d2}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst3_lane_s16 (int16_t *, int16x4x3_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst3.16 @{@var{d0}[@var{0}], @var{d1}[@var{0}], @var{d2}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst3_lane_s8 (int8_t *, int8x8x3_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst3.8 @{@var{d0}[@var{0}], @var{d1}[@var{0}], @var{d2}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst3_lane_f32 (float32_t *, float32x2x3_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst3.32 @{@var{d0}[@var{0}], @var{d1}[@var{0}], @var{d2}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst3_lane_p16 (poly16_t *, poly16x4x3_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst3.16 @{@var{d0}[@var{0}], @var{d1}[@var{0}], @var{d2}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst3_lane_p8 (poly8_t *, poly8x8x3_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst3.8 @{@var{d0}[@var{0}], @var{d1}[@var{0}], @var{d2}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst3q_lane_s32 (int32_t *, int32x4x3_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst3.32 @{@var{d0}[@var{0}], @var{d1}[@var{0}], @var{d2}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst3q_lane_s16 (int16_t *, int16x8x3_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst3.16 @{@var{d0}[@var{0}], @var{d1}[@var{0}], @var{d2}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst3q_lane_u32 (uint32_t *, uint32x4x3_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst3.32 @{@var{d0}[@var{0}], @var{d1}[@var{0}], @var{d2}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst3q_lane_u16 (uint16_t *, uint16x8x3_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst3.16 @{@var{d0}[@var{0}], @var{d1}[@var{0}], @var{d2}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst3q_lane_f32 (float32_t *, float32x4x3_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst3.32 @{@var{d0}[@var{0}], @var{d1}[@var{0}], @var{d2}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst3q_lane_p16 (poly16_t *, poly16x8x3_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst3.16 @{@var{d0}[@var{0}], @var{d1}[@var{0}], @var{d2}[@var{0}]@}, [@var{r0}]}
@end itemize




@subsubsection Element/structure loads, VLD4 variants

@itemize @bullet
@item uint32x2x4_t vld4_u32 (const uint32_t *)
@*@emph{Form of expected instruction(s):} @code{vld4.32 @{@var{d0}, @var{d1}, @var{d2}, @var{d3}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint16x4x4_t vld4_u16 (const uint16_t *)
@*@emph{Form of expected instruction(s):} @code{vld4.16 @{@var{d0}, @var{d1}, @var{d2}, @var{d3}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint8x8x4_t vld4_u8 (const uint8_t *)
@*@emph{Form of expected instruction(s):} @code{vld4.8 @{@var{d0}, @var{d1}, @var{d2}, @var{d3}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int32x2x4_t vld4_s32 (const int32_t *)
@*@emph{Form of expected instruction(s):} @code{vld4.32 @{@var{d0}, @var{d1}, @var{d2}, @var{d3}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int16x4x4_t vld4_s16 (const int16_t *)
@*@emph{Form of expected instruction(s):} @code{vld4.16 @{@var{d0}, @var{d1}, @var{d2}, @var{d3}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int8x8x4_t vld4_s8 (const int8_t *)
@*@emph{Form of expected instruction(s):} @code{vld4.8 @{@var{d0}, @var{d1}, @var{d2}, @var{d3}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item float32x2x4_t vld4_f32 (const float32_t *)
@*@emph{Form of expected instruction(s):} @code{vld4.32 @{@var{d0}, @var{d1}, @var{d2}, @var{d3}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item poly16x4x4_t vld4_p16 (const poly16_t *)
@*@emph{Form of expected instruction(s):} @code{vld4.16 @{@var{d0}, @var{d1}, @var{d2}, @var{d3}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item poly8x8x4_t vld4_p8 (const poly8_t *)
@*@emph{Form of expected instruction(s):} @code{vld4.8 @{@var{d0}, @var{d1}, @var{d2}, @var{d3}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item poly64x1x4_t vld4_p64 (const poly64_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.64 @{@var{d0}, @var{d1}, @var{d2}, @var{d3}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint64x1x4_t vld4_u64 (const uint64_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.64 @{@var{d0}, @var{d1}, @var{d2}, @var{d3}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int64x1x4_t vld4_s64 (const int64_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.64 @{@var{d0}, @var{d1}, @var{d2}, @var{d3}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint32x4x4_t vld4q_u32 (const uint32_t *)
@*@emph{Form of expected instruction(s):} @code{vld4.32 @{@var{d0}, @var{d1}, @var{d2}, @var{d3}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint16x8x4_t vld4q_u16 (const uint16_t *)
@*@emph{Form of expected instruction(s):} @code{vld4.16 @{@var{d0}, @var{d1}, @var{d2}, @var{d3}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint8x16x4_t vld4q_u8 (const uint8_t *)
@*@emph{Form of expected instruction(s):} @code{vld4.8 @{@var{d0}, @var{d1}, @var{d2}, @var{d3}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int32x4x4_t vld4q_s32 (const int32_t *)
@*@emph{Form of expected instruction(s):} @code{vld4.32 @{@var{d0}, @var{d1}, @var{d2}, @var{d3}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int16x8x4_t vld4q_s16 (const int16_t *)
@*@emph{Form of expected instruction(s):} @code{vld4.16 @{@var{d0}, @var{d1}, @var{d2}, @var{d3}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int8x16x4_t vld4q_s8 (const int8_t *)
@*@emph{Form of expected instruction(s):} @code{vld4.8 @{@var{d0}, @var{d1}, @var{d2}, @var{d3}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item float32x4x4_t vld4q_f32 (const float32_t *)
@*@emph{Form of expected instruction(s):} @code{vld4.32 @{@var{d0}, @var{d1}, @var{d2}, @var{d3}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item poly16x8x4_t vld4q_p16 (const poly16_t *)
@*@emph{Form of expected instruction(s):} @code{vld4.16 @{@var{d0}, @var{d1}, @var{d2}, @var{d3}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item poly8x16x4_t vld4q_p8 (const poly8_t *)
@*@emph{Form of expected instruction(s):} @code{vld4.8 @{@var{d0}, @var{d1}, @var{d2}, @var{d3}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint32x2x4_t vld4_lane_u32 (const uint32_t *, uint32x2x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld4.32 @{@var{d0}[@var{0}], @var{d1}[@var{0}], @var{d2}[@var{0}], @var{d3}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint16x4x4_t vld4_lane_u16 (const uint16_t *, uint16x4x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld4.16 @{@var{d0}[@var{0}], @var{d1}[@var{0}], @var{d2}[@var{0}], @var{d3}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint8x8x4_t vld4_lane_u8 (const uint8_t *, uint8x8x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld4.8 @{@var{d0}[@var{0}], @var{d1}[@var{0}], @var{d2}[@var{0}], @var{d3}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int32x2x4_t vld4_lane_s32 (const int32_t *, int32x2x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld4.32 @{@var{d0}[@var{0}], @var{d1}[@var{0}], @var{d2}[@var{0}], @var{d3}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int16x4x4_t vld4_lane_s16 (const int16_t *, int16x4x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld4.16 @{@var{d0}[@var{0}], @var{d1}[@var{0}], @var{d2}[@var{0}], @var{d3}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int8x8x4_t vld4_lane_s8 (const int8_t *, int8x8x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld4.8 @{@var{d0}[@var{0}], @var{d1}[@var{0}], @var{d2}[@var{0}], @var{d3}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item float32x2x4_t vld4_lane_f32 (const float32_t *, float32x2x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld4.32 @{@var{d0}[@var{0}], @var{d1}[@var{0}], @var{d2}[@var{0}], @var{d3}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item poly16x4x4_t vld4_lane_p16 (const poly16_t *, poly16x4x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld4.16 @{@var{d0}[@var{0}], @var{d1}[@var{0}], @var{d2}[@var{0}], @var{d3}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item poly8x8x4_t vld4_lane_p8 (const poly8_t *, poly8x8x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld4.8 @{@var{d0}[@var{0}], @var{d1}[@var{0}], @var{d2}[@var{0}], @var{d3}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int32x4x4_t vld4q_lane_s32 (const int32_t *, int32x4x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld4.32 @{@var{d0}[@var{0}], @var{d1}[@var{0}], @var{d2}[@var{0}], @var{d3}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int16x8x4_t vld4q_lane_s16 (const int16_t *, int16x8x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld4.16 @{@var{d0}[@var{0}], @var{d1}[@var{0}], @var{d2}[@var{0}], @var{d3}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint32x4x4_t vld4q_lane_u32 (const uint32_t *, uint32x4x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld4.32 @{@var{d0}[@var{0}], @var{d1}[@var{0}], @var{d2}[@var{0}], @var{d3}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint16x8x4_t vld4q_lane_u16 (const uint16_t *, uint16x8x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld4.16 @{@var{d0}[@var{0}], @var{d1}[@var{0}], @var{d2}[@var{0}], @var{d3}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item float32x4x4_t vld4q_lane_f32 (const float32_t *, float32x4x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld4.32 @{@var{d0}[@var{0}], @var{d1}[@var{0}], @var{d2}[@var{0}], @var{d3}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item poly16x8x4_t vld4q_lane_p16 (const poly16_t *, poly16x8x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vld4.16 @{@var{d0}[@var{0}], @var{d1}[@var{0}], @var{d2}[@var{0}], @var{d3}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint32x2x4_t vld4_dup_u32 (const uint32_t *)
@*@emph{Form of expected instruction(s):} @code{vld4.32 @{@var{d0}[], @var{d1}[], @var{d2}[], @var{d3}[]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint16x4x4_t vld4_dup_u16 (const uint16_t *)
@*@emph{Form of expected instruction(s):} @code{vld4.16 @{@var{d0}[], @var{d1}[], @var{d2}[], @var{d3}[]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint8x8x4_t vld4_dup_u8 (const uint8_t *)
@*@emph{Form of expected instruction(s):} @code{vld4.8 @{@var{d0}[], @var{d1}[], @var{d2}[], @var{d3}[]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int32x2x4_t vld4_dup_s32 (const int32_t *)
@*@emph{Form of expected instruction(s):} @code{vld4.32 @{@var{d0}[], @var{d1}[], @var{d2}[], @var{d3}[]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int16x4x4_t vld4_dup_s16 (const int16_t *)
@*@emph{Form of expected instruction(s):} @code{vld4.16 @{@var{d0}[], @var{d1}[], @var{d2}[], @var{d3}[]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int8x8x4_t vld4_dup_s8 (const int8_t *)
@*@emph{Form of expected instruction(s):} @code{vld4.8 @{@var{d0}[], @var{d1}[], @var{d2}[], @var{d3}[]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item float32x2x4_t vld4_dup_f32 (const float32_t *)
@*@emph{Form of expected instruction(s):} @code{vld4.32 @{@var{d0}[], @var{d1}[], @var{d2}[], @var{d3}[]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item poly16x4x4_t vld4_dup_p16 (const poly16_t *)
@*@emph{Form of expected instruction(s):} @code{vld4.16 @{@var{d0}[], @var{d1}[], @var{d2}[], @var{d3}[]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item poly8x8x4_t vld4_dup_p8 (const poly8_t *)
@*@emph{Form of expected instruction(s):} @code{vld4.8 @{@var{d0}[], @var{d1}[], @var{d2}[], @var{d3}[]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item poly64x1x4_t vld4_dup_p64 (const poly64_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.64 @{@var{d0}, @var{d1}, @var{d2}, @var{d3}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item uint64x1x4_t vld4_dup_u64 (const uint64_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.64 @{@var{d0}, @var{d1}, @var{d2}, @var{d3}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item int64x1x4_t vld4_dup_s64 (const int64_t *)
@*@emph{Form of expected instruction(s):} @code{vld1.64 @{@var{d0}, @var{d1}, @var{d2}, @var{d3}@}, [@var{r0}]}
@end itemize




@subsubsection Element/structure stores, VST4 variants

@itemize @bullet
@item void vst4_u32 (uint32_t *, uint32x2x4_t)
@*@emph{Form of expected instruction(s):} @code{vst4.32 @{@var{d0}, @var{d1}, @var{d2}, @var{d3}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst4_u16 (uint16_t *, uint16x4x4_t)
@*@emph{Form of expected instruction(s):} @code{vst4.16 @{@var{d0}, @var{d1}, @var{d2}, @var{d3}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst4_u8 (uint8_t *, uint8x8x4_t)
@*@emph{Form of expected instruction(s):} @code{vst4.8 @{@var{d0}, @var{d1}, @var{d2}, @var{d3}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst4_s32 (int32_t *, int32x2x4_t)
@*@emph{Form of expected instruction(s):} @code{vst4.32 @{@var{d0}, @var{d1}, @var{d2}, @var{d3}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst4_s16 (int16_t *, int16x4x4_t)
@*@emph{Form of expected instruction(s):} @code{vst4.16 @{@var{d0}, @var{d1}, @var{d2}, @var{d3}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst4_s8 (int8_t *, int8x8x4_t)
@*@emph{Form of expected instruction(s):} @code{vst4.8 @{@var{d0}, @var{d1}, @var{d2}, @var{d3}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst4_f32 (float32_t *, float32x2x4_t)
@*@emph{Form of expected instruction(s):} @code{vst4.32 @{@var{d0}, @var{d1}, @var{d2}, @var{d3}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst4_p16 (poly16_t *, poly16x4x4_t)
@*@emph{Form of expected instruction(s):} @code{vst4.16 @{@var{d0}, @var{d1}, @var{d2}, @var{d3}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst4_p8 (poly8_t *, poly8x8x4_t)
@*@emph{Form of expected instruction(s):} @code{vst4.8 @{@var{d0}, @var{d1}, @var{d2}, @var{d3}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst4_p64 (poly64_t *, poly64x1x4_t)
@*@emph{Form of expected instruction(s):} @code{vst1.64 @{@var{d0}, @var{d1}, @var{d2}, @var{d3}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst4_u64 (uint64_t *, uint64x1x4_t)
@*@emph{Form of expected instruction(s):} @code{vst1.64 @{@var{d0}, @var{d1}, @var{d2}, @var{d3}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst4_s64 (int64_t *, int64x1x4_t)
@*@emph{Form of expected instruction(s):} @code{vst1.64 @{@var{d0}, @var{d1}, @var{d2}, @var{d3}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst4q_u32 (uint32_t *, uint32x4x4_t)
@*@emph{Form of expected instruction(s):} @code{vst4.32 @{@var{d0}, @var{d1}, @var{d2}, @var{d3}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst4q_u16 (uint16_t *, uint16x8x4_t)
@*@emph{Form of expected instruction(s):} @code{vst4.16 @{@var{d0}, @var{d1}, @var{d2}, @var{d3}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst4q_u8 (uint8_t *, uint8x16x4_t)
@*@emph{Form of expected instruction(s):} @code{vst4.8 @{@var{d0}, @var{d1}, @var{d2}, @var{d3}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst4q_s32 (int32_t *, int32x4x4_t)
@*@emph{Form of expected instruction(s):} @code{vst4.32 @{@var{d0}, @var{d1}, @var{d2}, @var{d3}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst4q_s16 (int16_t *, int16x8x4_t)
@*@emph{Form of expected instruction(s):} @code{vst4.16 @{@var{d0}, @var{d1}, @var{d2}, @var{d3}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst4q_s8 (int8_t *, int8x16x4_t)
@*@emph{Form of expected instruction(s):} @code{vst4.8 @{@var{d0}, @var{d1}, @var{d2}, @var{d3}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst4q_f32 (float32_t *, float32x4x4_t)
@*@emph{Form of expected instruction(s):} @code{vst4.32 @{@var{d0}, @var{d1}, @var{d2}, @var{d3}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst4q_p16 (poly16_t *, poly16x8x4_t)
@*@emph{Form of expected instruction(s):} @code{vst4.16 @{@var{d0}, @var{d1}, @var{d2}, @var{d3}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst4q_p8 (poly8_t *, poly8x16x4_t)
@*@emph{Form of expected instruction(s):} @code{vst4.8 @{@var{d0}, @var{d1}, @var{d2}, @var{d3}@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst4_lane_u32 (uint32_t *, uint32x2x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst4.32 @{@var{d0}[@var{0}], @var{d1}[@var{0}], @var{d2}[@var{0}], @var{d3}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst4_lane_u16 (uint16_t *, uint16x4x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst4.16 @{@var{d0}[@var{0}], @var{d1}[@var{0}], @var{d2}[@var{0}], @var{d3}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst4_lane_u8 (uint8_t *, uint8x8x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst4.8 @{@var{d0}[@var{0}], @var{d1}[@var{0}], @var{d2}[@var{0}], @var{d3}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst4_lane_s32 (int32_t *, int32x2x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst4.32 @{@var{d0}[@var{0}], @var{d1}[@var{0}], @var{d2}[@var{0}], @var{d3}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst4_lane_s16 (int16_t *, int16x4x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst4.16 @{@var{d0}[@var{0}], @var{d1}[@var{0}], @var{d2}[@var{0}], @var{d3}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst4_lane_s8 (int8_t *, int8x8x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst4.8 @{@var{d0}[@var{0}], @var{d1}[@var{0}], @var{d2}[@var{0}], @var{d3}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst4_lane_f32 (float32_t *, float32x2x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst4.32 @{@var{d0}[@var{0}], @var{d1}[@var{0}], @var{d2}[@var{0}], @var{d3}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst4_lane_p16 (poly16_t *, poly16x4x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst4.16 @{@var{d0}[@var{0}], @var{d1}[@var{0}], @var{d2}[@var{0}], @var{d3}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst4_lane_p8 (poly8_t *, poly8x8x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst4.8 @{@var{d0}[@var{0}], @var{d1}[@var{0}], @var{d2}[@var{0}], @var{d3}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst4q_lane_s32 (int32_t *, int32x4x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst4.32 @{@var{d0}[@var{0}], @var{d1}[@var{0}], @var{d2}[@var{0}], @var{d3}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst4q_lane_s16 (int16_t *, int16x8x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst4.16 @{@var{d0}[@var{0}], @var{d1}[@var{0}], @var{d2}[@var{0}], @var{d3}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst4q_lane_u32 (uint32_t *, uint32x4x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst4.32 @{@var{d0}[@var{0}], @var{d1}[@var{0}], @var{d2}[@var{0}], @var{d3}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst4q_lane_u16 (uint16_t *, uint16x8x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst4.16 @{@var{d0}[@var{0}], @var{d1}[@var{0}], @var{d2}[@var{0}], @var{d3}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst4q_lane_f32 (float32_t *, float32x4x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst4.32 @{@var{d0}[@var{0}], @var{d1}[@var{0}], @var{d2}[@var{0}], @var{d3}[@var{0}]@}, [@var{r0}]}
@end itemize


@itemize @bullet
@item void vst4q_lane_p16 (poly16_t *, poly16x8x4_t, const int)
@*@emph{Form of expected instruction(s):} @code{vst4.16 @{@var{d0}[@var{0}], @var{d1}[@var{0}], @var{d2}[@var{0}], @var{d3}[@var{0}]@}, [@var{r0}]}
@end itemize




@subsubsection Logical operations (AND)

@itemize @bullet
@item uint32x2_t vand_u32 (uint32x2_t, uint32x2_t)
@*@emph{Form of expected instruction(s):} @code{vand @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint16x4_t vand_u16 (uint16x4_t, uint16x4_t)
@*@emph{Form of expected instruction(s):} @code{vand @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint8x8_t vand_u8 (uint8x8_t, uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vand @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int32x2_t vand_s32 (int32x2_t, int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vand @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int16x4_t vand_s16 (int16x4_t, int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vand @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int8x8_t vand_s8 (int8x8_t, int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vand @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint64x1_t vand_u64 (uint64x1_t, uint64x1_t)
@end itemize


@itemize @bullet
@item int64x1_t vand_s64 (int64x1_t, int64x1_t)
@end itemize


@itemize @bullet
@item uint32x4_t vandq_u32 (uint32x4_t, uint32x4_t)
@*@emph{Form of expected instruction(s):} @code{vand @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint16x8_t vandq_u16 (uint16x8_t, uint16x8_t)
@*@emph{Form of expected instruction(s):} @code{vand @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint8x16_t vandq_u8 (uint8x16_t, uint8x16_t)
@*@emph{Form of expected instruction(s):} @code{vand @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int32x4_t vandq_s32 (int32x4_t, int32x4_t)
@*@emph{Form of expected instruction(s):} @code{vand @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int16x8_t vandq_s16 (int16x8_t, int16x8_t)
@*@emph{Form of expected instruction(s):} @code{vand @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int8x16_t vandq_s8 (int8x16_t, int8x16_t)
@*@emph{Form of expected instruction(s):} @code{vand @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint64x2_t vandq_u64 (uint64x2_t, uint64x2_t)
@*@emph{Form of expected instruction(s):} @code{vand @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int64x2_t vandq_s64 (int64x2_t, int64x2_t)
@*@emph{Form of expected instruction(s):} @code{vand @var{q0}, @var{q0}, @var{q0}}
@end itemize




@subsubsection Logical operations (OR)

@itemize @bullet
@item uint32x2_t vorr_u32 (uint32x2_t, uint32x2_t)
@*@emph{Form of expected instruction(s):} @code{vorr @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint16x4_t vorr_u16 (uint16x4_t, uint16x4_t)
@*@emph{Form of expected instruction(s):} @code{vorr @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint8x8_t vorr_u8 (uint8x8_t, uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vorr @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int32x2_t vorr_s32 (int32x2_t, int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vorr @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int16x4_t vorr_s16 (int16x4_t, int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vorr @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int8x8_t vorr_s8 (int8x8_t, int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vorr @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint64x1_t vorr_u64 (uint64x1_t, uint64x1_t)
@end itemize


@itemize @bullet
@item int64x1_t vorr_s64 (int64x1_t, int64x1_t)
@end itemize


@itemize @bullet
@item uint32x4_t vorrq_u32 (uint32x4_t, uint32x4_t)
@*@emph{Form of expected instruction(s):} @code{vorr @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint16x8_t vorrq_u16 (uint16x8_t, uint16x8_t)
@*@emph{Form of expected instruction(s):} @code{vorr @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint8x16_t vorrq_u8 (uint8x16_t, uint8x16_t)
@*@emph{Form of expected instruction(s):} @code{vorr @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int32x4_t vorrq_s32 (int32x4_t, int32x4_t)
@*@emph{Form of expected instruction(s):} @code{vorr @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int16x8_t vorrq_s16 (int16x8_t, int16x8_t)
@*@emph{Form of expected instruction(s):} @code{vorr @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int8x16_t vorrq_s8 (int8x16_t, int8x16_t)
@*@emph{Form of expected instruction(s):} @code{vorr @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint64x2_t vorrq_u64 (uint64x2_t, uint64x2_t)
@*@emph{Form of expected instruction(s):} @code{vorr @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int64x2_t vorrq_s64 (int64x2_t, int64x2_t)
@*@emph{Form of expected instruction(s):} @code{vorr @var{q0}, @var{q0}, @var{q0}}
@end itemize




@subsubsection Logical operations (exclusive OR)

@itemize @bullet
@item uint32x2_t veor_u32 (uint32x2_t, uint32x2_t)
@*@emph{Form of expected instruction(s):} @code{veor @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint16x4_t veor_u16 (uint16x4_t, uint16x4_t)
@*@emph{Form of expected instruction(s):} @code{veor @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint8x8_t veor_u8 (uint8x8_t, uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{veor @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int32x2_t veor_s32 (int32x2_t, int32x2_t)
@*@emph{Form of expected instruction(s):} @code{veor @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int16x4_t veor_s16 (int16x4_t, int16x4_t)
@*@emph{Form of expected instruction(s):} @code{veor @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int8x8_t veor_s8 (int8x8_t, int8x8_t)
@*@emph{Form of expected instruction(s):} @code{veor @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint64x1_t veor_u64 (uint64x1_t, uint64x1_t)
@end itemize


@itemize @bullet
@item int64x1_t veor_s64 (int64x1_t, int64x1_t)
@end itemize


@itemize @bullet
@item uint32x4_t veorq_u32 (uint32x4_t, uint32x4_t)
@*@emph{Form of expected instruction(s):} @code{veor @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint16x8_t veorq_u16 (uint16x8_t, uint16x8_t)
@*@emph{Form of expected instruction(s):} @code{veor @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint8x16_t veorq_u8 (uint8x16_t, uint8x16_t)
@*@emph{Form of expected instruction(s):} @code{veor @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int32x4_t veorq_s32 (int32x4_t, int32x4_t)
@*@emph{Form of expected instruction(s):} @code{veor @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int16x8_t veorq_s16 (int16x8_t, int16x8_t)
@*@emph{Form of expected instruction(s):} @code{veor @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int8x16_t veorq_s8 (int8x16_t, int8x16_t)
@*@emph{Form of expected instruction(s):} @code{veor @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint64x2_t veorq_u64 (uint64x2_t, uint64x2_t)
@*@emph{Form of expected instruction(s):} @code{veor @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int64x2_t veorq_s64 (int64x2_t, int64x2_t)
@*@emph{Form of expected instruction(s):} @code{veor @var{q0}, @var{q0}, @var{q0}}
@end itemize




@subsubsection Logical operations (AND-NOT)

@itemize @bullet
@item uint32x2_t vbic_u32 (uint32x2_t, uint32x2_t)
@*@emph{Form of expected instruction(s):} @code{vbic @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint16x4_t vbic_u16 (uint16x4_t, uint16x4_t)
@*@emph{Form of expected instruction(s):} @code{vbic @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint8x8_t vbic_u8 (uint8x8_t, uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vbic @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int32x2_t vbic_s32 (int32x2_t, int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vbic @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int16x4_t vbic_s16 (int16x4_t, int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vbic @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int8x8_t vbic_s8 (int8x8_t, int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vbic @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint64x1_t vbic_u64 (uint64x1_t, uint64x1_t)
@end itemize


@itemize @bullet
@item int64x1_t vbic_s64 (int64x1_t, int64x1_t)
@end itemize


@itemize @bullet
@item uint32x4_t vbicq_u32 (uint32x4_t, uint32x4_t)
@*@emph{Form of expected instruction(s):} @code{vbic @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint16x8_t vbicq_u16 (uint16x8_t, uint16x8_t)
@*@emph{Form of expected instruction(s):} @code{vbic @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint8x16_t vbicq_u8 (uint8x16_t, uint8x16_t)
@*@emph{Form of expected instruction(s):} @code{vbic @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int32x4_t vbicq_s32 (int32x4_t, int32x4_t)
@*@emph{Form of expected instruction(s):} @code{vbic @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int16x8_t vbicq_s16 (int16x8_t, int16x8_t)
@*@emph{Form of expected instruction(s):} @code{vbic @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int8x16_t vbicq_s8 (int8x16_t, int8x16_t)
@*@emph{Form of expected instruction(s):} @code{vbic @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint64x2_t vbicq_u64 (uint64x2_t, uint64x2_t)
@*@emph{Form of expected instruction(s):} @code{vbic @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int64x2_t vbicq_s64 (int64x2_t, int64x2_t)
@*@emph{Form of expected instruction(s):} @code{vbic @var{q0}, @var{q0}, @var{q0}}
@end itemize




@subsubsection Logical operations (OR-NOT)

@itemize @bullet
@item uint32x2_t vorn_u32 (uint32x2_t, uint32x2_t)
@*@emph{Form of expected instruction(s):} @code{vorn @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint16x4_t vorn_u16 (uint16x4_t, uint16x4_t)
@*@emph{Form of expected instruction(s):} @code{vorn @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint8x8_t vorn_u8 (uint8x8_t, uint8x8_t)
@*@emph{Form of expected instruction(s):} @code{vorn @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int32x2_t vorn_s32 (int32x2_t, int32x2_t)
@*@emph{Form of expected instruction(s):} @code{vorn @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int16x4_t vorn_s16 (int16x4_t, int16x4_t)
@*@emph{Form of expected instruction(s):} @code{vorn @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item int8x8_t vorn_s8 (int8x8_t, int8x8_t)
@*@emph{Form of expected instruction(s):} @code{vorn @var{d0}, @var{d0}, @var{d0}}
@end itemize


@itemize @bullet
@item uint64x1_t vorn_u64 (uint64x1_t, uint64x1_t)
@end itemize


@itemize @bullet
@item int64x1_t vorn_s64 (int64x1_t, int64x1_t)
@end itemize


@itemize @bullet
@item uint32x4_t vornq_u32 (uint32x4_t, uint32x4_t)
@*@emph{Form of expected instruction(s):} @code{vorn @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint16x8_t vornq_u16 (uint16x8_t, uint16x8_t)
@*@emph{Form of expected instruction(s):} @code{vorn @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint8x16_t vornq_u8 (uint8x16_t, uint8x16_t)
@*@emph{Form of expected instruction(s):} @code{vorn @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int32x4_t vornq_s32 (int32x4_t, int32x4_t)
@*@emph{Form of expected instruction(s):} @code{vorn @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int16x8_t vornq_s16 (int16x8_t, int16x8_t)
@*@emph{Form of expected instruction(s):} @code{vorn @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int8x16_t vornq_s8 (int8x16_t, int8x16_t)
@*@emph{Form of expected instruction(s):} @code{vorn @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item uint64x2_t vornq_u64 (uint64x2_t, uint64x2_t)
@*@emph{Form of expected instruction(s):} @code{vorn @var{q0}, @var{q0}, @var{q0}}
@end itemize


@itemize @bullet
@item int64x2_t vornq_s64 (int64x2_t, int64x2_t)
@*@emph{Form of expected instruction(s):} @code{vorn @var{q0}, @var{q0}, @var{q0}}
@end itemize




@subsubsection Reinterpret casts

@itemize @bullet
@item poly8x8_t vreinterpret_p8_p16 (poly16x4_t)
@end itemize


@itemize @bullet
@item poly8x8_t vreinterpret_p8_f32 (float32x2_t)
@end itemize


@itemize @bullet
@item poly8x8_t vreinterpret_p8_p64 (poly64x1_t)
@end itemize


@itemize @bullet
@item poly8x8_t vreinterpret_p8_s64 (int64x1_t)
@end itemize


@itemize @bullet
@item poly8x8_t vreinterpret_p8_u64 (uint64x1_t)
@end itemize


@itemize @bullet
@item poly8x8_t vreinterpret_p8_s8 (int8x8_t)
@end itemize


@itemize @bullet
@item poly8x8_t vreinterpret_p8_s16 (int16x4_t)
@end itemize


@itemize @bullet
@item poly8x8_t vreinterpret_p8_s32 (int32x2_t)
@end itemize


@itemize @bullet
@item poly8x8_t vreinterpret_p8_u8 (uint8x8_t)
@end itemize


@itemize @bullet
@item poly8x8_t vreinterpret_p8_u16 (uint16x4_t)
@end itemize


@itemize @bullet
@item poly8x8_t vreinterpret_p8_u32 (uint32x2_t)
@end itemize


@itemize @bullet
@item poly16x4_t vreinterpret_p16_p8 (poly8x8_t)
@end itemize


@itemize @bullet
@item poly16x4_t vreinterpret_p16_f32 (float32x2_t)
@end itemize


@itemize @bullet
@item poly16x4_t vreinterpret_p16_p64 (poly64x1_t)
@end itemize


@itemize @bullet
@item poly16x4_t vreinterpret_p16_s64 (int64x1_t)
@end itemize


@itemize @bullet
@item poly16x4_t vreinterpret_p16_u64 (uint64x1_t)
@end itemize


@itemize @bullet
@item poly16x4_t vreinterpret_p16_s8 (int8x8_t)
@end itemize


@itemize @bullet
@item poly16x4_t vreinterpret_p16_s16 (int16x4_t)
@end itemize


@itemize @bullet
@item poly16x4_t vreinterpret_p16_s32 (int32x2_t)
@end itemize


@itemize @bullet
@item poly16x4_t vreinterpret_p16_u8 (uint8x8_t)
@end itemize


@itemize @bullet
@item poly16x4_t vreinterpret_p16_u16 (uint16x4_t)
@end itemize


@itemize @bullet
@item poly16x4_t vreinterpret_p16_u32 (uint32x2_t)
@end itemize


@itemize @bullet
@item float32x2_t vreinterpret_f32_p8 (poly8x8_t)
@end itemize


@itemize @bullet
@item float32x2_t vreinterpret_f32_p16 (poly16x4_t)
@end itemize


@itemize @bullet
@item float32x2_t vreinterpret_f32_p64 (poly64x1_t)
@end itemize


@itemize @bullet
@item float32x2_t vreinterpret_f32_s64 (int64x1_t)
@end itemize


@itemize @bullet
@item float32x2_t vreinterpret_f32_u64 (uint64x1_t)
@end itemize


@itemize @bullet
@item float32x2_t vreinterpret_f32_s8 (int8x8_t)
@end itemize


@itemize @bullet
@item float32x2_t vreinterpret_f32_s16 (int16x4_t)
@end itemize


@itemize @bullet
@item float32x2_t vreinterpret_f32_s32 (int32x2_t)
@end itemize


@itemize @bullet
@item float32x2_t vreinterpret_f32_u8 (uint8x8_t)
@end itemize


@itemize @bullet
@item float32x2_t vreinterpret_f32_u16 (uint16x4_t)
@end itemize


@itemize @bullet
@item float32x2_t vreinterpret_f32_u32 (uint32x2_t)
@end itemize


@itemize @bullet
@item poly64x1_t vreinterpret_p64_p8 (poly8x8_t)
@end itemize


@itemize @bullet
@item poly64x1_t vreinterpret_p64_p16 (poly16x4_t)
@end itemize


@itemize @bullet
@item poly64x1_t vreinterpret_p64_f32 (float32x2_t)
@end itemize


@itemize @bullet
@item poly64x1_t vreinterpret_p64_s64 (int64x1_t)
@end itemize


@itemize @bullet
@item poly64x1_t vreinterpret_p64_u64 (uint64x1_t)
@end itemize


@itemize @bullet
@item poly64x1_t vreinterpret_p64_s8 (int8x8_t)
@end itemize


@itemize @bullet
@item poly64x1_t vreinterpret_p64_s16 (int16x4_t)
@end itemize


@itemize @bullet
@item poly64x1_t vreinterpret_p64_s32 (int32x2_t)
@end itemize


@itemize @bullet
@item poly64x1_t vreinterpret_p64_u8 (uint8x8_t)
@end itemize


@itemize @bullet
@item poly64x1_t vreinterpret_p64_u16 (uint16x4_t)
@end itemize


@itemize @bullet
@item poly64x1_t vreinterpret_p64_u32 (uint32x2_t)
@end itemize


@itemize @bullet
@item int64x1_t vreinterpret_s64_p8 (poly8x8_t)
@end itemize


@itemize @bullet
@item int64x1_t vreinterpret_s64_p16 (poly16x4_t)
@end itemize


@itemize @bullet
@item int64x1_t vreinterpret_s64_f32 (float32x2_t)
@end itemize


@itemize @bullet
@item int64x1_t vreinterpret_s64_p64 (poly64x1_t)
@end itemize


@itemize @bullet
@item int64x1_t vreinterpret_s64_u64 (uint64x1_t)
@end itemize


@itemize @bullet
@item int64x1_t vreinterpret_s64_s8 (int8x8_t)
@end itemize


@itemize @bullet
@item int64x1_t vreinterpret_s64_s16 (int16x4_t)
@end itemize


@itemize @bullet
@item int64x1_t vreinterpret_s64_s32 (int32x2_t)
@end itemize


@itemize @bullet
@item int64x1_t vreinterpret_s64_u8 (uint8x8_t)
@end itemize


@itemize @bullet
@item int64x1_t vreinterpret_s64_u16 (uint16x4_t)
@end itemize


@itemize @bullet
@item int64x1_t vreinterpret_s64_u32 (uint32x2_t)
@end itemize


@itemize @bullet
@item uint64x1_t vreinterpret_u64_p8 (poly8x8_t)
@end itemize


@itemize @bullet
@item uint64x1_t vreinterpret_u64_p16 (poly16x4_t)
@end itemize


@itemize @bullet
@item uint64x1_t vreinterpret_u64_f32 (float32x2_t)
@end itemize


@itemize @bullet
@item uint64x1_t vreinterpret_u64_p64 (poly64x1_t)
@end itemize


@itemize @bullet
@item uint64x1_t vreinterpret_u64_s64 (int64x1_t)
@end itemize


@itemize @bullet
@item uint64x1_t vreinterpret_u64_s8 (int8x8_t)
@end itemize


@itemize @bullet
@item uint64x1_t vreinterpret_u64_s16 (int16x4_t)
@end itemize


@itemize @bullet
@item uint64x1_t vreinterpret_u64_s32 (int32x2_t)
@end itemize


@itemize @bullet
@item uint64x1_t vreinterpret_u64_u8 (uint8x8_t)
@end itemize


@itemize @bullet
@item uint64x1_t vreinterpret_u64_u16 (uint16x4_t)
@end itemize


@itemize @bullet
@item uint64x1_t vreinterpret_u64_u32 (uint32x2_t)
@end itemize


@itemize @bullet
@item int8x8_t vreinterpret_s8_p8 (poly8x8_t)
@end itemize


@itemize @bullet
@item int8x8_t vreinterpret_s8_p16 (poly16x4_t)
@end itemize


@itemize @bullet
@item int8x8_t vreinterpret_s8_f32 (float32x2_t)
@end itemize


@itemize @bullet
@item int8x8_t vreinterpret_s8_p64 (poly64x1_t)
@end itemize


@itemize @bullet
@item int8x8_t vreinterpret_s8_s64 (int64x1_t)
@end itemize


@itemize @bullet
@item int8x8_t vreinterpret_s8_u64 (uint64x1_t)
@end itemize


@itemize @bullet
@item int8x8_t vreinterpret_s8_s16 (int16x4_t)
@end itemize


@itemize @bullet
@item int8x8_t vreinterpret_s8_s32 (int32x2_t)
@end itemize


@itemize @bullet
@item int8x8_t vreinterpret_s8_u8 (uint8x8_t)
@end itemize


@itemize @bullet
@item int8x8_t vreinterpret_s8_u16 (uint16x4_t)
@end itemize


@itemize @bullet
@item int8x8_t vreinterpret_s8_u32 (uint32x2_t)
@end itemize


@itemize @bullet
@item int16x4_t vreinterpret_s16_p8 (poly8x8_t)
@end itemize


@itemize @bullet
@item int16x4_t vreinterpret_s16_p16 (poly16x4_t)
@end itemize


@itemize @bullet
@item int16x4_t vreinterpret_s16_f32 (float32x2_t)
@end itemize


@itemize @bullet
@item int16x4_t vreinterpret_s16_p64 (poly64x1_t)
@end itemize


@itemize @bullet
@item int16x4_t vreinterpret_s16_s64 (int64x1_t)
@end itemize


@itemize @bullet
@item int16x4_t vreinterpret_s16_u64 (uint64x1_t)
@end itemize


@itemize @bullet
@item int16x4_t vreinterpret_s16_s8 (int8x8_t)
@end itemize


@itemize @bullet
@item int16x4_t vreinterpret_s16_s32 (int32x2_t)
@end itemize


@itemize @bullet
@item int16x4_t vreinterpret_s16_u8 (uint8x8_t)
@end itemize


@itemize @bullet
@item int16x4_t vreinterpret_s16_u16 (uint16x4_t)
@end itemize


@itemize @bullet
@item int16x4_t vreinterpret_s16_u32 (uint32x2_t)
@end itemize


@itemize @bullet
@item int32x2_t vreinterpret_s32_p8 (poly8x8_t)
@end itemize


@itemize @bullet
@item int32x2_t vreinterpret_s32_p16 (poly16x4_t)
@end itemize


@itemize @bullet
@item int32x2_t vreinterpret_s32_f32 (float32x2_t)
@end itemize


@itemize @bullet
@item int32x2_t vreinterpret_s32_p64 (poly64x1_t)
@end itemize


@itemize @bullet
@item int32x2_t vreinterpret_s32_s64 (int64x1_t)
@end itemize


@itemize @bullet
@item int32x2_t vreinterpret_s32_u64 (uint64x1_t)
@end itemize


@itemize @bullet
@item int32x2_t vreinterpret_s32_s8 (int8x8_t)
@end itemize


@itemize @bullet
@item int32x2_t vreinterpret_s32_s16 (int16x4_t)
@end itemize


@itemize @bullet
@item int32x2_t vreinterpret_s32_u8 (uint8x8_t)
@end itemize


@itemize @bullet
@item int32x2_t vreinterpret_s32_u16 (uint16x4_t)
@end itemize


@itemize @bullet
@item int32x2_t vreinterpret_s32_u32 (uint32x2_t)
@end itemize


@itemize @bullet
@item uint8x8_t vreinterpret_u8_p8 (poly8x8_t)
@end itemize


@itemize @bullet
@item uint8x8_t vreinterpret_u8_p16 (poly16x4_t)
@end itemize


@itemize @bullet
@item uint8x8_t vreinterpret_u8_f32 (float32x2_t)
@end itemize


@itemize @bullet
@item uint8x8_t vreinterpret_u8_p64 (poly64x1_t)
@end itemize


@itemize @bullet
@item uint8x8_t vreinterpret_u8_s64 (int64x1_t)
@end itemize


@itemize @bullet
@item uint8x8_t vreinterpret_u8_u64 (uint64x1_t)
@end itemize


@itemize @bullet
@item uint8x8_t vreinterpret_u8_s8 (int8x8_t)
@end itemize


@itemize @bullet
@item uint8x8_t vreinterpret_u8_s16 (int16x4_t)
@end itemize


@itemize @bullet
@item uint8x8_t vreinterpret_u8_s32 (int32x2_t)
@end itemize


@itemize @bullet
@item uint8x8_t vreinterpret_u8_u16 (uint16x4_t)
@end itemize


@itemize @bullet
@item uint8x8_t vreinterpret_u8_u32 (uint32x2_t)
@end itemize


@itemize @bullet
@item uint16x4_t vreinterpret_u16_p8 (poly8x8_t)
@end itemize


@itemize @bullet
@item uint16x4_t vreinterpret_u16_p16 (poly16x4_t)
@end itemize


@itemize @bullet
@item uint16x4_t vreinterpret_u16_f32 (float32x2_t)
@end itemize


@itemize @bullet
@item uint16x4_t vreinterpret_u16_p64 (poly64x1_t)
@end itemize


@itemize @bullet
@item uint16x4_t vreinterpret_u16_s64 (int64x1_t)
@end itemize


@itemize @bullet
@item uint16x4_t vreinterpret_u16_u64 (uint64x1_t)
@end itemize


@itemize @bullet
@item uint16x4_t vreinterpret_u16_s8 (int8x8_t)
@end itemize


@itemize @bullet
@item uint16x4_t vreinterpret_u16_s16 (int16x4_t)
@end itemize


@itemize @bullet
@item uint16x4_t vreinterpret_u16_s32 (int32x2_t)
@end itemize


@itemize @bullet
@item uint16x4_t vreinterpret_u16_u8 (uint8x8_t)
@end itemize


@itemize @bullet
@item uint16x4_t vreinterpret_u16_u32 (uint32x2_t)
@end itemize


@itemize @bullet
@item uint32x2_t vreinterpret_u32_p8 (poly8x8_t)
@end itemize


@itemize @bullet
@item uint32x2_t vreinterpret_u32_p16 (poly16x4_t)
@end itemize


@itemize @bullet
@item uint32x2_t vreinterpret_u32_f32 (float32x2_t)
@end itemize


@itemize @bullet
@item uint32x2_t vreinterpret_u32_p64 (poly64x1_t)
@end itemize


@itemize @bullet
@item uint32x2_t vreinterpret_u32_s64 (int64x1_t)
@end itemize


@itemize @bullet
@item uint32x2_t vreinterpret_u32_u64 (uint64x1_t)
@end itemize


@itemize @bullet
@item uint32x2_t vreinterpret_u32_s8 (int8x8_t)
@end itemize


@itemize @bullet
@item uint32x2_t vreinterpret_u32_s16 (int16x4_t)
@end itemize


@itemize @bullet
@item uint32x2_t vreinterpret_u32_s32 (int32x2_t)
@end itemize


@itemize @bullet
@item uint32x2_t vreinterpret_u32_u8 (uint8x8_t)
@end itemize


@itemize @bullet
@item uint32x2_t vreinterpret_u32_u16 (uint16x4_t)
@end itemize


@itemize @bullet
@item poly8x16_t vreinterpretq_p8_p16 (poly16x8_t)
@end itemize


@itemize @bullet
@item poly8x16_t vreinterpretq_p8_f32 (float32x4_t)
@end itemize


@itemize @bullet
@item poly8x16_t vreinterpretq_p8_p64 (poly64x2_t)
@end itemize


@itemize @bullet
@item poly8x16_t vreinterpretq_p8_p128 (poly128_t)
@end itemize


@itemize @bullet
@item poly8x16_t vreinterpretq_p8_s64 (int64x2_t)
@end itemize


@itemize @bullet
@item poly8x16_t vreinterpretq_p8_u64 (uint64x2_t)
@end itemize


@itemize @bullet
@item poly8x16_t vreinterpretq_p8_s8 (int8x16_t)
@end itemize


@itemize @bullet
@item poly8x16_t vreinterpretq_p8_s16 (int16x8_t)
@end itemize


@itemize @bullet
@item poly8x16_t vreinterpretq_p8_s32 (int32x4_t)
@end itemize


@itemize @bullet
@item poly8x16_t vreinterpretq_p8_u8 (uint8x16_t)
@end itemize


@itemize @bullet
@item poly8x16_t vreinterpretq_p8_u16 (uint16x8_t)
@end itemize


@itemize @bullet
@item poly8x16_t vreinterpretq_p8_u32 (uint32x4_t)
@end itemize


@itemize @bullet
@item poly16x8_t vreinterpretq_p16_p8 (poly8x16_t)
@end itemize


@itemize @bullet
@item poly16x8_t vreinterpretq_p16_f32 (float32x4_t)
@end itemize


@itemize @bullet
@item poly16x8_t vreinterpretq_p16_p64 (poly64x2_t)
@end itemize


@itemize @bullet
@item poly16x8_t vreinterpretq_p16_p128 (poly128_t)
@end itemize


@itemize @bullet
@item poly16x8_t vreinterpretq_p16_s64 (int64x2_t)
@end itemize


@itemize @bullet
@item poly16x8_t vreinterpretq_p16_u64 (uint64x2_t)
@end itemize


@itemize @bullet
@item poly16x8_t vreinterpretq_p16_s8 (int8x16_t)
@end itemize


@itemize @bullet
@item poly16x8_t vreinterpretq_p16_s16 (int16x8_t)
@end itemize


@itemize @bullet
@item poly16x8_t vreinterpretq_p16_s32 (int32x4_t)
@end itemize


@itemize @bullet
@item poly16x8_t vreinterpretq_p16_u8 (uint8x16_t)
@end itemize


@itemize @bullet
@item poly16x8_t vreinterpretq_p16_u16 (uint16x8_t)
@end itemize


@itemize @bullet
@item poly16x8_t vreinterpretq_p16_u32 (uint32x4_t)
@end itemize


@itemize @bullet
@item float32x4_t vreinterpretq_f32_p8 (poly8x16_t)
@end itemize


@itemize @bullet
@item float32x4_t vreinterpretq_f32_p16 (poly16x8_t)
@end itemize


@itemize @bullet
@item float32x4_t vreinterpretq_f32_p64 (poly64x2_t)
@end itemize


@itemize @bullet
@item float32x4_t vreinterpretq_f32_p128 (poly128_t)
@end itemize


@itemize @bullet
@item float32x4_t vreinterpretq_f32_s64 (int64x2_t)
@end itemize


@itemize @bullet
@item float32x4_t vreinterpretq_f32_u64 (uint64x2_t)
@end itemize


@itemize @bullet
@item float32x4_t vreinterpretq_f32_s8 (int8x16_t)
@end itemize


@itemize @bullet
@item float32x4_t vreinterpretq_f32_s16 (int16x8_t)
@end itemize


@itemize @bullet
@item float32x4_t vreinterpretq_f32_s32 (int32x4_t)
@end itemize


@itemize @bullet
@item float32x4_t vreinterpretq_f32_u8 (uint8x16_t)
@end itemize


@itemize @bullet
@item float32x4_t vreinterpretq_f32_u16 (uint16x8_t)
@end itemize


@itemize @bullet
@item float32x4_t vreinterpretq_f32_u32 (uint32x4_t)
@end itemize


@itemize @bullet
@item poly64x2_t vreinterpretq_p64_p8 (poly8x16_t)
@end itemize


@itemize @bullet
@item poly64x2_t vreinterpretq_p64_p16 (poly16x8_t)
@end itemize


@itemize @bullet
@item poly64x2_t vreinterpretq_p64_f32 (float32x4_t)
@end itemize


@itemize @bullet
@item poly64x2_t vreinterpretq_p64_p128 (poly128_t)
@end itemize


@itemize @bullet
@item poly64x2_t vreinterpretq_p64_s64 (int64x2_t)
@end itemize


@itemize @bullet
@item poly64x2_t vreinterpretq_p64_u64 (uint64x2_t)
@end itemize


@itemize @bullet
@item poly64x2_t vreinterpretq_p64_s8 (int8x16_t)
@end itemize


@itemize @bullet
@item poly64x2_t vreinterpretq_p64_s16 (int16x8_t)
@end itemize


@itemize @bullet
@item poly64x2_t vreinterpretq_p64_s32 (int32x4_t)
@end itemize


@itemize @bullet
@item poly64x2_t vreinterpretq_p64_u8 (uint8x16_t)
@end itemize


@itemize @bullet
@item poly64x2_t vreinterpretq_p64_u16 (uint16x8_t)
@end itemize


@itemize @bullet
@item poly64x2_t vreinterpretq_p64_u32 (uint32x4_t)
@end itemize


@itemize @bullet
@item poly128_t vreinterpretq_p128_p8 (poly8x16_t)
@end itemize


@itemize @bullet
@item poly128_t vreinterpretq_p128_p16 (poly16x8_t)
@end itemize


@itemize @bullet
@item poly128_t vreinterpretq_p128_f32 (float32x4_t)
@end itemize


@itemize @bullet
@item poly128_t vreinterpretq_p128_p64 (poly64x2_t)
@end itemize


@itemize @bullet
@item poly128_t vreinterpretq_p128_s64 (int64x2_t)
@end itemize


@itemize @bullet
@item poly128_t vreinterpretq_p128_u64 (uint64x2_t)
@end itemize


@itemize @bullet
@item poly128_t vreinterpretq_p128_s8 (int8x16_t)
@end itemize


@itemize @bullet
@item poly128_t vreinterpretq_p128_s16 (int16x8_t)
@end itemize


@itemize @bullet
@item poly128_t vreinterpretq_p128_s32 (int32x4_t)
@end itemize


@itemize @bullet
@item poly128_t vreinterpretq_p128_u8 (uint8x16_t)
@end itemize


@itemize @bullet
@item poly128_t vreinterpretq_p128_u16 (uint16x8_t)
@end itemize


@itemize @bullet
@item poly128_t vreinterpretq_p128_u32 (uint32x4_t)
@end itemize


@itemize @bullet
@item int64x2_t vreinterpretq_s64_p8 (poly8x16_t)
@end itemize


@itemize @bullet
@item int64x2_t vreinterpretq_s64_p16 (poly16x8_t)
@end itemize


@itemize @bullet
@item int64x2_t vreinterpretq_s64_f32 (float32x4_t)
@end itemize


@itemize @bullet
@item int64x2_t vreinterpretq_s64_p64 (poly64x2_t)
@end itemize


@itemize @bullet
@item int64x2_t vreinterpretq_s64_p128 (poly128_t)
@end itemize


@itemize @bullet
@item int64x2_t vreinterpretq_s64_u64 (uint64x2_t)
@end itemize


@itemize @bullet
@item int64x2_t vreinterpretq_s64_s8 (int8x16_t)
@end itemize


@itemize @bullet
@item int64x2_t vreinterpretq_s64_s16 (int16x8_t)
@end itemize


@itemize @bullet
@item int64x2_t vreinterpretq_s64_s32 (int32x4_t)
@end itemize


@itemize @bullet
@item int64x2_t vreinterpretq_s64_u8 (uint8x16_t)
@end itemize


@itemize @bullet
@item int64x2_t vreinterpretq_s64_u16 (uint16x8_t)
@end itemize


@itemize @bullet
@item int64x2_t vreinterpretq_s64_u32 (uint32x4_t)
@end itemize


@itemize @bullet
@item uint64x2_t vreinterpretq_u64_p8 (poly8x16_t)
@end itemize


@itemize @bullet
@item uint64x2_t vreinterpretq_u64_p16 (poly16x8_t)
@end itemize


@itemize @bullet
@item uint64x2_t vreinterpretq_u64_f32 (float32x4_t)
@end itemize


@itemize @bullet
@item uint64x2_t vreinterpretq_u64_p64 (poly64x2_t)
@end itemize


@itemize @bullet
@item uint64x2_t vreinterpretq_u64_p128 (poly128_t)
@end itemize


@itemize @bullet
@item uint64x2_t vreinterpretq_u64_s64 (int64x2_t)
@end itemize


@itemize @bullet
@item uint64x2_t vreinterpretq_u64_s8 (int8x16_t)
@end itemize


@itemize @bullet
@item uint64x2_t vreinterpretq_u64_s16 (int16x8_t)
@end itemize


@itemize @bullet
@item uint64x2_t vreinterpretq_u64_s32 (int32x4_t)
@end itemize


@itemize @bullet
@item uint64x2_t vreinterpretq_u64_u8 (uint8x16_t)
@end itemize


@itemize @bullet
@item uint64x2_t vreinterpretq_u64_u16 (uint16x8_t)
@end itemize


@itemize @bullet
@item uint64x2_t vreinterpretq_u64_u32 (uint32x4_t)
@end itemize


@itemize @bullet
@item int8x16_t vreinterpretq_s8_p8 (poly8x16_t)
@end itemize


@itemize @bullet
@item int8x16_t vreinterpretq_s8_p16 (poly16x8_t)
@end itemize


@itemize @bullet
@item int8x16_t vreinterpretq_s8_f32 (float32x4_t)
@end itemize


@itemize @bullet
@item int8x16_t vreinterpretq_s8_p64 (poly64x2_t)
@end itemize


@itemize @bullet
@item int8x16_t vreinterpretq_s8_p128 (poly128_t)
@end itemize


@itemize @bullet
@item int8x16_t vreinterpretq_s8_s64 (int64x2_t)
@end itemize


@itemize @bullet
@item int8x16_t vreinterpretq_s8_u64 (uint64x2_t)
@end itemize


@itemize @bullet
@item int8x16_t vreinterpretq_s8_s16 (int16x8_t)
@end itemize


@itemize @bullet
@item int8x16_t vreinterpretq_s8_s32 (int32x4_t)
@end itemize


@itemize @bullet
@item int8x16_t vreinterpretq_s8_u8 (uint8x16_t)
@end itemize


@itemize @bullet
@item int8x16_t vreinterpretq_s8_u16 (uint16x8_t)
@end itemize


@itemize @bullet
@item int8x16_t vreinterpretq_s8_u32 (uint32x4_t)
@end itemize


@itemize @bullet
@item int16x8_t vreinterpretq_s16_p8 (poly8x16_t)
@end itemize


@itemize @bullet
@item int16x8_t vreinterpretq_s16_p16 (poly16x8_t)
@end itemize


@itemize @bullet
@item int16x8_t vreinterpretq_s16_f32 (float32x4_t)
@end itemize


@itemize @bullet
@item int16x8_t vreinterpretq_s16_p64 (poly64x2_t)
@end itemize


@itemize @bullet
@item int16x8_t vreinterpretq_s16_p128 (poly128_t)
@end itemize


@itemize @bullet
@item int16x8_t vreinterpretq_s16_s64 (int64x2_t)
@end itemize


@itemize @bullet
@item int16x8_t vreinterpretq_s16_u64 (uint64x2_t)
@end itemize


@itemize @bullet
@item int16x8_t vreinterpretq_s16_s8 (int8x16_t)
@end itemize


@itemize @bullet
@item int16x8_t vreinterpretq_s16_s32 (int32x4_t)
@end itemize


@itemize @bullet
@item int16x8_t vreinterpretq_s16_u8 (uint8x16_t)
@end itemize


@itemize @bullet
@item int16x8_t vreinterpretq_s16_u16 (uint16x8_t)
@end itemize


@itemize @bullet
@item int16x8_t vreinterpretq_s16_u32 (uint32x4_t)
@end itemize


@itemize @bullet
@item int32x4_t vreinterpretq_s32_p8 (poly8x16_t)
@end itemize


@itemize @bullet
@item int32x4_t vreinterpretq_s32_p16 (poly16x8_t)
@end itemize


@itemize @bullet
@item int32x4_t vreinterpretq_s32_f32 (float32x4_t)
@end itemize


@itemize @bullet
@item int32x4_t vreinterpretq_s32_p64 (poly64x2_t)
@end itemize


@itemize @bullet
@item int32x4_t vreinterpretq_s32_p128 (poly128_t)
@end itemize


@itemize @bullet
@item int32x4_t vreinterpretq_s32_s64 (int64x2_t)
@end itemize


@itemize @bullet
@item int32x4_t vreinterpretq_s32_u64 (uint64x2_t)
@end itemize


@itemize @bullet
@item int32x4_t vreinterpretq_s32_s8 (int8x16_t)
@end itemize


@itemize @bullet
@item int32x4_t vreinterpretq_s32_s16 (int16x8_t)
@end itemize


@itemize @bullet
@item int32x4_t vreinterpretq_s32_u8 (uint8x16_t)
@end itemize


@itemize @bullet
@item int32x4_t vreinterpretq_s32_u16 (uint16x8_t)
@end itemize


@itemize @bullet
@item int32x4_t vreinterpretq_s32_u32 (uint32x4_t)
@end itemize


@itemize @bullet
@item uint8x16_t vreinterpretq_u8_p8 (poly8x16_t)
@end itemize


@itemize @bullet
@item uint8x16_t vreinterpretq_u8_p16 (poly16x8_t)
@end itemize


@itemize @bullet
@item uint8x16_t vreinterpretq_u8_f32 (float32x4_t)
@end itemize


@itemize @bullet
@item uint8x16_t vreinterpretq_u8_p64 (poly64x2_t)
@end itemize


@itemize @bullet
@item uint8x16_t vreinterpretq_u8_p128 (poly128_t)
@end itemize


@itemize @bullet
@item uint8x16_t vreinterpretq_u8_s64 (int64x2_t)
@end itemize


@itemize @bullet
@item uint8x16_t vreinterpretq_u8_u64 (uint64x2_t)
@end itemize


@itemize @bullet
@item uint8x16_t vreinterpretq_u8_s8 (int8x16_t)
@end itemize


@itemize @bullet
@item uint8x16_t vreinterpretq_u8_s16 (int16x8_t)
@end itemize


@itemize @bullet
@item uint8x16_t vreinterpretq_u8_s32 (int32x4_t)
@end itemize


@itemize @bullet
@item uint8x16_t vreinterpretq_u8_u16 (uint16x8_t)
@end itemize


@itemize @bullet
@item uint8x16_t vreinterpretq_u8_u32 (uint32x4_t)
@end itemize


@itemize @bullet
@item uint16x8_t vreinterpretq_u16_p8 (poly8x16_t)
@end itemize


@itemize @bullet
@item uint16x8_t vreinterpretq_u16_p16 (poly16x8_t)
@end itemize


@itemize @bullet
@item uint16x8_t vreinterpretq_u16_f32 (float32x4_t)
@end itemize


@itemize @bullet
@item uint16x8_t vreinterpretq_u16_p64 (poly64x2_t)
@end itemize


@itemize @bullet
@item uint16x8_t vreinterpretq_u16_p128 (poly128_t)
@end itemize


@itemize @bullet
@item uint16x8_t vreinterpretq_u16_s64 (int64x2_t)
@end itemize


@itemize @bullet
@item uint16x8_t vreinterpretq_u16_u64 (uint64x2_t)
@end itemize


@itemize @bullet
@item uint16x8_t vreinterpretq_u16_s8 (int8x16_t)
@end itemize


@itemize @bullet
@item uint16x8_t vreinterpretq_u16_s16 (int16x8_t)
@end itemize


@itemize @bullet
@item uint16x8_t vreinterpretq_u16_s32 (int32x4_t)
@end itemize


@itemize @bullet
@item uint16x8_t vreinterpretq_u16_u8 (uint8x16_t)
@end itemize


@itemize @bullet
@item uint16x8_t vreinterpretq_u16_u32 (uint32x4_t)
@end itemize


@itemize @bullet
@item uint32x4_t vreinterpretq_u32_p8 (poly8x16_t)
@end itemize


@itemize @bullet
@item uint32x4_t vreinterpretq_u32_p16 (poly16x8_t)
@end itemize


@itemize @bullet
@item uint32x4_t vreinterpretq_u32_f32 (float32x4_t)
@end itemize


@itemize @bullet
@item uint32x4_t vreinterpretq_u32_p64 (poly64x2_t)
@end itemize


@itemize @bullet
@item uint32x4_t vreinterpretq_u32_p128 (poly128_t)
@end itemize


@itemize @bullet
@item uint32x4_t vreinterpretq_u32_s64 (int64x2_t)
@end itemize


@itemize @bullet
@item uint32x4_t vreinterpretq_u32_u64 (uint64x2_t)
@end itemize


@itemize @bullet
@item uint32x4_t vreinterpretq_u32_s8 (int8x16_t)
@end itemize


@itemize @bullet
@item uint32x4_t vreinterpretq_u32_s16 (int16x8_t)
@end itemize


@itemize @bullet
@item uint32x4_t vreinterpretq_u32_s32 (int32x4_t)
@end itemize


@itemize @bullet
@item uint32x4_t vreinterpretq_u32_u8 (uint8x16_t)
@end itemize


@itemize @bullet
@item uint32x4_t vreinterpretq_u32_u16 (uint16x8_t)
@end itemize





@itemize @bullet
@item poly128_t vldrq_p128(poly128_t const *)
@end itemize

@itemize @bullet
@item void vstrq_p128(poly128_t *, poly128_t)
@end itemize

@itemize @bullet
@item uint64x1_t vceq_p64 (poly64x1_t, poly64x1_t)
@end itemize

@itemize @bullet
@item uint64x1_t vtst_p64 (poly64x1_t, poly64x1_t)
@end itemize

@itemize @bullet
@item uint32_t vsha1h_u32 (uint32_t)
@*@emph{Form of expected instruction(s):} @code{sha1h.32 @var{q0}, @var{q1}}
@end itemize

@itemize @bullet
@item uint32x4_t vsha1cq_u32 (uint32x4_t, uint32_t, uint32x4_t)
@*@emph{Form of expected instruction(s):} @code{sha1c.32 @var{q0}, @var{q1}, @var{q2}}
@end itemize

@itemize @bullet
@item uint32x4_t vsha1pq_u32 (uint32x4_t, uint32_t, uint32x4_t)
@*@emph{Form of expected instruction(s):} @code{sha1p.32 @var{q0}, @var{q1}, @var{q2}}
@end itemize

@itemize @bullet
@item uint32x4_t vsha1mq_u32 (uint32x4_t, uint32_t, uint32x4_t)
@*@emph{Form of expected instruction(s):} @code{sha1m.32 @var{q0}, @var{q1}, @var{q2}}
@end itemize

@itemize @bullet
@item uint32x4_t vsha1su0q_u32 (uint32x4_t, uint32x4_t, uint32x4_t)
@*@emph{Form of expected instruction(s):} @code{sha1su0.32 @var{q0}, @var{q1}, @var{q2}}
@end itemize

@itemize @bullet
@item uint32x4_t vsha1su1q_u32 (uint32x4_t, uint32x4_t)
@*@emph{Form of expected instruction(s):} @code{sha1su1.32 @var{q0}, @var{q1}, @var{q2}}
@end itemize

@itemize @bullet
@item uint32x4_t vsha256hq_u32 (uint32x4_t, uint32x4_t, uint32x4_t)
@*@emph{Form of expected instruction(s):} @code{sha256h.32 @var{q0}, @var{q1}, @var{q2}}
@end itemize
 
@itemize @bullet
@item uint32x4_t vsha256h2q_u32 (uint32x4_t, uint32x4_t, uint32x4_t)
@*@emph{Form of expected instruction(s):} @code{sha256h2.32 @var{q0}, @var{q1}, @var{q2}}
@end itemize
 
@itemize @bullet
@item uint32x4_t vsha256su0q_u32 (uint32x4_t, uint32x4_t)
@*@emph{Form of expected instruction(s):} @code{sha256su0.32 @var{q0}, @var{q1}}
@end itemize
 
@itemize @bullet
@item uint32x4_t vsha256su1q_u32 (uint32x4_t, uint32x4_t, uint32x4_t)
@*@emph{Form of expected instruction(s):} @code{sha256su1.32 @var{q0}, @var{q1}, @var{q2}}
@end itemize

@itemize @bullet
@item poly128_t vmull_p64 (poly64_t a, poly64_t b)
@*@emph{Form of expected instruction(s):} @code{vmull.p64 @var{q0}, @var{d1}, @var{d2}}
@end itemize

@itemize @bullet
@item poly128_t vmull_high_p64 (poly64x2_t a, poly64x2_t b)
@*@emph{Form of expected instruction(s):} @code{vmull.p64 @var{q0}, @var{d1}, @var{d2}}
@end itemize

