- NAME
- SYNOPSIS
- DESCRIPTION
- OPTIONS
- KEY GENERATION OPTIONS

- RSA Key Generation Options
- EC Key Generation Options

- PARAMETER GENERATION OPTIONS

- DSA Parameter Generation Options
- DH Parameter Generation Options
- EC Parameter Generation Options

- GOST2001 KEY GENERATION AND PARAMETER OPTIONS
- NOTES
- EXAMPLES
- HISTORY

# NAME

openssl-genpkey, genpkey - generate a private key

# SYNOPSIS

openssl genpkey [-out filename] [-outform PEM|DER] [-pass arg] [-cipher] [-engine id] [-paramfile file] [-algorithm alg] [-pkeyopt opt:value] [-genparam] [-text]

# DESCRIPTION

The genpkey command generates a private key.

# OPTIONS

-out filename

  the output filename. If this argument is not specified then standard output is used.

-outform DER|PEM

  This specifies the output format DER or PEM. The default format is PEM.

-pass arg

  The output file password source. For more information about the format of arg see the PASS PHRASE ARGUMENTS section in openssl(1).

-cipher

  This option encrypts the private key with the supplied cipher. Any algorithm name accepted by `EVP_get_cipherbyname()` is acceptable such as des3.

-engine id

  Specifying an engine (by its unique id string) will cause genpkey to attempt to obtain a functional reference to the specified engine, thus initialising it if needed. The engine will then be set as the default for all available algorithms. If used this option should precede all other options.

-algorithm alg

  Public key algorithm to use such as RSA, DSA or DH. If used this option must precede any -pkeyopt options. The options -paramfile and -algorithm are mutually exclusive. Engines may add algorithms in addition to the standard built-in ones.

  Valid built-in algorithm names for private key generation are RSA and EC.

  Valid built-in algorithm names for parameter generation (see the -genparam option) are DH, DSA and EC.

  Note that the algorithm name X9.42 DH may be used as a synonym for the DH algorithm. These are identical and do not indicate the type of parameters that will be generated. Use the dh_paramgen_type option to indicate whether PKCS#3 or X9.42 DH parameters are required. See DH Parameter Generation Options below for more details.

-pkeyopt opt:value

  Set the public key algorithm option opt to value. The precise set of options supported depends on the public key algorithm used and its implementation. See KEY GENERATION OPTIONS and PARAMETER GENERATION OPTIONS below for more details.

-genparam

  Generate a set of parameters instead of a private key. If used this option must precede any -algorithm, -paramfile or -pkeyopt options.

-paramfile filename

  Some public key algorithms generate a private key based on a set of parameters. They can be supplied using this option. If this option is used the public key algorithm used is determined by the parameters. If used this option must precede and -pkeyopt options. The options -paramfile and -algorithm are mutually exclusive.

-text

  Print an (unencrypted) text representation of private and public keys and parameters along with the PEM or DER structure.

# KEY GENERATION OPTIONS

The options supported by each algorith and indeed each implementation of an algorithm can vary. The options for the OpenSSL implementations are detailed below.

## RSA Key Generation Options

rsa_keygen_bits:numbits

  The number of bits in the generated key. If not specified 2048 is used.

rsa_keygen_pubexp:value

  The RSA public exponent value. This can be a large decimal or hexadecimal value if preceded by 0x. Default value is 65537.

## EC Key Generation Options

The EC key generation options can also be used for parameter generation.

ec_paramgen_curve:curve

  The EC curve to use. OpenSSL supports NIST curve names such as ``P-256''.

ec_param_enc:encoding

  The encoding to use for parameters. The ``encoding'' parameter must be either ``named_curve'' or ``explicit''. The default value is ``named_curve''.

# PARAMETER GENERATION OPTIONS

The options supported by each algorithm and indeed each implementation of an algorithm can vary. The options for the OpenSSL implementations are detailed below.

## DSA Parameter Generation Options

dsa_paramgen_bits:numbits

  The number of bits in the generated prime. If not specified 2048 is used.

dsa_paramgen_q_bits:numbits

  The number of bits in the q parameter. Must be one of 160, 224 or 256. If not specified 224 is used.

dsa_paramgen_md:digest

  The digest to use during parameter generation. Must be one of sha1, sha224 or sha256. If set, then the number of bits in q will match the output size of the specified digest and the dsa_paramgen_q_bits parameter will be ignored. If not set, then a digest will be used that gives an output matching the number of bits in q, i.e. sha1 if q length is 160, sha224 if it 224 or sha256 if it is 256.

## DH Parameter Generation Options

dh_paramgen_prime_len:numbits

  The number of bits in the prime parameter p. The default is 2048.

dh_paramgen_subprime_len:numbits

  The number of bits in the sub prime parameter q. The default is 256 if the prime is at least 2048 bits long or 160 otherwise. Only relevant if used in conjunction with the dh_paramgen_type option to generate X9.42 DH parameters.

dh_paramgen_generator:value

  The value to use for the generator g. The default is 2.

dh_paramgen_type:value

  The type of DH parameters to generate. Use 0 for PKCS#3 DH and 1 for X9.42 DH. The default is 0.

dh_rfc5114:num

  If this option is set, then the appropriate RFC5114 parameters are used instead of generating new parameters. The value num can take the values 1, 2 or 3 corresponding to RFC5114 DH parameters consisting of 1024 bit group with 160 bit subgroup, 2048 bit group with 224 bit subgroup and 2048 bit group with 256 bit subgroup as mentioned in RFC5114 sections 2.1, 2.2 and 2.3 respectively. If present this overrides all other DH parameter options.

## EC Parameter Generation Options

The EC parameter generation options are the same as for key generation. See EC Key Generation Options above.

# GOST2001 KEY GENERATION AND PARAMETER OPTIONS

Gost 2001 support is not enabled by default. To enable this algorithm, one should load the ccgost engine in the OpenSSL configuration file. See README.gost file in the engines/ccgost directiry of the source distribution for more details.

Use of a parameter file for the GOST R 34.10 algorithm is optional. Parameters can be specified during key generation directly as well as during generation of parameter file.

paramset:name

  Specifies GOST R 34.10-2001 parameter set according to RFC 4357. Parameter set can be specified using abbreviated name, object short name or numeric OID. Following parameter sets are supported:

        paramset   OID               Usage
        A          1.2.643.2.2.35.1  Signature
        B          1.2.643.2.2.35.2  Signature
        C          1.2.643.2.2.35.3  Signature
        XA         1.2.643.2.2.36.0  Key exchange
        XB         1.2.643.2.2.36.1  Key exchange
        test       1.2.643.2.2.35.0  Test purposes

# NOTES

The use of the genpkey program is encouraged over the algorithm specific utilities because additional algorithm options and ENGINE provided algorithms can be used.

# EXAMPLES

Generate an RSA private key using default parameters:

     openssl genpkey -algorithm RSA -out key.pem

Encrypt output private key using 128 bit AES and the passphrase ``hello'':

     openssl genpkey -algorithm RSA -out key.pem -aes-128-cbc -pass pass:hello

Generate a 2048 bit RSA key using 3 as the public exponent:

     openssl genpkey -algorithm RSA -out key.pem -pkeyopt rsa_keygen_bits:2048 \
                                                    -pkeyopt rsa_keygen_pubexp:3

Generate 2048 bit DSA parameters:

     openssl genpkey -genparam -algorithm DSA -out dsap.pem \
                                                    -pkeyopt dsa_paramgen_bits:2048

Generate DSA key from parameters:

     openssl genpkey -paramfile dsap.pem -out dsakey.pem

Generate 2048 bit DH parameters:

     openssl genpkey -genparam -algorithm DH -out dhp.pem \
                                            -pkeyopt dh_paramgen_prime_len:2048

Generate 2048 bit X9.42 DH parameters:

     openssl genpkey -genparam -algorithm DH -out dhpx.pem \
                                            -pkeyopt dh_paramgen_prime_len:2048 \
                                            -pkeyopt dh_paramgen_type:1

Output RFC5114 2048 bit DH parameters with 224 bit subgroup:

     openssl genpkey -genparam -algorithm DH -out dhp.pem -pkeyopt dh_rfc5114:2

Generate DH key from parameters:

     openssl genpkey -paramfile dhp.pem -out dhkey.pem

Generate EC key directly:

     openssl genpkey -algorithm EC -out eckey.pem \
            -pkeyopt ec_paramgen_curve:P-384 \
            -pkeyopt ec_param_enc:named_curve

# HISTORY

The ability to use NIST curve names, and to generate an EC key directly, were added in OpenSSL 1.0.2.