- NAME
- SYNOPSIS
- DESCRIPTION
- COMMAND OPTIONS
- EXAMPLES
- NOTES
- SEE ALSO

# NAME

openssl-crl2pkcs7, crl2pkcs7 - Create a PKCS#7 structure from a CRL and certificates.

# SYNOPSIS

openssl crl2pkcs7 [-inform PEM|DER] [-outform PEM|DER] [-in filename] [-out filename] [-certfile filename] [-nocrl]

# DESCRIPTION

The crl2pkcs7 command takes an optional CRL and one or more certificates and converts them into a PKCS#7 degenerate ``certificates only'' structure.

# COMMAND OPTIONS

-inform DER|PEM

  This specifies the CRL input format. DER format is DER encoded CRL structure.PEM (the default) is a base64 encoded version of the DER form with header and footer lines.

-outform DER|PEM

  This specifies the PKCS#7 structure output format. DER format is DER encoded PKCS#7 structure.PEM (the default) is a base64 encoded version of the DER form with header and footer lines.

-in filename

  This specifies the input filename to read a CRL from or standard input if this option is not specified.

-out filename

  specifies the output filename to write the PKCS#7 structure to or standard output by default.

-certfile filename

  specifies a filename containing one or more certificates in PEM format. All certificates in the file will be added to the PKCS#7 structure. This option can be used more than once to read certificates form multiple files.

-nocrl

  normally a CRL is included in the output file. With this option no CRL is included in the output file and a CRL is not read from the input file.

# EXAMPLES

Create a PKCS#7 structure from a certificate and CRL:

     openssl crl2pkcs7 -in crl.pem -certfile cert.pem -out p7.pem

Creates a PKCS#7 structure in DER format with no CRL from several different certificates:

     openssl crl2pkcs7 -nocrl -certfile newcert.pem
            -certfile demoCA/cacert.pem -outform DER -out p7.der

# NOTES

The output file is a PKCS#7 signed data structure containing no signers and just certificates and an optional CRL.

This utility can be used to send certificates and CAs to Netscape as part of the certificate enrollment process. This involves sending the DER encoded output as MIME type application/x-x509-user-cert.

The PEM encoded form with the header and footer lines removed can be used to install user certificates and CAs in MSIE using the Xenroll control.

# SEE ALSO

pkcs7